**ITB18/1690-Technical Responsiveness Table**

**Bidders shall provide all the applicable data of the equipment offered, failing to do so may result in the bid being rejected. Corresponding documentation shall form part of the bidder’s offer.**

**LOT #1**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Item Description** | **Specifications** | **√****Yes** | **√****No** | **Technical Compliance** **Please provide details /description of offered feature)**  |
| **1** | **Waste Disposal Truck** |  |  |  |
| Condition | Brand New, year of production 2016 or later |  |  |  |
| Dimensions (± 5%) | Length, mm: max. 6500Width, mm: max. 2600Height, mm: max. 3200 |  |  |  |
| Total vehicle weight, kg, (± 5%) | max. 8,500 |  |  |  |
| Fuel | Diesel |  |  |  |
| Engine Horsepower HP, (± 5%) | min. 125  |  |  |  |
| European emission standards | Min. “Euro 3”  |  |  |  |
| Steering | Steering mechanism with the hydraulic booster |  |  |  |
| Standard equipment | Spare wheel. First aid kit. Emergency triangle and lantern, lifting jack. The bracket for the installation of fire extinguishers. Set of tools. |  |  |  |
| Warranty | 12 months |  |  |  |
| Technical specifications of the waste container |  |  |  |
| Loading type  | Back loading;1. Automatic loading:Small dustbins – minimum 120 litters; (euro-standard)Big dustbins - minimum 750 litters; (euro-standard)OR2. Manual loading  |  |  |  |
| Capacity of load container, m**3**, (± 10%) | 7,5 |  |  |  |
| Lifting capacity of manipulating arm, kg | Min. 600 (in case of manual loading) |  |  |  |
| Compaction ratio | 1,5 – 4 (depending on the density of the load) |  |  |  |
| Mass of loaded waste, kg | min. 3000  |  |  |  |

**LOT #2**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Item Description** | **Specifications** | **√****Yes** | **√****No** | **Technical Compliance** **Please provide details /description of offered feature)**  |
| **1** | **Waste Disposal Truck** |  |  |  |
| Condition | Brand New, year of production 2016 or later |  |  |  |
| Dimensions (± 5%) | Length, mm: max. 7500Width, mm: max. 2600Height, mm: max. 3500 |  |  |  |
| Total vehicle weight, kg (± 5%) | max. 13500 |  |  |  |
| Fuel | Diesel |  |  |  |
| Engine Horsepower HP, (± 5%) | min. 155 |  |  |  |
| European emission standards | Min. “Euro 3”  |  |  |  |
| Steering | Steering mechanism with the hydraulic booster |  |  |  |
| Standard equipment | Spare wheel. First aid kit. Emergency triangle and lantern, lifting jack. The bracket for the installation of fire extinguishers. Set of tools. |  |  |  |
| Warranty | 12 months |  |  |  |
| Technical specifications of the waste container |  |  |  |
| Loading type  | Back loading  |  |  |  |
| Capacity of load container, m**3**, (± 10%) | 10 |  |  |  |
| Mass of loaded waste, kg | min. 4000  |  |  |  |
| Types of loadable dustbins, liters (euro-standards) | Small dustbins – minimum 120 litters;Big dustbins - minimum 750 litters; |  |  |  |
| Additional options | Footboards and handles for operators |  |  |  |

**LOT #3**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Item Description** | **Specifications** | **√****Yes** | **√****No** | **Technical Compliance** **Please provide details /description of offered feature)**  |
| **1** | **Waste Disposal Truck** |  |  |  |
| Condition | Brand New, year of production 2016 or later |  |  |  |
| Dimensions (± 5%) | Length, mm: max. 8500Width, mm: max. 2600Height, mm: max. 3800 |  |  |  |
| Total vehicle weight, kg (± 5%) | max. 19500 |  |  |  |
| Fuel | Diesel |  |  |  |
| Engine Horsepower HP, (± 5%) | min. 155 |  |  |  |
| European emission standards | Min. “Euro 3”  |  |  |  |
| Steering | Steering mechanism with the hydraulic booster |  |  |  |
| Standard equipment | Spare wheel. First aid kit. Emergency triangle and lantern, lifting jack. The bracket for the installation of fire extinguishers. Set of tools. |  |  |  |
| Warranty | 12 months |  |  |  |
| Technical specifications of the waste container |  |  |  |
| Loading type  | Back loading  |  |  |  |
| Capacity of load container, m**3**, (± 10%) | 16 |  |  |  |
| Mass of loaded waste, kg | min. 7000  |  |  |  |
| Types of loadable dustbins, liters (euro-standards) | Small dustbins – minimum 120 litters;Big dustbins - minimum 750 litters; |  |  |  |
| Additional options | Footboards and handles for operators |  |  |  |