Annex 1

 **Technical Specifications**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Items to be Supplied\*** | **Quantity** | **UoM** | **Description / Specifications of Goods**  | **Latest Delivery Date**  |
|  | **500** | **Piece** | **Safety/Protective helmet****Materials: PVC or ABS resin; with mount for earmuffs****inner 6-8 point suspension space 30mm (1.2 inch) between the helmet shell and the head;****Standard ANSI Z89.1 or EN397** |  |
|  | **500** | **Piece** | **Safety Glasses****Materials: Polycarbonate;** **eye coverage with side shield, anti-fog and anti-scratch coatings;** **Flexible fitting frames****Standard ANSI Z87.1-2010** |  |
|  | **500** | **Piece** | **Respiratory mask****Disposable, Filter class N95, NIOSH approved;** **Type AS/NZS 1715 for organic vapor, fumes, thinner;** **Class P1 or P2 dust mask standard** |  |
|  | **10** | **Piece** | **Earmuffs****Reusable, cap-mounted;** **Materials: molded plastic, with soft ear cushion;****Noise Reduction Rating (NRR) 30 dB** |  |
|  | **2500** | **Pair** | **Gloves, Construction****'Materials: Soft leather hand gloves for Construction works;****Full Palm leather front and back; Safety rubberizes cuff for wrist protection;****Sizes: 8”, 11”, 14”, 16”, 18”** |  |
|  | **2500** | **Pair** | **Gloves, Chemical waste, disposable****Materials: Standard EN374 Nitrile for Chemical waste and Hazardous materials;****Sizes: 8”, 11”, 14”, 16”, 18”** |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **1000** | **piece** | **Work clothing** **Type: Overalls;** **Materials: cotton, polyester;** **Elasticated waist; Adjustable braces; 6 pockets** |  |
|  | **1000** | **Piece** | **Work vest****Materials: polyester;****High visibility with reflective bands; 2 pockets;** |  |
|  | **500** | **Pair** | **Boots****Materials: Nitrile rubber;** **anti-abrasion, anti-cut, oil-resistant, chemical-resistant** |  |
|  | **50** | **Piece** | **Long /surveyor's tape****Minimum 100 ft / 30 m blade long, 3/4" blade width;****Measurement scale in Metric, SAE, decimal foot****Materials: ABS case, stainless steel crank arm, fiberglass blade;****with automatic blade retract and stopper** |  |
|  | **50** | **Piece** | **Measuring tape****26 ft / 8 m blade long, 1/2 to 3/4" blade width;****Measurement scale in Metric, SAE, decimal foot****Materials: Metal/ABS case, fiberglass blade;****with automatic blade retract and stopper** |  |
|  | **50** | **Piece** | **Levels****3 vials magnetic I-Beam type;** **Materials: high impact ABS** |  |
|  | **50** | **Roll** | **String****Minimum 500 ft with reel;** **Materials: nylon** |  |
|  | **50** | **Piece** | **Pinch point / digging bar, 60"****Heavy duty design;****Materials: drop forged steel with enamel finishes** |  |
|  | **50** | **Piece** | **Long straight alignment pry bar, 30"****7/8" diameter;** **Materials: forged high carbon steel, enamel finishes** |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **50** | **Piece** | **Wrecking / pry / crow bar, 42"****Materials: forged high carbon steel, enamel finishes** |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **50** | **Piece** | **Wrecking / pry / crow bar, 24"****Materials: forged high carbon steel, enamel finishes** |  |
|  | **50** | **piece** | **Flat bar, half round 15"****Materials: forged high carbon steel, enamel finishes** |  |
|  | **50** | **Piece** | **Nail puller / claw****Size 10"** **Materials: forged, heat treated, tempered steel, enamel finishes** |  |
|  | **50** | **Set** | **Cold chisel****kit of minimum 3 pieces: 5/16", 5/8", and 3/4" cut sizes;** **Materials: forged, heat treated, tempered steel, enamel finishes** |  |
|  | **50** | **Piece** | **Hammer, claw****20 oz / 0.6 kg weight; 1 piece forged steel head and handle;****fiberglass-jacketed handle with ribbed grip** |  |
|  | **50** | **Piece** | **Hammer, blacksmith****64 oz / 1.8 kg weight;** **Materials: forged, heat treated, tempered steel head;** **fiberglass-jacketed handle with ribbed grip** |  |
|  | **50** | **Piece** | **Hammer, sledge****12 lbs / 5.5 kg weight;****Materials: forged, heat treated, tempered steel head;** **fiberglass-jacketed handle with ribbed grip** |  |
|  | **50** | **Piece** | **Concrete mesh cutter, 24"****Materials: Blades - chrome vanadium steel, forged, Handle - steel tube with comfort grip;****Cutting-edge hardness up to 48 HRC** |  |
|  | **50** | **Nos** | **Wheelbarrow****Materials: Tray - heavy-duty steel, Handle - steel tubes with comfort grip;****Load capacity: 6 cu. ft.****Dimensions: approx. 25 in. W x 58 in. D x 27 in. H** |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **50** | **set** | **Hacksaw****Approx. 10" standard, adjustable blade w/ wingnut;** **Materials: heavy-duty steel bar frame;** |  |
|  | **50** | **Piece** | **Shovel, digging, round point****approx. 26" length; with D-handle****Materials: tempered steel blade, hardwood handle** |  |
|  | **50** | **piece** | **Shovel, trenching spade****approx. 46" length;****Materials: tempered steel blade, hardwood handle** |  |
|  | **50** | **Piece** | **Shovel, square point****approx. 26" length; with D-handle****Materials: tempered steel blade, hardwood handle** |  |
|  | **50** | **Pieceset** | **Hoe****Blade / head dimension approx. 8"x8.5"; length approx. 40"****Materials: tempered steel head** |  |
|  | **50** | **Piece** | **Mutt****Blade / head dimension approx. 8"x4", length approx. 64"** **Materials: tempered steel head** |  |
|  | **50** | **Piece** | **Pick****Approx. weight 6 lbs / 2.7 kg; approx. length with handle 36"****Materials: tempered steel blade/tip, enamel coated, hardwood handle** |  |
|  | **50** | **Piece** | **Mattock****Approx. weight 6 lbs / 2.7 kg; approx. length with handle 36"****Materials: tempered steel blade/tip, enamel coated, hardwood handle** |  |
|  | 50 | **Piece** | **Rake****5-16 tine; approx 60" length****Materials: tempered steel head, hardwood handle** |  |
|  |  | **Piece** | **Machette****Approx 18"-22" length;****Materials: Blade - Carbon spring steel blade, Handle - wooden/plastic;** |  |
|  | **50** | **Piece** | **Axe, single tip****Approx. 38" length, 3.5 lbs / 1.6 kg weight;****Materials: drop-forged, heat treated steel head, hardwood handle** |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **50** | **Piece** | **Hatchet, single tip****'Approx. 12" length, 1.5 lbs / 0.7 kg weight;****Materials: drop-forged, heat treated steel head, hardwood handle** |  |
|  | **50** | **Piece** | **Utility knife / cutter****with retractable blades;****Dimension: approx 6" length** |  |
|  | **250** | **Piece** | **Bucket****Materials: plastic-rubber;** **Cap. 5L** |  |
|  | **50** | **Piece** | **Trowel, mason's / bricklayer's****Approx. blade size 10"x4-3/4";** **Materials: steel blade, wooden/plastic handle** |  |
|  | **50** | **Piece** | **Trowel, gauging****Approx. blade size 10"x4-3/4";** **Materials: steel blade, wooden/plastic handle** |  |
|  | **50** | **Piece** | **Trowel, margin****Approx. blade size 8"x2";** **Materials: steel blade, wooden/plastic handle** |  |
|  | **50** | **Piece** | **Trowel, pool****Approx. blade size 16"x4";** **Materials: steel blade, wooden/plastic handle** |  |
|  | **50** | **Piece** | **Trowel, concrete finishing****Approx. blade size 16"x4";** **Materials: steel blade, wooden/plastic handle** |  |
|  | **50** | **Piece** | **Rebar cutter and bender****Approx. 52" length;** **Materials: hardened steel alloy;****cuts and bends to 90 and 180 degrees;****max. cap. 5/8", hardness 60** |  |
|  | **50** | **piece** | **Handsaw, crosscut****approx. 24" length x 9 tooth per inch;****Hardened and tempered polished steel blade, wooden/plastic handle** |  |
|  | **20** | **Set** | **Hand/manual drill****keyless chuck for up to 1/4" bits;** **Materials: Metal and wood construction;** **package including drill bits** |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **20** | **Piece** | **Wood chisel****with grip;** **Materials: Hardened, tempered high-chrome carbon alloy steel blade;** **minimum set of 6, tip sizes 1/4", 1/2", 3/4", 1", 1-1/4", 1-1/2".** |  |
|  | **20** | **Set** | **Wooden plane, block****Approx. up to 6" length, with 1-3/8" blade width;****Materials: hardwood** |  |
|  | **20** | **set** | **Wooden plane, smoothing****Approx. up to 11" length, with 2" blade width;****Materials: hardwood** |  |
|  | **20** | **Set** | **Screwdriver set****6-piece set, 1/8", 3/16", 1/4" slotted head, #0, #1, #2 philips head;****Materials: chrome-vanadium steel** |  |
|  | **20** | **Piece** | **Plier, linesman****Approx. 8" length; insulated, slip resistant handle;****Materials: drop forged chrome-vanadium steel;****Meets ANSI specifications** |  |
|  | **20** | **Piece** | **Plier, long-nose****Approx. 8" length; insulated, slip resistant handle;****Materials: drop forged chrome-vanadium steel;****Meets ANSI specifications** |  |
|  | **20** | **Piece** | **Plier, diagonal/side cutting****Approx. 8" length; insulated, slip resistant handle;****Materials: drop forged chrome-vanadium steel;****Meets ANSI specifications** |  |
|  | **20** | **Piece** | **Plier, slip joint****Approx. 8" length; insulated, slip resistant handle;****Materials: drop forged chrome-vanadium steel;****Meets ANSI specifications** |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **20** | **Piece** | **Plier, groove joint****Approx. 12" length; insulated, slip resistant handle;****Materials: drop forged chrome-vanadium steel;****Meets ANSI specifications** |  |
|  | **20** | **Piece** | **Wire Cutter and Stripper****Approx. 7"length; insulated, slip resistant handle;****Jacket/wire cap: 10-18 AWG Solid and 12-20 AWG Stranded** |  |
|  | **20** | **Piece** | **Voltage tester/detector****with led indicator; detection 50 -1000 V AC 50-60Hz;****Materials: heavy-duty polycarbonate plastic resins; Class B FCC rules;****Dimension: approx. length 5"** |  |
|  | **20** | **Set** | **Adjustable wrench, set****6"and 10"length; slip resistant handle;****Materials: drop-forged chrome vanadium steel** |  |
|  | **20** | **Set** | **Wrench, rachet SAE sockets, set****minimum set of 13 SAE socket (inch): 1/4, 5/16, 3/8, 7/16, 1/2, 9/16, 5/8, 11/16, 3/4, 13/16, 7/8, 15/16, and 1 in.;****Materials: drop forged chrome-vanadium steel;****Package including storage rack/bag/box** |  |
|  | **20** | **set** | **Wrench, rachet Metric sockets, set****minimum set of 15 Metric socket (mm): 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22****Materials: drop forged chrome-vanadium steel;****Package including storage rack/bag/box** |  |
|  | **20** | **Set** | **Wrench, deep socket, set****minimum set of 3/8, 1/4, and 1/2 in. drives, with flex handles and extensions; minimum 30 combination of SAE and Metric sockets;****Materials: drop forged chrome-vanadium steel;****Package including storage rack/bag/box** |  |
|  | **20** | **Piece** | **Wrench, pipe****Approx. 24" length;****Materials: steel jaw, iron-cast handle** |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **20**  | **Piece** | **Plier, self-adjusting pipe clamping****Approx. 10"length;****Materials: steel alloy** |  |
|  | **20** | **Set** | **Hacksaw, mini, for PVC****Approx. 6" frame and blades;****Materials: steel alloy frame, carbon steel blade** |  |
|  | **20** | **Piece** | **PVC and Tube Cutter****Materials: heavy duty aluminium;****Cutting capacity up to 1-1/4"PVC, CPVC, PEX, PE, PB and rubber hose** |  |



Annex 2

**FORM FOR SUBMITTING SUPPLIER’S QUOTATION[[1]](#footnote-1)**

***(This Form must be submitted only using the Supplier’s Official Letterhead/Stationery[[2]](#footnote-2))***

We, the undersigned, hereby accept in full the UNDP General Terms and Conditions, and hereby offer to supply the items listed below in conformity with the specification and requirements of UNDP as per RFQ Reference No. \_\_\_\_\_\_\_:

**TABLE 1 : Offer to Supply Goods Compliant with Technical Specifications and Requirements**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **No.** | **QTY** | **UoM** | **Description / Specifications of Goods**  | **Latest Delivery Date**  | **Latest Delivery Date** | **Unit Price (IDR)** | **Total Price per Item****(IDR)** |
|  | **500** | **Piece** | **Safety/Protective helmet****Materials: PVC or ABS resin; with mount for earmuffs****inner 6-8 point suspension space 30mm (1.2 inch) between the helmet shell and the head;****Standard ANSI Z89.1 or EN397** |  |  |  |  |
|  | **500** | **Piece** | **Safety Glasses****Materials: Polycarbonate;** **eye coverage with side shield, anti-fog and anti-scratch coatings;** **Flexible fitting frames****Standard ANSI Z87.1-2010** |  |  |  |  |
|  | **500** | **Piece** | **Respiratory mask****Disposable, Filter class N95, NIOSH approved;** **Type AS/NZS 1715 for organic vapor, fumes, thinner;** **Class P1 or P2 dust mask standard** |  |  |  |  |
|  | **10** | **Piece** | **Earmuffs****Reusable, cap-mounted;** **Materials: molded plastic, with soft ear cushion;****Noise Reduction Rating (NRR) 30 dB** |  |  |  |  |
|  | **2500** | **Pair** | **Gloves, Construction****'Materials: Soft leather hand gloves for Construction works;****Full Palm leather front and back; Safety rubberizes cuff for wrist protection;****Sizes: 8”, 11”, 14”, 16”, 18”** |  |  |  |  |
|  | **2500** | **Pair** | **Gloves, Chemical waste, disposable****Materials: Standard EN374 Nitrile for Chemical waste and Hazardous materials;****Sizes: 8”, 11”, 14”, 16”, 18”** |  |  |  |  |
|  | **1000** | **Piece** | **Work clothing** **Type: Overalls;** **Materials: cotton, polyester;** **Elasticated waist; Adjustable braces; 6 pockets** |  |  |  |  |
|  | **1000** | **Piece** | **Work vest****Materials: polyester;****High visibility with reflective bands; 2 pockets;** |  |  |  |  |
|  | **500** | **Pair** | **Boots****Materials: Nitrile rubber;** **anti-abrasion, anti-cut, oil-resistant, chemical-resistant** |  |  |  |  |
|  | **50** | **Piece** | **Long /surveyor's tape****Minimum 100 ft / 30 m blade long, 3/4" blade width;****Measurement scale in Metric, SAE, decimal foot****Materials: ABS case, stainless steel crank arm, fiberglass blade;****with automatic blade retract and stopper** |  |  |  |  |
|  | **50** | **Piece** | **Measuring tape****26 ft / 8 m blade long, 1/2 to 3/4" blade width;****Measurement scale in Metric, SAE, decimal foot****Materials: Metal/ABS case, fiberglass blade;****with automatic blade retract and stopper** |  |  |  |  |
|  | **50** | **Piece** | **Levels****3 vials magnetic I-Beam type;** **Materials: high impact ABS** |  |  |  |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | **50** | **roll** | **String****Minimum 500 ft with reel;** **Materials: nylon** |  |  |  |  |
|  | **50** | **Piece** | **Pinch point / digging bar, 60"****Heavy duty design;****Materials: drop forged steel with enamel finishes** |  |  |  |  |
|  | **50** | **Piece** | **Long straight alignment pry bar, 30"****7/8" diameter;** **Materials: forged high carbon steel, enamel finishes** |  |  |  |  |
|  | **50** | **Piece** | **Wrecking / pry / crow bar, 42"****Materials: forged high carbon steel, enamel finishes** |  |  |  |  |
|  | **50** | **Piece** | **Wrecking / pry / crow bar, 24"****Materials: forged high carbon steel, enamel finishes** |  |  |  |  |
|  | **50** | **Piece** | **Flat bar, half round 15"****Materials: forged high carbon steel, enamel finishes** |  |  |  |  |
|  | **50** | **Piece** | **Nail puller / claw****Size 10"** **Materials: forged, heat treated, tempered steel, enamel finishes** |  |  |  |  |
|  | **50** | **Set**  | **Cold chisel****kit of minimum 3 pieces: 5/16", 5/8", and 3/4" cut sizes;** **Materials: forged, heat treated, tempered steel, enamel finishes** |  |  |  |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | **50** | **piece** | **Hammer, claw****20 oz / 0.6 kg weight; 1 piece forged steel head and handle;****fiberglass-jacketed handle with ribbed grip** |  |  |  |  |
|  | **50** | **Piece** | **Hammer, blacksmith****64 oz / 1.8 kg weight;** **Materials: forged, heat treated, tempered steel head;** **fiberglass-jacketed handle with ribbed grip** |  |  |  |  |
|  | **50** | **Piece** | **Hammer, sledge****12 lbs / 5.5 kg weight;****Materials: forged, heat treated, tempered steel head;** **fiberglass-jacketed handle with ribbed grip** |  |  |  |  |
|  | **50** | **piece** | **Concrete mesh cutter, 24"****Materials: Blades - chrome vanadium steel, forged, Handle - steel tube with comfort grip;****Cutting-edge hardness up to 48 HRC** |  |  |  |  |
|  | **50** | **Nos** | **Wheelbarrow****Materials: Tray - heavy-duty steel, Handle - steel tubes with comfort grip;****Load capacity: 6 cu. ft.****Dimensions: approx. 25 in. W x 58 in. D x 27 in. H** |  |  |  |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | **50** | **set** | **Hacksaw****Approx. 10" standard, adjustable blade w/ wingnut;** **Materials: heavy-duty steel bar frame;** |  |  |  |  |
|  | **50** | **Piece** | **Shovel, digging, round point****approx. 26" length; with D-handle****Materials: tempered steel blade, hardwood handle** |  |  |  |  |
|  | **50** | **Piece** | **Shovel, trenching spade****approx. 46" length;****Materials: tempered steel blade, hardwood handle** |  |  |  |  |
|  | **50** | **Piece** | **Shovel, square point****approx. 26" length; with D-handle****Materials: tempered steel blade, hardwood handle** |  |  |  |  |
|  | **50** | **Piece** | **Hoe****Blade / head dimension approx. 8"x8.5"; length approx. 40"****Materials: tempered steel head** |  |  |  |  |
|  | **50** | **Piece** | **Mutt****Blade / head dimension approx. 8"x4", length approx. 64"** **Materials: tempered steel head** |  |  |  |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | **50** | **piece** | **Pick****Approx. weight 6 lbs / 2.7 kg; approx. length with handle 36"****Materials: tempered steel blade/tip, enamel coated, hardwood handle** |  |  |  |  |
|  | **50** | **piece** | **Mattock****Approx. weight 6 lbs / 2.7 kg; approx. length with handle 36"****Materials: tempered steel blade/tip, enamel coated, hardwood handle** |  |  |  |  |
|  | 50 | **Piece** | **Rake****5-16 tine; approx 60" length****Materials: tempered steel head, hardwood handle** |  |  |  |  |
|  |  | **Piece** | **Machette****Approx 18"-22" length;****Materials: Blade - Carbon spring steel blade, Handle - wooden/plastic;** |  |  |  |  |
|  | **50** | **piece** | **Axe, single tip****Approx. 38" length, 3.5 lbs / 1.6 kg weight;****Materials: drop-forged, heat treated steel head, hardwood handle** |  |  |  |  |
|  | **50** | **piece** | **Hatchet, single tip****'Approx. 12" length, 1.5 lbs / 0.7 kg weight;****Materials: drop-forged, heat treated steel head, hardwood handle** |  |  |  |  |
|  | **50** | **Piece** | **Utility knife / cutter****with retractable blades;****Dimension: approx 6" length** |  |  |  |  |
|  | **250** | **piece** | **Bucket****Materials: plastic-rubber;** **Cap. 5L** |  |  |  |  |
|  | **50** | **piece** | **Trowel, mason's / bricklayer's****Approx. blade size 10"x4-3/4";** **Materials: steel blade, wooden/plastic handle** |  |  |  |  |
|  | **50** | **Piece** | **Trowel, gauging****Approx. blade size 10"x4-3/4";** **Materials: steel blade, wooden/plastic handle** |  |  |  |  |
|  | **50** | **Piece** | **Trowel, margin****Approx. blade size 8"x2";** **Materials: steel blade, wooden/plastic handle** |  |  |  |  |
|  | **50** | **Piece** | **Trowel, pool****Approx. blade size 16"x4";** **Materials: steel blade, wooden/plastic handle** |  |  |  |  |
|  | **50** | **Piece** | **Trowel, concrete finishing****Approx. blade size 16"x4";** **Materials: steel blade, wooden/plastic handle** |  |  |  |  |
|  | **50** | **Piece** | **Rebar cutter and bender****Approx. 52" length;** **Materials: hardened steel alloy;****cuts and bends to 90 and 180 degrees;****max. cap. 5/8", hardness 60** |  |  |  |  |
|  | **50** | **piece** | **Handsaw, crosscut****approx. 24" length x 9 tooth per inch;****Hardened and tempered polished steel blade, wooden/plastic handle** |  |  |  |  |
|  | **20** | **Set** | **Hand/manual drill****keyless chuck for up to 1/4" bits;** **Materials: Metal and wood construction;** **package including drill bits** |  |  |  |  |
|  | **20** | **Piece** | **Wood chisel****with grip;** **Materials: Hardened, tempered high-chrome carbon alloy steel blade;** **minimum set of 6, tip sizes 1/4", 1/2", 3/4", 1", 1-1/4", 1-1/2".** |  |  |  |  |
|  | **20** | **Set** | **Wooden plane, block****Approx. up to 6" length, with 1-3/8" blade width;****Materials: hardwood** |  |  |  |  |
|  | **20** | **Set** | **Wooden plane, smoothing****Approx. up to 11" length, with 2" blade width;****Materials: hardwood** |  |  |  |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | **20** | **set** | **Screwdriver set****6-piece set, 1/8", 3/16", 1/4" slotted head, #0, #1, #2 philips head;****Materials: chrome-vanadium steel** |  |  |  |  |
|  | **20** | **piece** | **Plier, linesman****Approx. 8" length; insulated, slip resistant handle;****Materials: drop forged chrome-vanadium steel;****Meets ANSI specifications** |  |  |  |  |
|  | **20** | **Piece** | **Plier, long-nose****Approx. 8" length; insulated, slip resistant handle;****Materials: drop forged chrome-vanadium steel;****Meets ANSI specifications** |  |  |  |  |
|  | **20** | **Piece** | **Plier, diagonal/side cutting****Approx. 8" length; insulated, slip resistant handle;****Materials: drop forged chrome-vanadium steel;****Meets ANSI specifications** |  |  |  |  |
|  | **20** | **Piece** | **Plier, slip joint****Approx. 8" length; insulated, slip resistant handle;****Materials: drop forged chrome-vanadium steel;****Meets ANSI specifications** |  |  |  |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | **20** | **piece** | **Plier, groove joint****Approx. 12" length; insulated, slip resistant handle;****Materials: drop forged chrome-vanadium steel;****Meets ANSI specifications** |  |  |  |  |
|  | **20** | **piece** | **Wire Cutter and Stripper****Approx. 7"length; insulated, slip resistant handle;****Jacket/wire cap: 10-18 AWG Solid and 12-20 AWG Stranded** |  |  |  |  |
|  | **20** | **piece** | **Voltage tester/detector****with led indicator; detection 50 -1000 V AC 50-60Hz;****Materials: heavy-duty polycarbonate plastic resins; Class B FCC rules;****Dimension: approx. length 5"** |  |  |  |  |
|  | **20** | **Set** | **Adjustable wrench, set****6"and 10"length; slip resistant handle;****Materials: drop-forged chrome vanadium steel** |  |  |  |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | **20** | **Set** | **Wrench, rachet SAE sockets, set****minimum set of 13 SAE socket (inch): 1/4, 5/16, 3/8, 7/16, 1/2, 9/16, 5/8, 11/16, 3/4, 13/16, 7/8, 15/16, and 1 in.;****Materials: drop forged chrome-vanadium steel;****Package including storage rack/bag/box** |  |  |  |  |
|  | **20** | **set** | **Wrench, rachet Metric sockets, set****minimum set of 15 Metric socket (mm): 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22****Materials: drop forged chrome-vanadium steel;****Package including storage rack/bag/box** |  |  |  |  |
|  | **20** | **set** | **Wrench, deep socket, set****minimum set of 3/8, 1/4, and 1/2 in. drives, with flex handles and extensions; minimum 30 combination of SAE and Metric sockets;****Materials: drop forged chrome-vanadium steel;****Package including storage rack/bag/box** |  |  |  |  |
|  | **20** | **piece** | **Wrench, pipe****Approx. 24" length;****Materials: steel jaw, iron-cast handle** |  |  |  |  |
|  | **20** | **Piece** | **Plier, self-adjusting pipe clamping****Approx. 10"length;****Materials: steel alloy** |  |  |  |  |
|  | **20** | **set** | **Hacksaw, mini, for PVC****Approx. 6" frame and blades;****Materials: steel alloy frame, carbon steel blade** |  |  |  |  |
|  | **20** | **piece** | **PVC and Tube Cutter****Materials: heavy duty aluminium;****Cutting capacity up to 1-1/4"PVC, CPVC, PEX, PE, PB and rubber hose** |  |  |  |  |
|  | Total Prices of Goods  |  |
|  |  Add : Cost of Transportation  |  |
|  |  Add : Cost of Insurance |  |
|  |  Add : Other Charges (pls. specify) |  |
|  | **Total Final and All – Inclusive Price Quotation** |  |

**TABLE 2 : Estimated Operating Costs (if applicable)**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **List of Consumable Item/s** *(Include fast moving parts, if any)* | **Estimated Average Consumption**  | **Unit of Measure** | **Unit Price** | **Total Price per Item** |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

**TABLE 3 : Offer to Comply with Other Conditions and Related Requirements**

|  |  |
| --- | --- |
| **Other Information pertaining to our Quotation are as follows :** | **Your Responses** |
| ***Yes, we will comply*** | ***No, we cannot comply*** | ***If you cannot comply, pls. indicate counter proposal*** |
| Delivery Lead Time |  |  |  |
| Estimated weight/volume/dimension of the Consignment:  |   |  |  |
| Validity of Quotation |  |  |  |
| All Provisions of the UNDP General Terms and Conditions |  |  |  |
| Other requirements *[pls. specify]* |  |  |  |

All other information that we have not provided automatically implies our full compliance with the requirements, terms and conditions of the RFQ.

*[Name and Signature of the Supplier’s Authorized Person]*

*[Designation]*

*[Date]*

1. *This serves as a guide to the Supplier in preparing the quotation and price schedule.*  [↑](#footnote-ref-1)
2. *Official Letterhead/Stationery must indicate contact details – addresses, email, phone and fax numbers – for verification purposes*  [↑](#footnote-ref-2)