{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":7,"n_cols":4,"rows_kept":7,"cut":false,"hidden":false,"merged":[[0,0,0,3],[3,0,3,3],[5,0,5,3]]}
["Compliance Sheet (to be filled by the Bidders)                                                    "]
[]
["Item # in BOQ","Item","Required Specifications","Submitted Specifications by Bidders"]
["Second/ Mechanical Works      الاعمال الميكانيكية    "]
[1,"Supply, install, operate and test air-conditioning split unit of 4 ton capacity (cooling and heating)","The system shall consist of outdoor air-cooled condensing unit and indoor evaporating unit. Both indoor and outdoor units should be fitted with hydrophilic aluminum fins for improved performance. Unit pipes should be made of a newly shaped inner groove copper, which enables refrigerant to flow through more effectively, thus improving heat exchange efficiency and reducing power consumptions. \nAll suction and liquid lines that connect the two units should be properly covered. Wooder’s cover while the outside lines should be well weather protected should nicely hide inside lines. The  indoor unit should be compact, stylish design, high energy efficiency and whisper quiet operation. The unit should be reverse cycle type (cooling and heating) with active carbon and dust filter. The condensing unit should be quiet operation, compact, pre-charged copper pipe kits and with anti rust cabinet made from electrolytic zinc steel sheet and anti-rust coated components.\nSplit unit should be designed for a high temperature performance and the numbers and capacities are presented in the bill of quantity while the installation locations and specifications are presented as shown on the drawings. Electrical heat suction shall be installed in the unit and served by the same power source as the rest of the unit. Only one power feed shall be required for the unit\n\n"]
["Third/ Electrical Works      الاعمال الكهربائية"]
[12,"Supply, install, operate and test electrical generator of 1000 kVA capacity 50Hz，380V- 400V, 3 Phase 1500 RPM","Reffer to Annex A"]