{"text_format":"2","workbook":"xlsx","n_sheets":21,"sheets":["SUMMARY","BOQ#1","BOQ#2","BOQ#3","BOQ#4","BOQ#5","BOQ#6","BOQ#7","BOQ#8","BOQ#9","BOQ#10","BOQ#11","BOQ#12","BOQ#13","BOQ#14","BOQ#15","BOQ#16","BOQ#17","BOQ#18","BOQ#19","BOQ#20"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"SUMMARY","index":0,"n_rows":22,"n_cols":2,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["NAME OF SCHOOL PROJECT","TOTAL COST US$"]
["BOQ#1-Renovation of Al-Moalem for Boys School"]
["BOQ#2-Renovation of Almutamayizin and Allmutamizat School"]
["BOQ#3-Renovation of Alrafidan for Girls Secondary School"]
["BOQ#4-Renovation of Al-Taghllubia for Boys School"]
["BOQ#5-Renovation of Al-Zawra Primary mixed School"]
["BOQ#6-Renovation of Ashur Banibal Alrayania for boys School"]
["BOQ#7-Renovation of Qarqoush First Alkindergarten"]
["BOQ#8-Renovation of Qarqoush for Boys Secondary School"]
["BOQ#9-Renovation of Qarqoush for Girls Secondary School"]
["BOQ#10-Renovation of Rasen Primary Mixed School"]
["BOQ#11-Qaraqush (2) Kindergarten"]
["BOQ#12-Renovation of Ashor Panepal School for Boys & Girls"]
["BOQ#13-Renovation of Ashur High School for Boys"]
["BOQ#14-Renovation of Bagdeda Intermediate School for Boys"]
["BOQ#15-Renovation of Mareem AL-Adhraa High School"]
["BOQ#16-Renovation of Najd Primary School for Boys"]
["BOQ#17-Renovation of Qaraqush High School for Boys"]
["BOQ#18-Renovation of Sanharib Industrial High School for Girls"]
["BOQ#19-Renovation of Store for Education Directorate Hamdanyiah"]
["BOQ#20-Renovation of Ur for Boys"]
["GRAND TOTAL"]

{"sheet":"BOQ#1","index":1,"n_rows":56,"n_cols":6,"rows_kept":56,"cut":false,"hidden":false,"merged":[[55,1,55,4],[0,0,0,5],[2,1,2,5],[3,1,3,5],[4,1,4,5],[24,0,25,0],[37,0,39,0]]}
["Renovation of Al-Moalem School for Boys & Girls - Alhamdain  Sub- District - Ninawa Governorate "]
[null,"General Specification "]
[null,"1- All the materials supplied by the contractor must be according to Iraq's standard Specifications"]
[null,"2- The contractor must provide samples , catalogues and specification of materials for testing and approval by the site engineer "]
[null,"3- Contractor must pay the cost for samples including any laboratory test required"]
[null,"4- The price of works includes all job requierements as per Iraq's standard specification."]
["#","Item Description","Unit","Qty","Price$","Total $"]
[null,"Civil Works"]
[1,"Site preparation:\nSupply of materials, tools, machineries and manpower for site preparation, by cleaning and removing all debris, rubble and dump it to locations approved by the local Authorities. ","LS",1]
[2,"Ceramic for walls:\nSupply of materials, tools and manpower to place a new ceramic 30x30 cm with cement morter. The price of works includes expantion joints (every 5m), the removal of old damaged ceramic and dumping of all debris to a site approved by local authorities, in case it is needed, as well as all needed works to complete the job.","m²",10]
[3,"Cement plastering:\nSupply materials, tools and manpower to repair wall cracks and to replace damaged cement plastering. The work includes removing the damaged cement plastering of external walls & fence, 25cm at each side of the crack, then filling the cracks with crack filler and cement mortar 1:3 and by using SBR at a rate of 200gr per m², including applying a layer of chicken wire on the area with  3 layers of cement plastering 1:3 mix ratio. Price of the work shall inlcude all requirements to complete  the job.","m2",30]
[4,"Gypsum plastering:\nSupply of all necessary materials, tools and manpower to remove the damaged gypsum plastering of internal walls & roofs and plastering with new gypsum plastering  in 2 layers minimum thickness 15mm.The work includes repairing of wall cracks by removing the damaged gypsum plastering 25cm at each side of the crack,then filling the cracks with cement morter 1:3 and using SBR at a rate of 200gr per m² , later putting a layer of plastic mesh on the area under the gypsum plastering. All needed works to complete the job, will be included within the price.","m2",420]
[5,"Main gate (2x2.6m):\nSupply materials , tools and manpower to install new main gate steel doors (2x2.6m), by using plate gauge16, steel frame of angel sheet dimensions 7.62x7.62 cm, 5mm thickness and steel pipe 40x40x1.5mm, including door handles, hinges and locks. Price of the work shall include painting of steel door with anti-rust and two coats of oil paints with all requirements to complete the job. See drawing nº 01","EA",1]
[6,"Wooden doors (1.0x2.1m):\nSupply of materials, tools and manpower to install wooden doors, dimensions 1.0x2.1m, including handles, lock , hinges and all accessories. Price of the work shall include, frame, painting two faces with oil paint and all requirements to complete the job. See drawing nº 02 ","EA",30]
[7,"Repair steel windows: \nSupply materials, tools and manpower to repair the damaged steel window, including anti-insects wire mesh.  Price of the work shall include hinges, handle and all requirements to complete the job.","EA",150]
[8,"Plastic painting works:\nSupply materials , tools and manpower to paint the external walls and fence with three-layer of silicon (water proof) painting . Price of the work shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",4000]
[9,"Emulsion painting works:\nSupply materials , tools and manpower to paint the interior walls with three-layer of emulsion painting . Price of the job shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",3000]
[10,"Oil Painting:\nSupply materials, tools and manpower to paint  steel doors, windows, and internal walls with a paint-stripe at 1.25m height, by using 3 layers of oil paint. Price of the work shall include all requirements to complete the job.","m²",750]
[11,"Expansion joints:\nSupply of materials, tools and manpower to inject expansion joints with foam and install aluminum plate 20 cm width, with rubber between the two pieces of plates and by using screws to fix. All needed works to complete the job, will be included within the price.","ml",15]
[12,"Suspended ceiling:\nSupply of materials, tools and manpower to install false ceiling 60x60 cm (Gypsum boards), by using necessary accessories Z, L, T sections, galvanized steel wire 2mm for fixing with the roof by screws. The price includes the removal of old damaged suspended ceiling, dumping of all debris to a site approved by local authorities, in case it is needed, as well as all needed works to complete the job.  See drawing nº 06","m²",190]
[13,"Crystal clear glass:\nSupply of materials, tools and manpower to remove the damaged glass and to install crysta clear glass 4 mm with with new paste, dumping of all debris to a site approved by local authorities, in case it is needed,  as well as all needed works to complete the job.","m²",150]
[14,"Flag pole : \nSupply materials , tools and man power to install Flag pole of  6 m high by using  2.5\" (64cm) pipe. Price of the work shall include anti rust and three layers oil painting and all  requirements  to complete the job.","EA",1]
[15,"Billboard:\nSupply materials, tools and man power to install the title of the school on  frame of size 3×1 m, with good quality LED printed sticker. The frame shall be made of square pipe section 4x4 cm. Price of the work shall  include all requirements to complete the job.","EA",1]
[16,"Class title board:\nSupply materials and manpower to install class title name made of plastic sheet size 15x25 cm, using screws to fix. Price of the work shall  include all requirements to complete the job.","EA",20]
[null,"Subtotal for Civil Works"]
[null,"Sanitary works"]
[1,"Water tank: \nSupply of materials , tools and manpower to install galvanized water tank of 1400 liters capacity with plate gauge 16 cylindrical shape supported by steel base made from 2 inch angle shape . Price of the work shall include connection of the inlet and outlet pipes, fittings, Valves, float valves, accessories and all requirements to complete the job. ","EA",6]
[2,"Drain pipes:\nSupply of materials, tools and manpower for removing damaged water drain pipes and for installing new galavnized steel pipes 3\" (76mm). Including all connections and needed accesories to fix on roof and walls. Price of the work shall  include all requirements to complete the job. See drawing nº 14","ml",30]
[3,"Galvanized iron water pipes:   \n Supply materials , tools and manpower  to inspect and repair the water network pipes (Hot & Cool) 1/2\" dia, 3/4\" dia, 1\" dia  and replace the damaged pipes. Price of the  work shall include all pipe fittings, connection works and all accessories and requirements to complete the job.","LS",1]
[4,"Ceramic lavatory pedestal:\nSupply of  materials, tools and manpower to install ceramic lavatory pedestal (1 sink), mixer taps, locks valves, mirror and all needed accessories with complete water connections. All needed works to complete the job, will be included within the price.","EA",4]
[5,"Mixer taps:\nSupply of materials, tools and manpower to install mixer taps, locks and all  needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",4]
[6,"Taps:\nSupply of all necessary materials, tools and manpower to connect chrome water taps 1/2\" or 3/4\" and to install water connections. All needed works to complete the job, will be included within the price.","EA",20]
[7,"Siphon:\nSupply of materials, tools and manpower to install siphon, locks valves and all needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",10]
[8,"Maintenance of sewerage pipes:\nSupply materials, machinary and manpower to clean the sewerage pipes net starting from the toilets groups, along manholes and the main septic tank. By using high pressure air/water to open the blockages in the network , and all requirements to complete a good work.","EA",1]
[9,"Manholes:                                                \nSupply  materials, tools and manpower to build  40x40 cm size  manholes, by using solid block of size (15x20x40)cm  with cement mortar(1: 3) mix ratio. The work includes cement plastering from inside and outside, with cover made of cast iron frame fixed with concrete slab of manhole and all requirements to complete good work . See drawing nº 04","EA",2]
[10,"Manholes covering:\nSupply of materials, tools and manpower for covering manholes, dimensions 80x115cm (jacker plate), by using steel frame fixed on the concrete slab. All needed works to complete the job, will be included within the price.","EA",1]
[11,"Water pump:\nSupply materials, tools and manpower to connect water pump (1hp), Q=3M³/Hrs., H=20m with, ball valve and all fitting and accessories for connection. The price of works includes all accessories needed, as well as all needed works to complete the job. See attached","EA",1]
[null,"Subtotal for Sanitary works "]
[null,"Electricals Works"]
[null,"Work includes replace the damaged wires with new suitable size , testing and operation"]
[1,"Socket Switch:Supplying materials , tools and manpower to install, connect and commissioning  of (220VAC/13A) socket switch using screws,using single core copper wire PVC insulated 1.0 kv grade  (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",180]
[2,"Light Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/6A) (single , double , triple and quadruple) light switches using screws,using single core copper wire (2*2.5mm2) 1.0 kV grade PVC insulated  installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",120]
[3,"Fluorescent Lighting:                \nSupplying materials, tools and manpower, to install, connect and commissioning Simple Fluorescent Lighting Fixture 1x36 W, 4 feet, (metal frame, tube and starter), using single core copper wire (2*1.5mm2)  PVC insulated 1.0 kV grade installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",50]
[4,"Lighting:\nSupplying materials, tools and manpower, to install, connect and commissioning (220VAC/20Watt) economic light lamp with Lamp, using single core copper wire (2*1.5mm2) 1.0o kV grade PVC insulated installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",80]
[5,"Fan Regulator:\nSupplying materials, tools and manpower to install, connect and commissioning best quality of  Ceiling Fans Regulator with 5 speeds/ fan speed switch/ Regulator and  all requirements to complete a good work. ","EA",10]
[6,"Ceiling Fan:\nSupplying materials, tools and manpower to install, connect and commissioning best quality of 56\" ceiling fan with power regulator using copper cable (2*1.5mm) 1.0 kV PVC insulated installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",12]
[7,"Exhaust fan:\nSupplying materials, tools and manpower, to install, connect and commissioning of exhaust fan 6 inch (220VAC), using single core copper wire (2*1.5mm2) 1.0 kV grade PVC insulated  installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way switch (6A) with all accessories and requirement to implement the work entirely.","LS",18]
[8,"Electrical bell:                           \nSupplying materials, tools and manpower, to install, connect and commissioning of electrical bell (220VAC), using single core copper wire (2*1.5mm2) 1.0 kV grade PVC insulated installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using 1 Gang 2 Way Single Pole Push Switch (6A) with all accessories and requirement to implement the work entirely.","LS",2]
[9,"Main Board:\nProviding materials, installation and operation test of distribution board, enclosed metal frame made of iron sheet 1mm thickness painted with two layers of gray color oil paint free, arrange the items shown below properly, with door,  dimensions (height x width x depth: 80cm x 80 cm x 40cm), using rubber gaskets and equipped with the following items, Plastic trunck for wiring, and Bus bars 100A 4No with earth bus bar, the price also include the required, glands, screws, insulators, and etc, all items should be arranged properly, affords a high degree of safety operation,\n\nA - [(1 No.)  100A,  3Ph. 415 VAC,25 kV BC MCCB type].\nB - [(6 No.)  25A,  3Ph. 145 VAC MCB type].\nC - [(6 No.)  25A,  1Ph. 220 VAC MCB type].\nD - (1 No.)Voltmeter (0- 400 V) with selector switch.\nE - (1 Set)Ammeter (0 -100 A), 100/5A with required CTs.\nF - (1 No.)Hertz meter (48- 52 )Hz.\nG - (1 No.) selector switch.\nH - (3 No.) Indicator lamp 220VAC/5A.\nI - Three-phase Kilowatt-hour meter \nJ - (1Set)Copper Bus-Bar 100A., for lines and the half for the neutral and             earth, length for each one not less than (40)cm., with all accessories.","EA",1,null,{"$f":"E49*D49","v":0}]
[10,"Sub Distribution Boards:\nSupply, installation, testing and commissioning of factory fabricated distribution boards for light/power, concealed type made of M.S sheet 16 SWG degreased, derusted, zinc phosphated finished with electrostatic powder coating, of approved colour with hinged door, lockable handle, protection plate, basbar, earth and neutral strip, complete internally wired, flexible earthing strap for door manufactured by any one of the approved manufacturers as specified and comprising as under: Distribution board (3 Phase/400V/50Hz ) , equipped with TPN DB 12ways,  (DIN type, horizontal/vertical) metal single door complete with all accessories to accommodate incoming  (1x 3 pole MCB , 1 x 63 Amps, 415 volt A.C),  includes outgoing  SP MCB (3 x 10 Amps), (3 x 16 Amps), (2 x 20 Amps),  (2 x 25 Amps) , (2 x 32 Amps )  and Neutral tapping bar/strip on/in prefabricated  MS cubical control panel board including drilling holes, connections, fixing etc. with all accessories to complete work as required.","EA",4]
[11,"Electrical water boiler:\nSupply materials, tools and manpower to install, establish, connect, and commissioning electrical heater 250 Liter with complete fittings & accessories . The work includes  Power Cable size (3x4mm2) .flexible cable copper conductor,PVC insulation,1.0 kV grade unarmoured,best type  inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories) or using (Plastic Cable Duct PVC Trunking) extend form SDB  to the wter boiler system, with all accessories and requirement to implement the work entirely. See attached","LS",2]
[12,"wire:\nSupplying materials, tools and manpower to install 1.0 KV grade PVC insualted 2*1.5mm2 copper wire, work includes all  requirements to complete a good work. ","M",1000]
[13,"Water- cooler:\nSupplying materials , tools and manpower to install best quality stainless steel electrical water-cooler with three taps, water connections using screws,using single core copper wire (2*2.5mm2) PVC insulated 1.0 kV grade installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",1]
[14," Wall Mounted Split Unit Air-Conditioning:\nSupply, installaytion , connect and commissioning best quality  Split unit Air-conditioning (Cool & Heat) 2  ton.(24000btuh) ,  ambiant temperature -10 to 55° C  using  Power Cable size (2x4mm2) .flexible cable copper conductor,1.0 kV grade PVC insulation, unarmoured,best type lay on plastic cable chanal or fixed on the wall or (ceiling) by special plastic clamps extend form the main board   to the workshop, the cabls should connected by cable lugs with all requirements & connections in both sides with switch 45  Amp , the price include steel base, installing condensation pipe with all accessories and requirements to complete a good work.In addition to the guarantee and maintenance of the unit  for two years. See attached","LS",4]
[null,"Subtotal for Electricals Works"]
[null,"Total "]

{"sheet":"BOQ#2","index":2,"n_rows":51,"n_cols":6,"rows_kept":51,"cut":false,"hidden":false,"merged":[[49,0,50,0],[50,1,50,4],[0,0,0,5],[2,1,2,5],[3,1,3,5],[4,1,4,5],[24,0,25,0],[36,0,37,0]]}
["Renovation of Al-Mutamayizin & Al-Mutamizat  School- Al_Hamdain Sub- District - Ninawa Governorate "]
[null,"General Specification "]
[null,"1- All the materials supplied by the contractor must be according to Iraq's standard Specifications"]
[null,"2- The contractor must provide samples , catalogues and specification of materials for testing and approval by the site engineer "]
[null,"3- Contractor must pay the cost for samples including any laboratory test required"]
[null,"4- The price of works includes all job requierements as per Iraq's standard specification."]
["#","Item Description","Unit","Qty","Price$","Total $"]
[null,"Civil Works"]
[1,"Site preparation:\nSupply of materials, tools, machineries and manpower for site preparation, by cleaning and removing all debris, rubble and dump it to locations approved by the local Authorities. ","LS",1]
[2,"Cement plastering:\nSupply materials, tools and manpower to repair wall cracks and to replace damaged cement plastering. The work includes removing the damaged cement plastering of external walls & fence, 25cm at each side of the crack, then filling the cracks with crack filler and cement mortar 1:3 and by using SBR at a rate of 200gr per m², including applying a layer of chicken wire on the area with  3 layers of cement plastering 1:3 mix ratio. Price of the work shall inlcude all requirements to complete  the job.","m²",10]
[3,"Gypsum plastering:\nSupply of all necessary materials, tools and manpower to remove the damaged gypsum plastering of internal walls & roofs and plastering with new gypsum plastering  in 2 layers minimum thickness 15mm.The work includes repairing of wall cracks by removing the damaged gypsum plastering 25cm at each side of the crack,then filling the cracks with cement morter 1:3 and using SBR at a rate of 200gr per m² , later putting a layer of plastic mesh on the area under the gypsum plastering. All needed works to complete the job, will be included within the price.","m²",700]
[4,"Ceramic for walls:\nSupply of materials, tools and manpower to place a new ceramic 30x30 cm with cement morter. The price of works includes expantion joints, the removal of old damaged ceramic and dumping of all debris to a site approved by local authorities, in case it is needed, as well as all needed works to complete the job.","m²",200]
[5,"Main gate (4x2.6m):\nSupply materials , tools and manpower to install new main gate steel doors (4x2.6m),by using plate gauge16, steel frame of angel sheet dimensions 7.62x7.62 cm, 5mm thickness and steel pipe 40x40x1.5mm, including door handles, hinges and locks. Price of the work shall include painting of steel door with anti-rust and two coats of oil paints with all requirements to complete the job. See drawing nº 17","EA",2]
[6,"Wooden doors (1.0x2.1m):\nSupply of materials, tools and manpower to install wooden doors, dimensions 1.0x2.1m, including handles, lock , hinges and all accessories. Price of the work shall include, frame, painting two faces with oil paint and all requirements to complete the job. See drawing nº 02 ","EA",6]
[7,"Repair steel doors:\nSupply materials , tools , machineries and manpower to repair the damaged steel doors. Price of the work shall include handles, hinges ,oil paint ,accessories and all requirements to complete the job.","EA",20]
[8,"Repair steel windows: \nSupply materials, tools and manpower to repair the damaged steel window, including anti-insects wire mesh.  Price of the work shall include hinges, handle and all requirements to complete the job.","EA",20]
[9,"Plastic painting works:\nSupply materials , tools and manpower to paint the external walls and fence with three-layer of silicon (water proof) painting . Price of the work shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",3500]
[10,"Emulsion painting works:\nSupply materials , tools and manpower to paint the interior walls with three-layer of emulsion painting . Price of the job shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",3000]
[11,"Oil Painting:\nSupply materials, tools and manpower to paint  steel doors, windows, and internal walls with a paint-stripe at 1.25m height, by using 3 layers of oil paint. Price of the work shall include all requirements to complete the job.","m²",1000]
[12,"Suspended ceiling:\nSupplying material tools and manpower to install false ceiling 60x60 cm (Gypsum boards). The price includes fixing galvanized steel sections (H-sections-beams) , inverted T-section , fixing with galvanized steel bar (Ø5mm ), installing the form of a square to diamension (1.2x1.2m). The price of works includes the removal of old damaged false ceiling and work of spot lights, dumping of all debris to a site approved by local authorities, in case it is needed, as well as all needed works to complete the job.  See attached drawing nº 06","m²",200]
[13,"Crystal clear glass:\nSupply of materials, tools and manpower to remove the damaged glass and to install crysta clear glass 4 mm with with new paste, dumping of all debris to a site approved by local authorities, in case it is needed,  as well as all needed works to complete the job.","m²",50]
[14,"Flag pole : \nSupply materials , tools and man power to install Flag pole of  6 m high by using  2.5\" (64cm) pipe. Price of the work shall include anti rust and three layers oil painting and all  requirements  to complete the job.","EA",1]
[15,"Billboard:\nSupply materials, tools and man power to install the title of the school on  frame of size 3×1 m, with good quality LED printed sticker. The frame shall be made of square pipe section 4x4 cm. Price of the work shall  include all requirements to complete the job.","EA",2]
[16,"Class title board:\nSupply materials and manpower to install class title name made of plastic sheet size 15x25 cm, using screws to fix. Price of the work shall  include all requirements to complete the job.","EA",30]
[null,"Subtotal for Civil Works"]
[null,"Sanitary works"]
[1,"Water tank: \nSupply of materials , tools and manpower to install galvanized water tank of 1400 liters capacity with plate gauge 16 cylindrical shape supported by steel base made from 2 inch angle shape . Price of the work shall include connection of the inlet and outlet pipes, fittings, Valves, float valves, accessories and all requirements to complete the job. ","EA",8]
[2,"Galvanized iron water pipes:   \n Supply materials , tools and manpower  to inspect and repair the water network pipes (Hot & Cool) 1/2\" dia, 3/4\" dia, 1\" dia  and replace the damaged pipes. Price of the  work shall include all pipe fittings, connection works and all accessories and requirements to complete the job.","LS",1]
[3,"Taps:\nSupply of all necessary materials, tools and manpower to connect chrome water taps 1/2\" or 3/4\" and to install water connections. All needed works to complete the job, will be included within the price.","EA",10]
[4,"Siphon:\nSupply of materials, tools and manpower to install siphon, locks valves and all needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",6]
[5,"Maintenance of sewerage pipes:\nSupply materials, machinary and manpower to clean the sewerage pipes net starting from the toilets groups, along manholes and the main septic tank. By using high pressure air/water to open the blockages in the network , and all requirements to complete a good work.","LS",1]
[6,"Manholes:                                                \nSupply  materials, tools and manpower to build  40x40 cm size  manholes, by using solid block of size (15x20x40)cm  with cement mortar(1: 3) mix ratio. The work includes cement plastering from inside and outside, with cover made of cast iron frame fixed with concrete slab of manhole and all requirements to complete good work . See drawing nº 04","EA",2]
[7,"Mixer taps:\nSupply of materials, tools and manpower to install mixer taps, locks and all  accessories with complete water connections. The price of works shall include all needed works to complete the job.","EA",4]
[8,"Manholes covering:\nSupply of materials, tools and manpower for covering manholes, dimensions 80x115cm (jacker plate), by using steel frame fixed on the concrete slab. All needed works to complete the job, will be included within the price.","EA",2]
[9,"Water pump:\nSupply materials, tools and manpower to connect water pump (1hp), Q=3M³/Hrs., H=20m with, ball valve and all fitting and accessories for connection. The price of works includes all accessories needed, as well as all needed works to complete the job. See attached","EA",1]
[null,"Subtotal for Sanitary works "]
[null,"Electricals Works"]
[null,"Work includes replace the damaged wires with new suitable size , testing and operation"]
[1,"Socket Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/13A) socket switch using screws,using single core copper  wire (2*2.5mm2) 1.0 kV grade PVC insulated installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",80]
[2,"Light Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/6A) (single , double , triple and quadruple) light switches using screws,using single core copper wire (2*2.5mm2) PVC insulated 1.0 KV grade  installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",40]
[3,"Fluorescent Lighting:\nSupplying materials, tools and manpower, to install, connect and commissioning Simple Fluorescent Lighting Fixture 1x36 W, 4 feet, (metal frame, tube and starter), using single core copper wire (2*1.5mm2) 1.0 kV grade PVC insulated installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",80]
[4,"Lighting:\nSupplying materials, tools and manpower, to install, connect and commissioning (220VAC/20Watt) economic light lamp with Lamp, using single core copper wire (2*1.5mm2) PVC insulated 1.0 kV grade installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",30]
[5,"Fan Regulator: \nSupplying materials, tools and manpower to install, connect and commissioning best quality of  Ceiling Fans Regulator with 5 speeds/ fan speed switch/ Regulator and  all requirements to complete a good work. ","EA",10]
[6,"Ceiling Fan:\nSupplying materials, tools and manpower to install, connect and commissioning best quality of 56\" ceiling fan with power regulator using copper cable (2*1.5mm2) 1.0 kV grade PVC insulated installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",10]
[7,"Exhaust fan:\nSupplying materials, tools and manpower, to install, connect and commissioning of exhaust fan 6 inch (220VAC), using single core copper wire (2*1.5mm2) PVC insulated 1.0 kV grade installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way switch (6A) with all accessories and requirement to implement the work entirely.","LS",8]
[8,"Electrical bell:\nSupplying materials, tools and manpower, to install, connect and commissioning of electrical bell (220VAC), using single core  copper wire (2*1.5mm2) PVC inulated 1.0 kV grade  installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using 1 Gang 2 Way Single Pole Push Switch (6A) with all accessories and requirement to implement the work entirely.","LS",2]
[9,"Wire:\nSupplying materials, tools and manpower to install 2*1.5mm  copper wire, PVC insulated 1.0 kV grade work includes all  requirements to complete a good work. ","ml",800]
[10,"Wall Mounted Split Unit Air-Conditioning:\nSupply, installaytion , connect and commissioning best quality  Split unit Air-conditioning (Cool & Heat) 2  ton.(24000btuh) ,ambiant temperature -10 to 55° C  using  Power Cable size (2x4mm2) .flexible cable copper conductor,PVC insulation, unarmoured,best type lay on plastic cable chanal or fixed on the wall or (ceiling) by special plastic clamps extend form the main board   to the workshop, the cabls should connected by cable lugs with all requirements & connections in both sides with switch 45  Amp , the price include steel base, installing condensation pipe with all accessories and requirements to complete a good work.In addition to the guarantee and maintenance of the unit  for two years. See attached","LS",4]
[11,"Water- cooler:\nSupplying materials , tools and manpower to install best quality stainless steel electrical water-cooler with three taps, water connections using screws,using single core copper wire PVC insulated (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",1]
[null,"Subtotal for Electricals Works"]
[null,"Total "]

{"sheet":"BOQ#3","index":3,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[[51,0,52,0],[52,1,52,4],[0,0,0,5],[2,1,2,5],[3,1,3,5],[4,1,4,5],[5,1,5,5],[37,0,39,0]]}
["Renovation of Al-Rafidan for Girls Secondary - Alhamdain  Sub- District - Ninawa Governorate "]
[null,"General Specification "]
[null,"1- All the materials supplied by the contractor must be according to Iraq's standard Specifications"]
[null,"2- The contractor must provide samples , catalogues and specification of materials for testing and approval by the site engineer "]
[null,"3- Contractor must pay the cost for samples including any laboratory test required"]
[null,"4- The price of works includes all job requierements as per Iraq's standard specification."]
["#","Item Description","Unit","Qty","Price$","Total $"]
[null,"Civil Works"]
[1,"Site preparation:\nSupply of materials, tools, machineries and manpower for site preparation, by cleaning and removing all debris, rubble and dump it to locations approved by the local Authorities. ","LS",1]
[2,"Main gate foundation and columns:\nSupply of materials, tools and manpower to casting reinforced concrete (1:2:4) in foundatios (0.8x0.8x0.25m) and columns (0.4x0.4x2m) for main gate. Inlcuding rebars, formworks and all requirements to complete the wrok. See drawing nº 08","m³",1]
[3,"Masonry works:  \nSupply materials, tools and manpower to  construct a fence by using solid blocks 15x20x40 cm, 20 cm width, 2.7m height and by using cement mortar (1: 3) mix ratio, the wall should be leveled vertically and horizontally. Price of the work shall inlcude all the requirement to complete the job.    ","m²",14]
[4,"Cement plastering:\nSupply materials, tools and manpower to repair wall cracks and to replace damaged cement plastering. The work includes removing the damaged cement plastering of external walls & fence, 25cm at each side of the crack, then filling the cracks with crack filler and cement mortar 1:3 and by using SBR at a rate of 200gr per m², including applying a layer of chicken wire on the area with  3 layers of cement plastering 1:3 mix ratio. Price of the work shall inlcude all requirements to complete  the job.","m²",35]
[5,"Gypsum plastering:\nSupply of all necessary materials, tools and manpower to remove the damaged gypsum plastering of internal walls & roofs and plastering with new gypsum plastering  in 2 layers minimum thickness 15mm.The work includes repairing of wall cracks by removing the damaged gypsum plastering 25cm at each side of the crack,then filling the cracks with cement morter 1:3 and using SBR at a rate of 200gr per m² , later putting a layer of plastic mesh on the area under the gypsum plastering. All needed works to complete the job, will be included within the price.","m²",10]
[6,"Main gate (2x2.6m):\nSupply materials , tools and manpower to install new main gate steel doors (2x2.6m), by using plate gauge16, steel frame of angel sheet dimensions 7.62x7.62 cm, 5mm thickness and steel pipe 40x40x1.5mm, including door handles, hinges and locks. Price of the work shall include painting of steel door with anti-rust and two coats of oil paints with all requirements to complete the job. See drawing nº 01","EA",1]
[7,"Wooden doors (1.0x2.1m):\nSupply of materials, tools and manpower to install wooden doors, dimensions 1.0x2.1m, including handles, lock , hinges and all accessories. Price of the work shall include, frame, painting two faces with oil paint and all requirements to complete the job. See drawing nº 02 ","EA",30]
[8,"Steel doors (1.0x2.0m): \nSupply of materials, tools and manpower to remove old steel doors and to install new steel double face doors (1x2m), including door handles, lock, mortise, fixing a stopper on the floor or wall. Price of works shall include painting by using 2 layers anti-rust and 3 layers of oil painting with all requirements to complete the job. See drawing nº 09","EA",18]
[9,"Repair steel doors:\nSupply materials , tools , machineries and manpower to repair the damaged steel doors. Price of the work shall include handles, hinges ,oil paint ,accessories and all requirements to complete the job.","EA",6]
[10,"Repair steel windows: \nSupply materials, tools and manpower to repair the damaged steel window, including anti-insects wire mesh.  Price of the work shall include hinges, handle and all requirements to complete the job.","EA",20]
[11,"Plastic painting works:\nSupply materials , tools and manpower to paint the external walls and fence with three-layer of silicon (water proof) painting . Price of the work shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",4000]
[12,"Emulsion painting works:\nSupply materials , tools and manpower to paint the interior walls with three-layer of emulsion painting . Price of the job shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",4000]
[13,"Oil Painting:\nSupply materials, tools and manpower to paint  steel doors, windows, and internal walls with a paint-stripe at 1.25m height, by using 3 layers of oil paint. Price of the work shall include all requirements to complete the job.","m²",1000]
[14,"Expansion joints:\nSupply of materials, tools and manpower to inject expansion joints with foam and install aluminum plate 20 cm width, with rubber between the two pieces of plates and by using screws to fix. All needed works to complete the job, will be included within the price.","ml",15]
[15,"Crystal clear glass:\nSupply of materials, tools and manpower to remove the damaged glass and to install crysta clear glass 4 mm with with new paste, dumping of all debris to a site approved by local authorities, in case it is needed,  as well as all needed works to complete the job.","m²",200]
[16,"Flag pole : \nSupply materials , tools and man power to install Flag pole of  6 m high by using  2.5\" (64cm) pipe. Price of the work shall include anti rust and three layers oil painting and all  requirements  to complete the job.","EA",1]
[17,"Billboard:\nSupply materials, tools and man power to install the title of the school on  frame of size 3×1 m, with good quality LED printed sticker. The frame shall be made of square pipe section 4x4 cm. Price of the work shall  include all requirements to complete the job.","EA",2]
[18,"Class title board:\nSupply materials and manpower to install class title name made of plastic sheet size 15x25 cm, using screws to fix. Price of the work shall  include all requirements to complete the job.","EA",20]
[null,"Subtotal for Civil Works"]
[null,"Sanitary works"]
[1,"Drain pipes:\nSupply of materials, tools and manpower for removing damaged water drain pipes and for installing new galavnized steel pipes 3\" (76mm). Including all connections and needed accesories to fix on roof and walls. Price of the work shall  include all requirements to complete the job. See attached drawing nº 14","ml",12]
[2,"Galvanized iron water pipes:   \n Supply materials , tools and manpower  to inspect and repair the water network pipes (Hot & Cool) 1/2\" dia, 3/4\" dia, 1\" dia  and replace the damaged pipes. Price of the  work shall include all pipe fittings, connection works and all accessories and requirements to complete the job.","LS",1]
[3,"Ceramic lavatory pedestal:\nSupply of  materials, tools and manpower to install ceramic lavatory pedestal (1 sink), mixer taps, locks valves, mirror and all needed accessories with complete water connections. All needed works to complete the job, will be included within the price.","EA",4]
[4,"Mixer taps:\nSupply of materials, tools and manpower to install mixer taps, locks and all  needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",4]
[5,"Taps:\nSupply of all necessary materials, tools and manpower to connect chrome water taps 1/2\" or 3/4\" and to install water connections. All needed works to complete the job, will be included within the price.","EA",10]
[6,"Siphon:\nSupply of materials, tools and manpower to install siphon, locks valves and all needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",12]
[7,"Maintenance of sewerage pipes:\nSupply materials, machinary and manpower to clean the sewerage pipes net starting from the toilets groups, along manholes and the main septic tank. By using high pressure air/water to open the blockages in the network , and all requirements to complete a good work.","LS",1]
[8,"Manholes covering:\nSupply of materials, tools and manpower for covering manholes, dimensions 80x115cm (jacker plate), by using steel frame fixed on the concrete slab. All needed works to complete the job, will be included within the price.","EA",1]
[9,"Water pump:\nSupply materials, tools and manpower to connect water pump (1hp), Q=3M³/Hrs., H=20m with, ball valve and all fitting and accessories for connection. The price of works includes all accessories needed, as well as all needed works to complete the job. See attached","EA",1]
[null,"Subtotal for Sanitary works "]
[null,"Electricals Works"]
[null,"Work includes replace the damaged wires with new suitable size , testing and operation"]
[1,"Socket Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/13A) socket switch using screws,using single core copper PVC insulated wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",32]
[2,"Light Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/6A) (single , double , triple and quadruple) light switches using screws,using single core coppper wire PVC insulated (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",20]
[3,"Fluorescent Lighting:\nSupplying materials, tools and manpower, to install, connect and commissioning Simple Fluorescent Lighting Fixture 1x36 W, 4 feet, (metal frame, tube and starter), using single core copper PVC insulated wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",160]
[4,"Lighting:\nSupplying materials, tools and manpower, to install, connect and commissioning (220VAC/20Watt) economic light lamp with Lamp, using single core copper  PVC insulated wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",10]
[5,"Fan Regulator: \nSupplying materials, tools and manpower to install, connect and commissioning best quality of  Ceiling Fans Regulator with 5 speeds/ fan speed switch/ Regulator and  all requirements to complete a good work. ","EA",7]
[6,"Ceiling Fan:\nSupplying materials, tools and manpower to install, connect and commissioning best quality of 56\" ceiling fan with power regulator using copper PVC insulated cable (2*1.5mm) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",12]
[7,"Electrical bell:\nSupplying materials, tools and manpower, to install, connect and commissioning of electrical bell (220VAC), using single core copper PVC insulated wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using 1 Gang 2 Way Single Pole Push Switch (6A) with all accessories and requirement to implement the work entirely.","LS",2]
[8,"Sub Distribution Boards:\nSupply, installation, testing and commissioning of factory fabricated distribution boards for light/power, concealed type made of M.S sheet 16 SWG degreased, derusted, zinc phosphated finished with electrostatic powder coating, of approved colour with hinged door, lockable handle, protection plate, basbar, earth and neutral strip, complete internally wired, flexible earthing strap for door manufactured by any one of the approved manufacturers as specified and comprising as under: Distribution board (3 Phase/400V/50Hz ) , equipped with TPN DB 12ways,  (DIN type, horizontal/vertical) metal single door complete with all accessories to accommodate incoming  (1x 3 pole MCB , 1 x 63 Amps, 415 volt A.C),  includes outgoing  SP MCB (3 x 10 Amps), (3 x 16 Amps), (2 x 20 Amps),  (2 x 25 Amps) , (2 x 32 Amps )  and Neutral tapping bar/strip on/in prefabricated  MS cubical control panel board including drilling holes, connections, fixing etc. with all accessories to complete work as required.","EA",2]
[9,"Electrical water boiler:\n Supply materials, tools and manpower to install, establish, connect, and commissioning electrical heater 250 Liter with complete fittings & accessories . The work includes  Power Cable size (3x4mm2) .flexible cable copper conductor,PVC insulation, unarmoured,best type  inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories) or using (Plastic Cable Duct PVC Trunking) extend form SDB  to the wter boiler system, with all accessories and requirement to implement the work entirely. See attached","LS",1]
[10,"wire:\nSupplying materials, tools and manpower to install PVC insulated copper 2*1.5mm2 wire, work includes all  requirements to complete a good work. ","ml",280]
[11,"Water- cooler:\nSupplying materials , tools and manpower to install best quality stainless steel electrical water-cooler with three taps, water connections using screws,using single core PVC insulated copper wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",1]
[null,"Subtotal for Electricals Works",null,null,null,{"$f":"SUM(F41:F51)","v":0}]
[null,"Total ",null,null,null,{"$f":"F52+F38+F27","v":0}]

{"sheet":"BOQ#4","index":4,"n_rows":48,"n_cols":6,"rows_kept":48,"cut":false,"hidden":false,"merged":[[46,0,47,0],[47,1,47,4],[0,0,0,5],[2,1,2,5],[3,1,3,5],[4,1,4,5],[21,0,22,0],[29,0,31,0]]}
["Renovation of Al-Taghllubia for Boys School - Alhamdain  Sub- District - Ninawa Governorate "]
[null,"General Specification "]
[null,"1- All the materials supplied by the contractor must be according to Iraq's standard Specifications"]
[null,"2- The contractor must provide samples , catalogues and specification of materials for testing and approval by the site engineer "]
[null,"3- Contractor must pay the cost for samples including any laboratory test required"]
[null,"4- The price of works includes all job requierements as per Iraq's standard specification."]
["#","Item Description","Unit","Qty","Price$","Total $"]
[null,"Civil Works"]
[1,"Site preparation :\nSupply of materials, tools, machineries and manpower for site preparation, by cleaning and removing all debris, rubble and dump it to locations approved by the local Authorities. ","LS",1]
[2,"Main gate (2x2.6m):\nSupply materials , tools and manpower to install new main gate steel doors (2x2.6m), by using plate gauge16, steel frame of angel sheet dimensions 7.62x7.62 cm, 5mm thickness and steel pipe 40x40x1.5mm, including door handles, hinges and locks. Price of the work shall include painting of steel door with anti-rust and two coats of oil paints with all requirements to complete the job. See drawing nº 01","EA",1]
[3,"Repair steel doors:\nSupply materials , tools , machineries and manpower to repair the damaged steel doors. Price of the work shall include handles, hinges ,oil paint ,accessories and all requirements to complete the job.","EA",20]
[4,"Repair steel windows: \nSupply materials, tools and manpower to repair the damaged steel window, including anti-insects wire mesh.  Price of the work shall include hinges, handle and all requirements to complete the job.","EA",20]
[5,"Plastic painting works:\nSupply materials , tools and manpower to paint the external walls and fence with three-layer of silicon (water proof) painting . Price of the work shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",3000]
[6,"Emulsion painting works:\nSupply materials , tools and manpower to paint the interior walls with three-layer of emulsion painting . Price of the job shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",2500]
[7,"Oil Painting:\nSupply materials, tools and manpower to paint  steel doors, windows, and internal walls with a paint-stripe at 1.25m height, by using 3 layers of oil paint. Price of the work shall include all requirements to complete the job.","m²",750]
[8,"Tiling expansion joints:\nSypply of materials, tools and manpower for cleaning of roofing and for applying mastic in expansion joints. All needed works to complete the job, will be included within the price.","ml",16]
[9,"Suspended ceiling:\nSupplying material tools and manpower to install false ceiling 60x60 cm (Gypsum boards). The price includes fixing galvanized steel sections (H-sections-beams) , inverted T-section , fixing with galvanized steel bar (Ø5mm ), installing the form of a square to diamension (1.2x1.2m). The price of works includes the removal of old damaged false ceiling and work of spot lights, dumping of all debris to a site approved by local authorities, in case it is needed, as well as all needed works to complete the job.  See attached drawing nº 06","m²",12]
[10,"Crystal clear glass: \nSupply materials, tools and manpower to remove the damaged glass and paste and then install new crystal clear 4mm glass  with high quality paste. Price of  work shall include  all  requirements to complete a good work. ","m²",90]
[11,"Flag pole : \nSupply materials , tools and man power to install Flag pole of  6 m high by using  2.5\" (64cm) pipe. Price of the work shall include anti rust and three layers oil painting and all  requirements  to complete the job.","EA",1]
[12,"Billboard:\nSupply materials, tools and man power to install the title of the school on  frame of size 3×1 m, with good quality LED printed sticker. The frame shall be made of square pipe section 4x4 cm. Price of the work shall  include all requirements to complete the job.","EA",2]
[13,"Class title board:\nSupply materials and manpower to install class title name made of plastic sheet size 15x25 cm, using screws to fix. Price of the work shall  include all requirements to complete the job.","EA",20]
[null,"Subtotal for Civil Works"]
[null,"Sanitary works"]
[1,"Water tank: \nSupply of materials , tools and manpower to install galvanized water tank of 1400 liters capacity with plate gauge 16 cylindrical shape supported by steel base made from 2 inch angle shape . Price of the work shall include connection of the inlet and outlet pipes, fittings, Valves, float valves, accessories and all requirements to complete the job. ","EA",6]
[2,"Galvanized Iron water pipes:   \nSupply materials , tools and manpower  to inspect and repair the water network pipes (Hot & Cool) 1/2\" dia, 3/4\" dia, 1\" dia  and replace the damaged pipes. Price of the  work shall include all pipe fittings, connection works and all accessories and requirements to complete the job.","LS",1]
[3,"Taps:\nSupply of all necessary materials, tools and manpower to connect chrome water taps 1/2\" or 3/4\" and to install water connections. All needed works to complete the job, will be included within the price.","EA",10]
[4,"Siphon:\nSupply of materials, tools and manpower to install siphon, locks valves and all needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",4]
[5,"Maintenance of sewerage pipes:\nSupply materials, machinary and manpower to clean the sewerage pipes net starting from the toilets groups, along manholes and the main septic tank. By using high pressure air/water to open the blockages in the network , and all requirements to complete a good work.","EA",1]
[6,"Water pump:\nSupply materials, tools and manpower to connect water pump (1hp), Q=3M³/Hrs., H=20m with, ball valve and all fitting and accessories for connection. The price of works includes all accessories needed, as well as all needed works to complete the job. See attached","EA",1]
[null,"Subtotal for Sanitary works "]
[null,"Electricals Works"]
[null,"Work includes replace the damaged wires with new suitable size , testing and operation"]
[1,"Socket Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/13A) socket switch using screws,using single core copper wire (2*2.5mm2)1.0 kV PVC insulated  installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",20]
[2,"Light Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/6A) (single , double , triple and quadruple) light switches using screws,using single core copper wire (2*2.5mm2) 1.0 kV grade PVC insulated installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",50]
[3,"Fluorescent Lighting:                \nSupplying materials, tools and manpower, to install, connect and commissioning Simple Fluorescent Lighting Fixture 1x36 W, 4 feet, (metal frame, tube and starter), using single core copper wire (2*1.5mm2) 1.0 kV grade PVC insulated installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",110]
[4,"Lighting:                \nSupplying materials, tools and manpower, to install, connect and commissioning (220VAC/20Watt) economic light lamp with Lamp, using single core copper wire (2*1.5mm2) 1.0 kV grade PVC insulated installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",20]
[5,"Fan Regulator:                                                 \nSupplying materials, tools and manpower to install, connect and commissioning best quality of  Ceiling Fans Regulator with 5 speeds/ fan speed switch/ Regulator and  all requirements to complete a good work. ","EA",5]
[6,"Ceiling Fan:\nSupplying materials, tools and manpower to install, connect and commissioning best quality of 56\" ceiling fan with power regulator using copper cable 1.0 kV PVC insulated  (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",5]
[7,"Exhaust fan:\nSupplying materials, tools and manpower, to install, connect and commissioning of exhaust fan 6 inch (220VAC), using single core copper wire 1.0 kV PVC insulated (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way switch (6A) with all accessories and requirement to implement the work entirely.","LS",10]
[8,"Electrical bell:\nSupplying materials, tools and manpower, to install, connect and commissioning of electrical bell (220VAC), using single core copper wire 1.0 kV grade PVC insulated (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using 1 Gang 2 Way Single Pole Push Switch (6A) with all accessories and requirement to implement the work entirely.","LS",2]
[9,"Main Board:\n Providing materials, installation and operation test of distribution board, enclosed metal frame made of iron sheet 1mm thickness painted with two layers of gray color oil paint free, arrange the items shown below properly, with door,  dimensions (height x width x depth: 80cm x 80 cm x 40cm), using rubber gaskets and equipped with the following items, Plastic trunck for wiring, and Bus bars 100A 4No with earth bus bar, the price also include the required, glands, screws, insulators, and etc, all items should be arranged properly, affords a high degree of safety operation,\n\nA - [(1 No.)  100A,  3Ph.415 VAC 25 kV BC MCCB type].\nB - [(6 No.)  25A,  3Ph.415 VAC MCB type].\nC - [(6 No.)  25A,  1Ph.220 VAC MCB type].\nD - (1 No.)Voltmeter (0- 400 V) with selector switch.\nE - (1 Set)Ammeter (0 -100 A), 100/5A with required CTs.\nF - (1 No.)Hertz meter (48- 52 )Hz.\nG - (1 No.) selector switch.\nH - (3 No.) Indicator lamp 220VAC/5A.\nI - Three-phase Kilowatt-hour meter \nJ - (1Set)Copper Bus-Bar 100A., for lines and the half for the neutral and             earth, length for each one not less than (40)cm., with all accessories.","EA",1]
[10,"Sub Distribution Boards:\nSupply, installation, testing and commissioning of factory fabricated distribution boards for light/power, concealed type made of M.S sheet 16 SWG degreased, derusted, zinc phosphated finished with electrostatic powder coating, of approved colour with hinged door, lockable handle, protection plate, basbar, earth and neutral strip, complete internally wired, flexible earthing strap for door manufactured by any one of the approved manufacturers as specified and comprising as under: Distribution board (3 Phase/400V/50Hz ) , equipped TPN DB 12ways,  (DIN type, horizontal/vertical) metal single door complete with all accessories to accommodate incoming  (1x 3 pole MCB , 1 x 63 Amps, 415 volt A.C),  includes outgoing  SP MCB (3 x 10 Amps), (3 x 16 Amps), (2 x 20 Amps),  (2 x 25 Amps) , (2 x 32 Amps )  and Neutral tapping bar/strip on/in prefabricated  MS cubical control panel board including drilling holes, connections, fixing etc. with all accessories to complete work as required.","EA",2]
[11,"Electrical water boiler:\nSupply materials, tools and manpower to install, establish, connect, and commissioning electrical heater 250 Liter 3 kW with complete fittings & accessories . The work includes  Power Cable size (3x4mm2) .flexible cable copper conductor,PVC insulation,1.0 kV grade unarmoured,best type  inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories) or using (Plastic Cable Duct PVC Trunking) extend form SDB  to the wter boiler system, with all accessories and requirement to implement the work entirely. See attached","EA",3]
[12,"wire:\nSupplying materials, tools and manpower to install 1.0 kV grade PVC coppere 2*1.5mm wire, work includes all  requirements to complete a good work. ","ml",350]
[13,"Water- cooler:                         \nSupplying materials , tools and manpower to install best quality stainless steel electrical water-cooler with three taps, water connections using screws,using single core copper wire (2*2.5mm2) 1.0 kV gradae PVC insulatedninstalled inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",1]
[14,"Wall Mounted Split Unit Air-Conditioning:                  \nSupply, installaytion , connect and commissioning best quality  Split unit Air-conditioning (Cool & Heat) 2  ton.(24000btuh) , ambiant temperature -10 to 50° C  using  Power Cable size (2x4mm2) .flexible cable copper conductor,1.0 kV grade PVC insulation, unarmoured,best type lay on plastic cable chanal or fixed on the wall or (ceiling) by special plastic clamps extend form the main board   to the workshop, the cabls should connected by cable lugs with all requirements & connections in both sides with switch 45  Amp , the price include steel base, installing condensation pipe with all accessories and requirements to complete a good work.In addition to the guarantee and maintenance of the unit  for two years. See attached","LS",1]
[null,"Subtotal for Electricals Works",null,null,null,{"$f":"SUM(F33:F46)","v":0}]
[null,"Total ",null,null,null,{"$f":"F47+F30+F22","v":0}]

{"sheet":"BOQ#5","index":5,"n_rows":51,"n_cols":6,"rows_kept":51,"cut":false,"hidden":false,"merged":[[34,1,34,3],[49,0,50,0],[50,1,50,4],[0,0,0,5],[2,1,2,5],[3,1,3,5],[4,1,4,5],[22,0,23,0],[32,0,33,0]]}
["Renovation of Al-Zawra Primary Mixed School - Al-Hamdaniya  Sub- District - Ninawa Governorate "]
[null,"General Specification "]
[null,"1- All the materials supplied by the contractor must be according to Iraq's standard Specifications"]
[null,"2- The contractor must provide samples , catalogues and specification of materials for testing and approval by the site engineer "]
[null,"3- Contractor must pay the cost for samples including any laboratory test required"]
[null,"4- The price of works includes all job requierements as per Iraq's standard specification."]
["#","Item Description","Unit","Qty","Price$","Total $"]
[null,"Civil Works"]
[1,"Site preparation :\nSupply of materials, tools, machineries and manpower for site preparation, by cleaning and removing all debris, rubble and dump it to locations approved by the local Authorities. ","LS",1]
[2,"Main gate (2x2.6m):\nSupply materials , tools and manpower to install new main gate steel doors (2x2.6m), by using plate gauge16, steel frame of angel sheet dimensions 7.62x7.62 cm, 5mm thickness and steel pipe 40x40x1.5mm, including door handles, hinges and locks. Price of the work shall include painting of steel door with anti-rust and two coats of oil paints with all requirements to complete the job. See drawing nº 01","EA",1]
[3,"Main gate (1.5x2m):\nSupply materials , tools and manpower to install new main gate steel doors (1.5x2m), by using plate gauge16 and steel pipe 40x40x1.5mm, including door handles, hinges and locks. Price of the work shall include painting of steel door with anti-rust and two coats of oil paints with all requirements to complete the job. See drawing nº 07","EA",2]
[4,"Repair steel doors:\nSupply materials , tools , machineries and manpower to repair the damaged steel doors. Price of the work shall include handles, hinges, painting by using 2 layers anti-rust and 3 layers of oil painting, accessories and all requirements to complete the job. ","EA",20]
[8,"Wooden doors (1.0x2.1m):\nSupply materials, tools and manpower to install wooden doors with dimensions 1.0x2.1m, including handles, lock , hinges and all accessories. The inner portions space of the door is not more than 12cm. Price of the work shall include, frame, painting two faces with oil paint and all requirements to complete the job.","EA",8]
[5,"Repair steel windows: \nSupply materials, tools and manpower to repair the damaged steel window, including anti-insects wire mesh.  Price of the work shall include hinges, handle and all requirements to complete the job.","EA",40]
[6,"Plastic painting works:\nSupply materials , tools and manpower to paint the external walls and fence with three-layer of silicon (water proof) painting . Price of the work shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",3500]
[7,"Emulsion painting works:\nSupply materials , tools and manpower to paint the interior walls with three-layer of emulsion painting . Price of the job shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",2500]
[8,"Oil Painting:\nSupply materials, tools and manpower to paint  steel doors, windows, and internal walls with a paint-stripe at 1.25m height, by using 3 layers of oil paint. Price of the work shall include all requirements to complete the job.","m²",750]
[9,"Expansion joints:\nSupply of materials, tools and manpower to inject expansion joints with foam and install aluminum plate 20 cm width, with rubber between the two pieces of plates and by using screws to fix. All needed works to complete the job, will be included within the price.","ml",20]
[10,"Crystal clear glass: \nSupply materials, tools and manpower to remove the damaged glass and paste and then install new crystal clear 4mm glass  with high quality paste. Price of  work shall include  all  requirements to complete a good work. ","m²",120]
[11,"Flag pole : \nSupply materials , tools and man power to install Flag pole of  6 m high by using  2.5\" (64cm) pipe. Price of the work shall include anti rust and three layers oil painting and all  requirements  to complete the job.","EA",1]
[12,"Billboard:\nSupply materials, tools and man power to install the title of the school on  frame of size 3×1 m, with good quality LED printed sticker. The frame shall be made of square pipe section 4x4 cm. Price of the work shall  include all requirements to complete the job.","EA",1]
[13,"Class title board:\nSupply materials and manpower to install class title name made of plastic sheet size 15x25 cm, using screws to fix. Price of the work shall  include all requirements to complete the job.","EA",20]
[null,"Subtotal for Civil Works"]
[null,"Sanitary works"]
[1,"Water tank: \nSupply of materials , tools and manpower to install galvanized water tank of 1400 liters capacity with plate gauge 16 cylindrical shape supported by steel base made from 2 inch angle shape . Price of the work shall include connection of the inlet and outlet pipes, fittings, Valves, float valves, accessories and all requirements to complete the job. ","EA",4]
[2,"Galvanized iron water pipes:   \nSupply of materials, tools and manpower to inspect and repair the water network pipes (Hot & Cool) 1/2\" dia, 3/4\" dia, 1\" dia  and replace the damaged pipes. Price of the  work shall include all pipe fittings, connection works and all accessories and requirements to complete the job.","LS",1]
[3,"Taps:\nSupply materials, tools and manpower necessary to connect chrome water taps 1/2\" or 3/4\", water connections. Price of the works shall include all requirements to complete the job.","EA",10]
[4,"Mixer taps:\nSupply of materials, tools and manpower to install mixer taps, locks and all  accessories with complete water connections. The price of works shall include all needed works to complete the job.","EA",6]
[5,"Siphon:\nSupply of materials, tools and manpower to install siphon, locks valves and all needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",6]
[6,"Manholes:                                                \nSupply  materials, tools and manpower to build  40x40 cm size  manholes, by using solid block of size (15x20x40)cm  with cement mortar(1: 3) mix ratio. The work includes cement plastering from inside and outside, with cover made of cast iron frame fixed with concrete slab of manhole and all requirements to complete good work . See drawing nº 04","EA",2]
[7,"Maintenance of sewerage pipes:\nSupply materials, machinary and manpower to clean the sewerage pipes net starting from the toilets groups, along manholes and the main septic tank. By using high pressure air/water to open the blockages in the network , and all requirements to complete a good work.","EA",1]
[8,"Water pump:\nSupply materials, tools and manpower to connect water pump (1hp), Q=3M³/Hrs., H=20m with, ball valve and all fitting and accessories for connection. The price of works includes all accessories needed, as well as all needed works to complete the job. See attached","EA",1]
[null,"Subtotal for Sanitary works "]
[null,"Electricals Works"]
[null,"Work includes replace the damaged wires with new suitable size , testing and operation"]
[1,"Socket Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/13A) socket switch using screws,using single core copper wire (2*2.5mm2) 1.0 kV  grade PVC insulated installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",20]
[2,"Light Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/6A) (single , double , triple and quadruple) light switches using screws,using single core copper wire (2*2.5mm2) 1.0 kV grade  PVC insulated copper installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",22]
[3,"Lighting:\nSupplying materials, tools and manpower, to install, connect and commissioning (220VAC/20Watt) economic light lamp with Lamp, using single core copper wire 1.0 kV grade PVC insulated (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",40]
[4,"Fluorescent Lighting:\nSupplying materials, tools and manpower, to install, connect and commissioning Simple Fluorescent Lighting Fixture 1x36 W, 4 feet, (metal frame, tube and starter), using single core copper wire (2*1.5mm2) 1.0 kV grade PVC insulated  installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",200]
[5,"Fan Regulator:\nSupplying materials, tools and manpower to install, connect and commissioning best quality of  Ceiling Fans Regulator with 5 speeds/ fan speed switch/ Regulator and  all requirements to complete a good work. ","EA",4]
[6,"Ceiling Fan:\nSupplying materials, tools and manpower to install, connect and commissioning best quality of 56\" ceiling fan with power regulator using copper cable  1.0 kV grade PVC insulated (2*1.5mm) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",8]
[7,"Exhaust fan:\nSupplying materials, tools and manpower, to install, connect and commissioning of exhaust fan 6 inch (220VAC), using single core copper wirePVC insulated  (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way switch (6A) with all accessories and requirement to implement the work entirely.","LS",10]
[8,"Electrical bell: \nSupplying materials, tools and manpower, to install, connect and commissioning of electrical bell (220VAC), using single core copper wire  PVC insulated 1.0 kV grade (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using 1 Gang 2 Way Single Pole Push Switch (6A) with all accessories and requirement to implement the work entirely.","LS",2]
[9,"Main Board:\nProviding materials, installation and operation test of Pre fabricated distribution board, enclosed metal frame made of iron sheet 1mm thickness painted with two layers of gray color oil paint free, arrange the items shown below properly, with door,  dimensions (height x width x depth: 80cm x 80 cm x 40cm), using rubber gaskets and equipped with the following items, Plastic trunck for wiring, and Bus bars 100A 4No with earth bus bar, the price also include the required, glands, screws, insulators, and etc, all items should be arranged properly, affords a high degree of safety operation,\n\nA - [(1 No.)  100A,  3Ph. 415 VAC ,25 kV BC,MCCB type].\nB - [(6 No.)  25A,  3Ph. 415 VAC MCB type].\nC - [(6 No.)  25A,  1Ph.220 VAC  MCB type].\nD - (1 No.)Voltmeter (0- 400 V) with selector switch.\nE - (1 Set)Ammeter (0 -100 A), 100/5A with required CTs.\nF - (1 No.)Hertz meter (48- 52 )Hz.\nG - (1 No.) selector switch.\nH - (3 No.) Indicator lamp 220VAC/5A.\nI - Three-phase Kilowatt-hour meter \nJ - (1Set)Copper Bus-Bar 100A., for lines and the half for the neutral and             earth, length for each one not less than (40)cm., with all accessories.","EA",1]
[10,"Sub Distribution Boards:\nSupply, installation, testing and commissioning of factory fabricated distribution boards for light/power, concealed type made of M.S sheet 16 SWG degreased, derusted, zinc phosphated finished with electrostatic powder coating, of approved colour with hinged door, lockable handle, protection plate, basbar, earth and neutral strip, complete internally wired, flexible earthing strap for door manufactured by any one of the approved manufacturers as specified and comprising as under: Distribution board (3 Phase/400V/50Hz ) , equipped with TPN DB 12ways,  (DIN type, horizontal/vertical) metal single door complete with all accessories to accommodate incoming  (1x 3 pole MCB , 1 x 63 Amps, 415 volt A.C),  includes outgoing  SP MCB (3 x 10 Amps), (3 x 16 Amps), (2 x 20 Amps),  (2 x 25 Amps) , (2 x 32 Amps )  and Neutral tapping bar/strip on/in prefabricated  MS cubical control panel board including drilling holes, connections, fixing etc. with all accessories to complete work as required.","EA",2]
[11,"Electrical water boiler:\nSupply materials, tools and manpower to install, establish, connect, and commissioning electrical heater 250 Liter 3 kW with complete fittings & accessories . The work includes  Power Cable size (3x4mm2) .flexible cable copper conductor,1.0 kV grade PVC insulation, unarmoured,best type  inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories) or using (Plastic Cable Duct PVC Trunking) extend form SDB  to the wter boiler system, with all accessories and requirement to implement the work entirely. See attached","EA",2]
[12,"Power Cable:\nProviding materials, installation and operation test of  Power Cable size (4x10mm2) .flexible cable copper conductor,1.0 kV grade PVC insulation, unarmoured,best type lay on plastic cable chanal or fixed on the wall or (ceiling) by special plastic clamps extend form the main pole to the main board, the cabls should connected by cable lugs with all requirements & connections in both sides , with all accessories and requirement to implement the work entirely.","M",100]
[13,"Wire:\nSupplying materials, tools and manpower to install 1.0 kV grade PVC insulated copper 2*1.5mm wire, work includes all  requirements to complete a good work. ","M",300]
[14,"Water- cooler:                         \nSupplying materials , tools and manpower to install best quality stainless steel electrical water-cooler with three taps, water connections using screws,using single core copper wire (2*2.5mm2) 1.0 kV PVC insulated installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",3]
[null,"Subtotal for Electricals Works"]
[null,"Total "]

{"sheet":"BOQ#6","index":6,"n_rows":54,"n_cols":6,"rows_kept":54,"cut":false,"hidden":false,"merged":[[53,1,53,4],[0,0,0,5],[2,1,2,5],[3,1,3,5],[4,1,4,5],[23,0,24,0],[35,0,37,0]]}
["Renovation of Ashur Banibal Alryania for Boys School - Alhamdain  Sub- District - Ninawa Governorate "]
[null,"General Specification "]
[null,"1- All the materials supplied by the contractor must be according to Iraq's standard Specifications"]
[null,"2- The contractor must provide samples , catalogues and specification of materials for testing and approval by the site engineer "]
[null,"3- Contractor must pay the cost for samples including any laboratory test required"]
[null,"4- The price of works includes all job requierements as per Iraq's standard specification."]
["#","Item Description","Unit","Qty","Price$","Total $"]
[null,"Civil Works"]
[1,"Site preparation:\nSupply of materials, tools, machineries and manpower for site preparation, by cleaning and removing all debris, rubble and dump it to locations approved by the local Authorities. ","LS",1]
[2,"Main gate (2x2.6m):\nSupply materials , tools and manpower to install new main gate steel doors (2x2.6m), by using plate gauge16, steel frame of angel sheet dimensions 7.62x7.62 cm, 5mm thickness and steel pipe 40x40x1.5mm, including door handles, hinges and locks. Price of the work shall include painting of steel door with anti-rust and two coats of oil paints with all requirements to complete the job. See drawing nº 01","EA",1]
[3,"Wooden doors (1.0x2.1m):\nSupply materials, tools and manpower to install wooden doors with dimensions 1.0x2.1m, including handles, lock , hinges and all accessories. The inner portions space of the door is not more than 12cm. Price of the work shall include, frame, painting two faces with oil paint and all requirements to complete the job.","EA",30]
[4,"Repair steel doors:\nSupply materials, tools, machineries and manpower to repair the damaged steel doors. Price of the work shall include handles, hinges, paiting, accessories and all requirements to complete the job.","EA",5]
[5,"Repair steel windows: \nSupply materials, tools and manpower to repair the damaged steel window, including anti-insects wire mesh.  Price of the work shall include hinges, handle and all requirements to complete the job.","EA",70]
[6,"Gypsum plastering:\nSupply of all necessary materials, tools and manpower to remove the damaged gypsum plastering of internal walls & roofs and plastering with new gypsum plastering  in 2 layers minimum thickness 15mm.The work includes repairing of wall cracks by removing the damaged gypsum plastering 25cm at each side of the crack,then filling the cracks with cement morter 1:3 and using SBR at a rate of 200gr per m² , later putting a layer of plastic mesh on the area under the gypsum plastering. All needed works to complete the job, will be included within the price.","m²",350]
[7,"Suspended ceiling:\nSupplying material tools and manpower to install false ceiling 60x60 cm (Gypsum boards). The price includes fixing galvanized steel sections (H-sections-beams) , inverted T-section , fixing with galvanized steel bar (Ø5mm ), installing the form of a square to diamension (1.2x1.2m). The price of works includes the removal of old damaged false ceiling and work of spot lights, dumping of all debris to a site approved by local authorities, in case it is needed, as well as all needed works to complete the job.  See attached drawing nº 06","m²",100]
[8,"Plastic painting:             \nSupply of materials, tools and manpower to paint the exterior walls and fence with three-layer of silicon (water proof) painting. The works include cleaning the walls and removing the fire waste, dirt and dust before painting, repairing wall cracks and filling with cement plastering. All needed works to complete the job, will be included within the price.","m²",4000]
[9,"Emulsion Painting:             \nSupply of materials, tools and manpower to paint walls and slabs with three-layer of emulsion painting. The works include cleaning the walls and removing the fire waste, dirt and dust before painting, repairing wall cracks and filling with cement plastering. All needed works to complete the job, will be included within the price.","m²",3000]
[10,"Oil Painting:\nSupply materials, tools and manpower to paint  steel doors, windows, and internal walls with a paint-stripe at 1.25m height, by using 3 layers of oil paint. Price of the work shall include all requirements to complete the job.","m²",750]
[11,"Expansion joints:\nSupply of materials, tools and manpower to inject expansion joints with foam and install aluminum plate 20 cm width, with rubber between the two pieces of plates and by using screws to fix. All needed works to complete the job, will be included within the price.","ml",15]
[12,"Crystal clear glass:\nSupply of materials, tools and manpower to remove the damaged glass and to install crysta clear glass 4 mm with with new paste, dumping of all debris to a site approved by local authorities, in case it is needed,  as well as all needed works to complete the job.","m²",140]
[13,"Flag pole : \nSupply materials , tools and man power to install Flag pole of  6 m high by using  2.5\" (64cm) pipe. Price of the work shall include anti rust and three layers oil painting and all  requirements  to complete the job.","EA",1]
[14,"Billboard:\nSupply materials, tools and man power to install the title of the school on  frame of size 3×1 m, with good quality LED printed sticker. The frame shall be made of square pipe section 4x4 cm. Price of the work shall  include all requirements to complete the job.","EA",1]
[15,"Class title board:\nSupply materials and manpower to install class title name made of plastic sheet size 15x25 cm, using screws to fix. Price of the work shall  include all requirements to complete the job.","EA",20]
[null,"Subtotal for Civil Works"]
[null,"Sanitary works"]
[1,"Water tank: \nSupply of materials , tools and manpower to install galvanized water tank of 1400 liters capacity with plate gauge 16 cylindrical shape supported by steel base made from 2 inch angle shape . Price of the work shall include connection of the inlet and outlet pipes, fittings, Valves, float valves, accessories and all requirements to complete the job. ","EA",6]
[2,"Drain pipes:\nSupply of materials, tools and manpower for removing damaged water drain pipes and for installing new galavnized steel pipes 3\" (76mm). Including all connections and needed accesories to fix on roof and walls. Price of the work shall  include all requirements to complete the job. See attached drawing nº 14","ml",30]
[3,"Galvanized iron water pipes:   \n Supply materials , tools and manpower  to inspect and repair the water network pipes (Hot & Cool) 1/2\" dia, 3/4\" dia, 1\" dia  and replace the damaged pipes. Price of the  work shall include all pipe fittings, connection works and all accessories and requirements to complete the job.","LS",1]
[4,"Ceramic lavatory pedestal:\nSupply of  materials, tools and manpower to install ceramic lavatory pedestal (1 sink), mixer taps, locks valves, mirror and all needed accessories with complete water connections. All needed works to complete the job, will be included within the price.","EA",4]
[5,"Mixer taps:\nSupply of materials, tools and manpower to install mixer taps, locks and all  needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",4]
[6,"Taps:\nSupply of all necessary materials, tools and manpower to connect chrome water taps 1/2\" or 3/4\" and to install water connections. All needed works to complete the job, will be included within the price.","EA",10]
[7,"Siphon:\nSupply of materials, tools and manpower to install siphon, locks valves and all needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",6]
[8,"Maintenance of sewerage pipes:\nSupply materials, machinary and manpower to clean the sewerage pipes net starting from the toilets groups, along manholes and the main septic tank. By using high pressure air/water to open the blockages in the network , and all requirements to complete a good work.","EA",1]
[9,"Manholes covering:\nSupply of materials, tools and manpower for covering manholes, dimensions 80x115cm (jacker plate), by using steel frame fixed on the concrete slab. All needed works to complete the job, will be included within the price.","EA",1]
[10,"Water pump:\nSupply materials, tools and manpower to connect water pump (1hp), Q=3M³/Hrs., H=20m with, ball valve and all fitting and accessories for connection. The price of works includes all accessories needed, as well as all needed works to complete the job.  See attached","EA",1]
[null,"Subtotal for Sanitary works "]
[null,"Electricals Works"]
[null,"Work includes replace the damaged wires with new suitable size , testing and operation"]
[1,"Socket Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/13A) socket switch using screws,using single core copper wire 1.0 kV grade PVC insulated (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",130]
[2,"Light Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/6A) (single , double , triple and quadruple) light switches using screws,using single core copper wire (2*2.5mm2) 1.0 kV grade PVC insulated installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",80]
[3,"Fluorescent Lighting:                \nSupplying materials, tools and manpower, to install, connect and commissioning Simple Fluorescent Lighting Fixture 1x36 W, 4 feet, (metal frame, tube and starter), using single core copper wire (2*1.5mm2)1.0 kV grade PVC insulated  installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",30]
[4,"Lighting:                \nSupplying materials, tools and manpower, to install, connect and commissioning (220VAC/20Watt) economic light lamp with Lamp, using single core copper wire (2*1.5mm2) 1.0 kV grade PVC insulated  installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",40]
[5,"Fan Regulator:                                                 \nSupplying materials, tools and manpower to install, connect and commissioning best quality of  Ceiling Fans Regulator with 5 speeds/ fan speed switch/ Regulator and  all requirements to complete a good work. ","EA",18]
[6,"Ceiling Fan:\nSupplying materials, tools and manpower to install, connect and commissioning best quality of 56\" ceiling fan with power regulator using copper cable 1.0 kV grade PVC insulated  (2*1.5mm) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",12]
[7,"Exhaust fan:                                       \nSupplying materials, tools and manpower, to install, connect and commissioning of exhaust fan 6 inch (220VAC), using single core copper wire1.0 kV grade PVC insulated (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way switch (6A) with all accessories and requirement to implement the work entirely.","LS",12]
[8,"Electrical bell:                           \nSupplying materials, tools and manpower, to install, connect and commissioning of electrical bell (220VAC), using single core copper wire 1.0 kV grade insulated(2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using 1 Gang 2 Way Single Pole Push Switch (6A) with all accessories and requirement to implement the work entirely.","LS",2]
[9,"Main Board:\nProviding materials, installation and operation test of distribution board, enclosed metal frame made of iron sheet 1mm thickness painted with two layers of gray color oil paint free, arrange the items shown below properly, with door,  dimensions (height x width x depth: 80cm x 80 cm x 40cm), using rubber gaskets and equipped with the following items, Plastic trunck for wiring, and Bus bars 100A 4No with earth bus bar, the price also include the required, glands, screws, insulators, and etc, all items should be arranged properly, affords a high degree of safety operation,\n\nA - [(1 No.)  100A,  3Ph.415 VAC 25 kV BC, MCCB type].\nB - [(6 No.)  25A,  3Ph. 415 VAC MCB type].\nC - [(6 No.)  25A,  1Ph.220 VAC MCB type].\nD - (1 No.)Voltmeter (0- 400 VAC) with selector switch.\nE - (1 Set)Ammeter (0 -100 A), 100/5A with required CTs.\nF - (1 No.)Hertz meter (48- 52 )Hz.\nG - (1 No.) selector switch.\nH - (3 No.) Indicator lamp 220VAC/5A.\nI - Three-phase Kilowatt-hour meter \nJ - (1Set)Copper Bus-Bar 100A., for lines and the half for the neutral and             earth, length for each one not less than (40)cm., with all accessories.","EA",1]
[10,"Sub Distribution Boards:\n                       Supply, installation, testing and commissioning of factory fabricated distribution boards for light/power, concealed type made of M.S sheet 16 SWG degreased, derusted, zinc phosphated finished with electrostatic powder coating, of approved colour with hinged door, lockable handle, protection plate, basbar, earth and neutral strip, complete internally wired, flexible earthing strap for door manufactured by any one of the approved manufacturers as specified and comprising as under: Distribution board (3 Phase/400V/50Hz ) , equipped with TPN DB 12ways,  (DIN type, horizontal/vertical) metal single door complete with all accessories to accommodate incoming  (1x 3 pole MCB , 1 x 63 Amps, 415 volt A.C),  includes outgoing  SP MCB (3 x 10 Amps), (3 x 16 Amps), (2 x 20 Amps),  (2 x 25 Amps) , (2 x 32 Amps )  and Neutral tapping bar/strip on/in prefabricated  MS cubical control panel board including drilling holes, connections, fixing etc. with all accessories to complete work as required.","EA",3]
[11,"Electrical water boiler: \nSupply materials, tools and manpower to install, establish, connect, and commissioning electrical heater 250 Liter 3kW with complete fittings & accessories . The work includes  Power Cable size (3x4mm2) .flexible cable copper conductor,1.0 kV grade PVC insulation, unarmoured,best type  inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories) or using (Plastic Cable Duct PVC Trunking) extend form SDB  to the wter boiler system, with all accessories and requirement to implement the work entirely.  See attached","EA",2]
[12,"Wire:                                    \nSupplying materials, tools and manpower to install copper 1.0 kV grade PVC insulated 2*1.5mm wire, work includes all  requirements to complete a good work. ","ml",1000]
[13,"Water- cooler:\nSupplying materials , tools and manpower to install best quality stainless steel electrical water-cooler with three taps, water connections using screws,using single core copper wire (2*2.5mm2) 1.0 kV grade PVC insulated installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",1]
[14,"Wall Mounted Split Unit Air-Conditioning:                  \nSupply, installaytion , connect and commissioning best quality  Split unit Air-conditioning (Cool & Heat) 2  ton.(24000btuh) , ambiant temperature -10 to 55° C  using  Power Cable size (2x4mm2) .flexible cable copper conductor,1.0 kV grade PVC insulation, unarmoured,best type lay on plastic cable chanal or fixed on the wall or (ceiling) by special plastic clamps extend form the main board   to the workshop, the cabls should connected by cable lugs with all requirements & connections in both sides with switch 45  Amp , the price include steel base, installing condensation pipe with all accessories and requirements to complete a good work.In addition to the guarantee and maintenance of the unit  for two years. See attached","LS",2]
[null,"Subtotal for Electricals Works"]
[null,"Total "]

{"sheet":"BOQ#7","index":7,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[[22,0,23,0],[34,0,36,0],[47,0,48,0],[48,1,48,4],[0,0,0,5],[2,1,2,5],[3,1,3,5],[4,1,4,5]]}
["Renovation of Qarqoush Frist Alkindergarten - Alhamdain  Sub- District - Ninawa Governorate "]
[null,"General Specification "]
[null,"1- All the materials supplied by the contractor must be according to Iraq's standard Specifications"]
[null,"2- The contractor must provide samples , catalogues and specification of materials for testing and approval by the site engineer "]
[null,"3- Contractor must pay the cost for samples including any laboratory test required"]
[null,"4- The price of works includes all job requierements as per Iraq's standard specification."]
["#","Item Description","Unit","Qty","Price$","Total $"]
[null,"Civil Works"]
[1,"Site preparation :\nSupply of materials, tools, machineries and manpower for site preparation, by cleaning and removing all debris, rubble and dump it to locations approved by the local Authorities. ","LS",1]
[2,"Main gate (2x2.6m):\nSupply materials , tools and manpower to install new main gate steel doors (2x2.6m), by using plate gauge16, steel frame of angel sheet dimensions 7.62x7.62 cm, 5mm thickness and steel pipe 40x40x1.5mm, including door handles, hinges and locks. Price of the work shall include painting of steel door with anti-rust and two coats of oil paints with all requirements to complete the job. See drawing nº 01","EA",1]
[3,"Repair steel doors:\nSupply materials , tools , machineries and manpower to repair the damaged steel doors. Price of the work shall include handles, hinges, painting by using 2 layers anti-rust and 3 layers of oil painting, accessories and all requirements to complete the job. ","EA",2]
[4,"Repair wooden doors:\nSupply materials , tools , machineries and manpower to repair the damaged wooden doors. Price of the work shall include handles, hinges, oil painting, accessories and all requirements to complete the job. ","EA",20]
[5,"Repair steel windows: \nSupply materials, tools and manpower to repair the damaged steel window, including anti-insects wire mesh.  Price of the work shall include hinges, handle and all requirements to complete the job.","EA",100]
[6,"Plastic painting works:\nSupply materials , tools and manpower to paint the external walls and fence with three-layer of silicon (water proof) painting . Price of the work shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",3000]
[7,"Emulsion Painting works:\nSupply materials , tools and manpower to paint the interior walls with three-layer of emulsion painting . Price of the job shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job. Interior walls painted with drawings, as per kindergarten administration requirements. ","m²",2500]
[8,"Oil Painting:\nSupply materials, tools and manpower to paint  steel doors, windows, and internal walls with a paint-stripe at 1.25m height, by using 3 layers of oil paint. Price of the work shall include all requirements to complete the job.","m²",750]
[9,"Steel stair:\nSupply materials, tools and manpower to install steel stair, width 1m by using plate 3mm, including hand rail of  90cm height. Price of work shall include anti rust and two coats of oil painting and all job requirements to complete good work. See drawing nº 03","ml",5]
[10,"Crystal clear glass: \nSupply materials, tools and manpower to remove the damaged glass and paste and then install new crystal clear 4mm glass  with high quality paste. Price of  work shall include  all  requirements to complete a good work. ","m²",100]
[11,"Suspended ceiling:\nSupplying material tools and manpower to install false ceiling 60x60 cm (Gypsum boards). The price includes fixing galvanized steel sections (H-sections-beams) , inverted T-section , fixing with galvanized steel bar (Ø5mm ), installing the form of a square to diamension (1.2x1.2m). The price of works includes the removal of old damaged false ceiling and work of spot lights, dumping of all debris to a site approved by local authorities, in case it is needed, as well as all needed works to complete the job.  See drawing nº 06","m²",10]
[12,"Flag pole : \nSupply materials , tools and man power to install Flag pole of  6 m high by using  2.5\" (64cm) pipe. Price of the work shall include anti rust and three layers oil painting and all  requirements  to complete the job.","EA",1]
[13,"Billboard:\nSupply materials, tools and man power to install the title of the school on  frame of size 3×1 m, with good quality LED printed sticker. The frame shall be made of square pipe section 4x4 cm. Price of the work shall  include all requirements to complete the job.","EA",1]
[14,"Class title board:\nSupply materials and manpower to install class title name made of plastic sheet size 15x25 cm, using screws to fix. Price of the work shall  include all requirements to complete the job.","EA",20]
[null,"Subtotal for Civil Works"]
[null,"Sanitary works"]
[1,"Water tank: \nSupply of materials , tools and manpower to install galvanized water tank of 1400 liters capacity with plate gauge 16 cylindrical shape supported by steel base made from 2 inch angle shape . Price of the work shall include connection of the inlet and outlet pipes, fittings, Valves, float valves, accessories and all requirements to complete the job. ","EA",2]
[2,"Galvanized iron water pipes:   \n Supply materials , tools and manpower  to inspect and repair the water network pipes (Hot & Cool) 1/2\" dia, 3/4\" dia, 1\" dia  and replace the damaged pipes. Price of the  work shall include all pipe fittings, connection works and all accessories and requirements to complete the job.","LS",1]
[3,"Ceramic lavatory pedestal:\nSupply of  materials, tools and manpower to install ceramic lavatory pedestal (1 sink), mixer taps, locks valves, mirror and all needed accessories with complete water connections. All needed works to complete the job, will be included within the price.","EA",4]
[4,"Mixer taps:\nSupply of materials, tools and manpower to install mixer taps, locks and all  needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",4]
[5,"Taps:\nSupply of all necessary materials, tools and manpower to connect chrome water taps 1/2\" or 3/4\" and to install water connections. All needed works to complete the job, will be included within the price.","EA",10]
[6,"Mixer taps:\nSupply of materials, tools and manpower to install mixer taps, locks and all  needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",4]
[7,"Manholes:                                                \nSupply  materials, tools and manpower to build  40x40 cm size  manholes, by using solid block of size (15x20x40)cm  with cement mortar(1: 3) mix ratio. The work includes cement plastering from inside and outside, with cover made of cast iron frame fixed with concrete slab of manhole and all requirements to complete good work . See drawing nº 04","EA",2]
[8,"Siphon:\nSupply of materials, tools and manpower to install siphon, locks valves and all needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",6]
[9,"Maintenance of sewerage pipes:\nSupply materials, machinary and manpower to clean the sewerage pipes net starting from the toilets groups, along manholes and the main septic tank. By using high pressure air/water to open the blockages in the network , and all requirements to complete a good work.","EA",1]
[10,"Water pump:\nSupply materials, tools and manpower to connect water pump (1hp), Q=3M³/Hrs., H=20m with, ball valve and all fitting and accessories for connection. The price of works includes all accessories needed, as well as all needed works to complete the job. See attached","EA",1]
[null,"Subtotal for Sanitary works "]
[null,"Electricals Works"]
[null,"Work includes replace the damaged wires with new suitable size , testing and operation"]
[1,"Socket Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/13A) socket switch using screws,using single core copper wire (2*2.5mm2) PVC insulated 1.0 kV grade installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",10]
[2,"Light Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/6A) (single , double , triple and quadruple) light switches using screws,using single core copper wire (2*2.5mm2) 1.0 kV PVC insulated  installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",10]
[3,"Lighting:                \nSupplying materials, tools and manpower, to install, connect and commissioning (220VAC/20Watt) economic light lamp with Lamp, using single core copper wire  1.0 kV PVC insulated (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",20]
[4,"Fluorescent Lamp : \nSupplying materials, tools and manpower, to install, connect and commissioning fluorescent light fixture (120 cm) (4 Foot)  with Lamp, and starte with all accessories and requirement to implement the work entirely.","EA",40]
[5,"Fan Regulator:                                                 \nSupplying materials, tools and manpower to install, connect and commissioning best quality of  Ceiling Fans Regulator with 5 speeds/ fan speed switch/ Regulator and  all requirements to complete a good work. ","EA",2]
[6,"Exhaust fan:                                       \nSupplying materials, tools and manpower, to install, connect and commissioning of exhaust fan 6 inch (220VAC), using single core copper wire (2*1.5mm2) 1.0 kV PVC insulated  installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way switch (6A) with all accessories and requirement to implement the work entirely.","LS",6]
[7,"Electrical bell:                           \nSupplying materials, tools and manpower, to install, connect and commissioning of electrical bell (220VAC), using single core copper wire (2*1.5mm2) PVC insulated 1.0 kV  installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using 1 Gang 2 Way Single Pole Push Switch (6A) with all accessories and requirement to implement the work entirely.","LS",1]
[8,"Main Board:\nProviding materials, installation and operation test of distribution board, enclosed metal frame made of iron sheet 1mm thickness painted with two layers of gray color oil paint free, arrange the items shown below properly, with door,  dimensions (height x width x depth: 80cm x 80 cm x 40cm), using rubber gaskets and equipped with the following items, Plastic trunck for wiring, and Bus bars 100A 4No with earth bus bar, the price also include the required, glands, screws, insulators, and etc, all items should be arranged properly, affords a high degree of safety operation,\n\nA - [(1 No.)  100A,  3Ph.415 VAC 25 kV BC MCCB type].\nB - [(6 No.)  25A,  3Ph.415 VAC MCB type].\nC - [(6 No.)  25A,  1Ph.220 VAC MCB type].\nD - (1 No.)Voltmeter (0- 400 V) with selector switch.\nE - (1 Set)Ammeter (0 -100 A), 100/5A with required CTs.\nF - (1 No.)Hertz meter (48- 52 )Hz.\nG - (1 No.) selector switch.\nH - (3 No.) Indicator lamp 220VAC/5A.\nI - Three-phase Kilowatt-hour meter \nJ - (1Set)Copper Bus-Bar 100A., for lines and the half for the neutral and             earth, length for each one not less than (40)cm., with all accessories.","EA",1]
[9,"Power Cable:\nProviding materials, installation and operation test of  Power Cable size (4x10mm2) .flexible cable copper conductor,PVC insulation, 1.0 kV grade unarmoured,best type lay on plastic cable chanal or fixed on the wall or (ceiling) by special plastic clamps extend form the main pole to the main board, the cabls should connected by cable lugs with all requirements & connections in both sides , with all accessories and requirement to implement the work entirely.","ml",80]
[10,"Water- cooler:                         \nSupplying materials , tools and manpower to install best quality stainless steel electrical water-cooler with three taps, water connections using screws,using single core Copper wire (2*2.5mm2)  1.0 kV grade PVC insulated installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",1]
[null,"Subtotal for Electricals Works"]
[null,"Total "]

{"sheet":"BOQ#8","index":8,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[[24,0,25,0],[34,0,35,0],[52,0,53,0],[52,1,52,4],[0,0,0,5],[2,1,2,5],[3,1,3,5],[4,1,4,5],[12,0,13,0],[12,2,13,2],[12,3,13,3],[12,4,13,4],[12,5,13,5]]}
["Renovation of Qarqoush for Boys - Secondary School - Alhamdain Sub- District - Ninawa Governorate "]
[null,"General Specification "]
[null,"1- All the materials supplied by the contractor must be according to Iraq's standard Specifications"]
[null,"2- The contractor must provide samples , catalogues and specification of materials for testing and approval by the site engineer "]
[null,"3- Contractor must pay the cost for samples including any laboratory test required"]
[null,"4- The price of works includes all job requierements as per Iraq's standard specification."]
["#","Item Description","Unit","Qty","Price$","Total $"]
[null,"Civil Works"]
[1,"Site preparation:\nSupply of materials, tools, machineries and manpower for site preparation, by cleaning and removing all debris, rubble and dump it to locations approved by the local Authorities. ","LS",1]
[2,"Masonry works :  \nSupply materials, tools and manpower to  construct a fence by using solid blocks 15x20x40 cm, 20 cm width, 2.7m height and by using cement mortar (1: 3) mix ratio, the wall should be leveled vertically and horizontally. Price of the work shall inlcude all the requirement to complete the job.    ","m²",25]
[3,"Cement plastering:\nSupply materials, tools and manpower to repair wall cracks and to replace damaged cement plastering. The work includes removing the damaged cement plastering of external walls & fence, 25cm at each side of the crack, then filling the cracks with crack filler and cement mortar 1:3 and by using SBR at a rate of 200gr per m², including applying a layer of chicken wire on the area with  3 layers of cement plastering 1:3 mix ratio. Price of the work shall inlcude all requirements to complete  the job.","m²",10]
[4,"Ceramic for walls:\nSupply of materials, tools and manpower to place a new ceramic 30x30 cm with cement morter. The price of works includes expantion joints, the removal of old damaged ceramic and dumping of all debris to a site approved by local authorities, in case it is needed, as well as all needed works to complete the job.","m²",200]
[5,"Main gate (2x2.6m):\nSupply materials , tools and manpower to install new main gate steel doors (2x2.6m), by using plate gauge16, steel frame of angel sheet dimensions 7.62x7.62 cm, 5mm thickness and steel pipe 40x40x1.5mm, including door handles, hinges and locks. Price of the work shall include painting of steel door with anti-rust and two coats of oil paints with all requirements to complete the job. See drawing nº 01","EA",1]
[null,"باب حديدى للبوابة الرئيسية:                                        تجهيز وتركيب بوابة للمدخل الرئيسي تتكون من فردتين قياس2.6*2 م باستخدام انابيب حديد مربعة 40*40*1.5 ملم وبليت كيج 16 مع الملبن و الكيلون وكافة الملحقات شاملا  السعر كل ما يتطلبه العمل ."]
[6,"Repair steel doors:\nSupply materials , tools , machineries and manpower to repair the damaged steel doors. Price of the work shall include handles, hinges ,oil paint ,accessories and all requirements to complete the job.","EA",20]
[7,"Repair steel windows: \nSupply materials, tools and manpower to repair the damaged steel window, including anti-insects wire mesh.  Price of the work shall include hinges, handle and all requirements to complete the job.","EA",20]
[8,"Plastic painting works:\nSupply materials , tools and manpower to paint the external walls and fence with three-layer of silicon (water proof) painting . Price of the work shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",2000]
[9,"Emulsion painting works:\nSupply materials , tools and manpower to paint the interior walls with three-layer of emulsion painting . Price of the job shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",2000]
[10,"Oil Painting:\nSupply materials, tools and manpower to paint  steel doors, windows, and internal walls with a paint-stripe at 1.25m height, by using 3 layers of oil paint. Price of the work shall include all requirements to complete the job.","m²",750]
[11,"Crystal clear glass: \nSupply materials, tools and manpower to remove the damaged glass and paste and then install new crystal clear 4mm glass  with high quality paste. Price of  work shall include  all  requirements to complete a good work. ","m²",100]
[12,"Steel stair:\nSupply materials, tools and manpower to install steel stair, width 1m by using plate 3mm, including hand rail of  90cm height. Price of work shall include anti rust and two coats of oil painting and all job requirements to complete good work. See drawing nº 03","ml",5]
[13,"Flag pole : \nSupply materials , tools and man power to install Flag pole of  6 m high by using  2.5\" (64cm) pipe. Price of the work shall include anti rust and three layers oil painting and all  requirements  to complete the job.","EA",1]
[14,"Billboard:\nSupply materials, tools and man power to install the title of the school on  frame of size 3×1 m, with good quality LED printed sticker. The frame shall be made of square pipe section 4x4 cm. Price of the work shall  include all requirements to complete the job.","EA",1]
[15,"Class title board:\nSupply materials and manpower to install class title name made of plastic sheet size 15x25 cm, using screws to fix. Price of the work shall  include all requirements to complete the job.","EA",20]
[null,"Subtotal for Civil Works"]
[null,"Sanitary works"]
[1,"Water tank: \nSupply of materials , tools and manpower to install galvanized water tank of 1400 liters capacity with plate gauge 16 cylindrical shape supported by steel base made from 2 inch angle shape . Price of the work shall include connection of the inlet and outlet pipes, fittings, Valves, float valves, accessories and all requirements to complete the job. ","EA",6]
[2,"Drain pipes (Yards):\nSupply of materials, tools and  equipment to fix plastic pipe from the main  yard, Ø6\" (15cm)  to the main network. Including plastic manholes (40x40cm) very 6m and consideration fo the slop of ground.  Including all connections and needed accesories to fix on roof and walls. Price of the work shall  include all requirements to complete the job. ","ml",90]
[3,"Galvanized iron water pipes:   \nSupply of materials, tools and manpower to inspect and repair the water network pipes (Hot & Cool) 1/2\" dia, 3/4\" dia, 1\" dia  and replace the damaged pipes. Price of the  work shall include all pipe fittings, connection works and all accessories and requirements to complete the job.","L.S.",1]
[4,"Taps:\nSupply materials, tools and manpower necessary to connect chrome water taps 1/2\" or 3/4\", water connections. Price of the works shall include all requirements to complete the job.","EA",10]
[5,"Maintenance of sewerage pipes:\nSupply materials, machinary and manpower to clean the sewerage pipes net starting from the toilets groups, along manholes and the main septic tank. By using high pressure air/water to open the blockages in the network , and all requirements to complete a good work.","EA",1]
[6,"Siphon:\nSupply of materials, tools and manpower to install siphon, locks valves and all needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",10]
[7,"Mixer taps:\nSupply of materials, tools and manpower to install mixer taps, locks and all  accessories with complete water connections. The price of works shall include all needed works to complete the job.","EA",8]
[8,"Water pump:\nSupply materials, tools and manpower to connect water pump (1hp), Q=3M³/Hrs., H=20m with, ball valve and all fitting and accessories for connection. The price of works includes all accessories needed, as well as all needed works to complete the job. See attached","EA",1]
[null,"Subtotal for Sanitary works "]
[null,"Electricals Works"]
[null,"Work includes replace the damaged wires with new suitable size , testing and operation"]
[1,"Socket Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/13A) socket switch using screws,using single core wire 1.0 kV grade  (2*2.5mm2) PVC insulated copper  installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",50]
[2,"Light Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/6A) (single , double , triple and quadruple) light switches using screws,using single core wire 1.0kV grade (2*2.5mm2) PVC copper installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",40]
[3,"Fluorescent Lighting:                \nSupplying materials, tools and manpower, to install, connect and commissioning Simple Fluorescent Lighting Fixture 1x36 W, 4 feet, (metal frame, tube and starter), using single core wire 1.0 kv grade  (2*1.5mm2) PVC insulated copper installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",180]
[4,"Lighting:                \nSupplying materials, tools and manpower, to install, connect and commissioning (220VAC/20Watt) economic light lamp with Lamp, using single core wire  1.0 kv grade (2*1.5mm2) PVC insulated copper installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",20]
[5,"Fluorescent Lamp : \nSupplying materials, tools and manpower, to install, connect and commissioning fluorescent light (120 cm) (4 Foot)  with Lamp, and starte with all accessories and requirement to implement the work entirely.","EA",20]
[6,"Fan Regulator:                                                 \nSupplying materials, tools and manpower to install, connect and commissioning best quality of  Ceiling Fans Regulator with 5 speeds/ fan speed switch/ Regulator and  all requirements to complete a good work. ","EA",15]
[7,"Exhaust fan:                                       \nSupplying materials, tools and manpower, to install, connect and commissioning of exhaust fan 6 inch (220VAC), using single core wire  1.0 kV grade(2*1.5mm2)  PVC insulated copper installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way switch (6A) with all accessories and requirement to implement the work entirely.","LS",10]
[8,"Electrical bell:                           \nSupplying materials, tools and manpower, to install, connect and commissioning of electrical bell (220VAC), using single core wire 1.0 kV grade (2*1.5mm2)  PVC insulated coppre installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using 1 Gang 2 Way Single Pole Push Switch (6A) with all accessories and requirement to implement the work entirely.","LS",2]
[9,"Main Board:\nProviding materials, installation and operation test of distribution board, enclosed metal frame made of iron sheet 1mm thickness painted with two layers of gray color oil paint free, arrange the items shown below properly, with door,  dimensions (height x width x depth: 80cm x 80 cm x 40cm), using rubber gaskets and equipped with the following items, Plastic trunck for wiring, and Bus bars 100A 4No with earth bus bar, the price also include the required, glands, screws, insulators, and etc, all items should be arranged properly, affords a high degree of safety operation,\n\nA - [(1 No.)  100A,  3Ph. 415 VAC 50 Hz TPN MCCB 26kV breaking capacity\nB - [(6 No.)  25A,  3Ph.415 V 50 Hz  MCB type].\nC - [(6 No.)  25A,  1Ph.220 VAC MCB type].\nD - (1 No.)Voltmeter (0- 400 V) with selector switch.\nE - (1 Set)Ammeter (0 -100 A), 100/5A with required CTs.\nF - (1 No.)Hertz meter (48- 52 )Hz.\nG - (1 No.) selector switch.\nH - (3 No.) Indicator lamp 220VAC/5A.\nI - Three-phase Kilowatt-hour meter  \nJ - (1Set)Copper Bus-Bar 100A., for lines and the half for the neutral and             earth, length for each one not less than (40)cm., with all accessories.","EA",1]
[10,"Sub Distribution Boards:\nSupplying,Installation, testing and commissioning of for TPN DB 12ways,  (DIN type, horizontal/vertical) metal single door complete with all accessories to accommodate incoming  (1x 3 pole MCB , 1 x 63 Amps, 415 volt A.C),  includes outgoing  SP MCB (3 x 10 Amps), (3 x 16 Amps), (2 x 20 Amps),  (2 x 25 Amps) , (2 x 32 Amps )  and Neutral tapping bar/strip on/in prefabricated  MS cubical control panel board including drilling holes, connections, fixing etc. with all accessories to complete work as required.","EA",3]
[11,"Electrical water boiler:\nSupply materials, tools and manpower to install, establish, connect, and commissioning electrical heater 250 Liter,3kV with complete fittings & accessories . The work includes  Power Cable size 1.0 kV grade(3x4mm2) .lexible cable copper conductor,PVC insulation, unarmoured,best type  inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories) or using (Plastic Cable Duct PVC Trunking) extend form SDB  to the wter boiler system, with all accessories and requirement to implement the work entirely. See attached","LS",2]
[12,"Wire:\nSupplying materials, tools and manpower to install   1.0 kV grade 2*1.5mm wire, work includes all  requirements to complete a good w. ","M",350]
[13,"Water- cooler:                         \nSupplying materials , tools and manpower to install best quality stainless steel electrical water-cooler with three taps, water connections using screws,using single core wire PVC insulated copper 1.0 kV grade  (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",1]
[14,"Wall Mounted Split Unit Air-Conditioning:                  \nSupply, installaytion , connect and commissioning best quality  Split unit Air-conditioning (Cool & Heat) 2  ton.(24000btuh) ,  max ambiant temperature  -10 to 55° C  using  Power Cable size 1.0 kV grade (2x4mm2) .flexible cable copper conductor,PVC insulation, unarmoured,best type lay on plastic cable chanal or fixed on the wall or (ceiling) by special plastic clamps extend form the main board   to the workshop, the cabls should connected by cable lugs with all requirements & connections in both sides with switch 45  Amp , the price include steel base, installing condensation pipe with all accessories and requirements to complete a good work.In addition to the guarantee and maintenance of the unit  for two years. See attached","LS",3]
[null,"Subtotal for Electricals Works"]
[null,"Total "]

{"sheet":"BOQ#9","index":9,"n_rows":51,"n_cols":6,"rows_kept":51,"cut":false,"hidden":false,"merged":[[34,1,34,5],[49,0,50,0],[50,1,50,4],[0,0,0,5],[2,1,2,5],[3,1,3,5],[4,1,4,5],[24,0,25,0],[32,0,33,0]]}
["Renovation of Qarqoush for Girls Secondary School - Alhamdain  Sub- District - Ninawa Governorate "]
[null,"General Specification "]
[null,"1- All the materials supplied by the contractor must be according to Iraq's standard Specifications"]
[null,"2- The contractor must provide samples , catalogues and specification of materials for testing and approval by the site engineer "]
[null,"3- Contractor must pay the cost for samples including any laboratory test required"]
[null,"4- The price of works includes all job requierements as per Iraq's standard specification."]
["#","Item Description","Unit","Qty","Price$","Total $"]
[null,"Civil Works"]
[1,"Site preparation:\nSupply of materials, tools, machineries and manpower for site preparation, by cleaning and removing all debris, rubble and dump it to locations approved by the local Authorities. ","LS",1]
[2,"Masonry works :  \nSupply materials, tools and manpower to  construct a fence by using solid blocks 15x20x40 cm, 20 cm width, 2.7m height and by using cement mortar (1:3) mix ratio, the wall should be leveled vertically and horizontally. Price of the work shall inlcude all the requirement to complete the job.    ","m²",25]
[3,"Limestone\nSupply materials, tools and manpower to install  Limestone (Hillan) for the building facade and at the entrance of the building. Quality and  texture of limestone shall be the same  as the existing one, with a width of 30 cm. The work includes the use of Ø3 mm iron (BRC) at 20x20 cm under the limestone for the purpose of strengthening. Price of the work shall include all requirements for completion of the job.","L.S",1]
[4,"Cement plastering:\nSupply materials, tools and manpower to repair wall cracks and to replace damaged cement plastering. The work includes removing the damaged cement plastering of external walls & fence, 25cm at each side of the crack, then filling the cracks with crack filler and cement mortar 1:3 and by using SBR at a rate of 200gr per m², including applying a layer of chicken wire on the area with  3 layers of cement plastering 1:3 mix ratio. Price of the work shall inlcude all requirements to complete  the job.","m²",50]
[5,"Main gate (2x2.6m):\nSupply materials , tools and manpower to install new main gate steel doors (2x2.6m), by using plate gauge16, steel frame of angel sheet dimensions 7.62x7.62 cm, 5mm thickness and steel pipe 40x40x1.5mm, including door handles, hinges and locks. Price of the work shall include painting of steel door with anti-rust and two coats of oil paints with all requirements to complete the job. See drawing nº 01","EA",1]
[6,"Repair steel doors:\nSupply materials , tools , machineries and manpower to repair the damaged steel doors. Price of the work shall include handles, hinges ,oil paint ,accessories and all requirements to complete the job.","EA",20]
[7,"Repair steel windows: \nSupply materials, tools and manpower to repair the damaged steel window, including anti-insects wire mesh.  Price of the work shall include hinges, handle and all requirements to complete the job.","EA",20]
[8,"Wooden doors (1.0x2.1m):\nSupply materials, tools and manpower to install wooden doors with dimensions 1.0x2.1m, including handles, lock , hinges and all accessories. The inner portions space of the door is not more than 12cm. Price of the work shall include, frame, painting two faces with oil paint and all requirements to complete the job.","EA",8]
[9,"Plastic painting works:\nSupply materials , tools and manpower to paint the external walls and fence with three-layer of silicon (water proof) painting . Price of the work shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",3000]
[10,"Emulsion painting works:\nSupply materials , tools and manpower to paint the interior walls with three-layer of emulsion painting . Price of the job shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",2500]
[11,"Oil Painting:\nSupply materials, tools and manpower to paint  steel doors, windows, and internal walls with a paint-stripe at 1.25m height, by using 3 layers of oil paint. Price of the work shall include all requirements to complete the job.","m²",750]
[12,"Crystal clear glass:\nSupply of materials, tools and manpower to remove the damaged glass and to install new crystal clear glass 4 mm with new paste, dumping of all debris to a site approved by local authorities, in case it is needed,  as well as all needed works to complete the job.","m²",100]
[13,"Steel stair:\nSupply materials, tools and manpower to install steel stair, width 1m by using plate 3mm, including hand rail of  90cm height. Price of work shall include anti rust and two coats of oil painting and all job requirements to complete good work. See drawing nº 03","ml",5]
[14,"Flag pole : \nSupply materials , tools and man power to install Flag pole of  6 m high by using  2.5\" (64cm) pipe. Price of the work shall include anti rust and three layers oil painting and all  requirements  to complete the job.","EA",1]
[15,"Billboard:\nSupply materials, tools and man power to install the title of the school on  frame of size 3×1 m, with good quality LED printed sticker. The frame shall be made of square pipe section 4x4 cm. Price of the work shall  include all requirements to complete the job.","EA",1]
[16,"Class title board:\nSupply materials and manpower to install class title name made of plastic sheet size 15x25 cm, using screws to fix. Price of the work shall  include all requirements to complete the job.","EA",20]
[null,"Subtotal for Civil Works"]
[null,"Sanitary works"]
[1,"Water tank: \nSupply of materials , tools and manpower to install galvanized water tank of 1400 liters capacity with plate gauge 16 cylindrical shape supported by steel base made from 2 inch angle shape . Price of the work shall include connection of the inlet and outlet pipes, fittings, Valves, float valves, accessories and all requirements to complete the job. ","EA",6]
[2,"Galvanized Iron water pipes:   \n Supply materials , tools and manpower  to inspect and repair the water network pipes (Hot & Cool) 1/2\" dia, 3/4\" dia, 1\" dia  and replace the damaged pipes using best quality one. Price of the  work shall include all pipe fittings, connection works and all accessories and requirements to complete the job.","L.S",1]
[3,"Taps:\nSupply materials, tools and manpower necessary to connect chrome water taps 1/2\" or 3/4\", water connections. Price of the works shall include all requirements to complete the job.","EA",10]
[4,"Manholes:                                                \nSupply  materials, tools and manpower to build  40x40 cm size  manholes, by using solid block of size (15x20x40)cm  with cement mortar(1: 3) mix ratio. The work includes cement plastering from inside and outside, with cover made of cast iron frame fixed with concrete slab of manhole and all requirements to complete good work . See drawing nº 04","EA",4]
[5,"Maintenance of sewerage pipes:\nSupply materials, machinary and manpower to clean the sewerage pipes net starting from the toilets groups, along manholes and the main septic tank. By using high pressure air/water to open the blockages in the network , and all requirements to complete a good work.","EA",1]
[6,"Water pump:\nSupply materials, tools and manpower to connect water pump (1hp), Q=3M³/Hrs., H=20m with, ball valve and all fitting and accessories for connection. The price of works includes all accessories needed, as well as all needed works to complete the job. See attached","EA",1]
[null,"Subtotal for Sanitary works "]
[null,"Electricals Works"]
[null,"Work includes replace the damaged wires with new suitable size , testing and operation"]
[1,"Socket Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/13A) socket switch using screws,using single core wire 1.0 kV grade  (2*2.5mm2) PVC insulated copper  installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",30]
[2,"Light Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/6A) (single , double , triple and quadruple) light switches using screws,using single core wire 1.0kV grade (2*2.5mm2) PVC copper installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",30]
[3,"Fluorescent Lighting:                \nSupplying materials, tools and manpower, to install, connect and commissioning Simple Fluorescent Lighting Fixture 1x36 W, 4 feet, (metal frame, tube and starter), using single core wire 1.0 kv grade  (2*1.5mm2) PVC insulated copper installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",280]
[4,"Lighting:                \nSupplying materials, tools and manpower, to install, connect and commissioning (220VAC/20Watt) economic light lamp with Lamp, using single core wire  1.0 kv grade (2*1.5mm2) PVC insulated copper installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",20]
[5,"Fluorescent Lamp : \nSupplying materials, tools and manpower, to install, connect and commissioning fluorescent light (120 cm) (4 Foot)  with Lamp, and starte with all accessories and requirement to implement the work entirely.","EA",20]
[6,"Fan Regulator:                                                 \nSupplying materials, tools and manpower to install, connect and commissioning best quality of  Ceiling Fans Regulator with 5 speeds/ fan speed switch/ Regulator and  all requirements to complete a good work. ","EA",10]
[7,"Exhaust fan:                                       \nSupplying materials, tools and manpower, to install, connect and commissioning of exhaust fan 6 inch (220VAC), using single core wire  1.0 kV grade(2*1.5mm2)  PVC insulated copper installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way switch (6A) with all accessories and requirement to implement the work entirely.","LS",5]
[8,"Electrical bell:                           \nSupplying materials, tools and manpower, to install, connect and commissioning of electrical bell (220VAC), using single core wire 1.0 kV grade (2*1.5mm2)  PVC insulated coppre installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using 1 Gang 2 Way Single Pole Push Switch (6A) with all accessories and requirement to implement the work entirely.","LS",2]
[9,"Main Board:\nProviding materials, installation and operation test of distribution board, enclosed metal frame made of iron sheet 1mm thickness painted with two layers of gray color oil paint free, arrange the items shown below properly, with door,  dimensions (height x width x depth: 80cm x 80 cm x 40cm), using rubber gaskets and equipped with the following items, Plastic trunck for wiring, and Bus bars 100A 4No with earth bus bar, the price also include the required, glands, screws, insulators, and etc, all items should be arranged properly, affords a high degree of safety operation,\n\nA - [(1X 100A,3Ph,4P 415V MCCB with 25 kV breaking capacity.\nB - [(6 No.) TPN,515 VAC  25A,  3Ph. MCB type].                               \nC - [(6 No.)  TP 220 VAC  25A,  1Ph. MCB type].\nD - (1 No.)Voltmeter (0- 400 V) with selector switch.\nE - (1 Set)Ammeter (0 -100 A), 100/5A with required CTs.\nF - (1 No.)Hertz meter (48- 52 )Hz.\nG - (1 No.) selector switch.\nH - (3 No.) Indicator lamp 220VAC/5A.\nI - Three-phase Kilowatt-hour meter 400V AC\nJ - (1Set)Copper Bus-Bar 100A., for lines and the half for the neutral and             earth, length for each one not less than (40)cm., with all accessories.","EA",1]
[10,"Sub Distribution Boards:\n                       Supply, installation, testing and commissioning of factory fabricated distribution boards for light/power, concealed type made of M.S sheet 16 SWG degreased, derusted, zinc phosphated finished with electrostatic powder coating, of approved colour with hinged door, lockable handle, protection plate, basbar, earth and neutral strip, complete internally wired, flexible earthing strap for door manufactured by any one of the approved manufacturers as specified and comprising as under: Distribution board (3 Phase/400V/50Hz ) , equipped with 12x1 phase ( Miniature circuit breakers) (10-16-20-25-32) Amps, with all accessories and requirement to implement the work entirely.  Supplying,Installation, testing and commissioning of for 12 ways, TPN DB (DIN type, horizontal/vertical) metal single door complete with all accessories to accommodate incoming  4 pole MCCB , 1 x 400 Amps  with electronic release, breaking capacity 25KA,, 415 volt A.C,  outgoing  SP MCB (3 x 10 Amps), (3 x 16 Amps), (2 x 20 Amps),  (2 x 25 Amps) , (2 x 32 Amps )  and Neutral tapping bar/strip on/in prefabricated  MS cubical control panel board including drilling holes, connections, fixing etc. with all accessories to complete work as required.","EA",2,null,{"$f":"E45*D45","v":0}]
[11,"Electrical water boiler:\nSupply materials, tools and manpower to install, establish, connect, and commissioning electrical heater 250 Liter,3kV with complete fittings & accessories . The work includes  Power Cable size 1.0 kV grade(3x4mm2) .lexible cable copper conductor,PVC insulation, unarmoured,best type  inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories) or using (Plastic Cable Duct PVC Trunking) extend form SDB  to the wter boiler system, with all accessories and requirement to implement the work entirely.  See attached","EA",2]
[12,"Wire:\nSupplying materials, tools and manpower to install   1.0 kV grade 2*1.5mm wire, work includes all  requirements to complete a good w. ","ml",350]
[13,"Water- cooler:                         \nSupplying materials , tools and manpower to install best quality stainless steel electrical water-cooler with three taps, water connections using screws,using single core wire PVC insulated copper 1.0 kV grade  (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",1]
[14,"Wall Mounted Split Unit Air-Conditioning:                  \nSupply, installaytion , connect and commissioning best quality  Split unit Air-conditioning (Cool & Heat) 2  ton.(24000btuh) ,  max ambiant temperature  -10 to 55° C  using  Power Cable size 1.0 kV grade (2x4mm2) .flexible cable copper conductor,PVC insulation, unarmoured,best type lay on plastic cable chanal or fixed on the wall or (ceiling) by special plastic clamps extend form the main board   to the workshop, the cabls should connected by cable lugs with all requirements & connections in both sides with switch 45  Amp , the price include steel base, installing condensation pipe with all accessories and requirements to complete a good work.In addition to the guarantee and maintenance of the unit  for two years. See attached","LS",3]
[null,"Subtotal for Electricals Works"]
[null,"Total "]

{"sheet":"BOQ#10","index":10,"n_rows":57,"n_cols":6,"rows_kept":57,"cut":false,"hidden":false,"merged":[[55,0,56,0],[56,1,56,4],[0,0,0,5],[2,1,2,5],[3,1,3,5],[4,1,4,5],[27,0,28,0],[37,0,39,0]]}
["Renovation of Rasen Primary Mixed School - Alhamdain  Sub- District - Ninawa Governorate "]
[null,"General Specification "]
[null,"1- All the materials supplied by the contractor must be according to Iraq's standard Specifications"]
[null,"2- The contractor must provide samples , catalogues and specification of materials for testing and approval by the site engineer "]
[null,"3- Contractor must pay the cost for samples including any laboratory test required"]
[null,"4- The price of works includes all job requierements as per Iraq's standard specification."]
["#","Item Description","Unit","Qty","Price$","Total $"]
[null,"Civil Works"]
[1,"Site preparation :\nSupply of materials, tools, machineries and manpower for site preparation, by cleaning and removing all debris, rubble and dump it to locations approved by the local Authorities. ","LS",1]
[2,"Masonry works :  \nSupply materials, tools and manpower to  construct a fence by using solid blocks 15x20x40 cm, 20 cm width, 2.7m height and by using cement mortar (1: 3) mix ratio, the wall should be leveled vertically and horizontally. Price of the work shall inlcude all the requirement to complete the job.    ","m²",10]
[3,"Cement plastering:\nSupply materials, tools and manpower to repair wall cracks and to replace damaged cement plastering. The work includes removing the damaged cement plastering of external walls & fence, 25cm at each side of the crack, then filling the cracks with crack filler and cement mortar 1:3 and by using SBR at a rate of 200gr per m², including applying a layer of chicken wire on the area with  3 layers of cement plastering 1:3 mix ratio. Price of the work shall inlcude all requirements to complete  the job.","m²",40]
[4,"Ceramic for walls:\nSupply of materials, tools and manpower to place a new ceramic 30x30 cm with cement morter. The price of works includes expantion joints, the removal of old damaged ceramic and dumping of all debris to a site approved by local authorities, in case it is needed, as well as all needed works to complete the job.","m²",15]
[5,"Limestone\nSupply materials, tools and manpower to install  Limestone (Hillan) for the building facade and at the entrance of the building. Quality and  texture of limestone shall be the same  as the existing one, with a width of 30 cm. The work includes the use of Ø3 mm iron (BRC) at 20x20 cm under the limestone for the purpose of strengthening. Price of the work shall include all requirements for completion of the job.","m²",20]
[6,"Main gate (2x2.6m):\nSupply materials , tools and manpower to install new main gate steel doors (2x2.6m), by using plate gauge16, steel frame of angel sheet dimensions 7.62x7.62 cm, 5mm thickness and steel pipe 40x40x1.5mm, including door handles, hinges and locks. Price of the work shall include painting of steel door with anti-rust and two coats of oil paints with all requirements to complete the job. See drawing nº 01","EA",1]
[7,"Repair steel doors:\nSupply materials , tools , machineries and manpower to repair the damaged steel doors. Price of the work shall include handles, hinges ,oil paint ,accessories and all requirements to complete the job.","EA",20]
[8,"Plastic painting works:                                  Supplying materials , tools and manpower necessary to paint the exterial walls and fence with three-layer of silicon (water proof) painting , the job includes cleaning the walls and removing the dirt and dust before painting with all requirements to complete a good work. ","m²",2500]
[9,"Emulsion Painting works:                       Supplying materials , tools and manpower necessary to paint the interior walls with three-layer of emulsion painting , the job includes cleaning the walls and removing the dirt and dust before painting with all requirements to complete a good work. ","m²",2000]
[10,"Oil Painting:                                                    Supplying materials , tools and manpower to paint the steel doors, windows, and internal walls with a paint-stripe at 1.25m height using 3 layers of oil paint, the price includes  all requirements to complete a good work. ","m²",750]
[11,"Repair PVC windows: \nSupply materials, tools and manpower to repair the damaged PVC windows, including anti-insects wire mesh.  Price of the work shall include hinges, handle and all requirements to complete the job.","EA",30]
[12,"Ceramic for walls:\nSupply of materials, tools and manpower forplacing new ceramic 30x60 cm with cement morter, by using cement mortar, filling joints by white cement mortar. All needed works to complete the job, will be included within the price.","m²",10]
[13,"Expansion joints:\nSupply of materials, tools and manpower to inject expansion joints with foam and install aluminum plate 20 cm width, with rubber between the two pieces of plates and by using screws to fix. All needed works to complete the job, will be included within the price.","ml",20]
[14,"Handrails:\nSupplyIing and installation of handrails, height of 1.20 cm with anti-rust paint and two coats of oil paint . All needed works to complete the job, will be included within the price. See drawing nº 05","ml",5]
[15,"Suspended ceiling:\nSupply of materials, tools and manpower to install false ceiling 60x60 cm (Gypsum boards), by using necessary accessories L, T sections, galvanized steel wire 2mm for fixing with the roof by screws. The price includes the removal of old damaged suspended ceiling, dumping of all debris to a site approved by local authorities, in case it is needed, as well as all needed works to complete the job.  See drawing nº 06","m²",30]
[16,"Crystal clear glass:\nSupply of materials, tools and manpower to remove the damaged glass and to install crysta clear glass 4 mm with with new paste, dumping of all debris to a site approved by local authorities, in case it is needed,  as well as all needed works to complete the job.","m²",120]
[17,"Flag pole : \nSupply materials , tools and man power to install Flag pole of  6 m high by using  2.5\" (64cm) pipe. Price of the work shall include anti rust and three layers oil painting and all  requirements  to complete the job.","EA",1]
[18,"Billboard:\nSupply materials, tools and man power to install the title of the school on  frame of size 3×1 m, with good quality LED printed sticker. The frame shall be made of square pipe section 4x4 cm. Price of the work shall  include all requirements to complete the job.","EA",1]
[19,"Class title board:\nSupply materials and manpower to install class title name made of plastic sheet size 15x25 cm, using screws to fix. Price of the work shall  include all requirements to complete the job.","EA",20]
[null,"Subtotal for Civil Works"]
[null,"Sanitary works"]
[1,"Water tank: \nSupply of materials , tools and manpower to install galvanized water tank of 1400 liters capacity with plate gauge 16 cylindrical shape supported by steel base made from 2 inch angle shape . Price of the work shall include connection of the inlet and outlet pipes, fittings, Valves, float valves, accessories and all requirements to complete the job. ","EA",4]
[2,"Galvanized Iron water pipes:   \n Supply materials , tools and manpower  to inspect and repair the water network pipes (Hot & Cool) 1/2\" dia, 3/4\" dia, 1\" dia  and replace the damaged pipes. Price of the  work shall include all pipe fittings, connection works and all accessories and requirements to complete the job.","L.S",1]
[3,"Taps:\nSupply materials, tools and manpower necessary to connect chrome water taps 1/2\" or 3/4\", water connections. Price of the works shall include all requirements to complete the job.","EA",10]
[4,"Mixer taps:\nSupply of materials, tools and manpower to install mixer taps, locks and all  accessories with complete water connections. The price of works shall include all needed works to complete the job.","EA",4]
[5,"Siphon:\nSupply of materials, tools and manpower to install siphon, locks valves and all needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",6]
[6,"Manholes:                                                \nSupply  materials, tools and manpower to build  40x40 cm size  manholes, by using solid block of size (15x20x40)cm  with cement mortar(1: 3) mix ratio. The work includes cement plastering from inside and outside, with cover made of cast iron frame fixed with concrete slab of manhole and all requirements to complete good work . See drawing nº 04","EA",4]
[7,"Maintenance of sewerage pipes:\nSupply materials, machinary and manpower to clean the sewerage pipes net starting from the toilets groups, along manholes and the main septic tank. By using high pressure air/water to open the blockages in the network , and all requirements to complete a good work.","EA",1]
[8,"Water pump:\nSupply materials, tools and manpower to connect water pump (1hp), Q=3M³/Hrs., H=20m with, ball valve and all fitting and accessories for connection. The price of works includes all accessories needed, as well as all needed works to complete the job. See attached","EA",1]
[null,"Subtotal for Sanitary works "]
[null,"Electricals Works"]
[null,"Work includes replace the damaged wires with new suitable size , testing and operation"]
[1,"Socket Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/13A) socket switch using screws,using single core copper wire 1.0 kV PVC insulated (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",30]
[2,"Light Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/6A) (single , double , triple and quadruple) light switches using screws,using single core copper wire (2*2.5mm2) 1.0 kV grade PVC insulated installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",20]
[3,"Lighting:                \nSupplying materials, tools and manpower, to install, connect and commissioning (220VAC/20Watt) economic light lamp with Lamp, using single core copper wire 1.0 Grade (2*1.5mm2) PVC insulated  installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",10]
[4,"Fluorescent Lighting:                \nSupplying materials, tools and manpower, to install, connect and commissioning Simple Fluorescent Lighting Fixture 1x36 W, 4 feet, (metal frame, tube and starter), using single core copper wire  1.0 grade PVC insulated (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",40]
[5,"Fan Regulator:                                                 \nSupplying materials, tools and manpower to install, connect and commissioning best quality of  Ceiling Fans Regulator with 5 speeds/ fan speed switch/ Regulator and  all requirements to complete a good work. ","EA",2]
[6,"Ceiling Fan:\nSupplying materials, tools and manpower to install, connect and commissioning best quality of 56\" ceiling fan with power regulator using copper cable 1.0 kV grade (2*1.5mm2) PVC insulated  installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",4]
[7,"Exhaust fan:                                       \nSupplying materials, tools and manpower, to install, connect and commissioning of exhaust fan 6 inch (220VAC), using single core copper wire (2*1.5mm2) 1.0 kV grade PVC insulated installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way switch (6A) with all accessories and requirement to implement the work entirely.","LS",4]
[8,"Electrical bell:                           \nSupplying materials, tools and manpower, to install, connect and commissioning of electrical bell (220VAC), using single core copper wire 1.0 kV grade (2*1.5mm2) PVC insulated installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using 1 Gang 2 Way Single Pole Push Switch (6A) with all accessories and requirement to implement the work entirely.","LS",2]
[9,"Main Board:\nProviding materials, installation and operation test of prefabricated distribution board, enclosed metal frame made of iron sheet 1mm thickness painted with two layers of gray color oil paint free, arrange the items shown below properly, with door,  dimensions (height x width x depth: 80cm x 80 cm x 40cm), using rubber gaskets and equipped with the following items, Plastic trunck for wiring, and Bus bars 100A 4No with earth bus bar, the price also include the required, glands, screws, insulators, and etc, all items should be arranged properly, affords a high degree of safety operation,\n\nA - [(1 No.)  100A,  3Ph.415 VAC 26 kV BC, MCCB type].\nB - [(6 No.)  25A,  3Ph. 415 VAC MCB type].\nC - [(6 No.)  25A,  1Ph.220 VAC MCB type].\nD - (1 No.)Voltmeter (0- 400 V) with selector switch.\nE - (1 Set)Ammeter (0 -100 A), 100/5A with required CTs.\nF - (1 No.)Hertz meter (48- 52 )Hz.\nG - (1 No.) selector switch.\nH - (3 No.) Indicator lamp 220VAC/5A.\nI - Three-phase Kilowatt-hour meter \nJ - (1Set)Copper Bus-Bar 100A., for lines and the half for the neutral and             earth, length for each one not less than (40)cm., with all accessories.","EA",1]
[10,"Sub Distribution Boards:\nSupplying,Installation, testing and commissioning of for TPN DB 12ways,  (DIN type, horizontal/vertical) metal single door complete with all accessories to accommodate incoming  (1x 3 pole MCB , 1 x 63 Amps, 415 volt A.C),  includes outgoing  SP MCB (3 x 10 Amps), (3 x 16 Amps), (2 x 20 Amps),  (2 x 25 Amps) , (2 x 32 Amps )  and Neutral tapping bar/strip on/in prefabricated  MS cubical control panel board including drilling holes, connections, fixing etc. with all accessories to complete work as required.","EA",2]
[11,"Electrical water boiler:\nSupply materials, tools and manpower to install, establish, connect, and commissioning electrical heater 250 Liter  3 kW with complete fittings & accessories . The work includes  Power Cable size (3x4mm2) .flexible cable copper conductor,PVC insulation,1.0 kV grade  unarmoured,best type  inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories) or using (Plastic Cable Duct PVC Trunking) extend form SDB  to the wter boiler system, with all accessories and requirement to implement the work entirely. See attached. ","LS",1]
[12,"Power Cable:\nProviding materials, installation and operation test of  Power Cable size (4x10mm2) .flexible cable copper conductor, 1.0 kV grade PVC insulation, unarmoured,best type lay on plastic cable chanal or fixed on the wall or (ceiling) by special plastic clamps extend form the main pole to the main board, the cabls should connected by cable lugs with all requirements & connections in both sides , with all accessories and requirement to implement the work entirely.","M",50]
[13,"Wire:\nSupplying materials, tools and manpower to install 1.0 kV grade PVC insulated copper  2*1.5mm2 wire, work includes all  requirements to complete a good work. ","M",500]
[14,"Water- cooler:                         \nSupplying materials , tools and manpower to install best quality stainless steel electrical water-cooler with three taps, water connections using screws,using single core copper wire (2*2.5mm2) 1.0 kV grade PVC insulated installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",3]
[15,"Wall Mounted Split Unit Air-Conditioning:                  \nSupply, installaytion , connect and commissioning best quality  Split unit Air-conditioning (Cool & Heat) 2  ton.(24000btuh) , ambiant temperature -10- 50° C  using  Power Cable size (2x4mm2) .flexible cable copper conductor,1.0 kV grade PVC insulation, unarmoured,best type lay on plastic cable chanal or fixed on the wall or (ceiling) by special plastic clamps extend form the main board   to the workshop, the cabls should connected by cable lugs with all requirements & connections in both sides with switch 45  Amp , the price include steel base, installing condensation pipe with all accessories and requirements to complete a good work.In addition to the guarantee and maintenance of the unit  for two years. See attached","LS",1]
[null,"Subtotal for Electricals Works",null,null,null,{"$f":"SUM(F41:F55)","v":0}]
[null,"Total ",null,null,null,{"$f":"F56+F38+F28","v":0}]

{"sheet":"BOQ#11","index":11,"n_rows":44,"n_cols":6,"rows_kept":44,"cut":false,"hidden":false,"merged":[[42,0,43,0],[42,1,42,4],[43,1,43,4],[0,0,0,5],[2,1,2,5],[3,1,3,5],[4,1,4,5],[18,0,19,0],[27,0,29,0]]}
["Renovation of Qaraqush (2) Kindergarten - Al Hamdanyiah  Sub- District - Ninawa Governorate "]
[null,"General Specification "]
[null,"1- All the materials supplied by the contractor must be according to Iraq's standard Specifications"]
[null,"2- The contractor must provide samples , catalogues and specification of materials for testing and approval by the site engineer "]
[null,"3- Contractor must pay the cost for samples including any laboratory test required"]
[null,"4- The price of works includes all job requierements as per Iraq's standard specification."]
["#","Item Description","Unit","Qty","Price$","Total $"]
[null,"Civil Works"]
[1,"Site preparation:\nSupply of materials, tools, machineries and manpower for site preparation, by cleaning and removing all debris, rubble and dump it to locations approved by the local Authorities. ","LS",1]
[2,"Wooden doors (1.0x2.1m):\nSupply of materials, tools and manpower to install wooden doors, dimensions 1.0x2.1m, including handles, lock , hinges and all accessories. Price of the work shall include, frame, painting two faces with oil paint and all requirements to complete the job. See drawing nº 02 ","m²",90]
[3,"Repair steel doors:\nSupply materials , tools , machineries and manpower to repair the damaged steel doors. Price of the work shall include handles, hinges, paiting, accessories and all requirements to complete the job.","EA",2]
[4,"Plastic painting works:\nSupply materials , tools and manpower to paint the external walls and fence with three-layer of silicon (water proof) painting . Price of the work shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",2500]
[5,"Emulsion painting works:\nSupply materials, tools and manpower to paint the interior walls with three-layer of emulsion painting . Price of the job shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job. Interior walls shall be painted with drawings acoording to the kindergarten's administration requirements","m²",1500]
[6,"Oil Painting:\nSupply materials, tools and manpower to paint  steel doors, windows, and internal walls with a paint-stripe at 1.25m height, by using 3 layers of oil paint. Price of the work shall include all requirements to complete the job.","m²",800]
[7,"Crystal clear glass:\nSupply of materials, tools and manpower to remove the damaged glass and to install new crystal clear glass 4 mm with new paste, dumping of all debris to a site approved by local authorities, in case it is needed,  as well as all needed works to complete the job.","m²",80]
[8,"Suspended ceiling:\nSupply of materials, tools and manpower to install false ceiling 60x60 cm (Gypsum boards), by using necessary accessories L, T sections, galvanized steel wire 2mm for fixing with the roof by screws. The price includes the removal of old damaged suspended ceiling, dumping of all debris to a site approved by local authorities, in case it is needed, as well as all needed works to complete the job.  See drawing nº 06","m²",40]
[9,"Billboard:\nSupply materials, tools and man power to install the title of the school on  frame of size 3×1 m, with good quality LED printed sticker. The frame shall be made of square pipe section 4x4 cm. Price of the work shall  include all requirements to complete the job.","EA",1]
[10,"Class title board:\nSupply materials and manpower to install class title name made of plastic sheet size 15x25 cm, using screws to fix. Price of the work shall  include all requirements to complete the job.","EA",10]
[null,"Subtotal for Civil Works"]
[null,"Sanitary works"]
[1,"Water tank: \nSupply of materials , tools and manpower to install galvanized water tank of 1400 liters capacity with plate gauge 16 cylindrical shape supported by steel base made from 2 inch angle shape . Price of the work shall include connection of the inlet and outlet pipes, fittings, Valves, float valves, accessories and all requirements to complete the job. ","EA",4]
[2,"Taps:\nSupply materials, tools and manpower necessary to connect chrome water taps 1/2\" or 3/4\", water connections. Price of the works shall include all requirements to complete the job.","EA",10]
[3,"Ceramic lavatory pedestal:\nSupply of  materials, tools and manpower to install ceramic lavatory pedestal (1 sink), mixer taps, locks valves, mirror and all needed accessories with complete water connections. All needed works to complete the job, will be included within the price.","EA",2]
[4,"Mixer taps:\nSupply of materials, tools and manpower to install mixer taps, locks and all  needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",2]
[5,"Siphon:\nSupply of materials, tools and manpower to install siphon, locks valves and all needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",6]
[6,"Maintenance of sewerage pipes:\nSupply materials, machinary and manpower to clean the sewerage pipes net starting from the toilets groups, along manholes and the main septic tank. By using high pressure air/water to open the blockages in the network , and all requirements to complete a good work.","LS",1]
[7,"Water pump:\nSupply materials, tools and manpower to connect water pump (1hp), Q=3M³/Hrs., H=20m with, ball valve and all fitting and accessories for connection. The price of works includes all accessories needed, as well as all needed works to complete the job. See attached","EA",1]
[null,"Subtotal for Sanitary works "]
[null,"Electricals Works"]
[null,"Work includes replace the damaged wires with new suitable size , testing and operation"]
[1,"Socket Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/13A) socket switch using screws,using single core PVC insulated copper wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",10]
[2,"Light Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/6A) (single , double , triple and quadruple) light switches using screws,using single core PVC insulated wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",10]
[3,"Lighting:                \nSupplying materials, tools and manpower, to install, connect and commissioning (220VAC/20Watt) economic light lamp with Lamp, using single core PVC insulated wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",25]
[4,"Fluorescent Lamp : \nSupplying materials, tools and manpower, to install, connect and commissioning fluorescent light fixture(120 cm) (4 Foot)  with Lamp, and starte with all accessories and requirement to implement the work entirely.","EA",25]
[5,"Ceiling Fan:\nSupplying materials, tools and manpower to install, connect and commissioning best quality of 56\" ceiling fan with power regulator using  PVC insulated copper cable (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",6]
[6,"Exhaust fan:\nSupplying materials, tools and manpower, to install, connect and commissioning of exhaust fan 6 inch (220VAC), using single core PVC insulated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way switch (6A) with all accessories and requirement to implement the work entirely.","LS",6]
[7,"Electrical bell:\nSupplying materials, tools and manpower, to install, connect and commissioning of electrical bell (220VAC), using single core PVC insulated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using 1 Gang 2 Way Single Pole Push Switch (6A) with all accessories and requirement to implement the work entirely.","LS",1]
[8,"Main Board:\nProviding materials, installation and operation test of distribution board, enclosed metal frame made of iron sheet 1mm thickness painted with two layers of gray color oil paint free, arrange the items shown below properly, with door,  dimensions (height x width x depth: 80cm x 80 cm x 40cm), using rubber gaskets and equipped with the following items, Plastic trunck for wiring, and Bus bars 100A 4No with earth bus bar, the price also include the required, glands, screws, insulators, and etc, all items should be arranged properly, affords a high degree of safety operation,\n\nA - [(1 No.)  100A,  3Ph.415 VAC, 25 kV BC, MCCB type].\nB - [(6 No.)  25A,  3Ph. 145 VAC MCB type].\nC - [(6 No.)  25A,  1Ph. 220 VAC MCB type].\nD - (1 No.)Voltmeter (0- 400 V) with selector switch.\nE - (1 Set)Ammeter (0 -100 A), 100/5A with required CTs.\nF - (1 No.)Hertz meter (48- 52 )Hz.\nG - (1 No.) selector switch.\nH - (3 No.) Indicator lamp 220VAC/5A.\nI - Three-phase Kilowatt-hour meter \nJ - (1Set)Copper Bus-Bar 100A., for lines and the half for the neutral and             earth, length for each one not less than (40)cm., with all accessories.","EA",1]
[9,"Sub Distribution Boards:\n                       Supply, installation, testing and commissioning of factory fabricated distribution boards for light/power, concealed type made of M.S sheet 16 SWG degreased, derusted, zinc phosphated finished with electrostatic powder coating, of approved colour with hinged door, lockable handle, protection plate, basbar, earth and neutral strip, complete internally wired, flexible earthing strap for door manufactured by any one of the approved manufacturers as specified and comprising TPN DB 12ways,  (DIN type, horizontal/vertical) metal single door complete with all accessories to accommodate incoming  (1x 3 pole MCB , 1 x 63 Amps, 415 volt A.C),  includes outgoing  SP MCB (3 x 10 Amps), (3 x 16 Amps), (2 x 20 Amps),  (2 x 25 Amps) , (2 x 32 Amps )  and Neutral tapping bar/strip on/in prefabricated  MS cubical control panel board including drilling holes, connections, fixing etc. with all accessories to complete work as required.","EA",1]
[10,"Electrical water boiler:\n Supply materials, tools and manpower to install, establish, connect, and commissioning electrical heater 250 Liter 3kW with complete fittings & accessories . The work includes  Power Cable size (3x4mm2) .flexible cable copper conductor,PVC insulation, unarmoured,best type  inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories) or using (Plastic Cable Duct PVC Trunking) extend form SDB  to the wter boiler system, with all accessories and requirement to implement the work entirely. See attached","LS",2]
[11,"Water- cooler:\nSupplying materials , tools and manpower to install best quality stainless steel electrical water-cooler with three taps, water connections using screws,using single core PVC insulated Coper wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",2]
[12," Wall Mounted Split Unit Air-Conditioning:\nSupply, installaytion , connect and commissioning best quality  Split unit Air-conditioning (Cool & Heat) 2  ton.(24000btuh) , ambiant temperature -10 to  50° C  using  Power Cable size (2x4mm2) .flexible cable copper conductor,PVC insulation, unarmoured,best type lay on plastic cable chanal or fixed on the wall or (ceiling) by special plastic clamps extend form the main board   to the workshop, the cabls should connected by cable lugs with all requirements & connections in both sides with switch 45  Amp , the price include steel base, installing condensation pipe with all accessories and requirements to complete a good work.In addition to the guarantee and maintenance of the unit  for two years. See attached","EA",2]
[null,"Subtotal for Electricals Works",null,null,null,{"$f":"SUM(F31:F42)","v":0}]
[null,"Total ",null,null,null,{"$f":"F43+F28+F19","v":0}]

{"sheet":"BOQ#12","index":12,"n_rows":51,"n_cols":6,"rows_kept":51,"cut":false,"hidden":false,"merged":[[49,0,50,0],[50,1,50,4],[0,0,0,5],[2,1,2,5],[3,1,3,5],[4,1,4,5],[25,0,26,0],[36,0,38,0]]}
["Renovation of Ashor Panepal School for Boys & Girls - Mosul Sub- District - Ninawa Governorate "]
[null,"General Specification "]
[null,"1- All the materials supplied by the contractor must be according to Iraq's standard Specifications"]
[null,"2- The contractor must provide samples , catalogues and specification of materials for testing and approval by the site engineer "]
[null,"3- Contractor must pay the cost for samples including any laboratory test required"]
[null,"4- The price of works includes all job requierements as per Iraq's standard specification."]
["#","Item Description","Unit","Qty","Price$","Total $"]
[null,"Civil Works"]
[1,"Site preparation:\nSupply of materials, tools, machineries and manpower for site preparation, by cleaning and removing all debris, rubble and dump it to locations approved by the local Authorities. ","LS",1]
[2,"Cement plastering:\nSupply materials, tools and manpower to repair wall cracks and to replace damaged cement plastering. The work includes removing the damaged cement plastering of external walls & fence, 25cm at each side of the crack, then filling the cracks with crack filler and cement mortar 1:3 and by using SBR at a rate of 200gr per m², including applying a layer of chicken wire on the area with  3 layers of cement plastering 1:3 mix ratio. Price of the work shall inlcude all requirements to complete  the job.","m²",25]
[3,"Gypsum plastering:\nSupply of all necessary materials, tools and manpower to remove the damaged gypsum plastering of internal walls & roofs and plastering with new gypsum plastering  in 2 layers minimum thickness 15mm.The work includes repairing of wall cracks by removing the damaged gypsum plastering 25cm at each side of the crack,then filling the cracks with cement morter 1:3 and using SBR at a rate of 200gr per m² , later putting a layer of plastic mesh on the area under the gypsum plastering. All needed works to complete the job, will be included within the price.","m²",50]
[4,"Steel doors (1.0x2.0m): \nSupply of materials, tools and manpower to remove old steel doors and to install new steel double face doors (1x2m), including door handles, lock, mortise, fixing a stopper on the floor or wall. Price of works shall include painting by using 2 layers anti-rust and 3 layers of oil painting with all requirements to complete the job. See drawing nº 09","EA",4]
[5,"Repair steel doors:\nSupply materials , tools , machineries and manpower to repair the damaged steel doors. Price of the work shall include handles, hinges, oil paint, accessories and all requirements to complete the job.","EA",28]
[6,"Steel windows:\nSupply of materials, tools and manpower to install new steel window (1.2x2m), with burglar protection (consisting of steel pipe frame 2\", sub dividers by using square bar 0.5\" every 15 cm). Including anti-insects wire mesh, handle and all requirements to complete the work. ","EA",10]
[7,"PVC doors (0.8x2m):\nSupply of materials, tools and manpower to remove old wooden doors and to install new PVC doors. Dimensions (0.8x2m). The price includes door handles, lock, mortise fixing asyopper on the floor or wall, accesories and all needed works to complete the job.","EA",8]
[8,"Repair steel windows: \nSupply materials, tools and manpower to repair the damaged steel window, including anti-insects wire mesh.  Price of the work shall include hinges, handle and all requirements to complete the job.","EA",2]
[9,"Room Partitions PVC panels:\nSupplying materials, tools and manpower for installing PVC partitions (3x3m), with door of dimensions (1.0x2.0m). The price of works includes accessories, and all needed requirements to complete the job. ","LS",1]
[10,"Plastic painting works:\nSupply materials , tools and manpower to paint the external walls and fence with three-layer of silicon (water proof) painting . Price of the work shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",1000]
[11,"Emulsion painting works:\nSupply materials , tools and manpower to paint the interior walls with three-layer of emulsion painting . Price of the job shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",1000]
[12,"Oil Painting:\nSupply materials, tools and manpower to paint  steel doors, windows, and internal walls with a paint-stripe at 1.25m height, by using 3 layers of oil paint. Price of the work shall include all requirements to complete the job.","m²",750]
[13,"Expansion joints:\nSupply of materials, tools and manpower to inject expansion joints with foam and install aluminum plate 20 cm width, with rubber between the two pieces of plates and by using screws to fix. All needed works to complete the job, will be included within the price.","ml",40]
[14,"Crystal clear glass:\nSupply of materials, tools and manpower to remove the damaged glass and to install crysta clear glass 4 mm with with new paste, dumping of all debris to a site approved by local authorities, in case it is needed,  as well as all needed works to complete the job.","m²",50]
[15,"Suspended ceiling:\nSupply of materials, tools and manpower to install false ceiling 60x60 cm (Gypsum boards), by using necessary accessories Z, L, T sections, galvanized steel wire 2mm for fixing with the roof by screws. The price includes the removal of old damaged suspended ceiling, dumping of all debris to a site approved by local authorities, in case it is needed, as well as all needed works to complete the job.  See drawing nº 06","m²",100]
[16,"Billboard:\nSupply materials, tools and man power to install the title of the school on  frame of size 3×1 m, with good quality LED printed sticker. The frame shall be made of square pipe section 4x4 cm. Price of the work shall  include all requirements to complete the job.","EA",1]
[17,"Class title board:\nSupply materials and manpower to install class title name made of plastic sheet size 15x25 cm, using screws to fix. Price of the work shall  include all requirements to complete the job.","EA",24]
[null,"Subtotal for Civil Works"]
[null,"Sanitary works"]
[1,"Water tank: \nSupply of materials , tools and manpower to install galvanized water tank of 1400 liters capacity with plate gauge 16 cylindrical shape supported by steel base made from 2 inch angle shape . Price of the work shall include connection of the inlet and outlet pipes, fittings, Valves, float valves, accessories and all requirements to complete the job. ","EA",3]
[2,"PPR water pipes:\nSupplying materials, tools and manpower  to inspect and repair the water net pipes (Hot & Cool) Ø1/2\", Ø3/4\", Ø1\" and to replace the damaged pipes. The work includes all pipe fittings, connection works and all accessories and requirements to complete a good work. ","ml",15]
[3,"Taps:\nSupply materials, tools and manpower necessary to connect chrome water taps 1/2\" or 3/4\", water connections. Price of the works shall include all requirements to complete the job.","EA",25]
[4,"Ceramic lavatory pedestal:\nSupply of  materials, tools and manpower to install ceramic lavatory pedestal (1 sink), mixer taps, locks valves, mirror and all needed accessories with complete water connections. All needed works to complete the job, will be included within the price.","EA",2]
[5,"Mixer taps:\nSupply of materials, tools and manpower to install mixer taps, locks and all  needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",2]
[6,"Water drinking bench:\nSupply of materials, tools and manpower to rehabilitationwater network and replacing the damaged part for the washing basin 6x1x0.4m, complete sanitary connections and all requirements to complete a good work. See drawing nº 18","EA",1]
[7,"Eastern style toilet:\nSupply of materials, tools and manpower to remove damaged easter style toilet and to install new easter style toilets, with flushing water tanks (siphon), all accessories and water connection. All needed works to complete the job, shall be included within the price.","EA",6]
[8,"Siphon:\nSupply of materials, tools and manpower to install siphon, locks valves and all needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",8]
[9,"Water pump:\nSupply materials, tools and manpower to connect water pump (1hp), Q=3M³/Hrs., H=20m with, ball valve and all fitting and accessories for connection. The price of works includes all accessories needed, as well as all needed works to complete the job. See attached","EA",150]
[null,"Subtotal for Sanitary works "]
[null,"Electricals Works"]
[null,"Work includes replace the damaged wires with new suitable size , testing and operation"]
[1,"Socket Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/13A) socket switch using screws,using single core  PVC insulated copper wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",15]
[2,"Light Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/6A) (single , double , triple and quadruple) light switches using screws,using single core PVC insulated copper wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",20]
[3,"Lighting:\nSupplying materials, tools and manpower, to install, connect and commissioning (220VAC/20Watt) economic light lamp with Lamp, using single core PVC insulated Copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",150]
[4,"Ceiling Fan:\nSupplying materials, tools and manpower to install, connect and commissioning best quality of 56\" ceiling fan with power regulator using PVC insulated copper cable (2*1.5mm) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",1]
[5,"Ceiling Fan( false ceiling)\nSupply connect and install electrical ceiling fan size 60x60 cm specially for false ceiling with remote control and multi speeds using PVC insulated copper wire size  (2*1.5mm) and all .accessories to complete the job","LS",1]
[6,"Exhaust fan:\nSupplying materials, tools and manpower, to install, connect and commissioning of exhaust fan 6 inch (220VAC), using single core PVC insulated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way switch (6A) with all accessories and requirement to implement the work entirely.","LS",4]
[7,"Electrical bell:\nSupplying materials, tools and manpower, to install, connect and commissioning of electrical bell (220VAC), using single core  PVC insulated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using 1 Gang 2 Way Single Pole Push Switch (6A) with all accessories and requirement to implement the work entirely.","LS",2]
[8,"Main Board:\nProviding materials, installation and operation test of  distribution board, enclosed metal frame made of iron sheet 1mm thickness painted with two layers of gray color oil paint free, arrange the items shown below properly, with door,  dimensions (height x width x depth: 80cm x 80 cm x 40cm), using rubber gaskets and equipped with the following items, Plastic trunck for wiring, and Bus bars 100A 4No with earth bus bar, the price also include the required, glands, screws, insulators, and etc, all items should be arranged properly, affords a high degree of safety operation,\n\nA - [(1 No.)  100A,  3Ph. 415 VAC 25 kV BC MCCB type].\nB - [(6 No.)  25A,  3Ph.145 VAC  MCB type].\nC - [(6 No.)  25A,  1Ph.220 VAC MCB type].\nD - (1 No.)Voltmeter (0- 400 V) with selector switch.\nE - (1 Set)Ammeter (0 -100 A), 100/5A with required CTs.\nF - (1 No.)Hertz meter (48- 52 )Hz.\nG - (1 No.) selector switch.\nH - (3 No.) Indicator lamp 220VAC/5A.\nI - Three-phase Kilowatt-hour meter \nJ - (1Set)Copper Bus-Bar 100A., for lines and the half for the neutral and             earth, length for each one not less than (40)cm., with all accessories.","EA",1]
[9,"Sub Distribution Boards:\nSupply, installation, testing and commissioning of factory fabricated distribution boards for light/power, concealed type made of M.S sheet 16 SWG degreased, derusted, zinc phosphated finished with electrostatic powder coating, of approved colour with hinged door, lockable handle, protection plate, basbar, earth and neutral strip, complete internally wired, flexible earthing strap for door manufactured by any one of the approved manufacturers as specified and comprising as under: Distribution board (3 Phase/400V/50Hz ) , equipped with TPN DB 12ways,  (DIN type, horizontal/vertical) metal single door complete with all accessories to accommodate incoming  (1x 3 pole MCB , 1 x 63 Amps, 415 volt A.C),  includes outgoing  SP MCB (3 x 10 Amps), (3 x 16 Amps), (2 x 20 Amps),  (2 x 25 Amps) , (2 x 32 Amps )  and Neutral tapping bar/strip on/in prefabricated  MS cubical control panel board including drilling holes, connections, fixing etc. with all accessories to complete work as required.","EA",2]
[10,"Power Cable:\nProviding materials, installation and operation test of  Power Cable size (4x10mm2) .flexible cable copper conductor,PVC insulation, unarmoured,best type lay on plastic cable chanal or fixed on the wall or (ceiling) by special plastic clamps extend form the main pole to the main board, the cabls should connected by cable lugs with all requirements & connections in both sides , with all accessories and requirement to implement the work entirely.","ml",25]
[null,"Subtotal for Electricals Works",null,null,null,{"$f":"SUM(F40:F49)","v":0}]
[null,"Total ",null,null,null,{"$f":"F50+F37+F26","v":0}]

{"sheet":"BOQ#13","index":13,"n_rows":61,"n_cols":6,"rows_kept":61,"cut":false,"hidden":false,"merged":[[43,0,44,0],[59,0,60,0],[60,1,60,4],[0,0,0,5],[2,1,2,5],[3,1,3,5],[4,1,4,5],[32,0,33,0],[41,0,42,0]]}
["Renovation of Ashur High School for Boys - Hamdanyiah Sub - District - Ninawa Governorate "]
[null,"General Specification "]
[null,"1- All the materials supplied by the contractor must be according to Iraq's standard Specifications"]
[null,"2- The contractor must provide samples , catalogues and specification of materials for testing and approval by the site engineer "]
[null,"3- Contractor must pay the cost for samples including any laboratory test required"]
[null,"4- The price of works includes all job requierements as per Iraq's standard specification."]
["#","Item Description","Unit","Qty","Price$","Total $"]
[null,"Civil Works"]
[1,"Site preparation:\nSupply of materials, tools, machineries and manpower for site preparation, by cleaning and removing all debris, rubble and dump it to locations approved by the local Authorities. ","LS",1]
[2,"Granite for stairs:\nSupplying materials, tools and manpower to place granite steps, 5 cm thickness (tread) and 3cm thickness (riser), 60cm width with 3cm nose. Length 5 meters. By using cement mortar (1:3) and grooving external edge, filling joints by white cement mortar. The price of works includes the removal of old damaged granite, as well as all needed works to complete the work.","EA",2]
[3,"Limestone :  \nSupply materials, tools and manpower to install  Limestone (Hillan) and to remplace the damaged parts of the existing one. Quality and  texture of limestone shall be the same  as the existing one. The work includes the use of galvanize wire 1mm thickness, screws and cement mortar. Price of works shall include all requirements for completion of the job.","m²",50]
[4,"Masonry works :  \nSupply materials, tools and manpower to  construct a fence by using solid blocks 15x20x40 cm, 20 cm width, 2.7m height and by using cement mortar (1: 3) mix ratio, the wall should be leveled vertically and horizontally. Price of the work shall inlcude all the requirement to complete the job.    ","m²",15]
[5,"Frosted glass:\nSupply of materials, tools and manpower to remove the damaged glass and to install new frosted glass 4 mm with new paste, dumping of all debris to a site approved by local authorities, in case it is needed,  as well as all needed works to complete the job.","m²",5]
[6,"Cement plastering:\nSupply materials, tools and manpower to repair wall cracks and to replace damaged cement plastering. The work includes removing the damaged cement plastering of external walls & fence, 25cm at each side of the crack, then filling the cracks with crack filler and cement mortar 1:3 and by using SBR at a rate of 200gr per m², including applying a layer of chicken wire on the area with  3 layers of cement plastering 1:3 mix ratio. Price of the work shall inlcude all requirements to complete  the job.","m²",110]
[7,"Gypsum plastering:\nSupply of all necessary materials, tools and manpower to remove the damaged gypsum plastering of internal walls & roofs and plastering with new gypsum plastering  in 2 layers minimum thickness 15mm.The work includes repairing of wall cracks by removing the damaged gypsum plastering 25cm at each side of the crack,then filling the cracks with cement morter 1:3 and using SBR at a rate of 200gr per m² , later putting a layer of plastic mesh on the area under the gypsum plastering. All needed works to complete the job, will be included within the price.","m²",50]
[8,"Repair main gate:\nSupplying materials, tools and manpower to repair steel main gate. The price of works includes the painting of steel door using anti-rust and oil paints with all requirements to complete a good work. ","EA",1]
[9,"Main gate (4x2m): \nSupply materials, tools and manpower to install new main gate steel doors (4x2m), by using plate gauge16, steel frame of angel sheet dimensions 7.62x7.62 cm, 5mm thickness and steel pipe 40x40x1.5mm, including door handles, hinges and locks. The price includes the removal of old damaged suspended ceiling, dumping of all debris to a site approved by local authorities, in case it is needed, as well as all needed works to complete the job.  See drawing nº 12","EA",2]
[10,"Steel doors (1.0x2.0m): \nSupply of materials, tools and manpower to remove old steel doors and to install new steel double face doors (1x2m), including door handles, lock, mortise, fixing a stopper on the floor or wall. Price of works shall include painting by using 2 layers anti-rust and 3 layers of oil painting with all requirements to complete the job. See drawing nº 09","EA",5]
[11,"Repair steel door:\nSupplying materials, tools, machineries and manpower to repair the damaged steel doors, work  includes handles, accessories and all the requirements to complete a good work.","EA",40]
[12,"Repair steel windows: \nSupply materials, tools and manpower to repair the damaged steel window, including anti-insects wire mesh.  Price of the work shall include hinges, handle and all requirements to complete the job.","EA",75]
[13,"Steel window:\nSupply and install steel windows, dimensions 100x50cm. Made of Z and T shape 1\" size, including clear cristal glass 4mm thickness.  Including anti-insects wire mesh, handle and all requirements to complete the work.","EA",40]
[14,"Maintenance of burglar steel bars:\nSupply of materials, tools and manpower to replace the damaged parts of the existing burglar steel bars, by new protection with the same texture, shape and size. Including 2 layes of anti-rust and 1 layer of oil painting, as well as all needed works to complete the job. ","m²",45]
[15,"Wooden doors (1.0x2.1m):\nSupply of materials, tools and manpower to install wooden doors, dimensions 1.0x2.1m, including handles, lock , hinges and all accessories. Price of the work shall include, frame, painting two faces with oil paint and all requirements to complete the job. See drawing nº 02 ","EA",12]
[16,"Plastic painting works:\nSupply materials , tools and manpower to paint the external walls and fence with three-layer of silicon (water proof) painting . Price of the work shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",3000]
[17,"Emulsion painting works:\nSupply materials , tools and manpower to paint the interior walls with three-layer of emulsion painting . Price of the job shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",2500]
[18,"Oil Painting:\nSupply materials, tools and manpower to paint  steel doors, windows, and internal walls with a paint-stripe at 1.25m height, by using 3 layers of oil paint. Price of the work shall include all requirements to complete the job.","m²",800]
[19,"Expansion joints:\nSupply of materials, tools and manpower to inject expansion joints with foam and install aluminum plate 20 cm width, with rubber between the two pieces of plates and by using screws to fix. All needed works to complete the job, will be included within the price.","ml",25]
[20,"Crystal clear glass:\nSupply of materials, tools and manpower to remove the damaged glass and to install new crystal clear glass 4 mm with new paste, dumping of all debris to a site approved by local authorities, in case it is needed,  as well as all needed works to complete the job.","m²",250]
[21,"Handrails:\nSupplyIing and installation of handrails, height of 1.20 cm with anti-rust paint and two coats of oil paint . All needed works to complete the job, will be included within the price. See drawing nº 05","ml",15]
[22,"Flag pole : \nSupply materials , tools and man power to install Flag pole of  6 m high by using  2.5\" (64cm) pipe. Price of the work shall include anti rust and three layers oil painting and all  requirements  to complete the job.","EA",1]
[23,"Billboard:\nSupply materials, tools and man power to install the title of the school on  frame of size 3×1 m, with good quality LED printed sticker. The frame shall be made of square pipe section 4x4 cm. Price of the work shall  include all requirements to complete the job.","EA",1]
[24,"Class title board:\nSupply materials and manpower to install class title name made of plastic sheet size 15x25 cm, using screws to fix. Price of the work shall  include all requirements to complete the job.","EA",15]
[null,"Subtotal for Civil Works"]
[null,"Sanitary works"]
[1,"Water tank: \nSupply of materials , tools and manpower to install galvanized water tank of 1400 liters capacity with plate gauge 16 cylindrical shape supported by steel base made from 2 inch angle shape . Price of the work shall include connection of the inlet and outlet pipes, fittings, Valves, float valves, accessories and all requirements to complete the job. ","EA",6]
[2,"Drain pipes:\nSupply of materials, tools and manpower for removing damaged water drain pipes and for installing new galavnized steel pipes 3\" (76mm). Including all connections and needed accesories to fix on roof and walls. Price of the work shall  include all requirements to complete the job. See attached drawing nº 14","ml",12]
[3,"Taps:\nSupply materials, tools and manpower necessary to connect chrome water taps 1/2\" or 3/4\", water connections. Price of the works shall include all requirements to complete the job.","EA",20]
[4,"Mixer taps:\nSupply of materials, tools and manpower to install mixer taps, locks and all  needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",4]
[5,"Siphon:\nSupply of materials, tools and manpower to install siphon, locks valves and all needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",2]
[6,"Maintenance of sewerage pipes:\nSupply materials, machinary and manpower to clean the sewerage pipes net starting from the toilets groups, along manholes and the main septic tank. By using high pressure air/water to open the blockages in the network , and all requirements to complete a good work.","LS",1]
[7,"Water pump:\nSupply materials, tools and manpower to connect water pump (1hp), Q=3M³/Hrs., H=20m with, ball valve and all fitting and accessories for connection. The price of works includes all accessories needed, as well as all needed works to complete the job. See attached","EA",1]
[null,"Subtotal for Sanitary works "]
[null,"Electricals Works"]
[1,"Work includes replace the damaged wires with new suitable size , testing and operation"]
[null,"Socket Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/13A) socket switch using screws,using single core PVC insulated copper wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",30]
[2,"Light Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/6A) (single , double , triple and quadruple) light switches using screws,using single core PVC isnulated copper wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",30]
[3,"Fluorescent Lighting:\nSupplying materials, tools and manpower, to install, connect and commissioning Simple Fluorescent Lighting Fixture 1x36 W, 4 feet, (metal frame, tube and starter), using single core copper PVC insulated wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",35]
[4,"Lighting:\nSupplying materials, tools and manpower, to install, connect and commissioning (220VAC/20Watt) economic light lamp with Lamp, using single core Copper PVC insulated wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",25]
[5,"Fluorescent lamp:\nSupplying materials, tools and manpower, to install, connect and commissioning best quality of fluorescent lamp fixture120 cm (4 Foot) with starter  with all requirements to complete a good work.","LS",150]
[6,"Fan Regulator:\nSupplying materials, tools and manpower to install, connect and commissioning best quality of  Ceiling Fans Regulator with 5 speeds/ fan speed switch/ Regulator and  all requirements to complete a good work. ","EA",3]
[7,"Ceiling Fan:\nSupplying materials, tools and manpower to install, connect and commissioning best quality of 56\" ceiling fan with power regulator using PVC insulated copper cable (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",8]
[8,"Exhaust fan:\nSupplying materials, tools and manpower, to install, connect and commissioning of exhaust fan 6 inch (220VAC), using single core PVC insulated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way switch (6A) with all accessories and requirement to implement the work entirely.","LS",6]
[9,"Electrical bell:\nSupplying materials, tools and manpower, to install, connect and commissioning of electrical bell (220VAC), using single core PVC insulated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using 1 Gang 2 Way Single Pole Push Switch (6A) with all accessories and requirement to implement the work entirely.","LS",2]
[10,"Main Board:\nProviding materials, installation and operation test of distribution board, enclosed metal frame made of iron sheet 1mm thickness painted with two layers of gray color oil paint free, arrange the items shown below properly, with door,  dimensions (height x width x depth: 80cm x 80 cm x 40cm), using rubber gaskets and equipped with the following items, Plastic trunck for wiring, and Bus bars 100A 4No with earth bus bar, the price also include the required, glands, screws, insulators, and etc, all items should be arranged properly, affords a high degree of safety operation,\n\nA - [(1 No.)  100A,  3Ph. 415 VAC 25 kV BC, MCCB type].\nB - [(6 No.)  25A,  3Ph.415 VAC MCB type].\nC - [(6 No.)  25A,  1Ph.220 VAC MCB type].\nD - (1 No.)Voltmeter (0- 400 V) with selector switch.\nE - (1 Set)Ammeter (0 -100 A), 100/5A with required CTs.\nF - (1 No.)Hertz meter (48- 52 )Hz.\nG - (1 No.) selector switch.\nH - (3 No.) Indicator lamp 220VAC/5A.\nI - Three-phase Kilowatt-hour meter \nJ - (1Set)Copper Bus-Bar 100A., for lines and the half for the neutral and             earth, length for each one not less than (40)cm., with all accessories.","EA",1]
[11,"Sub Distribution Boards:\nSupply, installation, testing and commissioning of factory fabricated distribution boards for light/power, concealed type made of M.S sheet 16 SWG degreased, derusted, zinc phosphated finished with electrostatic powder coating, of approved colour with hinged door, lockable handle, protection plate, basbar, earth and neutral strip, complete internally wired, flexible earthing strap for door manufactured by any one of the approved manufacturers as specified and comprising as under: Distribution board (3 Phase/400V/50Hz ) , equipped with  for TPN DB 12ways,  (DIN type, horizontal/vertical) metal single door complete with all accessories to accommodate incoming  (1x 3 pole MCB , 1 x 63 Amps, 415 volt A.C),  includes outgoing  SP MCB (3 x 10 Amps), (3 x 16 Amps), (2 x 20 Amps),  (2 x 25 Amps) , (2 x 32 Amps )  and Neutral tapping bar/strip on/in prefabricated  MS cubical control panel board including drilling holes, connections, fixing etc. with all accessories to complete work as required.","EA",2]
[12,"Power Cable:\nProviding materials, installation and operation test of  Power Cable size (4x10mm2) .flexible cable copper conductor,PVC insulation, unarmoured,best type lay on plastic cable chanal or fixed on the wall or (ceiling) by special plastic clamps extend form the main pole to the main board, the cabls should connected by cable lugs with all requirements & connections in both sides , with all accessories and requirement to implement the work entirely.","LS",65]
[13,"Electrical water boiler:\n Supply materials, tools and manpower to install, establish, connect, and commissioning electrical heater 250 Liter 3 kW with complete fittings & accessories . The work includes  Power Cable size (3x4mm2) .flexible cable copper conductor,PVC insulation, unarmoured,best type  inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories) or using (Plastic Cable Duct PVC Trunking) extend form SDB  to the wter boiler system, with all accessories and requirement to implement the work entirely. See attached","LS",1]
[14,"Water- cooler:\nSupplying materials , tools and manpower to install best quality stainless steel electrical water-cooler with three taps, water connections using screws,using single core PVC insulated copper wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",4]
[15,"Wall Mounted Split Unit Air-Conditioning:\nSupply, installaytion , connect and commissioning best quality  Split unit Air-conditioning (Cool & Heat) 2  ton.(24000btuh) ,ambiant temperature -10 to 55° C  using  Power Cable size (2x4mm2) .flexible cable copper conductor,PVC insulation, unarmoured,best type lay on plastic cable chanal or fixed on the wall or (ceiling) by special plastic clamps extend form the main board   to the workshop, the cabls should connected by cable lugs with all requirements & connections in both sides with switch 45  Amp , the price include steel base, installing condensation pipe with all accessories and requirements to complete a good work.In addition to the guarantee and maintenance of the unit  for two years. See attached","LS",2]
[null,"Subtotal for Electricals Works",null,null,null,{"$f":"SUM(F45:F59)","v":0}]
[null,"Total ",null,null,null,{"$f":"F60+F42+F33","v":0}]

{"sheet":"BOQ#14","index":14,"n_rows":57,"n_cols":6,"rows_kept":57,"cut":false,"hidden":false,"merged":[[55,0,56,0],[56,1,56,4],[0,0,0,5],[2,1,2,5],[3,1,3,5],[4,1,4,5],[29,0,30,0],[39,0,40,0]]}
["Renovation of Bagdeda Intermediate school for Boys - Mosul Sub- District - Ninawa Governorate "]
[null,"General Specification "]
[null,"1- All the materials supplied by the contractor must be according to Iraq's standard Specifications"]
[null,"2- The contractor must provide samples , catalogues and specification of materials for testing and approval by the site engineer "]
[null,"3- Contractor must pay the cost for samples including any laboratory test required"]
[null,"4- The price of works includes all job requierements as per Iraq's standard specification."]
["#","Item Description","Unit","Qty","Price$","Total $"]
[null,"Civil Works"]
[1,"Site preparation:\nSupply of materials, tools, machineries and manpower for site preparation, by cleaning and removing all debris, rubble and dump it to locations approved by the local Authorities. ","LS",1]
[2,"Masonry works :  \nSupply materials, tools and manpower to  construct a fence by using solid blocks 15x20x40 cm, 20 cm width, 2.7m height and by using cement mortar (1: 3) mix ratio, the wall should be leveled vertically and horizontally. Price of the work shall inlcude all the requirement to complete the job.    ","m²",100]
[3,"Limestone\nSupply materials, tools and manpower to install  Limestone (Hillan) for the building facade and at the entrance of the building. Quality and  texture of limestone shall be the same  as the existing one, with a width of 30 cm. The work includes the use of Ø3 mm iron (BRC) at 20x20 cm under the limestone for the purpose of strengthening. Price of the work shall include all requirements for completion of the job.","m²",35]
[4,"Ceramic for walls:\nSupply of materials, tools and manpower to place a new ceramic 30x30 cm with cement morter. The price of works includes expantion joints, the removal of old damaged ceramic and dumping of all debris to a site approved by local authorities, in case it is needed, as well as all needed works to complete the job.","m²",70]
[5,"Granite for stairs:\nSupplying materials, tools and manpower to place granite steps, 5 cm thickness (tread) and 3cm thickness (riser), 60cm width with 3cm nose. By using cement mortar (1:3) and grooving external edge, filling joints by white cement mortar. The price of works includes the removal of old damaged granite, as well as all needed works to complete the work.","ml",10]
[6,"Cement plastering:\nSupply materials, tools and manpower to repair wall cracks and to replace damaged cement plastering. The work includes removing the damaged cement plastering of external walls & fence, 25cm at each side of the crack, then filling the cracks with crack filler and cement mortar 1:3 and by using SBR at a rate of 200gr per m², including applying a layer of chicken wire on the area with  3 layers of cement plastering 1:3 mix ratio. Price of the work shall inlcude all requirements to complete  the job.","m²",30]
[7,"Gypsum plastering:\nSupply of all necessary materials, tools and manpower to remove the damaged gypsum plastering of internal walls & roofs and plastering with new gypsum plastering  in 2 layers minimum thickness 15mm.The work includes repairing of wall cracks by removing the damaged gypsum plastering 25cm at each side of the crack,then filling the cracks with cement morter 1:3 and using SBR at a rate of 200gr per m² , later putting a layer of plastic mesh on the area under the gypsum plastering. All needed works to complete the job, will be included within the price.","m²",450]
[8,"Suspended ceiling:\nSupply of materials, tools and manpower to install false ceiling 60x60 cm (Gypsum boards), by using necessary accessories Z, L, T sections, galvanized steel wire 2mm for fixing with the roof by screws. The price includes the removal of old damaged suspended ceiling, dumping of all debris to a site approved by local authorities, in case it is needed, as well as all needed works to complete the job.  See drawing nº 06","m²",150]
[9,"Main gate (4x2m): \nSupply materials, tools and manpower to install new main gate steel doors (4x2m), by using plate gauge16 and steel pipe 40x40x1.5mm, including door handles, hinges and locks. The price includes the removal of old damaged suspended ceiling, dumping of all debris to a site approved by local authorities, in case it is needed, as well as all needed works to complete the job.  See drawing nº 12","EA",2]
[10,"Steel doors (1.0x2.0m): \nSupply of materials, tools and manpower to remove old steel doors and to install new steel double face doors (1x2m), including door handles, lock, mortise, fixing a stopper on the floor or wall. Price of works shall include painting by using 2 layers anti-rust and 3 layers of oil painting with all requirements to complete the job. See drawing nº 09","EA",2]
[11,"Repair steel doors:\nSupply materials , tools , machineries and manpower to repair the damaged steel doors. Price of the work shall include handles, hinges ,oil paint ,accessories and all requirements to complete the job.","EA",23]
[12,"Room Partitions PVC panels:\nSupplying materials, tools and manpower for installing PVC partitions (3x3m), with door of dimensions (1.0x2.0m). The price of works includes accessories, and all needed requirements to complete the job. ","m²",30]
[13,"Repair PVC windows: \nSupply materials, tools and manpower to repair the damaged PVC windows, including anti-insects wire mesh.  Price of the work shall include hinges, handle and all requirements to complete the job.","EA",10]
[14,"PVC doors (0.8x2m):\nSupply of materials, tools and manpower to remove old wooden doors and to install new PVC doors. Dimensions (0.8x2m). The price includes door handles, lock, mortise fixing asyopper on the floor or wall, accesories and all needed works to complete the job.","EA",3]
[15,"Plastic painting works:\nSupply materials , tools and manpower to paint the external walls and fence with three-layer of silicon (water proof) painting . Price of the work shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",1500]
[16,"Emulsion painting works:\nSupply materials , tools and manpower to paint the interior walls with three-layer of emulsion painting . Price of the job shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",1500]
[17,"Oil Painting:\nSupply materials, tools and manpower to paint  steel doors, windows, and internal walls with a paint-stripe at 1.25m height, by using 3 layers of oil paint. Price of the work shall include all requirements to complete the job.","m²",750]
[18,"Crystal clear glass:\nSupply of materials, tools and manpower to remove the damaged glass and to install crysta clear glass 4 mm with with new paste, dumping of all debris to a site approved by local authorities, in case it is needed,  as well as all needed works to complete the job.","m²",300]
[19,"Flag pole : \nSupply materials , tools and man power to install Flag pole of  6 m high by using  2.5\" (64cm) pipe. Price of the work shall include anti rust and three layers oil painting and all  requirements  to complete the job.","EA",2]
[20,"Billboard:\nSupply materials, tools and man power to install the title of the school on  frame of size 3×1 m, with good quality LED printed sticker. The frame shall be made of square pipe section 4x4 cm. Price of the work shall  include all requirements to complete the job.","EA",2]
[21,"Class title board:\nSupply materials and manpower to install class title name made of plastic sheet size 15x25 cm, using screws to fix. Price of the work shall  include all requirements to complete the job.","EA",24]
[null,"Subtotal for Civil Works"]
[null,"Sanitary works"]
[1,"Water tank: \nSupply of materials , tools and manpower to install galvanized water tank of 1400 liters capacity with plate gauge 16 cylindrical shape supported by steel base made from 2 inch angle shape . Price of the work shall include connection of the inlet and outlet pipes, fittings, Valves, float valves, accessories and all requirements to complete the job. ","EA",4]
[2,"Drain pipes:\nSupply of materials, tools and manpower for removing damaged water drain pipes and for installing new galavnized steel pipes 3\" (76mm). Including all connections and needed accesories to fix on roof and walls. Price of the work shall  include all requirements to complete the job. See attached drawing nº 14","ml",30]
[3,"Ceramic lavatory pedestal:\nSupply of  materials, tools and manpower to install ceramic lavatory pedestal (1 sink), mixer taps, locks valves, mirror and all needed accessories with complete water connections. All needed works to complete the job, will be included within the price.","EA",4]
[4,"Mixer taps:\nSupply of materials, tools and manpower to install mixer taps, locks and all  needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",2]
[5,"Water drinking bench:\nSupply of materials, tools and manpower to rehabilitationwater network and replacing the damaged part for the washing basin 6x1x0.4m, complete sanitary connections and all requirements to complete a good work. See drawing nº 18","EA",1]
[6,"Siphon:\nSupply of materials, tools and manpower to install siphon, locks valves and all needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",4]
[7,"Maintenance of sewerage pipes:\nSupply materials, machinary and manpower to clean the sewerage pipes net starting from the toilets groups, along manholes and the main septic tank. By using high pressure air/water to open the blockages in the network , and all requirements to complete a good work.","EA",1]
[8,"Water pump:\nSupply materials, tools and manpower to connect water pump (1hp), Q=3M³/Hrs., H=20m with, ball valve and all fitting and accessories for connection. The price of works includes all accessories needed, as well as all needed works to complete the job. See attached","EA",2]
[null,"Subtotal for Sanitary works "]
[null,"Electricals Works"]
[null,"Work includes replace the damaged wires with new suitable size , testing and operation"]
[1,"Socket Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/13A) socket switch using screws,using single core PVC insulated copper wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",25]
[2,"Light Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/6A) (single , double , triple and quadruple) light switches using screws,using single core PVC insulated wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",15]
[3,"Lighting:\nSupplying materials, tools and manpower, to install, connect and commissioning (220VAC/20Watt) economic light lamp with Lamp, using single core PVC insulated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",25]
[4,"Fluorescent Lamp :\nSupplying materials, tools and manpower, to install, connect and commissioning fluorescent light fixture (120 cm) (4 Foot)  with Lamp, and starte with all accessories and requirement to implement the work entirely.","EA",100]
[5,"Ceiling Fan:\nSupplying materials, tools and manpower to install, connect and commissioning best quality of 56\" ceiling fan with power regulator using PVC insulated copper cable (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",4]
[6,"Ceiling Fan( false ceiling)\n Supply connect and install electrical ceiling fan size 60x60 cm specially for false ceiling with remote control and multi speeds using wire PVC copper insulated cable size (2*1.5mm) and all .accessories to complete the job","LS",8]
[7,"Exhaust fan:\nSupplying materials, tools and manpower, to install, connect and commissioning of exhaust fan 6 inch (220VAC), using single core PVC insulated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way switch (6A) with all accessories and requirement to implement the work entirely.","LS",6]
[8,"Electrical bell:\nSupplying materials, tools and manpower, to install, connect and commissioning of electrical bell (220VAC), using single core PVC insulated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using 1 Gang 2 Way Single Pole Push Switch (6A) with all accessories and requirement to implement the work entirely.","LS",2]
[9,"Main Board:\nProviding materials, installation and operation test of distribution board, enclosed metal frame made of iron sheet 1mm thickness painted with two layers of gray color oil paint free, arrange the items shown below properly, with door,  dimensions (height x width x depth: 80cm x 80 cm x 40cm), using rubber gaskets and equipped with the following items, Plastic trunck for wiring, and Bus bars 100A 4No with earth bus bar, the price also include the required, glands, screws, insulators, and etc, all items should be arranged properly, affords a high degree of safety operation,\n\nA - [(1 No.)  100A,  3Ph. 415 VAC 25 kV BC MCCB type].\nB - [(6 No.)  25A,  3Ph. 415 VAC MCB type].\nC - [(6 No.)  25A,  1Ph. 220 VAC MCB type].\nD - (1 No.)Voltmeter (0- 400 V) with selector switch.\nE - (1 Set)Ammeter (0 -100 A), 100/5A with required CTs.\nF - (1 No.)Hertz meter (48- 52 )Hz.\nG - (1 No.) selector switch.\nH - (3 No.) Indicator lamp 220VAC/5A.\nI - Three-phase Kilowatt-hour meter \nJ - (1Set)Copper Bus-Bar 100A., for lines and the half for the neutral and             earth, length for each one not less than (40)cm., with all accessories.","EA",1]
[10,"Sub Distribution Boards:\nSupply, installation, testing and commissioning of factory fabricated distribution boards for light/power, concealed type made of M.S sheet 16 SWG degreased, derusted, zinc phosphated finished with electrostatic powder coating, of approved colour with hinged door, lockable handle, protection plate, basbar, earth and neutral strip, complete internally wired, flexible earthing strap for door manufactured by any one of the approved manufacturers as specified and comprising as under: Distribution board (3 Phase/400V/50Hz ) , equipped with TPN DB 12ways,  (DIN type, horizontal/vertical) metal single door complete with all accessories to accommodate incoming  (1x 3 pole MCB , 1 x 63 Amps, 415 volt A.C),  includes outgoing  SP MCB (3 x 10 Amps), (3 x 16 Amps), (2 x 20 Amps),  (2 x 25 Amps) , (2 x 32 Amps )  and Neutral tapping bar/strip on/in prefabricated  MS cubical control panel board including drilling holes, connections, fixing etc. with all accessories to complete work as required.","EA",1]
[11,"Electrical water boiler:\nSupply materials, tools and manpower to install, establish, connect, and commissioning electrical heater 250 Liter 3 kW with complete fittings & accessories . The work includes  Power Cable size (3x4mm2) .flexible cable copper conductor,PVC insulation, unarmoured,best type  inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories) or using (Plastic Cable Duct PVC Trunking) extend form SDB  to the wter boiler system, with all accessories and requirement to implement the work entirely. See attached","LS",2]
[12,"Water- cooler:\nSupplying materials , tools and manpower to install best quality stainless steel electrical water-cooler with three taps, water connections using screws,using single core PVC insulated copper wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",2]
[13," Wall Mounted Split Unit Air-Conditioning:\nSupply, installaytion , connect and commissioning best quality  Split unit Air-conditioning (Cool & Heat) 2  ton.(24000btuh) ,ambiant temperature -10 to 55° C  using  Power Cable size (2x4mm2) .flexible cable copper conductor,PVC insulation, unarmoured,best type lay on plastic cable chanal or fixed on the wall or (ceiling) by special plastic clamps extend form the main board   to the workshop, the cabls should connected by cable lugs with all requirements & connections in both sides with switch 45  Amp , the price include steel base, installing condensation pipe with all accessories and requirements to complete a good work.In addition to the guarantee and maintenance of the unit  for two years. See attached","LS",4]
[null,"Subtotal for Electricals Works"]
[null,"Total "]

{"sheet":"BOQ#15","index":15,"n_rows":57,"n_cols":6,"rows_kept":57,"cut":false,"hidden":false,"merged":[[55,0,56,0],[56,1,56,4],[0,0,0,5],[2,1,2,5],[3,1,3,5],[4,1,4,5],[26,0,27,0],[37,0,38,0]]}
["Renovation of  Mareem AL Adhraa High School  - Hamdanyiah Sub- District - Ninawa Governorate "]
[null,"General Specification "]
[null,"1- All the materials supplied by the contractor must be according to Iraq's standard Specifications"]
[null,"2- The contractor must provide samples , catalogues and specification of materials for testing and approval by the site engineer "]
[null,"3- Contractor must pay the cost for samples including any laboratory test required"]
[null,"4- The price of works includes all job requierements as per Iraq's standard specification."]
["#","Item Description","Unit","Qty","Price$","Total $"]
[null,"Civil Works"]
[1,"Site preparation:\nSupply of materials, tools, machineries and manpower for site preparation, by cleaning and removing all debris, rubble and dump it to locations approved by the local Authorities. ","LS",1]
[2,"Repair main gate:\nSupplying materials, tools and manpower to repair steel main gate. The price of works includes the painting of steel door using anti-rust and oil paints with all requirements to complete a good work. ","EA",1]
[3,"Cement plastering:\nSupply materials, tools and manpower to repair wall cracks and to replace damaged cement plastering. The work includes removing the damaged cement plastering of external walls & fence, 25cm at each side of the crack, then filling the cracks with crack filler and cement mortar 1:3 and by using SBR at a rate of 200gr per m², including applying a layer of chicken wire on the area with  3 layers of cement plastering 1:3 mix ratio. Price of the work shall inlcude all requirements to complete  the job.","m²",15]
[4,"Gypsum plastering:\nSupply of all necessary materials, tools and manpower to remove the damaged gypsum plastering of internal walls & roofs and plastering with new gypsum plastering  in 2 layers minimum thickness 15mm.The work includes repairing of wall cracks by removing the damaged gypsum plastering 25cm at each side of the crack,then filling the cracks with cement morter 1:3 and using SBR at a rate of 200gr per m² , later putting a layer of plastic mesh on the area under the gypsum plastering. All needed works to complete the job, will be included within the price.","m²",15]
[5,"Main gate (4x2m): \nSupply materials, tools and manpower to install new main gate steel doors (4x2m),by using plate gauge16, steel frame of angel sheet dimensions 7.62x7.62 cm, including door handles, hinges and locks. The price includes the removal of old damaged suspended ceiling, dumping of all debris to a site approved by local authorities, in case it is needed, as well as all needed works to complete the job.  See drawing nº 12","EA",1]
[6,"Steel doors (1.0x2.0m): \nSupply of materials, tools and manpower to remove old steel doors and to install new steel double face doors (1x2m), including door handles, lock, mortise, fixing a stopper on the floor or wall. Price of works shall include painting by using 2 layers anti-rust and 3 layers of oil painting with all requirements to complete the job. See drawing nº 09","EA",2]
[7,"Repair steel doors:\nSupply materials , tools , machineries and manpower to repair the damaged steel doors. Price of the work shall include handles, hinges, paiting, accessories and all requirements to complete the job.","EA",15]
[8,"Repair steel windows: \nSupply materials, tools and manpower to repair the damaged steel window, including anti-insects wire mesh.  Price of the work shall include hinges, handle and all requirements to complete the job.","EA",45]
[9,"Wooden doors (1.0x2.1m):\nSupply of materials, tools and manpower to install wooden doors, dimensions 1.0x2.1m, including handles, lock , hinges and all accessories. Price of the work shall include, frame, painting two faces with oil paint and all requirements to complete the job. See drawing nº 02 ","EA",4]
[10,"Plastic painting works:\nSupply materials , tools and manpower to paint the external walls and fence with three-layer of silicon (water proof) painting . Price of the work shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",3500]
[11,"Emulsion painting works:\nSupply materials , tools and manpower to paint the interior walls with three-layer of emulsion painting . Price of the job shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",3000]
[12,"Oil Painting:\nSupply materials, tools and manpower to paint  steel doors, windows, and internal walls with a paint-stripe at 1.25m height, by using 3 layers of oil paint. Price of the work shall include all requirements to complete the job.","m²",1000]
[13,"Roof waterproofing:\nSupplying of materials, tools and manpower to clean, wash and paint the roof by using rubble membrane paint thinckness 2mm. The price of works shall include all requirements to complet the job.","m²",10]
[14,"Expansion joints:\nSupply of materials, tools and manpower to inject expansion joints with foam and install aluminum plate 20 cm width, with rubber between the two pieces of plates and by using screws to fix. All needed works to complete the job, will be included within the price.","ml",20]
[15,"Crystal clear glass:\nSupply of materials, tools and manpower to remove the damaged glass and to install new crystal clear glass 4 mm with new paste, dumping of all debris to a site approved by local authorities, in case it is needed,  as well as all needed works to complete the job.","m²",55]
[16,"Flag pole : \nSupply materials , tools and man power to install Flag pole of  6 m high by using  2.5\" (64cm) pipe. Price of the work shall include anti rust and three layers oil painting and all  requirements  to complete the job.","EA",1]
[17,"Billboard:\nSupply materials, tools and man power to install the title of the school on  frame of size 3×1 m, with good quality LED printed sticker. The frame shall be made of square pipe section 4x4 cm. Price of the work shall  include all requirements to complete the job.","EA",1]
[18,"Class title board:\nSupply materials and manpower to install class title name made of plastic sheet size 15x25 cm, using screws to fix. Price of the work shall  include all requirements to complete the job.","EA",20]
[null,"Subtotal for Civil Works"]
[null,"Sanitary works"]
[1,"Water tank: \nSupply of materials , tools and manpower to install galvanized water tank of 1400 liters capacity with plate gauge 16 cylindrical shape supported by steel base made from 2 inch angle shape . Price of the work shall include connection of the inlet and outlet pipes, fittings, Valves, float valves, accessories and all requirements to complete the job. ","EA",6]
[2,"Drain pipes:\nSupply of materials, tools and manpower for removing damaged water drain pipes and for installing new galavnized steel pipes 3\" (76mm). Including all connections and needed accesories to fix on roof and walls. Price of the work shall  include all requirements to complete the job. See attached drawing nº 14","ml",18]
[3,"Galvanized iron water pipes:   \n Supply materials , tools and manpower  to inspect and repair the water network pipes (Hot & Cool) 1/2\" dia, 3/4\" dia, 1\" dia  and replace the damaged pipes. Price of the  work shall include all pipe fittings, connection works and all accessories and requirements to complete the job.","LS",1]
[4,"Taps:\nSupply materials, tools and manpower necessary to connect chrome water taps 1/2\" or 3/4\", water connections. Price of the works shall include all requirements to complete the job.","EA",12]
[5,"Mixer taps:\nSupply of materials, tools and manpower to install mixer taps, locks and all  needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",2]
[6,"Water drinking bench:\nSupply of materials, tools and manpower to rehabilitationwater network and replacing the damaged part for the washing basin 6x1x0.4m, complete sanitary connections and all requirements to complete a good work. See drawing nº 18","EA",1]
[7,"Siphon:\nSupply of materials, tools and manpower to install siphon, locks valves and all needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",5]
[8,"Maintenance of sewerage pipes:\nSupply materials, machinary and manpower to clean the sewerage pipes net starting from the toilets groups, along manholes and the main septic tank. By using high pressure air/water to open the blockages in the network , and all requirements to complete a good work.","LS",1]
[9,"Water pump:\nSupply materials, tools and manpower to connect water pump (1hp), Q=3M³/Hrs., H=20m with, ball valve and all fitting and accessories for connection. The price of works includes all accessories needed, as well as all needed works to complete the job. See attached","EA",1]
[null,"Subtotal for Sanitary works "]
[null,"Electricals Works"]
[null,"Work includes replace the damaged wires with new suitable size , testing and operation"]
[1,"Socket Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/13A) socket switch using screws,using single core PVC insulated copper wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",36]
[2,"Light Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/6A) (single , double , triple and quadruple) light switches using screws,using single core PVC insulated copper wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",25]
[3,"Fluorescent Lighting:\nSupplying materials, tools and manpower, to install, connect and commissioning Simple Fluorescent Lighting Fixture 1x36 W, 4 feet, (metal frame, tube and starter), using single core PVC insulated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",35]
[4,"Lighting:\nSupplying materials, tools and manpower, to install, connect and commissioning (220VAC/20Watt) economic light lamp with Lamp, using single core PVC insulated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",15]
[5,"Fluorescent Lamp:\nSupplying materials, tools and manpower, to install, connect and commissioning fluorescent light fixture (120 cm) (4 Foot)  with Lamp, and starte with all accessories and requirement to implement the work entirely.","EA",90]
[6,"Fan Regulator:\n Supplying materials, tools and manpower to install, connect and commissioning best quality of  Ceiling Fans Regulator with 5 speeds/ fan speed switch/ Regulator and  all requirements to complete a good work. ","EA",3]
[7,"Ceiling Fan:\nSupplying materials, tools and manpower to install, connect and commissioning best quality of 56\" ceiling fan with power regulator using PVC insulated copper cable (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",4]
[8,"Exhaust fan:\nSupplying materials, tools and manpower, to install, connect and commissioning of exhaust fan 6 inch (220VAC), using single core PVC insulated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way switch (6A) with all accessories and requirement to implement the work entirely.","LS",5]
[9,"Electrical bell:\nSupplying materials, tools and manpower, to install, connect and commissioning of electrical bell (220VAC), using single core PVC insulated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using 1 Gang 2 Way Single Pole Push Switch (6A) with all accessories and requirement to implement the work entirely.","LS",2]
[10,"Main Board:\nProviding materials, installation and operation test of distribution board, enclosed metal frame made of iron sheet 1mm thickness painted with two layers of gray color oil paint free, arrange the items shown below properly, with door,  dimensions (height x width x depth: 80cm x 80 cm x 40cm), using rubber gaskets and equipped with the following items, Plastic trunck for wiring, and Bus bars 100A 4No with earth bus bar, the price also include the required, glands, screws, insulators, and etc, all items should be arranged properly, affords a high degree of safety operation,\n\nA - [(1 No.)  100A,  3Ph.415 VAC 25 kV BC, MCCB type].\nB - [(6 No.)  25A,  3Ph. 415 VAC MCB type].\nC - [(6 No.)  25A,  1Ph. 220 VAC MCB type].\nD - (1 No.)Voltmeter (0- 400 V) with selector switch.\nE - (1 Set)Ammeter (0 -100 A), 100/5A with required CTs.\nF - (1 No.)Hertz meter (48- 52 )Hz.\nG - (1 No.) selector switch.\nH - (3 No.) Indicator lamp 220VAC/5A.\nI - Three-phase Kilowatt-hour meter \nJ - (1Set)Copper Bus-Bar 100A., for lines and the half for the neutral and             earth, length for each one not less than (40)cm., with all accessories.","EA",1]
[11,"Sub Distribution Boards:\n  Supply, installation, testing and commissioning of factory fabricated distribution boards for light/power, concealed type made of M.S sheet 16 SWG degreased, derusted, zinc phosphated finished with electrostatic powder coating, of approved colour with hinged door, lockable handle, protection plate, basbar, earth and neutral strip, complete internally wired, flexible earthing strap for door manufactured by any one of the approved manufacturers as specified and comprising as under: Distribution board (3 Phase/400V/50Hz ) , equipped with TPN DB 12ways,  (DIN type, horizontal/vertical) metal single door complete with all accessories to accommodate incoming  (1x 3 pole MCB , 1 x 63 Amps, 415 volt A.C),  includes outgoing  SP MCB (3 x 10 Amps), (3 x 16 Amps), (2 x 20 Amps),  (2 x 25 Amps) , (2 x 32 Amps )  and Neutral tapping bar/strip on/in prefabricated  MS cubical control panel board including drilling holes, connections, fixing etc. with all accessories to complete work as required.","EA",3]
[12,"Power Cable:\nProviding materials, installation and operation test of  Power Cable size (4x10mm2) .flexible cable copper conductor,PVC insulation, unarmoured,best type lay on plastic cable chanal or fixed on the wall or (ceiling) by special plastic clamps extend form the main pole to the main board, the cabls should connected by cable lugs with all requirements & connections in both sides , with all accessories and requirement to implement the work entirely.","LS",75]
[13,"Electrical water boiler:\nSupply materials, tools and manpower to install, establish, connect, and commissioning electrical heater 250 Liter  3 kWwith complete fittings & accessories . The work includes  Power Cable size (3x4mm2) .flexible cable copper conductor,PVC insulation, unarmoured,best type  inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories) or using (Plastic Cable Duct PVC Trunking) extend form SDB  to the wter boiler system, with all accessories and requirement to implement the work entirely. See attached","EA",1]
[14,"Water- cooler:\nSupplying materials , tools and manpower to install best quality stainless steel electrical water-cooler with three taps, water connections using screws,using single core PVC insulated copper wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",4]
[15,"Wall Mounted Split Unit Air-Conditioning:\nSupply, installaytion , connect and commissioning best quality  Split unit Air-conditioning (Cool & Heat) 2  ton.(24000btuh) ,ambiant temperature -10 to 55° C  using  Power Cable size (2x4mm2) .flexible cable copper conductor,PVC insulation, unarmoured,best type lay on plastic cable chanal or fixed on the wall or (ceiling) by special plastic clamps extend form the main board   to the workshop, the cabls should connected by cable lugs with all requirements & connections in both sides with switch 45  Amp , the price include steel base, installing condensation pipe with all accessories and requirements to complete a good work.In addition to the guarantee and maintenance of the unit  for two years. See attached","LS",1]
[null,"Subtotal for Electricals Works"]
[null,"Total "]

{"sheet":"BOQ#16","index":16,"n_rows":59,"n_cols":6,"rows_kept":59,"cut":false,"hidden":false,"merged":[[57,0,58,0],[58,1,58,4],[0,0,0,5],[2,1,2,5],[3,1,3,5],[4,1,4,5],[29,0,30,0],[38,0,39,0]]}
["Renovation of Najd Primary School for Boys- Hamdanyiah Sub- District - Ninawa Governorate "]
[null,"General Specification "]
[null,"1- All the materials supplied by the contractor must be according to Iraq's standard Specifications"]
[null,"2- The contractor must provide samples , catalogues and specification of materials for testing and approval by the site engineer "]
[null,"3- Contractor must pay the cost for samples including any laboratory test required"]
[null,"4- The price of works includes all job requierements as per Iraq's standard specification."]
["#","Item Description","Unit","Qty","Price$","Total $"]
[null,"Civil Works"]
[1,"Site preparation:\nSupply of materials, tools, machineries and manpower for site preparation, by cleaning and removing all debris, rubble and dump it to locations approved by the local Authorities. ","LS",1]
[2,"Cement plastering:\nSupply materials, tools and manpower to repair wall cracks and to replace damaged cement plastering. The work includes removing the damaged cement plastering of external walls & fence, 25cm at each side of the crack, then filling the cracks with crack filler and cement mortar 1:3 and by using SBR at a rate of 200gr per m², including applying a layer of chicken wire on the area with  3 layers of cement plastering 1:3 mix ratio. Price of the work shall inlcude all requirements to complete  the job.","m²",45]
[3,"Gypsum plastering:\nSupply of all necessary materials, tools and manpower to remove the damaged gypsum plastering of internal walls & roofs and plastering with new gypsum plastering  in 2 layers minimum thickness 15mm.The work includes repairing of wall cracks by removing the damaged gypsum plastering 25cm at each side of the crack,then filling the cracks with cement morter 1:3 and using SBR at a rate of 200gr per m² , later putting a layer of plastic mesh on the area under the gypsum plastering. All needed works to complete the job, will be included within the price.","m²",1250]
[4,"Repair main gate:\nSupplying materials, tools and manpower to repair steel main gate. The price of works includes the painting of steel door using anti-rust and oil paints with all requirements to complete a good work. ","EA",1]
[5,"Main gate (4x2m): \nSupply materials, tools and manpower to install new main gate steel doors (4x2m), by using plate gauge16, steel frame of angel sheet dimensions 7.62x7.62 cm, including door handles, hinges and locks. The price includes the removal of old damaged suspended ceiling, dumping of all debris to a site approved by local authorities, in case it is needed, as well as all needed works to complete the job.  See drawing nº 12","EA",2]
[6,"Steel doors (1.0x2.0m): \nSupply of materials, tools and manpower to remove old steel doors and to install new steel double face doors (1x2m), including door handles, lock, mortise, fixing a stopper on the floor or wall. Price of works shall include painting by using 2 layers anti-rust and 3 layers of oil painting with all requirements to complete the job. See drawing nº 09","EA",14]
[7,"Repair steel doors:\nSupply materials , tools , machineries and manpower to repair the damaged steel doors. Price of the work shall include handles, hinges, paiting, accessories and all requirements to complete the job.","EA",33]
[8,"Repair steel windows: \nSupply materials, tools and manpower to repair the damaged steel window, including anti-insects wire mesh.  Price of the work shall include hinges, handle and all requirements to complete the job.","EA",50]
[9,"Steel window: \nSupply of materials, tools and manpower to install new steel window (1x0.5m), with burglar protection (consisting of steel pipe frame 2\", sub dividers by using square bar 0.5\" every 15 cm). Including anti-insects wire mesh, handle and all requirements to complete the work. ","EA",95]
[10,"Maintenance of burglar steel bars:\nSupply of materials, tools and manpower to replace the damaged parts of the existing burglar steel bars, by new protection with the same texture, shape and size. Including 2 layes of anti-rust and 1 layer of oil painting, as well as all needed works to complete the job. ","m²",55]
[11,"Wooden doors (1.0x2.1m):\nSupply of materials, tools and manpower to install wooden doors, dimensions 1.0x2.1m, including handles, lock , hinges and all accessories. Price of the work shall include, frame, painting two faces with oil paint and all requirements to complete the job. See drawing nº 02 ","EA",6]
[12,"Plastic painting works:\nSupply materials , tools and manpower to paint the external walls and fence with three-layer of silicon (water proof) painting . Price of the work shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",2500]
[13,"Emulsion painting works:\nSupply materials , tools and manpower to paint the interior walls with three-layer of emulsion painting . Price of the job shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",2500]
[14,"Oil Painting:\nSupply materials, tools and manpower to paint  steel doors, windows, and internal walls with a paint-stripe at 1.25m height, by using 3 layers of oil paint. Price of the work shall include all requirements to complete the job.","m²",800]
[15,"Repair Sun Shed:\nSupply of materials, tools and manpower for repairing sun shed by placing new plastic corrugated sheet 1 mm thickness. The price of works shall include all accesories and works needed to complete the job. ","m²",130]
[16,"Expansion joints:\nSupply of materials, tools and manpower to inject expansion joints with foam and install aluminum plate 20 cm width, with rubber between the two pieces of plates and by using screws to fix. All needed works to complete the job, will be included within the price.","ml",25]
[17,"Crystal clear glass:\nSupply of materials, tools and manpower to remove the damaged glass and to install new crystal clear glass 4 mm with new paste, dumping of all debris to a site approved by local authorities, in case it is needed,  as well as all needed works to complete the job.","m²",160]
[18,"Suspended ceiling:\nSupply of materials, tools and manpower to install false ceiling 60x60 cm (Gypsum boards), by using necessary accessories L, T sections, galvanized steel wire 2mm for fixing with the roof by screws. The price includes the removal of old damaged suspended ceiling, dumping of all debris to a site approved by local authorities, in case it is needed, as well as all needed works to complete the job.  See drawing nº 06","m²",350]
[19,"Flag pole : \nSupply materials , tools and man power to install Flag pole of  6 m high by using  2.5\" (64cm) pipe. Price of the work shall include anti rust and three layers oil painting and all  requirements  to complete the job.","EA",2]
[20,"Billboard:\nSupply materials, tools and man power to install the title of the school on  frame of size 3×1 m, with good quality LED printed sticker. The frame shall be made of square pipe section 4x4 cm. Price of the work shall  include all requirements to complete the job.","EA",1]
[21,"Class title board:\nSupply materials and manpower to install class title name made of plastic sheet size 15x25 cm, using screws to fix. Price of the work shall  include all requirements to complete the job.","EA",15]
[null,"Subtotal for Civil Works"]
[null,"Sanitary works"]
[1,"Water tank: \nSupply of materials , tools and manpower to install galvanized water tank of 1400 liters capacity with plate gauge 16 cylindrical shape supported by steel base made from 2 inch angle shape . Price of the work shall include connection of the inlet and outlet pipes, fittings, Valves, float valves, accessories and all requirements to complete the job. ","EA",8]
[2,"Drain pipes:\nSupply of materials, tools and manpower for removing damaged water drain pipes and for installing new galavnized steel pipes 3\" (76mm). Including all connections and needed accesories to fix on roof and walls. Price of the work shall  include all requirements to complete the job. See attached drawing nº 14","ml",10]
[3,"Galvanized iron water pipes:   \n Supply materials , tools and manpower  to inspect and repair the water network pipes (Hot & Cool) 1/2\" dia, 3/4\" dia, 1\" dia  and replace the damaged pipes. Price of the  work shall include all pipe fittings, connection works and all accessories and requirements to complete the job.","LS",1]
[4,"Taps:\nSupply materials, tools and manpower necessary to connect chrome water taps 1/2\" or 3/4\", water connections. Price of the works shall include all requirements to complete the job.","EA",30]
[5,"Siphon:\nSupply of materials, tools and manpower to install siphon, locks valves and all needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",8]
[6,"Maintenance of sewerage pipes:\nSupply materials, machinary and manpower to clean the sewerage pipes net starting from the toilets groups, along manholes and the main septic tank. By using high pressure air/water to open the blockages in the network , and all requirements to complete a good work.","LS",1]
[7,"Water pump:\nSupply materials, tools and manpower to connect water pump (1hp), Q=3M³/Hrs., H=20m with, ball valve and all fitting and accessories for connection. The price of works includes all accessories needed, as well as all needed works to complete the job. See attached","EA",1]
[null,"Subtotal for Sanitary works "]
[null,"Electricals Works"]
[null,"Work includes replace the damaged wires with new suitable size , testing and operation"]
[1,"Socket Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/13A) socket switch using screws,using single core PVC insulated copper wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",70]
[2,"Light Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/6A) (single , double , triple and quadruple) light switches using screws,using single core PVC insulated copper wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",75]
[3,"Fluorescent Lighting: \nSupplying materials, tools and manpower, to install, connect and commissioning Simple Fluorescent Lighting Fixture 1x36 W, 4 feet, (metal frame, tube and starter), using single core PVC insulated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",60]
[4,"Lighting:\nSupplying materials, tools and manpower, to install, connect and commissioning (220VAC/20Watt) economic light lamp with Lamp, using single core PVC insulated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",15]
[5,"Fluorescent lamp:\nSupplying materials, tools and manpower, to install, connect and commissioning best quality of fluorescent lamp fixtures 120 cm (4 Foot) with starter  with all requirements to complete a good work.","EA",150]
[6,"Fan Regulator:\nSupplying materials, tools and manpower to install, connect and commissioning best quality of  Ceiling Fans Regulator with 5 speeds/ fan speed switch/ Regulator and  all requirements to complete a good work. ","EA",8]
[7,"Ceiling Fan:\nSupplying materials, tools and manpower to install, connect and commissioning best quality of 56\" ceiling fan with power regulator using PVC insulaed copper cable (2*1.5mm) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",10]
[8,"Exhaust fan:\nSupplying materials, tools and manpower, to install, connect and commissioning of exhaust fan 6 inch (220VAC), using single core PVC insulated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way switch (6A) with all accessories and requirement to implement the work entirely.","LS",10]
[9,"Electrical bell:\nSupplying materials, tools and manpower, to install, connect and commissioning of electrical bell (220VAC), using single core PVC insulated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using 1 Gang 2 Way Single Pole Push Switch (6A) with all accessories and requirement to implement the work entirely.","LS",2]
[10,"Main Board:\nProviding materials, installation and operation test of distribution board, enclosed metal frame made of iron sheet 1mm thickness painted with two layers of gray color oil paint free, arrange the items shown below properly, with door,  dimensions (height x width x depth: 80cm x 80 cm x 40cm), using rubber gaskets and equipped with the following items, Plastic trunck for wiring, and Bus bars 100A 4No with earth bus bar, the price also include the required, glands, screws, insulators, and etc, all items should be arranged properly, affords a high degree of safety operation,\n\nA - [(1 No.)  100A,  3Ph.415 VAC,25 kV BC, MCCB type].\nB - [(6 No.)  25A,  3Ph. 1415 VAC MCB type].\nC - [(6 No.)  25A,  1Ph.220 VAC MCB type].\nD - (1 No.)Voltmeter (0- 400 V) with selector switch.\nE - (1 Set)Ammeter (0 -100 A), 100/5A with required CTs.\nF - (1 No.)Hertz meter (48- 52 )Hz.\nG - (1 No.) selector switch.\nH - (3 No.) Indicator lamp 220VAC/5A.\nI - Three-phase Kilowatt-hour meter \nJ - (1Set)Copper Bus-Bar 100A., for lines and the half for the neutral and             earth, length for each one not less than (40)cm., with all accessories.","EA",2]
[11,"Sub Distribution Boards:\nSupply, installation, testing and commissioning of factory fabricated distribution boards for light/power, concealed type made of M.S sheet 16 SWG degreased, derusted, zinc phosphated finished with electrostatic powder coating, of approved colour with hinged door, lockable handle, protection plate, basbar, earth and neutral strip, complete internally wired, flexible earthing strap for door manufactured by any one of the approved manufacturers as specified and comprising as under: Distribution board (3 Phase/400V/50Hz ) , equipped with  TPN DB 12ways,  (DIN type, horizontal/vertical) metal single door complete with all accessories to accommodate incoming  (1x 3 pole MCB , 1 x 63 Amps, 415 volt A.C),  includes outgoing  SP MCB (3 x 10 Amps), (3 x 16 Amps), (2 x 20 Amps),  (2 x 25 Amps) , (2 x 32 Amps )  and Neutral tapping bar/strip on/in prefabricated  MS cubical control panel board including drilling holes, connections, fixing etc. with all accessories to complete work as required.","EA",3]
[12,"Power Cable:\nProviding materials, installation and operation test of  Power Cable size (4x10mm2) .flexible cable copper conductor,PVC insulation, unarmoured,best type lay on plastic cable chanal or fixed on the wall or (ceiling) by special plastic clamps extend form the main pole to the main board, the cabls should connected by cable lugs with all requirements & connections in both sides , with all accessories and requirement to implement the work entirely.","ml",60]
[13,"Wire:\nSupply materials, Installation and operation test of Electric items below flush mounting by using PVC insulated copper wires of size (2x1.5mm2, 2x2.5mm2 and 2x4mm2)  installed inside best type of cable tray& heavy  duty PVC( 20mm & 25mm dia. 2mm) respectively  thickness conduits, circular junction box, square GI box , adapter, couplings with all accessories) the work also include switch  and all requirement to implement the works entirely.","LS",250]
[14,"Electrical water boiler:\nSupply materials, tools and manpower to install, establish, connect, and commissioning electrical heater 250 Liter 3 kW  with complete fittings & accessories . The work includes  Power Cable size (3x4mm2) .flexible cable copper conductor,PVC insulation, unarmoured,best type  inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories) or using (Plastic Cable Duct PVC Trunking) extend form SDB  to the wter boiler system, with all accessories and requirement to implement the work entirely. See attached","LS",1]
[15,"Water- cooler:\nSupplying materials , tools and manpower to install best quality stainless steel electrical water-cooler with three taps, water connections using screws,using single core PVC insulated copper wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",4]
[16,"Wall Mounted Split Unit Air-Conditioning:                  \nSupply, installaytion , connect and commissioning best quality  Split unit Air-conditioning (Cool & Heat) 2  ton.(24000btuh) ,  ambiant temperature -10 to  55° C  using  Power Cable size (2x4mm2) .flexible cable copper conductor,PVC insulation, unarmoured,best type lay on plastic cable chanal or fixed on the wall or (ceiling) by special plastic clamps extend form the main board   to the workshop, the cabls should connected by cable lugs with all requirements & connections in both sides with switch 45  Amp , the price include steel base, installing condensation pipe with all accessories and requirements to complete a good work.In addition to the guarantee and maintenance of the unit  for two years. See attached","LS",2]
[null,"Subtotal for Electricals Works"]
[null,"Total "]

{"sheet":"BOQ#17","index":17,"n_rows":61,"n_cols":6,"rows_kept":61,"cut":false,"hidden":false,"merged":[[59,0,60,0],[60,1,60,4],[0,0,0,5],[2,1,2,5],[3,1,3,5],[4,1,4,5],[31,0,32,0],[41,0,43,0]]}
["Renovation of Qaraqush High School for Boys- Hamdanyiah Sub- District - Ninawa Governorate "]
[null,"General Specification "]
[null,"1- All the materials supplied by the contractor must be according to Iraq's standard Specifications"]
[null,"2- The contractor must provide samples , catalogues and specification of materials for testing and approval by the site engineer "]
[null,"3- Contractor must pay the cost for samples including any laboratory test required"]
[null,"4- The price of works includes all job requierements as per Iraq's standard specification."]
[]
["#","Item Description","Unit","Qty","Price$","Total $"]
[null,"Civil Works"]
[1,"Site preparation:\nSupply of materials, tools, machineries and manpower for site preparation, by cleaning and removing all debris, rubble and dump it to locations approved by the local Authorities. ","LS",1]
[2,"Masonry works :  \nSupply materials, tools and manpower to  construct a fence by using solid blocks 15x20x40 cm, 20 cm width, 2.7m height and by using cement mortar (1: 3) mix ratio, the wall should be leveled vertically and horizontally. Price of the work shall inlcude all the requirement to complete the job.    ","m²",7]
[3,"Frosted glass:\nSupply of materials, tools and manpower to remove the damaged glass and to install new frosted glass 4 mm with new paste, dumping of all debris to a site approved by local authorities, in case it is needed,  as well as all needed works to complete the job.","m²",5]
[4,"Cement plastering:\nSupply materials, tools and manpower to repair wall cracks and to replace damaged cement plastering. The work includes removing the damaged cement plastering of external walls & fence, 25cm at each side of the crack, then filling the cracks with crack filler and cement mortar 1:3 and by using SBR at a rate of 200gr per m², including applying a layer of chicken wire on the area with  3 layers of cement plastering 1:3 mix ratio. Price of the work shall inlcude all requirements to complete  the job.","m²",110]
[5,"Gypsum plastering:\nSupply of all necessary materials, tools and manpower to remove the damaged gypsum plastering of internal walls & roofs and plastering with new gypsum plastering  in 2 layers minimum thickness 15mm.The work includes repairing of wall cracks by removing the damaged gypsum plastering 25cm at each side of the crack,then filling the cracks with cement morter 1:3 and using SBR at a rate of 200gr per m² , later putting a layer of plastic mesh on the area under the gypsum plastering. All needed works to complete the job, will be included within the price.","m²",90]
[6,"Repair main gate:\nSupplying materials, tools and manpower to repair steel main gate. The price of works includes the painting of steel door using anti-rust and oil paints with all requirements to complete a good work. ","EA",1]
[7,"Main gate (4x2m): \nSupply materials, tools and manpower to install new main gate steel doors (4x2m), by using plate gauge16, steel frame of angel sheet dimensions 7.62x7.62 cm, including door handles, hinges and locks. The price includes the removal of old damaged suspended ceiling, dumping of all debris to a site approved by local authorities, in case it is needed, as well as all needed works to complete the job.  See drawing nº 12","EA",1]
[8,"Steel doors (1.0x2.0m): \nSupply of materials, tools and manpower to remove old steel doors and to install new steel double face doors (1x2m), including door handles, lock, mortise, fixing a stopper on the floor or wall. Price of works shall include painting by using 2 layers anti-rust and 3 layers of oil painting with all requirements to complete the job. See drawing nº 09","EA",6]
[9,"Repair steel doors:\nSupply materials , tools , machineries and manpower to repair the damaged steel doors. Price of the work shall include handles, hinges, paiting, accessories and all requirements to complete the job.","EA",38]
[10,"Repair steel windows: \nSupply materials, tools and manpower to repair the damaged steel window, including anti-insects wire mesh.  Price of the work shall include hinges, handle and all requirements to complete the job.","EA",75]
[11,"PVC doors:\nSupply of materials, tools and manpower to remove old wooden doors and to install new PVC doors. Dimensions (1x2.0m). The price includes door handles, lock, mortise fixing asyopper on the floor or wall, accesories and all needed works to complete the job.","EA",3]
[12,"Wooden doors (1x2.1m): \nSupply materials, tools and manpower to remove old wooden doors and to install new wooden doors with handles, lock and all accessories. The inner portions space of the door is not more than 12cm. Price of the work shall include painting two faces with oil paint and all requirements to complete the job. See drawing nº 02","EA",6]
[13,"Plastic painting works:\nSupply materials , tools and manpower to paint the external walls and fence with three-layer of silicon (water proof) painting . Price of the work shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",6000]
[14,"Emulsion painting works:\nSupply materials , tools and manpower to paint the interior walls with three-layer of emulsion painting . Price of the job shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",6000]
[15,"Oil Painting:\nSupply materials, tools and manpower to paint  steel doors, windows, and internal walls with a paint-stripe at 1.25m height, by using 3 layers of oil paint. Price of the work shall include all requirements to complete the job.","m²",4000]
[16,"Expansion joints:\nSupply of materials, tools and manpower to inject expansion joints with foam and install aluminum plate 20 cm width, with rubber between the two pieces of plates and by using screws to fix. All needed works to complete the job, will be included within the price.","ml",40]
[17,"Crystal clear glass:\nSupply of materials, tools and manpower to remove the damaged glass and to install new crystal clear glass 4 mm with new paste, dumping of all debris to a site approved by local authorities, in case it is needed,  as well as all needed works to complete the job.","m²",70]
[18,"PVC Partition:   \nSupply of materials, tools and manpower to install PVC partitions. The price of works includes, windows, doors, glaas, accessories and all needed requirements to complete the job. ","m²",35]
[19,"PVC windows :                                      \nSupply of materials, tools and manpower to install PVC windows. By openig a hole on the wall and including gypsum plastering from inside and cement plastering form outside, installation of PVC windows, glass, handles and all requiered works to complete the job. ","m²",18]
[20,"Flag pole : \nSupply materials , tools and man power to install Flag pole of  6 m high by using  2.5\" (64cm) pipe. Price of the work shall include anti rust and three layers oil painting and all  requirements  to complete the job.","EA",2]
[21,"Billboard:\nSupply materials, tools and man power to install the title of the school on  frame of size 3×1 m, with good quality LED printed sticker. The frame shall be made of square pipe section 4x4 cm. Price of the work shall  include all requirements to complete the job.","EA",2]
[22,"Class title board:\nSupply materials and manpower to install class title name made of plastic sheet size 15x25 cm, using screws to fix. Price of the work shall  include all requirements to complete the job.","EA",45]
[null,"Subtotal for Civil Works"]
[null,"Sanitary works"]
[1,"Water tank: \nSupply of materials , tools and manpower to install galvanized water tank of 1400 liters capacity with plate gauge 16 cylindrical shape supported by steel base made from 2 inch angle shape . Price of the work shall include connection of the inlet and outlet pipes, fittings, Valves, float valves, accessories and all requirements to complete the job. ","EA",6]
[2,"Drain pipes:\nSupply of materials, tools and manpower for removing damaged water drain pipes and for installing new galavnized steel pipes 3\" (76mm). Including all connections and needed accesories to fix on roof and walls. Price of the work shall  include all requirements to complete the job. See attached drawing nº 14","ml",18]
[3,"Galvanized iron water pipes:   \n Supply materials , tools and manpower  to inspect and repair the water network pipes (Hot & Cool) 1/2\" dia, 3/4\" dia, 1\" dia  and replace the damaged pipes. Price of the  work shall include all pipe fittings, connection works and all accessories and requirements to complete the job.","LS",1]
[4,"Taps:\nSupply materials, tools and manpower necessary to connect chrome water taps 1/2\" or 3/4\", water connections. Price of the works shall include all requirements to complete the job.","EA",12]
[5,"Mixer taps:\nSupply of materials, tools and manpower to install mixer taps, locks and all  needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",1]
[6,"Siphon:\nSupply of materials, tools and manpower to install siphon, locks valves and all needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",9]
[7,"Maintenance of sewerage pipes:\nSupply materials, machinary and manpower to clean the sewerage pipes net starting from the toilets groups, along manholes and the main septic tank. By using high pressure air/water to open the blockages in the network , and all requirements to complete a good work.","LS",1]
[8,"Water pump:\nSupply materials, tools and manpower to connect water pump (1hp), Q=3M³/Hrs., H=20m with, ball valve and all fitting and accessories for connection. The price of works includes all accessories needed, as well as all needed works to complete the job. See attached","EA",2]
[null,"Subtotal for Sanitary works "]
[null,"Electricals Works"]
[null,"Work includes replace the damaged wires with new suitable size , testing and operation"]
[1,"Socket Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/13A) socket switch using screws,using single core PVC  insulated copper wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",20]
[2,"Light Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/6A) (single , double , triple and quadruple) light switches using screws,using single core PVC insulated copper wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",20]
[3,"Fluorescent Lighting:\nSupplying materials, tools and manpower, to install, connect and commissioning Simple Fluorescent Lighting Fixture 1x36 W, 4 feet, (metal frame, tube and starter), using single core PVC insulated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",25]
[4,"Lighting:                \nSupplying materials, tools and manpower, to install, connect and commissioning (220VAC/20Watt) economic light lamp with Lamp, using single core PVC insulated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",20]
[5,"Fluorescent lamp:\nSupplying materials, tools and manpower, to install, connect and commissioning best quality of fluorescent lamp fixture 120 cm (4 Foot) with starter  with all requirements to complete a good work.","EA",250]
[6,"Fan Regulator:\nSupplying materials, tools and manpower to install, connect and commissioning best quality of  Ceiling Fans Regulator with 5 speeds/ fan speed switch/ Regulator and  all requirements to complete a good work. ","EA",10]
[7,"Ceiling Fan:\nSupplying materials, tools and manpower to install, connect and commissioning best quality of 56\" ceiling fan with power regulator using PVC insulated copper cable (2*1.5mm) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",5]
[8,"Exhaust fan:\nSupplying materials, tools and manpower, to install, connect and commissioning of exhaust fan 6 inch (220VAC), using single core PVC insulated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way switch (6A) with all accessories and requirement to implement the work entirely.","LS",5]
[9,"Electrical bell:\nSupplying materials, tools and manpower, to install, connect and commissioning of electrical bell (220VAC), using single core PVC insulated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using 1 Gang 2 Way Single Pole Push Switch (6A) with all accessories and requirement to implement the work entirely.","LS",2]
[10,"Main Board:\nProviding materials, installation and operation test of distribution board, enclosed metal frame made of iron sheet 1mm thickness painted with two layers of gray color oil paint free, arrange the items shown below properly, with door,  dimensions (height x width x depth: 80cm x 80 cm x 40cm), using rubber gaskets and equipped with the following items, Plastic trunck for wiring, and Bus bars 100A 4No with earth bus bar, the price also include the required, glands, screws, insulators, and etc, all items should be arranged properly, affords a high degree of safety operation,\n\nA - [(1 No.)  100A,  3Ph. 415VAC,25 kV BC,MCCB type].\nB - [(6 No.)  25A,  3Ph. 415 VAC,MCB type].\nC - [(6 No.)  25A,  1Ph. 220 VAC MCB type].\nD - (1 No.)Voltmeter (0- 400 V) with selector switch.\nE - (1 Set)Ammeter (0 -100 A), 100/5A with required CTs.\nF - (1 No.)Hertz meter (48- 52 )Hz.\nG - (1 No.) selector switch.\nH - (3 No.) Indicator lamp 220VAC/5A.\nI - Three-phase Kilowatt-hour meter \nJ - (1Set)Copper Bus-Bar 100A., for lines and the half for the neutral and             earth, length for each one not less than (40)cm., with all accessories.","EA",1]
[11,"Sub Distribution Boards:\nSupply, installation, testing and commissioning of factory fabricated distribution boards for light/power, concealed type made of M.S sheet 16 SWG degreased, derusted, zinc phosphated finished with electrostatic powder coating, of approved colour with hinged door, lockable handle, protection plate, basbar, earth and neutral strip, complete internally wired, flexible earthing strap for door manufactured by any one of the approved manufacturers as specified and comprising as under: Distribution board (3 Phase/400V/50Hz ) , equipped with TPN DB 12ways,  (DIN type, horizontal/vertical) metal single door complete with all accessories to accommodate incoming  (1x 3 pole MCB , 1 x 63 Amps, 415 volt A.C),  includes outgoing  SP MCB (3 x 10 Amps), (3 x 16 Amps), (2 x 20 Amps),  (2 x 25 Amps) , (2 x 32 Amps )  and Neutral tapping bar/strip on/in prefabricated  MS cubical control panel board including drilling holes, connections, fixing etc. with all accessories to complete work as required.","EA",4]
[12,"Power Cable:\nProviding materials, installation and operation test of  Power Cable size (4x10mm2) .flexible cable copper conductor,PVC insulation, unarmoured,best type lay on plastic cable chanal or fixed on the wall or (ceiling) by special plastic clamps extend form the main pole to the main board, the cabls should connected by cable lugs with all requirements & connections in both sides , with all accessories and requirement to implement the work entirely.","LS",50]
[13,"Electrical water boiler:\nSupply materials, tools and manpower to install, establish, connect, and commissioning electrical heater 250 Liter 3 kW with complete fittings & accessories . The work includes  Power Cable size (3x4mm2) .flexible cable copper conductor,PVC insulation, unarmoured,best type  inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories) or using (Plastic Cable Duct PVC Trunking) extend form SDB  to the wter boiler system, with all accessories and requirement to implement the work entirely. See attached","LS",2]
[14,"Water- cooler:\n Supplying materials , tools and manpower to install best quality stainless steel electrical water-cooler with three taps, water connections using screws,using single core PVC insulated copper wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",4]
[15,"Wall Mounted Split Unit Air-Conditioning:\nSupply, installation , connect and commissioning best quality  Split unit Air-conditioning (Cool & Heat) 2  ton.(24000btuh) , ambiant temperature -10 to 55° C  using  Power Cable size (2x4mm2) .flexible cable copper conductor,PVC insulation, unarmoured,best type lay on plastic cable chanal or fixed on the wall or (ceiling) by special plastic clamps extend form the main board   to the workshop, the cabls should connected by cable lugs with all requirements & connections in both sides with switch 45  Amp , the price include steel base, installing condensation pipe with all accessories and requirements to complete a good work.In addition to the guarantee and maintenance of the unit  for two years. See attached","LS",2]
[null,"Subtotal for Electricals Works"]
[null,"Total "]

{"sheet":"BOQ#18","index":18,"n_rows":44,"n_cols":6,"rows_kept":44,"cut":false,"hidden":false,"merged":[[42,0,43,0],[43,1,43,4],[0,0,0,5],[2,1,2,5],[3,1,3,5],[4,1,4,5],[21,0,22,0],[28,0,29,0]]}
["Renovation of Sanharib Industrial High School for  Girls - Hamdaniah Sub- District - Ninawa Governorate "]
[null,"General Specification "]
[null,"1- All the materials supplied by the contractor must be according to Iraq's standard Specifications"]
[null,"2- The contractor must provide samples , catalogues and specification of materials for testing and approval by the site engineer "]
[null,"3- Contractor must pay the cost for samples including any laboratory test required"]
[null,"4- The price of works includes all job requierements as per Iraq's standard specification."]
["#","Item Description","Unit","Qty","Price$","Total $"]
[null,"Civil Works"]
[1,"Site preparation:\nSupply of materials, tools, machineries and manpower for site preparation, by cleaning and removing all debris, rubble and dump it to locations approved by the local Authorities. ","LS",1]
[2,"Cement plastering:\nSupply materials, tools and manpower to repair wall cracks and to replace damaged cement plastering. The work includes removing the damaged cement plastering of external walls & fence, 25cm at each side of the crack, then filling the cracks with crack filler and cement mortar 1:3 and by using SBR at a rate of 200gr per m², including applying a layer of chicken wire on the area with  3 layers of cement plastering 1:3 mix ratio. Price of the work shall inlcude all requirements to complete  the job.","m²",8]
[3,"Gypsum plastering:\nSupply of all necessary materials, tools and manpower to remove the damaged gypsum plastering of internal walls & roofs and plastering with new gypsum plastering  in 2 layers minimum thickness 15mm.The work includes repairing of wall cracks by removing the damaged gypsum plastering 25cm at each side of the crack,then filling the cracks with cement morter 1:3 and using SBR at a rate of 200gr per m² , later putting a layer of plastic mesh on the area under the gypsum plastering. All needed works to complete the job, will be included within the price.","m²",8]
[4,"Repair main gate:\nSupplying materials, tools and manpower to repair steel main gate. The price of works includes frame, the painting of steel door using anti-rust and oil paints with all requirements to complete a good work. ","EA",2]
[5,"Steel doors (1.0x2.0m): \nSupply of materials, tools and manpower to remove old steel doors and to install new steel double face doors (1x2m), including door handles, lock, mortise, fixing a stopper on the floor or wall. Price of works shall include painting by using 2 layers anti-rust and 3 layers of oil painting with all requirements to complete the job. See drawing nº 09","EA",3]
[6,"Repair steel doors:\nSupply materials , tools , machineries and manpower to repair the damaged steel doors. Price of the work shall include handles, hinges, paiting, accessories and all requirements to complete the job.","EA",5]
[7,"Plastic painting works:\nSupply materials , tools and manpower to paint the external walls and fence with three-layer of silicon (water proof) painting . Price of the work shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",1500]
[8,"Emulsion painting works:\nSupply materials , tools and manpower to paint the interior walls with three-layer of emulsion painting . Price of the job shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",1500]
[9,"Oil Painting:\nSupply materials, tools and manpower to paint  steel doors, windows, and internal walls with a paint-stripe at 1.25m height, by using 3 layers of oil paint. Price of the work shall include all requirements to complete the job.","m²",750]
[10,"Crystal clear glass:\nSupply of materials, tools and manpower to remove the damaged glass and to install new crystal clear glass 4 mm with new paste, dumping of all debris to a site approved by local authorities, in case it is needed,  as well as all needed works to complete the job.","m²",30]
[11,"Flag pole : \nSupply materials , tools and man power to install Flag pole of  6 m high by using  2.5\" (64cm) pipe. Price of the work shall include anti rust and three layers oil painting and all  requirements  to complete the job.","EA",1]
[12,"Billboard:\nSupply materials, tools and man power to install the title of the school on  frame of size 3×1 m, with good quality LED printed sticker. The frame shall be made of square pipe section 4x4 cm. Price of the work shall  include all requirements to complete the job.","EA",1]
[13,"Class title board:\nSupply materials and manpower to install class title name made of plastic sheet size 15x25 cm, using screws to fix. Price of the work shall  include all requirements to complete the job.","EA",12]
[null,"Subtotal for Civil Works"]
[null,"Sanitary works"]
[1,"Water tank: \nSupply of materials , tools and manpower to install galvanized water tank of 1400 liters capacity with plate gauge 16 cylindrical shape supported by steel base made from 2 inch angle shape . Price of the work shall include connection of the inlet and outlet pipes, fittings, Valves, float valves, accessories and all requirements to complete the job. ","EA",6]
[2,"Drain pipes:\nSupply of materials, tools and manpower for removing damaged water drain pipes and for installing new galavnized steel pipes 3\" (76mm). Including all connections and needed accesories to fix on roof and walls. Price of the work shall  include all requirements to complete the job. See attached drawing nº 14","ml",10]
[3,"Taps:\nSupply materials, tools and manpower necessary to connect chrome water taps 1/2\" or 3/4\", water connections. Price of the works shall include all requirements to complete the job.","EA",10]
[4,"Mixer taps:\nSupply of materials, tools and manpower to install mixer taps, locks and all  needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",3]
[5,"Water pump:\nSupply materials, tools and manpower to connect water pump (1hp), Q=3M³/Hrs., H=20m with, ball valve and all fitting and accessories for connection. The price of works includes all accessories needed, as well as all needed works to complete the job. See attached","EA",1]
[null,"Subtotal for Sanitary works "]
[null,"Electricals Works"]
[null,"Work includes replace the damaged wires with new suitable size , testing and operation"]
[1,"Socket Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/13A) socket switch using screws,using single core PVC insulated copper wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",45]
[2,"Light Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/6A) (single , double , triple and quadruple) light switches using screws,using single core PVC insulated copper wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",15]
[3,"Fluorescent Lighting:                \nSupplying materials, tools and manpower, to install, connect and commissioning Simple Fluorescent Lighting Fixture 1x36 W, 4 feet, (metal frame, tube and starter), using single core PVC insultated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",50]
[4,"Fluorescent lamp:                                 \nSupplying materials, tools and manpower, to install, connect and commissioning best quality of fluorescent lamp fixtures 120 cm (4 Foot) with starter  with all requirements to complete a good work.","EA",30]
[5,"Exhaust fan:                                       \nSupplying materials, tools and manpower, to install, connect and commissioning of exhaust fan 6 inch (220VAC), using single core PVC insualted copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way switch (6A) with all accessories and requirement to implement the work entirely.","LS",5]
[6,"Electrical bell:\nSupplying materials, tools and manpower, to install, connect and commissioning of electrical bell (220VAC), using single core PVC insulated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using 1 Gang 2 Way Single Pole Push Switch (6A) with all accessories and requirement to implement the work entirely.","LS",1]
[7,"Main Board:\nProviding materials, installation and operation test of distribution board, enclosed metal frame made of iron sheet 1mm thickness painted with two layers of gray color oil paint free, arrange the items shown below properly, with door,  dimensions (height x width x depth: 80cm x 80 cm x 40cm), using rubber gaskets and equipped with the following items, Plastic trunck for wiring, and Bus bars 100A 4No with earth bus bar, the price also include the required, glands, screws, insulators, and etc, all items should be arranged properly, affords a high degree of safety operation,\n\nA - [(1 No.)  100A,  3Ph. 415 VAC 25 kV BC MCCB type].\nB - [(6 No.)  25A,  3Ph 415 VAC. MCB type].\nC - [(6 No.)  25A,  1Ph.220 VAC MCB type].\nD - (1 No.)Voltmeter (0- 400 V) with selector switch.\nE - (1 Set)Ammeter (0 -100 A), 100/5A with required CTs.\nF - (1 No.)Hertz meter (48- 52 )Hz.\nG - (1 No.) selector switch.\nH - (3 No.) Indicator lamp 220VAC/5A.\nI - Three-phase Kilowatt-hour meter \nJ - (1Set)Copper Bus-Bar 100A., for lines and the half for the neutral and             earth, length for each one not less than (40)cm., with all accessories.","EA",1]
[8,"Sub Distribution Boards:\nSupply, installation, testing and commissioning of factory fabricated distribution boards for light/power, concealed type made of M.S sheet 16 SWG degreased, derusted, zinc phosphated finished with electrostatic powder coating, of approved colour with hinged door, lockable handle, protection plate, basbar, earth and neutral strip, complete internally wired, flexible earthing strap for door manufactured by any one of the approved manufacturers as specified and comprising as under: Distribution board (3 Phase/400V/50Hz ) , equipped withTPN DB 12ways,  (DIN type, horizontal/vertical) metal single door complete with all accessories to accommodate incoming  (1x 3 pole MCB , 1 x 63 Amps, 415 volt A.C),  includes outgoing  SP MCB (3 x 10 Amps), (3 x 16 Amps), (2 x 20 Amps),  (2 x 25 Amps) , (2 x 32 Amps )  and Neutral tapping bar/strip on/in prefabricated  MS cubical control panel board including drilling holes, connections, fixing etc. with all accessories to complete work as required.","EA",1]
[9,"Power Cable:\nProviding materials, installation and operation test of  Power Cable size (4x10mm2) .flexible cable copper conductor,PVC insulation, unarmoured,best type lay on plastic cable chanal or fixed on the wall or (ceiling) by special plastic clamps extend form the main pole to the main board, the cabls should connected by cable lugs with all requirements & connections in both sides , with all accessories and requirement to implement the work entirely.","ml",25]
[10,"Electrical water boiler:\nSupply materials, tools and manpower to install, establish, connect, and commissioning electrical heater 250 Liter 3 kW with complete fittings & accessories . The work includes  Power Cable size (3x4mm2) .flexible cable copper conductor,PVC insulation, unarmoured,best type  inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories) or using (Plastic Cable Duct PVC Trunking) extend form SDB  to the wter boiler system, with all accessories and requirement to implement the work entirely. See attached","LS",2]
[11,"Water- cooler:\nSupplying materials , tools and manpower to install best quality stainless steel electrical water-cooler with three taps, water connections using screws,using single core PVC insulated copper wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",3]
[null,"Subtotal for Electricals Works",null,null,null,{"$f":"SUM(F32:F42)","v":0}]
[null,"Total ",null,null,null,{"$f":"F43+F29+F22","v":0}]

{"sheet":"BOQ#19","index":19,"n_rows":46,"n_cols":6,"rows_kept":46,"cut":false,"hidden":false,"merged":[[44,0,45,0],[45,1,45,4],[0,0,2,5],[4,1,4,5],[5,1,5,5],[6,1,6,5],[21,0,22,0],[30,0,31,0]]}
["Renovation of Store for Education Directorate Hamdanyiah - Hamdanyiah Sub- District - Ninawa Governorate "]
[]
[]
[null,"General Specification "]
[null,"1- All the materials supplied by the contractor must be according to Iraq's standard Specifications"]
[null,"2- The contractor must provide samples , catalogues and specification of materials for testing and approval by the site engineer "]
[null,"3- Contractor must pay the cost for samples including any laboratory test required"]
[null,"4- The price of works includes all job requierements as per Iraq's standard specification."]
["#","Item Description","Unit","Qty","Price$","Total $"]
[null,"Civil Works"]
[1,"Site preparation:\nSupply of materials, tools, machineries and manpower for site preparation, by cleaning and removing all debris, rubble and dump it to locations approved by the local Authorities. ","LS",1]
[2,"Concrete works (Play Yard): \nSapplying materials, tools and man power and casting concrete with compressive streagth 30 Mpa, 15 cm thickness for play yards and walkways, reinforced with B.R.C (Ø4mm)  (15x15) cm, having expantion joints every 4 m in each direction , the price includes all job requirements ","m²",30]
[3,"Masonry works :  \nSupply materials, tools and manpower to  construct a fence by using solid blocks 15x20x40 cm, 20 cm width, 2.7m height and by using cement mortar (1: 3) mix ratio, the wall should be leveled vertically and horizontally. Price of the work shall inlcude all the requirement to complete the job.    ","m²",100]
[4,"Roof repairing:\nSupply of material, tools and manpower to remplace old corrugated sheet roofing and to install new panel sandwich (5 cm thickness). The pice of works shall include the repairing horizontal steel  purlins (rectangular steel pipe) by remplazing the damaged parts and by painting with anti-rust and oil paints. the price include transfer all the corrugated made sheets‬‏ to the place specified by the Directorate of Education  with all requirements to complete a good work. ","m²",1600]
[5,"Cement plastering:\nSupply materials, tools and manpower to repair wall cracks and to replace damaged cement plastering. The work includes removing the damaged cement plastering of external walls & fence, 25cm at each side of the crack, then filling the cracks with crack filler and cement mortar 1:3 and by using SBR at a rate of 200gr per m², including applying a layer of chicken wire on the area with  3 layers of cement plastering 1:3 mix ratio. Price of the work shall inlcude all requirements to complete  the job.","m²",250]
[6,"Gypsum plastering:\nSupply of all necessary materials, tools and manpower to remove the damaged gypsum plastering of internal walls & roofs and plastering with new gypsum plastering  in 2 layers minimum thickness 15mm.The work includes repairing of wall cracks by removing the damaged gypsum plastering 25cm at each side of the crack,then filling the cracks with cement morter 1:3 and using SBR at a rate of 200gr per m² , later putting a layer of plastic mesh on the area under the gypsum plastering. All needed works to complete the job, will be included within the price.","M2",40]
[7,"Repair main gate (6x6m):\nSupplying materials, tools and manpower to repair steel main gate. Dimensions 6x6m. The price of works includes the painting of steel door using anti-rust and oil paints with all requirements to complete a good work. ","EA",3]
[8,"Plastic painting works:\nSupply materials , tools and manpower to paint the external walls and fence with three-layer of silicon (water proof) painting . Price of the work shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",250]
[9,"Crystal clear glass:\nSupply of materials, tools and manpower to remove the damaged glass and to install new crystal clear glass 4 mm with new paste, dumping of all debris to a site approved by local authorities, in case it is needed,  as well as all needed works to complete the job.","m²",10]
[10,"Flag pole : \nSupply materials , tools and man power to install Flag pole of  6 m high by using  2.5\" (64cm) pipe. Price of the work shall include anti rust and three layers oil painting and all  requirements  to complete the job.","EA",2]
[11,"Billboard:\nSupply materials, tools and man power to install the title of the school on  frame of size 3×1 m, with good quality LED printed sticker. The frame shall be made of square pipe section 4x4 cm. Price of the work shall  include all requirements to complete the job.","EA",1]
[null,"Subtotal for Civil Works"]
[null,"Sanitary works"]
[1,"Water tank: \nSupply of materials , tools and manpower to install galvanized water tank of 1400 liters capacity with plate gauge 16 cylindrical shape supported by steel base made from 2 inch angle shape . Price of the work shall include connection of the inlet and outlet pipes, fittings, Valves, float valves, accessories and all requirements to complete the job. ","EA",4]
[2,"Taps:\nSupply materials, tools and manpower necessary to connect chrome water taps 1/2\" or 3/4\", water connections. Price of the works shall include all requirements to complete the job.","EA",5]
[3,"Mixer taps:\nSupply of materials, tools and manpower to install mixer taps, locks and all  needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",2]
[4,"Ceramic lavatory pedestal:\nSupply of  materials, tools and manpower to install ceramic lavatory pedestal (1 sink), mixer taps, locks valves, mirror and all needed accessories with complete water connections. All needed works to complete the job, will be included within the price.","EA",1]
[5,"Siphon:\nSupply of materials, tools and manpower to install siphon, locks valves and all needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",1]
[6,"Maintenance of sewerage pipes:\nSupply materials, machinary and manpower to clean the sewerage pipes net starting from the toilets groups, along manholes and the main septic tank. By using high pressure air/water to open the blockages in the network , and all requirements to complete a good work.","LS",1]
[7,"Water pump:\nSupply materials, tools and manpower to connect water pump (1hp), Q=3M³/Hrs., H=20m with, ball valve and all fitting and accessories for connection. The price of works includes all accessories needed, as well as all needed works to complete the job. See attached","EA",2]
[null,"Subtotal for Sanitary works ",null,null,null,{"$f":"SUM(F24:F30)","v":0}]
[null,"Electricals Works"]
[null,"Work includes replace the damaged wires with new suitable size , testing and operation"]
[1,"Socket Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/13A) socket switch using screws,using single core PVC insulated copper wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",10]
[2,"Light Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/6A) (single , double , triple and quadruple) light switches using screws,using single core PVC insulated copper wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",10]
[3,"Fluorescent Lighting:\nSupplying materials, tools and manpower, to install, connect and commissioning Simple Fluorescent Lighting Fixture 1x36 W, 4 feet, (metal frame, tube and starter), using single core PVC insulated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",100]
[4,"Outdoor Lighting:\nSupplying materials , tools and manpower to install, connect and commissioning  of  Out door lighting fixtures, Projector (220VAC/200 W), LED type, water proof, over wall mounting,  metal shape with photocell connection in the control board and all requirements to complete a good work. ","EA",30]
[5,"Ceiling Fan:\nSupplying materials, tools and manpower to install, connect and commissioning best quality of 56\" ceiling fan with power regulator using PVC insulated copper cable (2*1.5mm) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",25]
[6,"Exhaust fan:\nSupplying materials, tools and manpower, to install, connect and commissioning of exhaust fan 6 inch (220VAC), using single core PVC insulated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way switch (6A) with all accessories and requirement to implement the work entirely.","LS",4]
[7,"Main Board:\nProviding materials, installation and operation test of distribution board, enclosed metal frame made of iron sheet 1mm thickness painted with two layers of gray color oil paint free, arrange the items shown below properly, with door,  dimensions (height x width x depth: 80cm x 80 cm x 40cm), using rubber gaskets and equipped with the following items, Plastic trunck for wiring, and Bus bars 100A 4No with earth bus bar, the price also include the required, glands, screws, insulators, and etc, all items should be arranged properly, affords a high degree of safety operation,\n\nA - [(1 No.)  100A,  3Ph. 415 VAC ,25 kV BC, MCCB type].\nB - [(6 No.)  25A,  3Ph. 415 VAC MCB type].\nC - [(6 No.)  25A,  1Ph. 220 VAC MCB type].\nD - (1 No.)Voltmeter (0- 400 V) with selector switch.\nE - (1 Set)Ammeter (0 -100 A), 100/5A with required CTs.\nF - (1 No.)Hertz meter (48- 52 )Hz.\nG - (1 No.) selector switch.\nH - (3 No.) Indicator lamp 220VAC/5A.\nI - Three-phase Kilowatt-hour meter \nJ - (1Set)Copper Bus-Bar 100A., for lines and the half for the neutral and             earth, length for each one not less than (40)cm., with all accessories.","EA",1]
[8,"Sub Distribution Boards:\nSupply, installation, testing and commissioning of factory fabricated distribution boards for light/power, concealed type made of M.S sheet 16 SWG degreased, derusted, zinc phosphated finished with electrostatic powder coating, of approved colour with hinged door, lockable handle, protection plate, basbar, earth and neutral strip, complete internally wired, flexible earthing strap for door manufactured by any one of the approved manufacturers as specified and comprising as under: Distribution board (3 Phase/400V/50Hz ) , equipped with TPN DB 12ways,  (DIN type, horizontal/vertical) metal single door complete with all accessories to accommodate incoming  (1x 3 pole MCB , 1 x 63 Amps, 415 volt A.C),  includes outgoing  SP MCB (3 x 10 Amps), (3 x 16 Amps), (2 x 20 Amps),  (2 x 25 Amps) , (2 x 32 Amps )  and Neutral tapping bar/strip on/in prefabricated  MS cubical control panel board including drilling holes, connections, fixing etc. with all accessories to complete work as required.","EA",3]
[9,"Electrical water boiler:\nSupply materials, tools and manpower to install, establish, connect, and commissioning electrical heater 250 Liter 3 kW with complete fittings & accessories . The work includes  Power Cable size (3x4mm2) .flexible cable copper conductor,PVC insulation, unarmoured,best type  inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories) or using (Plastic Cable Duct PVC Trunking) extend form SDB  to the wter boiler system, with all accessories and requirement to implement the work entirely. See attached","LS",2]
[10,"Water- cooler:\nSupplying materials , tools and manpower to install best quality stainless steel electrical water-cooler with three taps, water connections using screws,using single core PVC insulated copper wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",1]
[11,"Wall Mounted Split Unit Air-Conditioning:\nSupply, installaytion , connect and commissioning best quality  Split unit Air-conditioning (Cool & Heat) 2  ton.(24000btuh) ,  ambiant temperature -10 to 55° C  using  Power Cable size (2x4mm2) .flexible cable copper conductor,PVC insulation, unarmoured,best type lay on plastic cable chanal or fixed on the wall or (ceiling) by special plastic clamps extend form the main board   to the workshop, the cabls should connected by cable lugs with all requirements & connections in both sides with switch 45  Amp , the price include steel base, installing condensation pipe with all accessories and requirements to complete a good work.In addition to the guarantee and maintenance of the unit  for two years. See attached","LS",2]
[null,"Subtotal for Electricals Works"]
[null,"Total "]

{"sheet":"BOQ#20","index":20,"n_rows":60,"n_cols":6,"rows_kept":60,"cut":false,"hidden":false,"merged":[[58,0,59,0],[59,1,59,4],[0,0,0,5],[2,1,2,5],[3,1,3,5],[4,1,4,5],[28,0,29,0],[40,0,41,0]]}
["Renovation of Ur for Boys- Hamdanyiah Sub- District - Ninawa Governorate "]
[null,"General Specification "]
[null,"1- All the materials supplied by the contractor must be according to Iraq's standard Specifications"]
[null,"2- The contractor must provide samples , catalogues and specification of materials for testing and approval by the site engineer "]
[null,"3- Contractor must pay the cost for samples including any laboratory test required"]
[null,"4- The price of works includes all job requierements as per Iraq's standard specification."]
["#","Item Description","Unit","Qty","Price$","Total $"]
[null,"Civil Works"]
[1,"Site preparation:\nSupply of materials, tools, machineries and manpower for site preparation, by cleaning and removing all debris, rubble and dump it to locations approved by the local Authorities. ","LS",1]
[2,"Concrete works (Play Yard): \nSapplying materials, tools and man power and casting concrete with compressive streagth 30 Mpa, 15 cm thickness for play yards and walkways, reinforced with B.R.C (Ø4mm)  (15x15) cm, having expantion joints every 4 m in each direction , the price includes all job requirements ","m²",200]
[3,"Cement plastering:\nSupply materials, tools and manpower to repair wall cracks and to replace damaged cement plastering. The work includes removing the damaged cement plastering of external walls & fence, 25cm at each side of the crack, then filling the cracks with crack filler and cement mortar 1:3 and by using SBR at a rate of 200gr per m², including applying a layer of chicken wire on the area with  3 layers of cement plastering 1:3 mix ratio. Price of the work shall inlcude all requirements to complete  the job.","m²",15]
[4,"Gypsum plastering:\nSupply of all necessary materials, tools and manpower to remove the damaged gypsum plastering of internal walls & roofs and plastering with new gypsum plastering  in 2 layers minimum thickness 15mm.The work includes repairing of wall cracks by removing the damaged gypsum plastering 25cm at each side of the crack,then filling the cracks with cement morter 1:3 and using SBR at a rate of 200gr per m² , later putting a layer of plastic mesh on the area under the gypsum plastering. All needed works to complete the job, will be included within the price.","m²",15]
[5,"Repair main gate:\nSupplying materials, tools and manpower to repair steel main gate. The price of works includes the painting of steel door using anti-rust and oil paints with all requirements to complete a good work. ","EA",1]
[6,"Main gate (4x2m): \nSupply materials, tools and manpower to install new main gate steel doors (4x2m),by using plate gauge16, steel frame of angel sheet dimensions 7.62x7.62 cm, 5mm thickness and steel pipe 40x40x1.5mm. The price includes the removal of old damaged suspended ceiling, dumping of all debris to a site approved by local authorities, in case it is needed, as well as all needed works to complete the job.  See drawing nº 12","EA",1]
[7,"Steel doors (1.0x2.0m): \nSupply of materials, tools and manpower to remove old steel doors and to install new steel double face doors (1x2m), including door handles, lock, mortise, fixing a stopper on the floor or wall. Price of works shall include painting by using 2 layers anti-rust and 3 layers of oil painting with all requirements to complete the job. See drawing nº 09","EA",5]
[8,"Repair steel doors:\nSupply materials , tools , machineries and manpower to repair the damaged steel doors. Price of the work shall include handles, hinges, paiting, accessories and all requirements to complete the job.","EA",26]
[9,"Repair steel windows: \nSupply materials, tools and manpower to repair the damaged steel window, including anti-insects wire mesh.  Price of the work shall include hinges, handle and all requirements to complete the job.","EA",55]
[10,"Wooden doors (1.0x2.1m):\nSupply of materials, tools and manpower to install wooden doors, dimensions 1.0x2.1m, including handles, lock , hinges and all accessories. Price of the work shall include, frame, painting two faces with oil paint and all requirements to complete the job. See drawing nº 02 ","EA",5]
[11,"Repair Sun Shed:\nSupply of materials, tools and manpower for repairing sun shed by placing new plastic corrugated sheet 1 mm thickness. The price of works shall include all accesories and works needed to complete the job. ","m²",130]
[12,"Plastic painting works:\nSupply materials , tools and manpower to paint the external walls and fence with three-layer of silicon (water proof) painting . Price of the work shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",3000]
[13,"Emulsion painting works:\nSupply materials , tools and manpower to paint the interior walls with three-layer of emulsion painting . Price of the job shall include cleaning the walls and removing the dirt and dust before painting with all requirements to complete the job.","m²",3000]
[14,"Oil Painting:\nSupply materials, tools and manpower to paint  steel doors, windows, and internal walls with a paint-stripe at 1.25m height, by using 3 layers of oil paint. Price of the work shall include all requirements to complete the job.","m²",850]
[15,"Expansion joints:\nSupply of materials, tools and manpower to inject expansion joints with foam and install aluminum plate 20 cm width, with rubber between the two pieces of plates and by using screws to fix. All needed works to complete the job, will be included within the price.","ml",20]
[16,"Crystal clear glass:\nSupply of materials, tools and manpower to remove the damaged glass and to install new crystal clear glass 4 mm with new paste, dumping of all debris to a site approved by local authorities, in case it is needed,  as well as all needed works to complete the job.","m²",180]
[17,"Porcelanic tiling:\nSupplying materials, tools and manpower to remove the damaged and broken porcelain floor tiles and to place new tiles (30x30cm), by using cement mortar, expantion joints every 5m and filling joints by white cement mortar.All needed works to complete the job, will be included within the price.","m²",30]
[18,"Flag pole : \nSupply materials , tools and man power to install Flag pole of  6 m high by using  2.5\" (64cm) pipe. Price of the work shall include anti rust and three layers oil painting and all  requirements  to complete the job.","EA",2]
[19,"Billboard:\nSupply materials, tools and man power to install the title of the school on  frame of size 3×1 m, with good quality LED printed sticker. The frame shall be made of square pipe section 4x4 cm. Price of the work shall  include all requirements to complete the job.","EA",2]
[20,"Class title board:\nSupply materials and manpower to install class title name made of plastic sheet size 15x25 cm, using screws to fix. Price of the work shall  include all requirements to complete the job.","EA",30]
[null,"Subtotal for Civil Works"]
[null,"Sanitary works"]
[1,"Water tank: \nSupply of materials , tools and manpower to install galvanized water tank of 1400 liters capacity with plate gauge 16 cylindrical shape supported by steel base made from 2 inch angle shape . Price of the work shall include connection of the inlet and outlet pipes, fittings, Valves, float valves, accessories and all requirements to complete the job. ","EA",6]
[2,"Drain pipes:\nSupply of materials, tools and manpower for removing damaged water drain pipes and for installing new galavnized steel pipes 3\" (76mm). Including all connections and needed accesories to fix on roof and walls. Price of the work shall  include all requirements to complete the job. See attached drawing nº 14","ml",18]
[3,"Galvanized iron water pipes:   \n Supply materials , tools and manpower  to inspect and repair the water network pipes (Hot & Cool) 1/2\" dia, 3/4\" dia, 1\" dia  and replace the damaged pipes. Price of the  work shall include all pipe fittings, connection works and all accessories and requirements to complete the job.","LS",1]
[4,"Taps:\nSupply materials, tools and manpower necessary to connect chrome water taps 1/2\" or 3/4\", water connections. Price of the works shall include all requirements to complete the job.","EA",30]
[5,"Ceramic lavatory pedestal:\nSupply of  materials, tools and manpower to install ceramic lavatory pedestal (1 sink), mixer taps, locks valves, mirror and all needed accessories with complete water connections. All needed works to complete the job, will be included within the price.","EA",4]
[6,"Water drinking bench:\nSupply of materials, tools and manpower to rehabilitationwater network and replacing the damaged part for the washing basin 6x1x0.4m, complete sanitary connections and all requirements to complete a good work. See drawing nº 18","EA",3]
[7,"Eastern style toilet:\nSupply of materials, tools and manpower to remove damaged eastern style toilets with flushing water tanks (siphon), and install new toilets with all accessories, gully trap and water connection. All needed works to complete the job, shall be included within the price.","EA",3]
[8,"Siphon:\nSupply of materials, tools and manpower to install siphon, locks valves and all needed accessories for completing water connections. All needed works to complete the job, will be included within the price.","EA",4]
[9,"Maintenance of sewerage pipes:\nSupply materials, machinary and manpower to clean the sewerage pipes net starting from the toilets groups, along manholes and the main septic tank. By using high pressure air/water to open the blockages in the network , and all requirements to complete a good work.","LS",1]
[10,"Water pump:\nSupply materials, tools and manpower to connect water pump (1hp), Q=3M³/Hrs., H=20m with, ball valve and all fitting and accessories for connection. The price of works includes all accessories needed, as well as all needed works to complete the job. See attached","EA",1]
[null,"Subtotal for Sanitary works "]
[null,"Electricals Works"]
[null,"Work includes replace the damaged wires with new suitable size , testing and operation"]
[1,"Socket Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/13A) socket switch using screws,using single core PVC insulated copper wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",20]
[2,"Light Switch:\nSupplying materials , tools and manpower to install, connect and commissioning  of (220VAC/6A) (single , double , triple and quadruple) light switches using screws,using single core PVC insulated copper wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",20]
[3,"Fluorescent Lighting:                \nSupplying materials, tools and manpower, to install, connect and commissioning Simple Fluorescent Lighting Fixture 1x36 W, 4 feet, (metal frame, tube and starter), using single core PVC insulated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",50]
[4,"Lighting:                \nSupplying materials, tools and manpower, to install, connect and commissioning (220VAC/20Watt) economic light lamp with Lamp, using single core PVC insulated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way  lighting switch (6A) with all accessories and requirement to implement the work entirely.","LS",20]
[5,"Fluorescent lamp:\nSupplying materials, tools and manpower, to install, connect and commissioning best quality of fluorescent lamp fixtures 120 cm (4 Foot) with starter  with all requirements to complete a good work.","EA",220]
[6,"Fan Regulator:\nSupplying materials, tools and manpower to install, connect and commissioning best quality of  Ceiling Fans Regulator with 5 speeds/ fan speed switch/ Regulator and  all requirements to complete a good work. ","EA",2]
[7,"Ceiling Fan:\nSupplying materials, tools and manpower to install, connect and commissioning best quality of 56\" ceiling fan with power regulator using PVC insualted copper cable (2*1.5mm) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",10]
[8,"Exhaust fan:\nSupplying materials, tools and manpower, to install, connect and commissioning of exhaust fan 6 inch (220VAC), using single core PVC insulated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using single way switch (6A) with all accessories and requirement to implement the work entirely.","LS",4]
[9,"Electrical bell:\nSupplying materials, tools and manpower, to install, connect and commissioning of electrical bell (220VAC), using single core PVCi insulated copper wire (2*1.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories), or using (Plastic Cable Duct PVC Trunking) using 1 Gang 2 Way Single Pole Push Switch (6A) with all accessories and requirement to implement the work entirely.","LS",2]
[10,"Main Board:\nProviding materials, installation and operation test of distribution board, enclosed metal frame made of iron sheet 1mm thickness painted with two layers of gray color oil paint free, arrange the items shown below properly, with door,  dimensions (height x width x depth: 80cm x 80 cm x 40cm), using rubber gaskets and equipped with the following items, Plastic trunck for wiring, and Bus bars 100A 4No with earth bus bar, the price also include the required, glands, screws, insulators, and etc, all items should be arranged properly, affords a high degree of safety operation,\n\nA - [(1 No.)  100A,  3Ph. 415 VAC , 25 kV BC,MCCB type].\nB - [(6 No.)  25A,  3Ph. 415 VAC MCB type].\nC - [(6 No.)  25A,  1Ph. 220VAC MCB type].\nD - (1 No.)Voltmeter (0- 400 V) with selector switch.\nE - (1 Set)Ammeter (0 -100 A), 100/5A with required CTs.\nF - (1 No.)Hertz meter (48- 52 )Hz.\nG - (1 No.) selector switch.\nH - (3 No.) Indicator lamp 220VAC/5A.\nI - Three-phase Kilowatt-hour meter \nJ - (1Set)Copper Bus-Bar 100A., for lines and the half for the neutral and             earth, length for each one not less than (40)cm., with all accessories.","EA",1]
[11,"Sub Distribution Boards:\nSupply, installation, testing and commissioning of factory fabricated distribution boards for light/power, concealed type made of M.S sheet 16 SWG degreased, derusted, zinc phosphated finished with electrostatic powder coating, of approved colour with hinged door, lockable handle, protection plate, basbar, earth and neutral strip, complete internally wired, flexible earthing strap for door manufactured by any one of the approved manufacturers as specified and comprising as under: Distribution board (3 Phase/400V/50Hz ) , equipped with TPN DB 12ways,  (DIN type, horizontal/vertical) metal single door complete with all accessories to accommodate incoming  (1x 3 pole MCB , 1 x 63 Amps, 415 volt A.C),  includes outgoing  SP MCB (3 x 10 Amps), (3 x 16 Amps), (2 x 20 Amps),  (2 x 25 Amps) , (2 x 32 Amps )  and Neutral tapping bar/strip on/in prefabricated  MS cubical control panel board including drilling holes, connections, fixing etc. with all accessories to complete work as required.","EA",2]
[12,"Power Cable:\nProviding materials, installation and operation test of  Power Cable size (4x10mm2) .flexible cable copper conductor,PVC insulation, unarmoured,best type lay on plastic cable chanal or fixed on the wall or (ceiling) by special plastic clamps extend form the main pole to the main board, the cabls should connected by cable lugs with all requirements & connections in both sides , with all accessories and requirement to implement the work entirely.","ml",50]
[13,"Electrical water boiler:\nSupply materials, tools and manpower to install, establish, connect, and commissioning electrical heater 250 Liter 3 kV with complete fittings & accessories . The work includes  Power Cable size (3x4mm2) .flexible cable copper conductor,PVC insulation, unarmoured,best type  inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings with all accessories) or using (Plastic Cable Duct PVC Trunking) extend form SDB  to the wter boiler system, with all accessories and requirement to implement the work entirely. See attached","LS",3]
[14,"Water- cooler: \nSupplying materials , tools and manpower to install best quality stainless steel electrical water-cooler with three taps, water connections using screws,using single core PVC insualted copper wire (2*2.5mm2) installed inside best type heavy duty PVC( 20mm dia. thickness conduits, circular junction box, square plastic box, adapter, couplings, with all accessories), or using (Plastic Cable Duct PVC Trunking) with all accessories and requirement to implement the work entirely.","LS",4]
[15,"Wall Mounted Split Unit Air-Conditioning:\nSupply, installaytion , connect and commissioning best quality  Split unit Air-conditioning (Cool & Heat) 2  ton.(24000btuh) , ambiant temperature -10 to 55° C  using  Power Cable size (2x4mm2) .flexible cable copper conductor,PVC insulation, unarmoured,best type lay on plastic cable chanal or fixed on the wall or (ceiling) by special plastic clamps extend form the main board   to the workshop, the cabls should connected by cable lugs with all requirements & connections in both sides with switch 45  Amp , the price include steel base, installing condensation pipe with all accessories and requirements to complete a good work.In addition to the guarantee and maintenance of the unit  for two years. See attached","EA",1]
[null,"Subtotal for Electricals Works"]
[null,"Total "]