{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":231,"n_cols":6,"rows_kept":231,"cut":false,"hidden":false,"merged":[[156,1,156,4],[4,0,4,5],[1,1,1,5],[0,1,0,5],[2,1,2,5]]}
[null,"Bill of Quantity"]
[" ","ITB 274/17 - Reconstruction of the Central Workshop of Municipality DG in Falluja"]
[null,"Falluja - Anbar"]
["#","Item/Description","Unit","Quantity","Price $","Total $"]
["Part 1: Construction of Administration Building "]
["A- Civil Works"]
[1,"Supply equipment and manpower to prepare the site, work should include leveling the ground, removing the surplus soil  in accordance with specified level, marking the ground and compacting the soil with 95% degree of compaction, price should include removal of all debris material to a dump site approved by the relevant local authority, provision of level devise type (lica spriner 250 M) to be handed to the Fallujah municipality DG after completion of project, and all the works required to complete the Job.","L.s",1]
[2,"Supply materials, tools and manpower to excavate and backfill with sub-base layer\" class C\" under and beside foundation and \" class B\" for floors and passage ways, layer thickness should not less than 20 cm according to the heights in the attached drawings with compaction not less than 95% degree, price should include spry chlordane (treatment liquid of termite ) with all the required works to complete the Job","m3",200]
[3,"Supply materials, tools and manpower to spread crashed stone or boulder layer of 7 cm under the foundation, floors and passage ways with compaction,  price should include spry chlordane (treatment liquid of termite ) with all the required works to complete the Job.","m2",260]
[null,"Casting Concrete works:"]
[4,"Supply materials, tools and manpower to cast the blinding with 21 Map compressive strength and 10 cm thick under foundations, floors and passage ways, using sulphate resistant Cement and Sika proof with all the required works to complete the Job","m2",250]
[5,"Supply materials, tools and manpower to cast 21MPa concrete for D.P.C level with  15 cm thickness and as per the drawings ,using sulphate resistant Cement and Sika proof with all the required works to complete the Job.","m.l.",75]
[6,"Supply materials, tools and manpower to cast 28 MPa  sulphate resistance reinforced concrete for continuous footing foundation as per attached drawings, the price should include high yield (420N/mm2) deformed steel reinforcement , timber formwork shuttering, with all the required works to complete the Job","m3",22]
[7,"Supply materials, tools and manpower to cast reinforced concrete with compressive strength 26 Map for building roofs, beams, water baffles and doors and windows lintel as per the technical specifications and drawings attached, the work includes  high yield (420N/mm2) deformed steel reinforcement, works of the  wooden frames and all accessories, with all the required works to complete the Job.","m3",41]
[null,"Building Bricks Works:"]
[8,"Supply materials, tools and manpower to build the walls under D.P.C level with bricks of (24x12x7.5) cm dimension and sulphate resistance cement-sand mortar (1:3) of graded width (48 - 36 - 24) as per attached drawings, the work includes plastering the walls with sulphate resistance cement – sand mortar (1:3), spreading for both sides of the walls with tar with all the required works to complete the Job.","m3",5]
[9,"Supply materials, tools and manpower to build passage ways retaining walls with bricks of (24x12x7.5) cm dimension and sulphate resistance cement-sand mortar (1:3) of (24) cm width as per attached drawings, the work includes casting of footing foundation of (40*20) dimension, plastering the walls with sulphate resistance cement – sand mortar (1:3), spreading for both sides of the walls with tar with all the required works to complete the Job.","m3",8]
[10,"Supply materials, tools and manpower build with bricks of (24x12x7.5) cm dimension and cement mortar (1:3) above D.P.C level of 24 cm thick for interior and exterior walls of 24 cm width as per attached drawings and technical specification, with all the required works to complete the Job","m3",70]
[null,"Finishing Works:"]
[11," Supply materials, tools and manpower to finish the floors with mosaic tiles of (40*40)cm dimension and sulphate resistant cement mortar (1:3) the work includes filling the joints with white cement and polishing the mosaic tiles, with all the required works to complete the Job.","m2",95]
[12,"Supply materials, tools and manpower to finish with 15 cm rounded edge mosaic board and cement - sand mortar (1:3) for the walls above the floor finish level, the work includes filling the joints with white cement with all the required works to complete the Job.","m.l.",110]
[13,"Supply materials, tools and manpower to finish sanitary unit walls with (60x30) cm dimension ceramic tiles and sulphate resistant cement - sand mortar (1:3) as per the attached drawings, the work include filling the joints using white cement, and all the required works to complete the Job.","m2",50]
[14,"Supply materials, tools and manpower to plaster with cement- sand mortar (1:3) of 2 cm thick for the external walls and bathrooms and kitchen rooms ceiling , price should include leveling the plaster in vertical and horizontal directions, with all the required works to complete the Job.   ","m2",236]
[15,"Supply materials, tools and manpower to render with cement finishing coat for the external walls with all the required works to complete the Job.   ","m2",220]
[16,"Supply materials, tools and manpower to plaster with 2 cm  of brown and white stucco finish coat for internal walls and ceilings, the work includes spreading the walls before plastering with cement –sand mortar (1:3) and leveling the finish in horizontal and vertical directions, with all the required works to complete the Job.","m2",450]
[17,"Supply materials, tools and manpower to paint the internal walls and ceiling with three layers of water based (plastic) paints, the work includes cleaning the walls and ceiling before painting and all the required works to complete the Job.","m2",450]
[18,"Supply materials, tools and manpower to paint the external walls and  kitchen and bathrooms ceiling with three layers of oil based paints, the work includes cleaning the walls and ceiling before painting and all the required works to complete the Job.","m2",16]
[19,"Supply materials, tools and manpower to finish with concrete tiles as per the technical specifications and drawings as following:\n- clean the roof, paint with bitumen emulsion materials, spreading two opposite 10 mm thick layers of tar and spreading two  opposite water-proof (membrane) layer of 4 mm.\n- spreading corks layer with 5 cm thickness\n- spreading nylon layer over the corks and then spread clean river sand layer with 10 cm thickness.\n- finishing with concrete tiles of(80x80x4) cm thickness as per the slopes and levels in the attached drawings.\n- filling the joints with mastic and burn\n- supply and install PVC water drainage pipe of 4 inch diameter as per the drawing.\nwith all work requirements to complete the Job.","m2",120]
[null,"Doors and Windows works:"]
[20,"Supply and install steel door of 2 side plate of G16 with square section steel frame of 2 inch dimension and  2mm thickness as per the drawings, the work includes painting with 3 layers of oil based paints in addition to Anti rust Primer, locks, connections accessories, and all the required works to complete the Job."]
["a","·    D1 (1.5 X 2.4) m","Ea.",1]
["b","·    D2 (1 X 2.1) m","Ea.",5]
["c ","·    D3 (1 X 2.1) m","Ea.",1]
["d","·    D4 (0.8 X 2.1) m","Ea.",3]
[21,"Supply and install of steel windows, price should include supplying and installation steel frames, installation of glass  6 mm thick, anti insect netting mesh, steel guard frame and painting the window with 3 layer of oil based paint in addition to anti rust prime coat, with all accessories and all work requirements to complete the Job."]
["a","·    W1 (2 X 2) m","Ea.",6]
["b","·    W2 (1 X 1.6) m","Ea.",1]
["c","·    W3 (1 X 1) m","Ea.",2]
["d","·    W4 (0.6 X 0.6) m","Ea.",3]
["B- Water and Sewage works"]
[22,"Supply and install Fire Extinguishers of (6) Kg wright, the price includes installation on the wall as per technical specification the drawings with all the required works to complete the Job."]
["a","ABC Fire Extinguishers","Ea.",3]
["b","CO2 Fire Extinguishers","Ea.",2]
[23,"Supply, install and connect galvanized water tank of 1m3 capacity using gage 16 plate ,the work includes installation on concrete bases with all connection and installations accessories and with all the required works to complete the Job","Ea.",2]
[24,"Supply and install water heater of 200-liter capacity and (3) KW, the price includes all installation  and connections accessories, and valves, with all the required works to complete the Job.","Ea.",1]
[25,"Supply, install and connect (2) taps electrical water cooler of 40 liter/hr. cooling capacity and stainless steel cover, price includes all electrical and water connections accessories and required works to complete the Job","Ea.",1]
[26,"Supply, install and connect (3.5) m3/hr. water pump (centrifugal) water pump of (15) m head. The price should include provision and installation of flow meter, check valves and electrical and water connections, with  all accessories and required works to complete the Job.","Ea.",1]
[27,"Supply and install wash basin ceramic of (56*40) cm dimension with mixer, price includes installation work with all requirements and accessories to complete the job.","Ea.",3]
[28," Supply, install, connect and test eastern ceramic toilet base of (56) length with carbon steel siphon of (32) mm down pipe price should include all installations and connection accessories and all the required works to complete the Job.","Ea.",3]
[29,"Supply, install and connect PVC pipes for sewage net of sanitary units for the  building, the work includes excavation, backfill, covering it with concrete from all sides using sulphate resistant cement, with all connection and installations accessories, and all the required works to complete the Job"]
["a",".    Pipe (2) inch diameter and 3 bar pressure","m.l.",10]
["b",".    Pipe (4) inch diameter and 6 bar pressure","m.l.",35]
["c",".    Pipe (6) inch diameter and 6 bar pressure","m.l.",20]
["d",".    P- type gully trap ","Ea.",10]
[30,"Supply, install and connect galvanized water pipe with three lines (water source, water heater and water tank), price should include all connection and installations accessories and water chrome taps with all the required works to complete the Job."]
["a",".       Galvanized pip (1/2) inch diameter","m.l.",150]
["b",".       Galvanized pip (3/4) inch diameter","m.l.",40]
[31,"Supply, install and connect carbon steel pipes of (4) inch diameter for raining water for the  building, the work includes installation work with all connection and installations accessories, and all the required works to complete the Job","m.l.",16]
[32,"Supply materials, tools and manpower to build the septic tank of (2.55 * 3.5 * 6.75) m dimension using concrete block and sulphate resistant cement - sand mortar (3:1), price should include soil excavations, casting  (20 * 40) cm dimensions foundation for walls and 18 cm thick roof with two layers reinforcement with 21 Map Concrete sulphate resistant cement, plastering the walls with cement- sand mortar (1:3), execute maintenance opening (60 * 60) and installation manhole steel covers of (40x40)cm and installation of relief pipe of (50) mm diameter and 3 m height with all the required works to complete the Job.","Ea.",1]
[33,"Supply materials, tools and manpower to cast concrete manhole of (50*50) dimension using sulphate resistant cement, the work includes excavation, coating with tar, installation of cast iron manhole cover of (40x40) cm dimension and all the required works to complete the Job.","Ea.",4]
[34,"Supply, install, connect and test two hole stainless steel kitchen sink with mixer and drainage pipes, with all requirements and accessories.","Ea.",1]
["C: Electrical works"]
[35,"Supply, install, connect and test light installations, price should include provision wires, wiring with (1*2.5) mm2 wire works inside PVC conduits with all installation accessories and all the required works to complete the Job."]
[null,"تجهيز وتثبيت وربط وفحص التاسيسات الكهربائية للانارة باستخدام واير بقطر (1*2.5) ملم2 شاملا السعر اعمال التسليك داخل انابيب بلاستك مع كافة ملحقات الربط وكل ما يتطلبه العمل."]
["a","Single fluorescent tube bases (1 *40) watt with bulb and switch","Ea.",16]
["b","Ceiling lights (100) watt with switch","Ea.",10]
["c","Wall lights Quanta (200) Watts  with switch","Ea.",10]
[36,"Supply, install, connect and test Ceiling fan  with the regulator,230 V,   price should include provision wires, wiring works inside PVC conduits with all installation accessories and all the required works to complete the Job.","Ea.",5]
[null,"تجهيز وتركيب وتشغيل مروحة هواء سقفية مع منظم السرعة  شاملا السعر تجهيز وايرات واعمال التسليك داخل انابيب بلاستك مع كافة ملحقات الربط وكل ما يتطلبه العمل."]
[37,"Supply, install, connect and test Air ventilator fan of 300 mm diameter with 6A switch & frame ,  price should include provision wires, wiring works inside PVC conduits with all installation accessories and all the required works to complete the Job.","Ea.",3]
[null,"تجهيز وتركيب وتشغيل ساحبة هواء جداريه قطر 300 ملم  شاملا السعر تجهيز وايرات واعمال التسليك داخل انابيب بلاستك مع كافة ملحقات الربط وكل ما يتطلبه العمل.  ."]
[38,"Supply, install, connect and operate wall and ceiling  electrical points with all electrical installations using single wire of (3x2.5) mm2 as per the drawings, the price should include pulling wires inside PVC conduits with all installation and connection accessories and all the required works to complete the Job, as described below:","Ea.",15]
[null,"تجهيز مواد وتأسيس وفحص وتشغيل نقطة كهربائية سقفية أو جداريه باستخدام أسلاك نحاسية مفردة قياس 3×2.5 ملم2 وكما موضح في المخططات شاملا السعر تسليك الوايرات داخل انابيب بلاستيكية مع كل ملحقات التثبيت والربط وكل ما يتطلبه العمل. "]
[39,"Supply, connect and operate electrical point with plug switch using single copper wires of (1 x 4)mm2, the work includes  pulling wires inside PVC conduits and connecting it from sub-distribution board with all installation and connection accessories all the required works to complete the Job. As following :"]
[null,"تحهيز وربط وتسليك وتشغيل  نقطة كهربائية مع ماخذ باستخدام اسلاك نحاسية مفردة قياس (1*4) ملم2 تمرر داخل انابيب بلاستيكية  تربط من لوحة التوزيع الفرعية مع كافة ملحقات الربط والتوصيل مع كل ما يتطلبه العمل وكما يلي"]
["a",".    Plug switch of 13 amp capacity","Ea.",12]
["b",".    water proof Plug switch of 13 amp capacity","Ea.",3]
["c",".    Plug switch of 15 amp capacity","Ea.",8]
["d",".    Plug switch of 20 amp capacity","Ea.",5]
[40,"Supply, connect and operate phone plug switch point using wires of (2 x 0.6)mm2, the work includes  pulling wires inside PVC conduits of (20) mm diameter with all installation and connection accessories all the required works to complete the Job.","Ea.",5]
[null,"تجهيز وربط وتسليك وتشغيل مأخذ تلفون باستخدام اسلاك قياس (2*0.6) ملم2 تمرر داخل انابيب بلاستيكية  قطر 20 ملم مع كافة ملحقات الربط والتوصيل مع كل ما يتطلبه العمل."]
[41,"Supply, connect and operate (T.T.B) phone connection board (5) pair capacity, the work includes installation  of sealed board in the  pulling wires inside PVC conduits with all installation and connection accessories all the required works to complete the Job.","Ea.",1]
[null,"تجهيز المواد والعمل لتركيب وربط وفحص صندوق اسلاك هاتف  T.T.B صالحة للتثبيت داخل الحائط مع باب يمنع تسرب الغبار ويحتوي على الموصلات (Connectors) وكما موضح في المخططات الكهربائية صندوق سعة (5) زوج مع كل ما يتطلبه العمل."]
[42,"Supply, connect and operate electrical point with electric bell with wiring using single copper wires of (1 x 2.5) mm2, the work includes  pulling wires inside PVC conduits and doorbell Switch, with all installation and connection accessories all the required works to complete the Job.","Ea.",2]
[null,"تجهيز وربط وتشغيل نقطة جرس مع الجرس الكهربائي  باستخدام اسلاك نحاسية مفردة قياس (1*2.5) ملم2 تمرر داخل انابيب بلاستيكية مع مفتاح التشغيل الخاص بالجرس مع كافة ملحقات الربط والتوصيل وكل ما يتطلبه العمل. "]
[43,"Supply and connect the cable of low pressure type armored (PVC/SWA/PVC)  and unarmored (PVC/PVC) to connect and feed the distribution boards, the work includes bury it underground using PVC conduits,  pulling wires and according to the following measurements:"]
[null,"تجهيز وربط كيبل ضغط واطى معزولة نوع غير مسلحة (PVC/PVC) ومسلحة (PVC/SWA/PVC) لتغذية لوحات التوزيع الكهربائية شاملا العمل دفنها تحت الارض بواسطة انابيب PVC وحسب القياسات التالية :  "]
["a","Armoured  cable of (3x35/25) mm2+(1x16) mm2 inside PVC of 3 inch with executing maintenance opening every 10 m","m.l.",300]
["b"," Unarmoured cable of (4x16) mm2+(1x10) mm2 inside PVC of 3 inch with executing maintenance opening every 10 m","m.l.",50]
["c",".    Maintenance manhole of (30x30) cm  ","Ea.",20]
[44,"Supply, install and connect earthling system for the building consists of three copper rods  , the length of each one of them 1.8m and diameter 16 mm, connected together  by copper wire of (1 x95) m2 to form a triangle shape ,the side length it 3 m and 2 m deep; Interred at a depth of 2m by salt and coal up to a wet area and all the required works to complete the Job.","L.s",1]
[null," تجهيز المواد والعمل على تاسيس وفحص نظام ارضي للبنايه تتكون من ثلاث قضبان نحاسية طول كل منهم1.5م وقطر 16ملم مربوطه مع بعضها باللوحه الرئيسيه بواسطة سلك نحاس قياس (1 * 16) ملم2  على شكل مثلث طول ضلعه3م مدفون عمق 2م بواسطة ملح وفحم يصل الى منطقة رطبه مع كل ما يتطلبه العمل"]
[45,"Supply, install and connect Main distribution board consist of metal board box, digital screens of Ammeter, voltage and frequency meters, signal lamps, with all connection and installations accessories, and consist of:\n1- Main circuit breaker , 3 phase of 150 A capacity / 1 \n2- Sub circuit breaker three phase of 30 A capacity / 5\n3- bus bar of 200 A capacity /1  ( short ciucuit breaking capacity of circuit breakers shall not be less than 15  KA)","SET",1]
[null,"تجهيز وتثبيت وربط وتشغيل لوحة توزيع كهربائية رئيسية (MDB) ذات هيكل حديدي يحتوي على مقياس دجتل للفولتية والتيار التردد ومصابيح دلاله مع كافة الملحقات اللازمة ويتكون من:-\nأ‌- قاطع دورة رئيسي(150) أمبيرعدد 1 \nب‌- قاطع دورة فرعي ثلاثي الطور سعة (30) أمبير عدد 5 \nج- باز بار سعة (200) أمبير عدد 1 .\n"]
["D: Mechanical Works"]
[46,"Supply, install and connect floor standing air-conditioning split unit (cooling and heating) of 3 ton capacity the price includes the plug switch with capacity (63) A, with the protection device and installation of the outdoor part on steel frames, and all the required works","Ea.",5]
[null,"تجهيز وتثبيت وربط مكيف هواء سبلت يونت كنتوري (تدفئة تبريد) سعة (3 طن), شاملا السعر نقطة الماخذ بسعة (63) امبير والتاسيسات الكهربائية مع جهاز الحماية وتثبيت القطع الخارجية بحمالات حديدية مع كافة متطلبات العمل ."]
[null,"Sub Total"]
["Part 2: Construction of Rooms Enclosed to the Gamelan"]
["A- Civil Works"]
[1,"Supply materials, equipment and  manpower to prepare the site, the work include cutting and leveling the original ground as per the drawings and technical specifications,  remove surplus soil, plants and debris to dump site approved by relevant authorization with all required work to complete the job.","L.S",1]
[2,"Supply materials, tools and manpower to excavate and backfill using  sub-base class B under and beside foundations, under floors and passageways, with 20 cm thick layers and compaction rate 95%, price should include spraying of chlordane (treatment liquid of termite) for each layer as per technical specifications, with all required work to complete the job.","m3",310]
[3,"Supply materials, tools and manpower to spread crashed stone or boulder layer of 7 cm under the foundation, floors and passage ways with compaction,  price should include spry chlordane (treatment liquid of termite ) with all the required works to complete the Job.","m2",410]
[null,"Casting Concrete works:"]
[4,"Supply tools and manpower to cast concrete (21 Mpa) for blinding layer of 10 cm under the foundation using sulphate resistant cement with all required work to complete the job.","m2",70]
[5,"Supply tools and manpower to cast concrete (22 Mpa) using sulphate resistant cement for building floors and passage ways of 10 cm thick, price should include executing of expansion joins and filling the joints with tar, with all required work to complete the job.","m2",410]
[6,"Supply tools and manpower to cast concrete (25 Mpa) for (D.C.P) of (15x24) cm dimensions using sulphate resistant cement and sika prove with all required work to complete the job.","m.l.",115]
[7,"Supply materials, tools and manpower to cast 28 MPa  reinforced concrete using sulphhate resistance cement for footing foundation of (60x40) cm dimensions, the price should include high yield (420N/mm2) deformed steel reinforcement, timber formwork shuttering, as per attached drawings, with all the required works to complete the Job.","m3",25]
[8,"Supply materials, tools and manpower to cast 30 MPa  reinforced concrete for roof, beams, water buffls and lintel beams, the price should include high yield (420N/mm2) deformed steel reinforcement, timber formwork shuttering, as per attached drawings, with all the required works to complete the Job.","m3",93]
[null,"Building Bricks Works:"]
[9,"Supply materials, tools and manpower to build with brick of (7.5x12x24) cm dimensions and sulphate resistant cement mortar (1:3) under and above (D.P.C) level or height of 3.5 m, work should include building 2 rows with 48 cm width, 2 rows with 36 width and 2 rows with 24 width under (D.P.C) level, with all the required works to complete the Job.","m3",145]
[10,"Supply materials, tools and manpower to build passage ways retaining walls with bricks of (24x12x7.5) cm dimension and sulphate resistance cement-sand mortar (1:3) of (24) cm width as per attached drawings, the work includes casting of footing foundation of (40*20) dimension, plastering the walls with sulphate resistance cement – sand mortar (1:3) with all the required works to complete the Job.","m3",11]
[11,"Supply materials, tools and manpower to plaster the walls under (D.P.C) level using sulphate resistant cement - sand mortar (3:1) as per the technical specifications with all required work to complete the job.","m2",42]
[12,"Supply materials, tools and manpower to spray with bitumen emulsion coat for foundation and walls under (D.P.C) level with all required work to complete the job.","m2",125]
[null,"Finishing Works:"]
[13," Supply materials, tools and manpower to finish the floors with mosaic tiles of (40*40)cm dimension and sulphate resistant cement mortar (1:3) the work includes filling the joints with white cement and polishing the mosaic tiles, with all the required works to complete the Job.","m2",180]
[14,"Supply materials, tools and manpower to finish with 15 cm rounded edge mosaic board and cement - sand mortar (1:3) for the walls above the floor finish level, the work includes filling the joints with white cement with all the required works to complete the Job.","m.l.",230]
[15,"Supply materials, tools and manpower to plaster with cement- sand mortar (1:3) of 2 cm thick for the external walls, price should include leveling the plaster in vertical and horizontal directions, with all the required works to complete the Job.   ","m2",450]
[16,"Supply materials, tools and manpower to render with cement finishing coat for the external walls with all the required works to complete the Job.   ","m2",450]
[17,"Supply materials, tools and manpower to plaster with 2 cm  of brown and white stucco finish coat for internal walls and ceilings, the work includes spreading the walls before plastering with cement –sand mortar (1:3) and leveling the finish in horizontal and vertical directions, with all the required works to complete the Job.","m2",645]
[18,"Supply materials, tools and manpower to paint the internal walls and ceiling with three layers of water based (plastic) paints, the work includes cleaning the walls and ceiling before painting and all the required works to complete the Job.","m2",645]
[19,"Supply materials, tools and manpower to paint the external walls with three layers of oil based paints, the work includes cleaning the walls and ceiling before painting and all the required works to complete the Job.","m2",450]
[20,"Supply materials, tools and manpower to finish with concrete tiles as per the technical specifications and drawings as following:\n- clean the roof, paint with bitumen emulsion materials, spreading two opposite 10 mm thick layers of tar and spreading two  opposite water-proof (membrane) layer of 4 mm.\n- spreading corks layer with 5 cm thickness\n- spreading nylon layer over the corks and then spread clean river sand layer with 10 cm thickness.\n- finishing with concrete tiles of(80x80x4) cm thickness as per the slopes and levels in the attached drawings.\n- filling the joints with mastic and burn\n- supply and install PVC water drainage pipe of 4 inch diameter as per the drawing.\nwith all work requirements to complete the Job.","m2",310]
[null,"Doors and Windows works:"]
[21,"Supply and install steel door (1 X 2.1) m dimension of 2 side plate of G16 with square section steel frame of 2 inch  and  2mm thickness as per the drawings, the work includes painting with 3 layers of oil based paints in addition to Anti rust Primer, locks, connections accessories, and all the required works to complete the Job.","Ea.",5]
[22,"Supply and install of steel windows of (1,5×1,5) m dimensions, price should include supplying and installation steel frames, installation of glass  6 mm thick, anti insect netting mesh, steel guard frame and painting the window with 3 layer of oil based paint in addition to anti rust prime coat, with all accessories and all work requirements to complete the Job.","Ea.",10]
["B: Electrical works"]
[23,"Supply, install, connect and test light installations, price should include provision wires, wiring with (1*2.5) mm2 wire works inside PVC conduits with all installation accessories and all the required works to complete the Job."]
[null,"تجهيز وتثبيت وربط وفحص التاسيسات الكهربائية للانارة باستخدام واير بقطر (1*2.5) ملم2 شاملا السعر اعمال التسليك داخل انابيب بلاستك مع كافة ملحقات الربط وكل ما يتطلبه العمل."]
["a","Single fluorescent tube bases (2 *40) watt with bulb and switch","Ea.",16]
["b","Ceiling lights (100) watt with switch","Ea.",10]
["c","Wall lights Quanta (200) Watts  with switch","Ea.",10]
[24,"Supply, install, connect and test Ceiling fan  with the regulator & 6A switch,  price should include provision wires, wiring works inside PVC conduits with all installation accessories and all the required works to complete the Job.","Ea.",5]
[null,"تجهيز وتركيب وتشغيل مروحة هواء سقفية مع منظم السرعة  شاملا السعر تجهيز وايرات واعمال التسليك داخل انابيب بلاستك مع كافة ملحقات الربط وكل ما يتطلبه العمل."]
[25,"Supply, install, connect and test Air ventilator fan of 300 mm diameter with 6A switch and frame,  price should include provision wires, wiring works inside PVC conduits with all installation accessories and all the required works to complete the Job.","Ea.",1]
[null,"تجهيز وتركيب وتشغيل ساحبة هواء جداريه قطر 300 ملم  شاملا السعر تجهيز وايرات واعمال التسليك داخل انابيب بلاستك مع كافة ملحقات الربط وكل ما يتطلبه العمل.  ."]
[26,"Supply, install, connect and operate wall and ceiling  electrical points with all electrical installations using single wire of (3x2.5) mm2 as per the drawings, the price should include pulling wires inside PVC conduits with all installation and connection accessories and all the required works to complete the Job, as described below:","Ea.",15]
[null,"تجهيز مواد وتأسيس وفحص وتشغيل نقطة كهربائية سقفية أو جداريه باستخدام أسلاك نحاسية مفردة قياس 3×2.5 ملم2 وكما موضح في المخططات شاملا السعر تسليك الوايرات داخل انابيب بلاستيكية مع كل ملحقات التثبيت والربط وكل ما يتطلبه العمل. "]
[27,"Supply, connect and operate electrical point with plug switch using single copper wires of (1 x 4)mm2, the work includes  pulling wires inside PVC conduits and connecting it from sub-distribution board with all installation and connection accessories all the required works to complete the Job. As following :"]
[null,"تحهيز وربط وتسليك وتشغيل  نقطة كهربائية مع ماخذ باستخدام اسلاك نحاسية مفردة قياس (1*4) ملم2 تمرر داخل انابيب بلاستيكية  تربط من لوحة التوزيع الفرعية مع كافة ملحقات الربط والتوصيل مع كل ما يتطلبه العمل وكما يلي"]
["a",".    Plug switch of 13 amp capacity","Ea.",12]
["b",".    water proof Plug switch of 13 amp capacity","Ea.",3]
["c",".    Plug switch of 15 amp capacity","Ea.",8]
["d",".    Plug switch of 20 amp capacity","Ea.",5]
[28,"Supply and connect the cable of low pressure type armoured (PVC/SWA/PVC)  and unarmoured (PVC/PVC) to connect and feed the distribution boards, the work includes bury it underground using PVC conduits,  pulling wires and according to the following measurements:"]
[null,"تجهيز وربط كيبل ضغط واطى معزولة نوع غير مسلحة (PVC/PVC) ومسلحة (PVC/SWA/PVC) لتغذية لوحات التوزيع الكهربائية شاملا العمل دفنها تحت الارض بواسطة انابيب PVC وحسب القياسات التالية :  "]
["a","Armoured  cable of (3x35/25) mm2+(1x16) mm2 inside PVC of 3 inch with executing maintenance opening every 10 m","m.l.",100]
["b","Unarmoured cable of (4x16) mm2+(1x10) mm2 inside PVC of 3 inch with executing maintenance opening every 10 m","m.l.",50]
["c",".    Maintenance manhole of (30x30) cm  ","Ea.",4]
[29,"Supply, install and connect earthling system for the building consists of three copper rods  , the length of each one of them 1.8m and diameter 16 mm, connected together  by copper wire of (1 x95) m2 to form a triangle shape ,the side length it 3 m and 2 m deep; Interred at a depth of 2m by salt and coal up to a wet area and all the required works to complete the Job.","L.s",1]
[null," تجهيز المواد والعمل على تاسيس وفحص نظام ارضي للبنايه تتكون من ثلاث قضبان نحاسية طول كل منهم1.5م وقطر 16ملم مربوطه مع بعضها باللوحه الرئيسيه بواسطة سلك نحاس قياس (1 * 16) ملم2  على شكل مثلث طول ضلعه3م مدفون عمق 2م بواسطة ملح وفحم يصل الى منطقة رطبه مع كل ما يتطلبه العمل"]
[30,"Supply, install and connect Main distribution board consist of metal board box, digital screens of Ammeter, voltage and frequency meters, signal lamps, with all connection and installations accessories, and consist of:\n1- Main circuit breaker of 150 A capacity / 1 \n2- Sub circuit breaker three phase of 30 A capacity / 5 ( short circuit breaking capacity of circuit breakers shall not be less than 15 kA.\n3- bus bar of 200 A capacity /1 ","Set",1]
[null,"تجهيز وتثبيت وربط وتشغيل لوحة توزيع كهربائية رئيسية (MDB) ذات هيكل حديدي يحتوي على مقياس دجتل للفولتية والتيار التردد ومصابيح دلاله مع كافة الملحقات اللازمة ويتكون من:-\nأ‌- قاطع دورة رئيسي(150) أمبيرعدد 1 \nب‌- قاطع دورة فرعي ثلاثي الطور سعة (30) أمبير عدد 5 \nج- باز بار سعة (200) أمبير عدد 1 ."]
["C: Mechanical Works"]
[31,"Supply, install and connect floor standing air-conditioning split unit (cooling and heating) of 3 ton capacity the price includes the plug switch with capacity (63) A, with the protection device and installation of the outdoor part on steel frames, and all the required works","Ea.",2]
[null,"تجهيز وتثبيت وربط مكيف هواء سبلت يونت كنتوري (تدفئة تبريد) سعة (3 طن), شاملا السعر نقطة الماخذ بسعة (63) امبير والتاسيسات الكهربائية مع جهاز الحماية وتثبيت القطع الخارجية بحمالات حديدية مع كافة متطلبات العمل ."]
[null,"Sub Total"]
["Part 3: Construction of Steel Gamelan Workshop"]
[1,"Supply materials, equipment and  manpower to prepare the site, the work include cutting and leveling the original ground as per the drawings and technical specifications,  remove surplus soil, plants and debris to dump site approved by relevant authorization with all required work to complete the job.","L.S",1]
[2,"Supply materials, tools and manpower to excavate and backfill using  sub-base class B for depths 50 cm under foundations and 90 cm under floors, with 25 cm thick layers and compaction, price should include spraying of chlordane (treatment liquid of termite) with all required work to complete the job.","m3",500]
[3,"Supply tools and manpower to cast concrete (21 Mpa) for blinding layer of 10 cm using sulphate resistant cement with all required work to complete the job.","m3",18]
[4,"Supply materials, tools and manpower to cast 30 MPa  reinforced concrete using sulphhate resistance cement for columns foundation F1 of (300×200 x 60) cm dimensions no/22 and F2 of (200x200x60) cm dimensions no/ 6, and column nicks of (60x60x85) cm dimensions, the price should include high yield (420N/mm2) deformed steel reinforcement, timber formwork shuttering, as per attached drawings, with all the required works to complete the Job.","m3",103]
[5,"Supply materials, tools and manpower to cast 30 MPa  reinforced concrete using sulphhate resistance cement for tie beam (T.B) of (50×100 +85×50) cm dimensions, the price should include high yield (420N/mm2) deformed steel reinforcement, timber formwork shuttering, as per attached drawings, with all the required works to complete the Job.","m3",108]
[6,"Supply materials, tools and manpower to spray with bitumen emulsion coat for foundation and walls under (D.P.C) level with all required work to complete the job.","m2",635]
[7,"Supply tools and manpower to cast concrete (25 Mpa) for (D.C.P) of 10 cm using sulphate resistant cement with all required work to complete the job.","m.l.",130]
[8,"Supply tools and manpower to cast concrete (25 Mpa)  using double (BRC) mesh of 6.3 mm thick and sulphate resistant cement for building floors and passage ways of 15 cm thick, price should include executing of expansion joins and filling the joints with tar, with all required work to complete the job.","m2",1300]
[9,"Supply materials, tools and manpower to build with brick of (7.5x12x24) cm dimensions and sulphate resistant cement mortar (1:3) for passageways retaining walls of 24 cm width and 40 cm height as per attached drawings, price includes casting concrete of (40x20) cm dimensions as foundation using sulphate resistant cement and plastering both side with cement, with all the required works to complete the Job.","m.l.",150]
[10,"Supply materials, tools and manpower to install steel structure of Gamelan dimensions (23.10X44.2), height 7.4m in the middle and 6.0m in the sides from concrete ground level as per attached drawings include the following:\n- Supply and install base plate of (600x600x10) mm dimensions no/28 to be install on the concrete foundations using  (L) section steel bolts of (650) mm length and 16 mm diameter no/ 336.\n- Installation of steel columns (I Section) of (15*200*45.72) mm dimensions (18 inch) no/ 28, work includes welding the columns on the base plate as per attached drawings.\n- Installation of (I) steel section Rafter  (I Section) of (15*200*45.72) mm dimensions (18 inch) between the columns of triangle shape with connections parts as per the drawing using welding and bolts.\n- Installation of U channel steel section purlins of (3) inch height and 5 mm thickness every (1) m with installation of L angle steel section of (3) inch dimension and 5 mm thick every 1 m using welding. \n- Installation of sub beams of Rectangular Steel section of (8x4x0.3) cm dimensions every (1) m with welding a triangular frame every (1) m using Rectangular Steel section of (16x8x0.4) cm dimensions fixed by bolts and welding with total length of (540) m. \n- Installation of sandwich panels 5cm thick for the roof fixed on purlins by bolts with washers to prevent any water seepage.\n- Installation of galvanizes plate rainwater channel of (250x250x0.2) fixed on both side of gamelan with installation of PVC pipe of 3 inch diameter ever 6 m.\n- fixing a plate between the roof and walls along the sides line.\n- painting the steel structure with anti-rust paint and oiled paints (three layers) as per the drawing and technical specifications with all accessories and required work to complete the job.\n","m.l.\nof Sec.",44.2]
[null,"تجهيز المواد والعمل وتجهيز المواد والعمل للقيام باعمال تركيب وتثبيت الهيكل الحديدي للجملون بابعاد ( 23.10 * 44.20) متر وبارتفاع 6  ن الجوانب و 7.40 من الوسط من مستوى صبة الأرضية كما موضح بالمخطط المرفق ويشمل العمل:\n- تجهيز بليت (Base plate ) مغلون بالابعاد (500×500×10)ملم عدد28 وتثبيته بالقاعدة الكونكريتية بواسطة البولتات المغلونة بطول650ملم شكل (L) عدد 224 قطر 16ملم.\n- تثبيت اعمدة حديدية مقطع شكل (I) بقياس (300×150×15)ملم (12 انج) عدد 28 ويثبت باللحام على البليت الخاص بقاعدة العمود  وحسب المخططات .\n-  تثبيت مقطع حديدي (Rafter)على شكل مثلث يثبت بين الاعمدة يتكون من مقطع (I) مع لحام اجزاء رابطة اخرى وحسبب المخططات.\n-  تثبيت مقطع حديدي شكل ساقية (channel) قياس 3 انج وبسمك 6 ملم  كل 1 متر مع تثبيت مقطع زاوية (L) قياس  3 انج  وبسمك 5 ملم كل 1 متر بواسطة اللحام وكما موضح بالمخططات.\n- تثبيت طراحيات شكل مستطيل بابعاد (8×4×0,3) سم كل 1متر مع عمل محيط ثلاثي كل 1 متر من البوري المستطيل بابعاد )16×8×0,4) سم  ويثبت بالبراغي واللحام ويكون الطول الكلي (540)متر\n- تثبيت ساندويج بنل سمك 5 سم لسقف الجملون باستخدام براغي التثبيت الخاصة.\n- ثبيت مجرى مياة امطار قياس 250×250× 0,2 سم من البليت المغلون على جانبي الجملون بصورة جيدة مع تثبيت نزالات للمياه قطر 3 انج كل 6 م.\n- معالجة مناطق التقاء السقف مع الجدران الجانبية بالبليت المغلون لكلا جانبي الجملون وعلى طول الخط للجانبين.\n- صبغ الهيكل الحديدي بالصبغ الرادليت ثم الصبغ الدهني ثلالث طبقات وحسب المخططات والمواصفات الفنية وتوجيهات المهندس المشرف وكل ما يتطلبه العمل.\n"]
[11,"Supply materials, tools and manpower to build with thermostone block of (20x20x40) cm dimensions and sulphate resistant cement mortar (1:3) for warehouse walls as per attached drawings with all the required works to complete the Job.","m3",170]
[null,"تجهيز المواد والعمل للبناء بالثرمستون 20×20×40سم فوق مستوى مانع الرطوبة لجدران الجملون بنسبة خلط 3:1 وباستخدام الاسمنت المقاوم للاملاح وحسب المخططات مع كل ما يتطلبه العمل."]
[12,"Supply materials, tools, and manpower for plastering the external and external walls with cement sand mortar (1:3), with all the required works to complete the Job.","m2",1610]
[null,"تجهيز المواد والعمل لبخ الحدران الخارجية والداخلية بمادة الاسمنت والرمل بنسبة خلط (3:1) مع كل ما يتطلبه العمل ."]
[13," Supply materials, tools and manpower to paint the internal and internal walls with three layers of oil based paints with all the required works to complete the Job.","m2",1610]
[null," تجهيز المواد والعمل على صبغ الجدران الحارجية والداخلية بصبغ البوية الجيدة وبثلاث طبقات  مع كل ما يتطلبه العمل"]
[14,"Supply and install steel door of (4x4) m dimensions and steel plate of (2) mm thickness on both sides with frame of 4 inch and 5mm thickness. the work  including all necessary fixings, fittings, locks with  key, glazing, insulation foam, accessories, mastic, hardware and painting with anti-rust paint and 3 layers of oil paints, locks, connections accessories, and all the required works to complete the work","Ea.",1]
[null,"تجهيز وتنصيب ابواب حديدية  بابعاد (4x4) كبس وجهين سمك الاطار 4 انج و البليت (2) ملم شاملا العمل الصبع بالرادليت وبثلاث طبقات من الاصباغ الدهنية والاقفال مع كافة ملحقات التثبيت مع كل ما يتطلبه العمل. "]
[15,"Supply materials, tools and manpower to install PVC pipe of 6 atmospheric pressure for the sewage net, price should include all connections, fittings, Joints, excavations, casting sulfate resistant cement, with all the required works to complete the Job."]
[null,"تجهيز المواد والعمل على  مد انابيب بلاستيكية PVC لشبكة مياه المجاري  بضغط 6 بار مع جميع الملحقات التوصيل والربط شاملا السعر الحفر والتغليف بالخرسانه الاعتيادية وباستخدام السمنت المقاوم للاملاح وكل مايتطلبه العمل."]
["a",".        (4) inch diameter pipe","m.l.",100]
["b",".        (6) inch diameter pipe","m.l.",20]
["B: Electrical works"]
[16,"Supply, install, connect and test light installations, price should include provision wires, wiring with (1*2.5) mm2 wire works inside PVC conduits with all installation accessories and all the required works to complete the Job."]
[null,"تجهيز وتثبيت وربط وفحص التاسيسات الكهربائية للانارة باستخدام واير بقطر (1*2.5) ملم2 شاملا السعر اعمال التسليك داخل انابيب بلاستك مع كافة ملحقات الربط وكل ما يتطلبه العمل."]
["a","Single fluorescent tube bases (2 *40) watt with bulb and switch","Ea.",16]
["b","Ceiling lights (100) watt with switch","Ea.",10]
["c","Wall lights Quanta (200)Watts  with switch","Ea.",10]
[17,"Supply, install, connect and test Ceiling fan, 230 V  with the regulator,  price should include provision wires, wiring works inside PVC conduits with all installation accessories and all the required works to complete the Job.","Ea.",5]
[null,"تجهيز وتركيب وتشغيل مروحة هواء سقفية مع منظم السرعة  شاملا السعر تجهيز وايرات واعمال التسليك داخل انابيب بلاستك مع كافة ملحقات الربط وكل ما يتطلبه العمل."]
[18,"Supply, install, connect and test Air ventilator fan of 300 mm diameter, 230 V. with 6 A switch and frame the price should include provision wires, wiring works inside PVC conduits with all installation accessories and all the required works to complete the Job.","Ea.",3]
[null,"تجهيز وتركيب وتشغيل ساحبة هواء جداريه قطر 300 ملم  شاملا السعر تجهيز وايرات واعمال التسليك داخل انابيب بلاستك مع كافة ملحقات الربط وكل ما يتطلبه العمل.  ."]
[19,"Supply, install, connect and operate wall and ceiling  electrical points with all electrical installations using single wire of (3x2.5) mm2 as per the drawings, the price should include pulling wires inside PVC conduits with all installation and connection accessories and all the required works to complete the Job, as described below:","Ea.",15]
[null,"تجهيز مواد وتأسيس وفحص وتشغيل نقطة كهربائية سقفية أو جداريه باستخدام أسلاك نحاسية مفردة قياس 3×2.5 ملم2 وكما موضح في المخططات شاملا السعر تسليك الوايرات داخل انابيب بلاستيكية مع كل ملحقات التثبيت والربط وكل ما يتطلبه العمل. "]
[20,"Supply, connect and operate electrical point with plug switch using single copper wires of (1 x 4)mm2, the work includes  pulling wires inside PVC conduits and connecting it from sub-distribution board with all installation and connection accessories all the required works to complete the Job. As following :"]
[null,"تحهيز وربط وتسليك وتشغيل  نقطة كهربائية مع ماخذ باستخدام اسلاك نحاسية مفردة قياس (1*4) ملم2 تمرر داخل انابيب بلاستيكية  تربط من لوحة التوزيع الفرعية مع كافة ملحقات الربط والتوصيل مع كل ما يتطلبه العمل وكما يلي"]
["a",".    Plug switch of 13 amp capacity","Ea.",12]
["b","Water proof Plug switch of 13 amp capacity","Ea.",3]
["c",".    Plug switch of 15 amp capacity","Ea.",8]
["d",".    Plug switch of 20 amp capacity","Ea.",5]
[21,"Supply and connect the cable of low pressure type armoured (PVC/SWA/PVC)  and unarmoured (PVC/PVC) to connect and feed the distribution boards, the work includes bury it underground using PVC conduits,  pulling wires and according to the following measurements:"]
[null,"تجهيز وربط كيبل ضغط واطى معزولة نوع غير مسلحة (PVC/PVC) ومسلحة (PVC/SWA/PVC) لتغذية لوحات التوزيع الكهربائية شاملا العمل دفنها تحت الارض بواسطة انابيب PVC وحسب القياسات التالية :  "]
["a","Aarmoured  cable of (3x35/25) mm2+(1x16) mm2 inside PVC of 3 inch with executing maintenance opening every 10 m","m.l.",100]
["b","Unarmoured cable of (4x16) mm2+(1x10) mm2 inside PVC of 3 inch with executing maintenance opening every 10 m","m.l.",50]
["c",".  Maintenance manhole of (30x30) cm  ","Ea.",4]
[22,"Supply, install and connect earthling system for the building consists of three copper rods  , the length of each one of them 1.8m and diameter 16 mm, connected together  by copper wire of (1 x95) m2 to form a triangle shape ,the side length it 3 m and 2 m deep; Interred at a depth of 2m by salt and coal up to a wet area and all the required works to complete the Job.","L.s",1]
[null," تجهيز المواد والعمل على تاسيس وفحص نظام ارضي للبنايه تتكون من ثلاث قضبان نحاسية طول كل منهم1.5م وقطر 16ملم مربوطه مع بعضها باللوحه الرئيسيه بواسطة سلك نحاس قياس (1 * 16) ملم2  على شكل مثلث طول ضلعه3م مدفون عمق 2م بواسطة ملح وفحم يصل الى منطقة رطبه مع كل ما يتطلبه العمل"]
[23,"Supply, install and connect Main distribution board consist of metal board box, digital screens of Ammeter, voltage and frequency meters, signal lamps, with all connection and installations accessories, and consist of:\n1- Main circuit breaker of 150 A capacity / 1 \n2- Sub circuit breaker three phase of 30 A capacity / 5\n3- bus bar of 200 A capacity /1  ( short circuit breaking capacity of circuit breakers shall not be less that 15 kA.)","Set",1]
[null,"تجهيز وتثبيت وربط وتشغيل لوحة توزيع كهربائية رئيسية (MDB) ذات هيكل حديدي يحتوي على مقياس دجتل للفولتية والتيار التردد ومصابيح دلاله مع كافة الملحقات اللازمة ويتكون من:-\nأ‌- قاطع دورة رئيسي(150) أمبيرعدد 1 \nب‌- قاطع دورة فرعي ثلاثي الطور سعة (30) أمبير عدد 5 \nج- باز بار سعة (200) أمبير عدد 1 ."]
[24,"Supply, install, test and operate new diesel generator of 150 kVA capacity inside silencer canopy from best brands and well known generator manufactories; the work should include cables, ATS, all electrical connections with the change over and main circuit breaker, provision and connection of external fuel tank  of 2000 litre capacity, all mechanical connections, and provision of spare parts (oil filter set Qty.5, gas filter set Qty.10, air filter set Qty.3) with all works required to complete the job.  See the Technical Data Sheet for the required technical specifications.","Ea.",1]
[null,"تجهيز ونصب وفحص وتشغيل مولدة كهربائية جديدة سعة 150 كي في اي داخل حاوية كاتمة للصوت شاملا السعر  محول ATS وجميع الكيبلات والتوصيلات الكهربائية بين المولد والقاطع الرئيسي والتوصيلات مع تجهيز وربط خزان الوقود(5000) م3 وتجهيز مواد احتياطية تشمل (سيت فلتر دهن عدد 5، سيت فلتر كاز عدد 10، سيت فلتر هواء عدد 3) مع كل ما يتطلبه العمل. شهادة المنشأ واوراق الفحص مطلوبة. راجع ملحق المواصفات الفنية لمزيد من التفاصيل."]
[null,"Sub Total"]
["Part 4: Construction of Fence and Workshop ground "]
[1,"Supply materials, equipment and  manpower to prepare the site include removing of surplus soil, plants and debris to dump site approved by relevant authorization with all required work to complete the job.","L.S",1]
[2,"Supply materials, tools and manpower to backfill using two layer sub-base class B  of 20 cm thickness with (2%) slope and compaction rate 95%, price should include spraying of chlordane (treatment liquid of termite) for each layer as per technical specifications, with all required work to complete the job.","m3",500]
[3,"Supply tools and manpower to cast concrete (30 Mpa)  using double (BRC) mesh of 6.3 mm thick and sulphate resistant cement for sunshade floors of 20 cm thick, price should include executing of expansion joins and filling the joints with tar, with all required work to complete the job.","m2",1600]
[4,"Supply, install and connect 200 mm UPVC pipes of 6 bar for sewage net, the work includes excavation of trench with (400 to 600) mm width and backfill with river sand around and  25 cm over the pipe, and sub-base class B  of 20 cm thickness layers for the rest height with watering and compaction, price should include the retaining walls, dewatering ground water (if needed), covering it with concrete from all sides using sulphate resistant cement, with all connection and installations accessories, and all the required works to complete the Job","m.l.",560]
[5,"Supply materials, tools and manpower to cast manholes of (1100-1300) mm diameter with various depth depending of the pipe depth using sulphate resistant concrete, the work includes spreading boulder layer of 20 cm thick, casting reinforced concrete for base of 30 cm thick and 160 cm diameter beneath the pipe with one layer reinforcement Ø 12 @ 15 cm, casting reinforced concrete for wall of 20 cm  with one layer reinforcement Ø 12 @ 15 cm and casting the reinforced concrete cover of 25 cm thick and 130 cm diameter with two layers reinforcement Ø 12 @ 15 cm, price should include soil excavations,  installation heavy manhole cast iron cover of (55)cm diameter, spray with bitumen emulsion coat the external and epoxy coat two layers for internal walls, using water stop strips between the base and wall and timber work with all the required works to complete the Job.","Ea.",6]
[6,"Supply materials, tools and manpower to excavate the soil with the required dimension to cast sewer concrete trap, the work includes casting (40x60) bases with various depth (50 - 90) cm, casting 30 MPa  reinforced concrete using sulphhate resistant cement for trap base of (500x80) cm dimension and 15 cm thick and casting 30 MPa  reinforced concrete using sulphhate resistant cement for trap walls of (40 x 60) cm dimension and 15 cm thick with depth of 75 cm, price should include high yield (420N/mm2) deformed steel reinforcement, timber formwork shuttering, heavy cast iron grate cover with all the required works to complete the Job.","Ea.",16]
[7,"Supply materials, tools and manpower to build the septic tank of (2.55 * 3.5 * 6.75) m dimension (21 Map) reinforced concrete (20) cm thick using sulphate resistant cement, price should include soil excavations,  execute maintenance opening (80 * 80) and installation manhole cast iron covers of (60x60)cm, spray with bitumen emulsion coat the external and epoxy coat for internal walls and installation of relief pipe of (50) mm diameter and 3 m height with all the required works to complete the Job.","Ea.",1]
[8,"Supply materials, tools and manpower to remove the damaged parts of the fence and rebuild wall of 24 cm width with brick of (7.5x12x24) cm dimensions and cement-sand mortar (1:3), with all the required works to complete the Job.","m3",20]
[9,"Supply materials, tools, and manpower for plastering the external and external walls with cement sand mortar (1:3), with all the required works to complete the Job.","m2",500]
[10,"Supply materials, tools and manpower to paint the fence with three layers of water based (plastic) paints, the work includes cleaning the walls and ceiling before painting and all the required works to complete the Job.","m2",3120]
[11,"Supply materials, tools and manpower repair and maintain the fence doors, the work includes all welding and fixing work, replacing the handles, key and hinges, painting with oily paint three layers with all required works to complete the work","L.s",1]
[12,"Supply materials, tools and manpower to install a lighting system as following:\na- casting reinforced concrete bases of (60x60x120) cm dimension using sulphate concrete cement with mixture ratio (4:2:1).\nb- supply and install lighting tower of (9) m height with two light holder and pedestal base of (30x30x1) cm dimension of 4 bolts holes.\nc- supply, connect and test sodium bulb projector (400) watt,  Two Nos.\nd- supply and connect unarmoured cable (2x4) mm2 (30) m and circuit breaker of 10 A. \ne- connection between the light towers with (4x16) mm2 cable pulled inside PVC pipe (2) inch buried in to ground.\nf- electrical board for the lighting system includes 3 x single phase 32 A circuit breaker  and auto switch photocell.\nwith all required work to complete the job.","Ea.",10]
[13,"Supply materials, tools and manpower to excavate for sun shade bases and backfill using  sub-base class B for depths 25 cm under foundations and foundation sides, with 25 cm thick layers and compaction, price should include spraying of chlordane (treatment liquid of termite) with all required work to complete the job.","m3",380]
[14,"Supply tools and manpower to cast concrete (21 Mpa) for blinding layer of 10 cm using sulphate resistant cement with all required work to complete the job.","m3",25]
[15,"Supply materials, tools and manpower to spray with bitumen emulsion coat for foundation under (D.P.C) level with all required work to complete the job.","m2",400]
[16,"Supply materials, tools and manpower to cast 30 MPa  reinforced concrete using sulphhate resistance cement for columns foundation F3 of (100×100 x 600) cm dimensions no/82, and column nicks of (60x60x35) cm dimensions, the price should include high yield (420N/mm2) deformed steel reinforcement, timber formwork shuttering, as per attached drawings, with all the required works to complete the Job.","m3",75]
[17,"Supply materials, tools and manpower to install iron sun shade for the garage of (5x7) m dimension and (5) m height for one panel as per attached drawings, the work includes:\n- Supply and install galvanized base plate of (500x500x10) mm dimension to be installed on the concrete bases using (650) mm long bolts.\n- Supply and install steel column of (I) shaped section (8) inch size and (5) m height on the base plate and side connection of  (I) shaped section (6) inch no. 2 for each two columns. \n- Supply and install steel longitudinal beams of (I) shaped section (6) inch size and (7) m length, and steel latitude beams of (I) shaped section (6) inch size and (5) m length no. 4\n- Supply and install steel angle (L) shaped section of (4) inch size and (4) mm thick to be installed inclined with  angle of (85 and 73) between the columns and longitudinal beams.\n- Supply and install sub beams steel angle (L) shaped section of (3) inch size and (4) mm thick in both direction every (1) m  \n- Supply and install sandwich panel of (5) cm thick and (2) mm plate thick on the main and sub beams using the specific bolts every (50) cm.\n- Supply and install galvanized rainwater gutters of (25x25) m dimension and 2 mm plate thick to be installed along the sunshade with covering the connection area with plate strips, and installing galvanized down pipe of (3) inch diameter. \nwith all the required works to complete the Job.\nthe price should includes painting the frame with primer layer and oily paints three layers, all cutting and welding processes, and all required work as per the technical specifications and drawings to complete the work.","m2",1330]
[null,"Sub Total"]
[null,"Total"]