{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["1- CONCRETING WORKS"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"1- CONCRETING WORKS","index":0,"n_rows":9,"n_cols":11,"rows_kept":9,"cut":false,"hidden":false,"merged":[[3,5,3,10],[8,5,8,6],[8,7,8,10]]}
[]
[{"$nulls":5},"CONCRETING WORKS ( Annex 4 )"]
[]
[{"$nulls":5},"Rates of Concrete Works shall include: ‐.\n• All form works and shuttering shall be new.\n• Supplying, Casting, vibrating and curing as per specifications.\n• Approved additives and admixtures.\n• Incurred costs on New Concrete Job Mix Designs, Sampling, testing and providing test results certificates, storing and saving of samples.\n• Painting of exposed surfaces of underground reinforced concrete elements with two coats of hot bituminous paint (75/25) the strokes of each layer to be opposite to each other.\n• Preliminary installations for Electrical, plumbing and floor drainage in concrete slabs, beams, and any concrete elements wherever required.\n• Compaction and testing under the foundation, ground beams, ground slabs. The compaction should not be less than 98% of MDD.\n• All works according to specifications, drawings and supervisor engineer instructions.\n• due to excavation of foundations will be individual pits, the price of foundations item shall include build up automatic cement solid blocks 10x20x40cm instead of formwork with cement mortar 1:3.\n• All prices of concrete items are include the steel reinforcement works Fy = 280 Mpa (Grade 40) as mentioned in drawings."]
[]
[{"$nulls":5},"NO","DESCRIPTION","UNIT","QTY","UNIT PRICE USD","TOTAL COST USD"]
[{"$nulls":5},1.1000000000000001,"Supply and cast ready mix reinforced concrete Fcu = 25 Mpa for the  first floor slab 12 cm thick with steel 5Ø10/m for both side as per drawings ","m²",60]
[{"$nulls":5},1.2,"Supply and cast ready mix reinforced concrete Fcu = 25 Mpa for the ground floor thick 10cm with 10mm net bars steel reinforcement as per drawings and engineer instruction.","m²",60]
[{"$nulls":5},"TOTAL DEV. 01",null,{"$f":"SUM(K$5:K8)","v":0}]