{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["3- FLOOR AND WALL TILING."],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"3- FLOOR AND WALL TILING.","index":0,"n_rows":13,"n_cols":11,"rows_kept":13,"cut":false,"hidden":false,"merged":[[3,5,3,10],[12,5,12,6],[12,7,12,10]]}
[]
[{"$nulls":5},"FLOOR AND WALL TILING ( Annex 6 )"]
[]
[{"$nulls":5},"• Prices of Tiles works shall include supply of all materials, testing, mortar, 5cm sand under tiles or back the tiles (wall), skirting, workmanship, opening areas and all materials & tool sand anywhere else, needed, all according to drawings, specifications, conditions and directed instructions by the Engineer."]
[]
[{"$nulls":5},"NO","DESCRIPTION","UNIT","QTY","UNIT PRICE USD","TOTAL COST USD"]
[{"$nulls":5},3.1,"Supply and install non-slip 60x33*0.8cm ceramic tiles, with all required works, for flooring (offices and corridors), as specified and approved by the Engineer. The price includes the mortar (1:3) the sand cement fills. The color of the tiles shall be as chosen by the Engineer.","m²",36]
[{"$nulls":5},3.2,"Supply and install non-slip 33x33*0.6cm ceramic tiles, with all required works, for flooring (baths,kitchen), as specified and approved by the Engineer. The price includes the mortar (1:3) the sand cement fills. The color of the tiles shall be as chosen by the Engineer.","m²",11.5]
[{"$nulls":5},3.3,"Supply and install glazed tiles for walls (baths,kitchen), cladding 30x45x0.8mm class. The tiles shall be laid and fixed to the walls by approved bonding agents. Price includes cost of surface preparation to receive tiles, which shall include two coats of cement plaster (scratch and float coat) and approved adhesive materials, accessories and grounding. Color of the tiles shall be as chosen by the Engineer.","m²",35]
[{"$nulls":5},3.4,"Supply & install a good quality ceramic skirting tiles from the same type with the same color, size 33×7×0.8 cm chips, according to specifications and engineer's instructions","L.M.",35]
[{"$nulls":5},3.5,"Supply and install interlock tiles , with all required works, for walk side, as specified and approved by the Engineer. The color of the tiles shall be as chosen by the Engineer.","m²",15.5]
[{"$nulls":5},3.6,"Supply and install cement tiles , with all required works, for floor slab, as specified and approved by the Engineer. The color of the tiles shall be as chosen by the Engineer.","m²",56]
[{"$nulls":5},"TOTAL DEV. 03",null,{"$f":"SUM(K$5:K12)","v":0}]