{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["5- INSULATION WORKS."],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"5- INSULATION WORKS.","index":0,"n_rows":6,"n_cols":11,"rows_kept":6,"cut":false,"hidden":false,"merged":[[5,5,5,6],[5,7,5,10]]}
[]
[{"$nulls":5},"INSULATION WORKS    ( Annex 8 )"]
[]
[{"$nulls":5},"NO","DESCRIPTION","UNIT","QTY","UNIT PRICE USD","TOTAL COST USD"]
[{"$nulls":5},5.0999999999999996,"Supply and install roof water proofing membrane of bitumen rolls 5mm thick covered with quartz granules for main roof and primer coat GS at rate 25 kg/m² installation of 15x15cm angle fillet 474 groove, groove sealant, groove cover, joints over lapping, backing sheets or pieces all around external and internal corners roof drains, and all necessary material to complete the works as shown in the drawings and as per manufacture instructions and codes of practice.","m²",56]
[{"$nulls":5},"TOTAL DEV. 05",null,{"$f":"SUM(K$5:K5)","v":0}]