{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["7-  ELECTRICAL"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"7-  ELECTRICAL","index":0,"n_rows":14,"n_cols":11,"rows_kept":14,"cut":false,"hidden":false,"merged":[[13,7,13,10],[13,5,13,6]]}
[]
[{"$nulls":5},"7-  ELECTRICAL WORKS ( Annex 10 )"]
[{"$nulls":5},6]
[{"$nulls":5},"NO","DESCRIPTION","UNIT","QTY","UNIT PRICE USD","TOTAL COST USD"]
[{"$nulls":5},"7.1","B-LIGHTING POINT ( Annex 10 )\nSupply, install, test & commission a complete internal lighting point with 2x2.5sq.mm + E = 1.5 sq. mm PVC insulated multistrand copper conductor cable (Saudi cable or equivalent) in recessed 25mm dia PVC pipe including all conductors, cables, conduits, switches, boxes, and all other accessories from distribution board to lighting points, as specified and detailed on drawings.","No.",9]
[{"$nulls":5},"8","SOCKET OUTLET.\nSupply, install, test and commission a complete socket outlet point (Legrand or equivalent) or power point with 2x4sq.mm + E = 2.5 sq. mm PVC insulated multistrand copper conductor cable (Saudi cable or equivalent) in recessed 25mm dia PVC pipe, including all conductors, cables, conduits, boxes. Socket outlets and all connections between the distribution boards and the socket outlet or power connection point for the following:"]
[{"$nulls":5},"8.1","2P+E BRITICH STANDARD SINGLE SOCKET (13A-220V)","No.",13]
[{"$nulls":5},"8.2","2P+E BRITICH OR UNIVERSAL STANDARD SINGLE SOCKET (16A-220V)","No.",1]
[{"$nulls":5},"9","DISTRIBUTION BOARDS"]
[{"$nulls":5},"9.1","MAIN AND SUB-MAIN DISTRIBUTION BOARDS.\nSupply, install, test & commission complete main and sub-main distribution boards inclusive of all circuit breakers for outgoing cables, incoming cables, busbar and their coupling unit, casing cable clamps/terminals. price include connect with cables to premises power room.The board shall be of the free standing, cubicle type operating at 440/230 volts 3 phase, 4 wire and 50 hertz incorporating a TPN and E busbar of the same size. It shall be of robust construction to withstand the mechanical forces it endures while clearing a short circuit current or clearing faulty conditions. It shall be furnished with molded case circuit breakers (Schnieder, Legrand, Simense, Hager or equivalent) with rated capacities as indicated on the drawings. All as required to form a complete unit. All shall be in accordance with the drawings, specifications, codes of practice and highest prevailing standards of engineering for the following : "]
[{"$nulls":5},"9.1.1","SUB-MAIN DISTRIBUTION BOARD (SMDB).","No.",1]
[{"$nulls":5},"10","POWER CABLES:\nSupply, install, test and commission 600/1000v.XLPE/PVC/CU/4C, multi-core copper cables (Saudi cable or equivalent) including all necessary cleats, supports, brackets, glands, cable terminals, underground cable trenches excavation and backfilling, ducts, pipes, Boxes, manholes …etc. All of which shall be according to the specifications, drawings. Codes of practice and highest prevailing engineering standards, for the following:"]
[{"$nulls":5},"10.1","4C x 16 mm² XLPE/PVC/CU + E = 6 mm²","m",85]
[{"$nulls":5},"TOTAL DEV. 7 TO DEV. 10",null,{"$f":"SUM(K$5:K14)","v":0}]