

|  |
| --- |
|  |

**REQUEST FOR QUOTATION (RFQ 42/2020)**

**(Goods)**

|  |  |
| --- | --- |
| **RFQ 42/2020 for Supply of agricultural equipment (LOTs 1 – 12)** | **DATE: 20.05.2020** |
| **REFERENCE: 00096178 Restoration of Strumica River Basin** |

Dear Sir / Madam:

Quotations may be submitted on or before **05 June 2020 by 10:00** **via dedicated email**: [offers.mk@undp.org](mailto:offers.mk@undp.org).

Subject: **RFQ 42/2020 for Supply of agricultural equipment**

We kindly request you to submit your quotation for **RfQ 42/20** **Supply of agricultural equipment (LOTs 1 – 12), as** detailed in Annex 1 of this RFQ. When preparing your quotation, please be guided by the form attached hereto as Annex 2.

Quotations may be submitted on or before **05 June 2020 by 10:00** **via dedicated email**: [offers.mk@undp.org](mailto:offers.mk@undp.org).

Subject: RFQ 42/2020 for Supply of agricultural equipment

It shall remain your responsibility to ensure that your quotation will reach UNDP before the deadline. Quotations that are received by UNDP after the deadline indicated above, for whatever reason, shall not be considered for evaluation.

Please take note of the following requirements and conditions pertaining to the supply of the abovementioned good/s:

|  |  |  |
| --- | --- | --- |
| Delivery Terms  [[INCOTERMS 2020](https://www.kn-portal.com/incoterms_2020/)]  *(Pls. link this to price schedule)* | FCA  CPT  CIP  DAP  Other *[pls. specify]* | |
| Customs clearance[[1]](#footnote-1), if needed, shall be done by: | UNDP  Supplier/Offeror  Freight Forwarder | |
| Exact Address/es of Delivery Location/s (identify all, if multiple) | Strumica | |
| UNDP Preferred Freight Forwarder, if any[[2]](#footnote-2) | N/A | |
| Distribution of shipping documents *(if using freight forwarder)* | N/A | |
| Latest Expected Delivery Date and Time *(if delivery time exceeds this, quote may be rejected by UNDP)* | 60 days from the issuance of the Purchase Order (PO) | |
| Delivery Schedule | Required  Not Required | |
| Packing Requirements | N/A | |
| Mode of Transport | AIR | LAND |
| SEA | OTHER *[pls. specify]* |
| Preferred  Currency of Quotation[[3]](#footnote-3) | United States Dollars  Euro  Local Currency : MKD | |
| Value Added Tax on Price Quotation[[4]](#footnote-4) | Must be inclusive of VAT and other applicable indirect taxes  Must be exclusive of VAT | |
| After-sales services required | Warranty on Parts and Labor for minimum period of Click to type  Technical Support  Provision of Service Unit when pulled out for maintenance/ repair  Others *[pls. specify]* | |
| Deadline for the Submission of Quotation | COB,Indicate date *and* Time zone | |
| All documentations, including catalogs, instructions and operating manuals, shall be in this language | English  French  Spanish  Others *[pls. specify, including dialects, if needed]* | |
| Documents to be submitted[[5]](#footnote-5) | Duly Accomplished Form as provided in Annex 2, and in accordance with the list of requirements in Annex 1;  A statement whether any import or export licenses are required in respect of the goods to be purchased including any restrictions on the country of origin, use/dual use nature of goods or services, including and disposition to end users;  Confirmation that licenses of this nature have been obtained in the past and an expectation of obtaining all the necessary licenses should the quotation be selected;  Quality Certificates (ISO, etc.) and/or other similar certificates, accreditations, awards and citations received by the Bidder, if any;  Latest Business Registration Certificate ;  Company profile ;  Latest Internal Revenue Certificate / Tax Clearance;  Manufacturer’s Authorization of the Company as a Sales Agent (if Supplier is not the manufacturer);  Certificate of Exclusive Distributorship in the country (if applicable, and if Supplier is not the manufacturer);  Evidence/Certification of Environmental Sustainability (“Green” Standards) of the Company or the Product being supplied ;  Complete documentation, information and declaration of any goods classified or may be classified as “Dangerous Goods”.  Patent Registration Certificates (if any of technologies submitted in the quotation is patented by the Supplier);  Written Self-Declaration of not being included in the UN Security Council 1267/1989 list, UN Procurement Division List or other UN Ineligibility List;  Technical description of items: Full detail including technical and performance characteristics and exact model and country of origin for all listed items  ☒ Manufacturer’s Authorization of the Company or from authorized dealer for after-sale service  **☒** Warranty statement for all items listed in the specification  **☒** At least 2 references from beneficiary institutions/companies to whom you have supplied such or similar equipment  Others *[pls. specify as many as required]* | |
| Period of Validity of Quotes starting the Submission Date | 60 days  90 days  120 days  In exceptional circumstances, UNDP may request the Vendor to extend the validity of the Quotation beyond what has been initially indicated in this RFQ. The Proposal shall then confirm the extension in writing, without any modification whatsoever on the Quotation. | |
| Partial Quotes | Not permitted  Permitted **per LOTs** **(1-12)** | |
| Payment Terms[[6]](#footnote-6) | 100% upon complete delivery of goods  Others *[pls. specify]* | |
| Liquidated Damages | Will not be imposed  Will be imposed under the following conditions :  Percentage of contract price per day of delay : \_\_\_\_\_\_  Max. no. of days of delay : \_\_\_\_\_\_  After which UNDP may terminate the contract. | |
| Evaluation Criteria  *[check as many as applicable]* | Technical responsiveness/Full compliance to requirements and lowest price[[7]](#footnote-7)  Comprehensiveness of after-sales services  Full acceptance of the PO/Contract General Terms and Conditions *[this is a mandatory criteria and cannot be deleted regardless of the nature of services required]*  Earliest Delivery / Shortest Lead Time[[8]](#footnote-8)  Others *[pls. specify]* | |
| UNDP will award to: | One and only one supplier  One or more Supplier, depending on the following factors: **depending on the offers per LOTs** | |
| Type of Contract to be Signed | Purchase Order  Contract Face Sheet (Goods and-or Services) UNDP (this template is also utilised for Long-Term Agreement[[9]](#footnote-9) and *if LTA will be signed, specify the document that will trigger the call-off. E.g., PO, etc.)*  Other Type/s of Contract *[pls. specify]* | |
| Contract General Terms and Conditions | General Terms and Conditions for contracts (goods and/or services)  General Terms and Conditions for de minimis contracts (services only, less than $50,000)  Applicable Terms and Conditions are available at  <http://www.undp.org/content/undp/en/home/procurement/business/how-we-buy.html> | |
| Special conditions of Contract | Cancellation of PO/Contract if the delivery/completion is delayed by 60 days  Others *[pls. specify]* | |
| Conditions for Release of Payment | Passing Inspection *[specify method, if possible]*  Complete Installation  Passing all Testing *[specify standard, if possible]*  Completion of Training on Operation and Maintenance *[specify no. of trainees, and location of training, if possible*  Written Acceptance of Goods based on full compliance with RFQ requirements  Others *[pls. specify]* | |
| Annexes to this RFQ[[10]](#footnote-10) | Specifications of the Goods Required (Annex 1)  Form for Submission of Quotation (Annex 2)  [General Terms and Conditions / Special Conditions](https://popp.undp.org/_Layouts/15/POPPOpenDoc.aspx?ID=POPP-11-2493)  Others *[pls. specify, if any]*  Non-acceptance of the terms of the General Terms and Conditions (GTC) shall be grounds for disqualification from this procurement process. | |
| Contact Person for Inquiries  (Written inquiries only)[[11]](#footnote-11) | *Procurement Unit*    *procurement.mk@undp.org*  Any delay in UNDP’s response shall be not used as a reason for extending the deadline for submission, unless UNDP determines that such an extension is necessary and communicates a new deadline to the Proposers. | |

Goods offered shall be reviewed based on completeness and compliance of the quotation with the minimum specifications described above and any other annexes providing details of UNDP requirements.

The quotation that complies with all of the specifications, requirements and offers the lowest price, as well as all other evaluation criteria indicated, shall be selected. Any offer that does not meet the requirements shall be rejected.

Any discrepancy between the unit price and the total price (obtained by multiplying the unit price and quantity) shall be re-computed by UNDP. The unit price shall prevail and the total price shall be corrected. If the supplier does not accept the final price based on UNDP’s re-computation and correction of errors, its quotation will be rejected.

After UNDP has identified the lowest price offer, UNDP reserves the right to award the contract based only on the prices of the goods in the event that the transportation cost (freight and insurance) is found to be higher than UNDP’s own estimated cost if sourced from its own freight forwarder and insurance provider.

At any time during the validity of the quotation, no price variation due to escalation, inflation, fluctuation in exchange rates, or any other market factors shall be accepted by UNDP after it has received the quotation. At the time of award of Contract or Purchase Order, UNDP reserves the right to vary (increase or decrease) the quantity of services and/or goods, by up to a maximum twenty-five per cent (25%) of the total offer, without any change in the unit price or other terms and conditions.

Any Purchase Order that will be issued as a result of this RFQ shall be subject to the General Terms and Conditions attached hereto. The mere act of submission of a quotation implies that the vendor accepts without question the General Terms and Conditions of UNDP indicated above - <http://www.undp.org/content/undp/en/home/procurement/business/how-we-buy.html> .

UNDP is not bound to accept any quotation, nor award a contract/Purchase Order, nor be responsible for any costs associated with a Supplier’s preparation and submission of a quotation, regardless of the outcome or the manner of conducting the selection process.

Please be advised that UNDP’s vendor protest procedure is intended to afford an opportunity to appeal for persons or firms not awarded a purchase order or contract in a competitive procurement process. **In the event that** you believe you have not been fairly treated, you can find detailed information about vendor protest procedures in the following link:

<http://www.undp.org/content/undp/en/home/operations/procurement/protestandsanctions/>

**UNDP encourages every prospective Vendor to** avoid and prevent conflicts of interest, by disclosing to UNDP if you, or any of your affiliates or personnel, were involved in the preparation of the requirements, design, specifications, cost estimates, and other information used in this RFQ.

UNDP implements a zero tolerance on fraud and other proscribed practices, and is committed to identifying and addressing all such acts and practices against UNDP, as well as third parties involved in UNDP activities. UNDP expects its suppliers to adhere to the UN Supplier Code of Conduct found in this link : <http://www.un.org/depts/ptd/pdf/conduct_english.pdf>

**Thank you and we look forward to receiving your quotation.**

**Annex 1**

**Technical Specification**

**Remark:** Please note that the given specifications are the minimum requirements that must be met by your offer. UNDP will not accept any specification that is below these requirements. You may, however, offer better performance and higher specifications.

Contract will be awarded to a company/companies that will meet the specifications and offer the lowest price.

**LOT 1: Влечен атомизер/Trailed atomizer (sprayer)**

|  |  |  |
| --- | --- | --- |
| **Technical specification** | **Техничка спецификација** |  |
| **Atomizer 1000 liters - 1 pieces** | **Атомизер 1000 литри - 1 парчиња** | Indicate “yes” if min. requirements are met or indicate “your” specs. If exceeding the required ones |
| Tank capacity 1000 liters | Капацитет на буре 1000 литри | YES/NO |
| Pump-minimum 5 piston, Minimum 125 liters/min flow | Пумпа минимум 5 клипна, проток минимум 125 литри/минута | YES/NO |
| Number of nozzles: min.12 | Број на бренери: најмалку 12 | YES/NO |
| Tank material: polyethylene | Материјал на буре: полиетилен | YES/NO |
| Fan diameter minimum Ø F800 | Вентилатор: минимум Ø 800 дијаметар | YES/NO |
| Light signaling in transport | Светлосна сигнализација при транспорт | YES/NO |
| Speed reducer for controlling fan speed /rotation | Редуктор за регулирање на бројот на вртежи на перката | YES/NO |
| Self-charging from a water tank | Самополнење од резервоар со вода | YES/NO |
| Additional small tank with clean water for washing hands | Дополнителен мал резервоар со чиста вода за миење на раце | YES/NO |
| Main cleaning filter | Главен филтер за прочистување | YES/NO |
| Secondary filters for fine filtration | Секундарни филтри за фина филтрација | YES/NO |
| Valve for liquid discharge in the tank | Вентил за испуштање на течноста во резервоарот | YES/NO |
| Warranty – 24 months minimum | Гаранција – минимум 24 месеци | YES/NO |
| Service/Repair provided to the equipment within 30 days upon reported issue | Обезбеден сервис/поправка на опремата во рок од 30 дена максимум од денот на пријавување на проблемот | YES/NO |
| Evidence that the service support is regulated between the offeror and authorized service provider in the country, if the offeror is not also service provider. Please provide proof if your company is an authorized service provider | Доказ за регулирање на сервисната поддршка помеѓу понудувачот и авторизираниот сервисер во земјата, ако понудувачот не е истовремено овластен сервис. Да се достави доказ ако компанијата е авторизиран сервисер. | YES/NO |
| Operation and maintenance | Обука за користење и одржување на опремата | YES/NO |

**LOT 2: Мулчер/Flail mower**

|  |  |  |
| --- | --- | --- |
| **Technical specifications** | **Техничка Спецификација** | Indicate “yes” if min. requirements are met or indicate “your” specs. If exceeding the required ones |
| **Flail Mower - 2 pieces** | **Мулчер - 2 парчиња** | YES/NO |
| Mechanic offset | Механички страничен помест | YES/NO |
| Metal flaps | Метални завеси | YES/NO |
| Height adjustable rear roller | Заден ваљак подесив по висина | YES/NO |
| Working units hammers | Работни тела чекани | YES/NO |
| P.T.O shaft | Карданско вратило | YES/NO |
| Power requirements: minimum 35 HP | Потребна снага на трактор: минумум 35 кс | YES/NO |
| Maximal diameter of mulched branches: up to 5 cm | Можност за кршење дрвца со дебелина до 5 см. | YES/NO |
| Weight: minimum 290 kg, maximum 400kg | Тежина на мулчер: минимум 290 кг, максимум 400 кг | YES/NO |
| Working width: minimum 1,55 meters, maximum –1,65 meters | Работна ширина: минимум 1,55, максимум 1,65 метри | YES/NO |
| Warranty – 24 months minimum | Гаранција – минимум 24 месеци | YES/NO |
| Service/Repair provided to the equipment within 30 days upon reported issue | Обезбеден сервис/поправка на опремата во рок од 30 дена максимум од денот на пријавување на проблемот | YES/NO |
| Evidence that the service support is regulated between the offeror and authorized service provider in the country, if the offeror is not also service provider. Please provide proof if your company is an authorized service provider | Доказ за регулирање на сервисната поддршка помеѓу понудувачот и авторизираниот сервисер во земјата, ако понудувачот не е истовремено овластен сервис. Да се достави доказ ако компанијата е авторизиран сервисер. | YES/NO |
| Operation and maintenance | Обука за користење и одржување на опремата | YES/NO |

**LOT 3: Рото фреза/Rotary tiller**

|  |  |  |
| --- | --- | --- |
| **Technical specifications** | **Техничка Спецификација** | Indicate “yes” if min. requirements are met or indicate “your” specs. If exceeding the required ones |
| **Rotary tiller**  **(8 pieces)** | **Рото-фреза**  **(8 парчиња)** | YES/NO |
| Working width 85 cm | Работен зафат од 185 см | YES/NO |
| Weight size minimum -250 kg | Тежина минимум 250 кг | YES/NO |
| Tractor required power: minimum 35 HP | Потребна снага на трактор: минимум 35 КС | YES/NO |
| Included shaft | Вклучен кардан | YES/NO |
| Warranty – 24 months minimum | Гаранција – минимум 24 месеци | YES/NO |
| Service/Repair provided to the equipment within 30 days upon reported issue | Обезбеден сервис/поправка на опремата во рок од 30 дена максимум од денот на пријавување на проблемот | YES/NO |
| Evidence that the service support is regulated between the offeror and authorized service provider in the country, if the offeror is not also service provider. Please provide proof if your company is an authorized service provider | Доказ за регулирање на сервисната поддршка помеѓу понудувачот и авторизираниот сервисер во земјата, ако понудувачот не е истовремено овластен сервис. Да се достави доказ ако компанијата е авторизиран сервисер. | YES/NO |
| Operation and maintenance | Обука за користење и одржување на опремата | YES/NO |

**LOT 4: Тањирача/Disk Harrow**

|  |  |  |
| --- | --- | --- |
| **Technical specifications** | **Техничка Спецификација** | Indicate “yes” if min. requirements are met or indicate “your” specs. If exceeding the required ones |
| **Disk Harrow**  **(5 pieces)** | **Тањирача**  **(5 парчиња)** | YES/NO |
| Working bodies-min 20 | Работни тела-min 20 | YES/NO |
| With 4 axles | Со 4 осовини | YES/NO |
| With 5 disks per axle | Со 5 дискови по осовина | YES/NO |
| 3 points of connection | 3 точки на приклучување | YES/NO |
| Tractor required power: minimum 25 HP | Потребна снага на трактор: минимум 25 КС | YES/NO |
| Warranty – 24 months minimum | Гаранција – минимум 24 месеци | YES/NO |
| Service/Repair provided to the equipment within 30 days upon reported issue | Обезбеден сервис/поправка на опремата во рок од 30 дена максимум од денот на пријавување на проблемот | YES/NO |
| Evidence that the service support is regulated between the offeror and authorized service provider in the country, if the offeror is not also service provider. Please provide proof if your company is an authorized service provider | Доказ за регулирање на сервисната поддршка помеѓу понудувачот и авторизираниот сервисер во земјата, ако понудувачот не е истовремено овластен сервис. Да се достави доказ ако компанијата е авторизиран сервисер. | YES/NO |
| Operation and maintenance | Обука за користење и одржување на опремата | YES/NO |

**LOT 5: Носен атомизер/ Mounted atomizer**

|  |  |  |
| --- | --- | --- |
| **Technical specifications** | **Техничка Спецификација** | Indicate “yes” if min. requirements are met or indicate “your” specs. If exceeding the required ones |
| **Mounted atomizer - 5 pieces** | **Носен атомизер –**  **5 парчиња** | YES/NO |
| Tank capacity 350 liters | Капацитет на буре 350 литри | YES/NO |
| Pump capacity min 75 l per minute | Пумпа капацитет минимум 75 литри во минута | YES/NO |
| Piston pump minimum 3 cylinders | Клипна пумпа со минимум 3 цилиндри | YES/NO |
| Tank material: polyester | Материјал на буре: полиестер | YES/NO |
| Self-charging from a water tank | Самополнење од резервоар со вода | YES/NO |
| Warranty – 24 months minimum | Гаранција – минимум 24 месеци | YES/NO |
| Service/Repair provided to the equipment within 30 days upon reported issue | Обезбеден сервис/поправка на опремата во рок од 30 дена максимум од денот на пријавување на проблемот | YES/NO |
| Evidence that the service support is regulated between the offeror and authorized service provider in the country, if the offeror is not also service provider. Please provide proof if your company is an authorized service provider | Доказ за регулирање на сервисната поддршка помеѓу понудувачот и авторизираниот сервисер во земјата, ако понудувачот не е истовремено овластен сервис. Да се достави доказ ако компанијата е авторизиран сервисер. | YES/NO |
| Operation and maintenance | Обука за користење и одржување на опремата | YES/NO |

**LOT 6: Носен атомизер/ Mounted atomizer**

|  |  |  |
| --- | --- | --- |
| **Technical specifications** | **Техничка Спецификација** | Indicate “yes” if min. requirements are met or indicate “your” specs. If exceeding the required ones |
| **Mounted atomizer - 1 piece** | **Носен атомизер –**  **1 парче** | YES/NO |
| Tank capacity 450 liters | Капацитет на буре 450 литри | YES/NO |
| Pump capacity min 75 l per minute | Пумпа капацитет минимум 75 литри во минута | YES/NO |
| Tank material: polyester | Материјал на буре: полиестер | YES/NO |
| Piston pump minimum 3 cylinders | Клипна пумпа со минимум 3 цилиндри | YES/NO |
| Self-charging from a water tank | Самополнење од резервоар со вода | YES/NO |
| Warranty – 24 months minimum | Гаранција – минимум 24 месеци | YES/NO |
| Service/Repair provided to the equipment within 30 days upon reported issue | Обезбеден сервис/поправка на опремата во рок од 30 дена максимум од денот на пријавување на проблемот | YES/NO |
| Evidence that the service support is regulated between the offeror and authorized service provider in the country, if the offeror is not also service provider. Please provide proof if your company is an authorized service provider | Доказ за регулирање на сервисната поддршка помеѓу понудувачот и авторизираниот сервисер во земјата, ако понудувачот не е истовремено овластен сервис. Да се достави доказ ако компанијата е авторизиран сервисер. | YES/NO |
| Operation and maintenance | Обука за користење и одржување на опремата | YES/NO |

**LOT 7: Inter row rotary tiller / Меѓуредна рото фреза**

|  |  |  |
| --- | --- | --- |
| **Technical specifications** | **Техничка Спецификација** | Indicate “yes” if min. requirements are met or indicate “your” specs. If exceeding the required ones |
| **Inter row rotary tiller**  **(5 piece)** | **Меѓуредна рото-фреза**  **(5 парче)** | YES/NO |
| Number of working blades: min 15 – max 20 | Број на работни тела: min 15 –max 20 | YES/NO |
| Working width min 60 – max 70 cm | Работен зафат од min 60 до max 70 см | YES/NO |
| Weight min 390 – max 440 kg | Тежина од min 390 до max 440 кг | YES/NO |
| Distance between rows min 220 – max 270 cm | Растојание меѓу редови од min 220 – max 270 см | YES/NO |
| Height of working blades: minimum 35 | Висина на работно тело: минимум 35 см | YES/NO |
| Tractor required power: minimum 35 HP | Потребна снага на трактор: минимум 35 КС | YES/NO |
| Two wheels for machine control | Две тркала за контрола на машината | YES/NO |
| Warranty – 24 months minimum | Гаранција – минимум 24 месеци | YES/NO |
| Service/Repair provided to the equipment within 30 days upon reported issue | Обезбеден сервис/поправка на опремата во рок од 30 дена максимум од денот на пријавување на проблемот | YES/NO |
| Evidence that the service support is regulated between the offeror and authorized service provider in the country, if the offeror is not also service provider. Please provide proof if your company is an authorized service provider | Доказ за регулирање на сервисната поддршка помеѓу понудувачот и авторизираниот сервисер во земјата, ако понудувачот не е истовремено овластен сервис. Да се достави доказ ако компанијата е авторизиран сервисер. | YES/NO |
| Operation and maintenance | Обука за користење и одржување на опремата | YES/NO |

**LOT 8: Електрични ножици за кроење/ Electronic pruning shears**

|  |  |  |
| --- | --- | --- |
| **Technical specifications** | **Техничка Спецификација** | Indicate “yes” if min. requirements are met or indicate “your” specs. If exceeding the required ones |
| **Electronic pruning shears**  **(5 pieces)** | **Електрични ножици за кроење**  **(5 парчиња)** | YES/NO |
| Cutting diameter min 30- max 40 mm | кроење на гранки со дијаметар min 30-max 40 мм | YES/NO |
| Complete harness | Елек со батерија | YES/NO |
| Battery LI-ION: 4 до 5 Ah | Батерија LI-ION од 4 до 5 Ah | YES/NO |
| Power: minimum 90W | Јачина минимум 90W | YES/NO |
| Battery charger included | Полнач за батерија вклучен | YES/NO |
| Cary case kit included | Кутија за носење вклучена |  |
| Warranty – 24 months minimum | Гаранција – минимум 24 месеци | YES/NO |
| Service/Repair provided to the equipment within 30 days upon reported issue | Обезбеден сервис/поправка на опремата во рок од 30 дена максимум од денот на пријавување на проблемот | YES/NO |
| Evidence that the service support is regulated between the offeror and authorized service provider in the country, if the offeror is not also service provider. Please provide proof if your company is an authorized service provider | Доказ за регулирање на сервисната поддршка помеѓу понудувачот и авторизираниот сервисер во земјата, ако понудувачот не е истовремено овластен сервис. Да се достави доказ ако компанијата е авторизиран сервисер. | YES/NO |
| Operation and maintenance | Обука за користење и одржување на опремата | YES/NO |

**LOT 9: Мулч фолија/Mulch film**

|  |  |  |
| --- | --- | --- |
| **Technical specifications** | **Техничка Спецификација** | Indicate “yes” if min. requirements are met or indicate “your” specs. If exceeding the required ones |
| **Mulch film - 10.000 m2** | **Фолија за мулчирање - 10.000 m2** |  |
| Silver / Brown | Сребрена боја / кафеава (двобојна) | YES/NO |
| Thickness minimum 20 micron | Дебелина минимум 20 микрона | YES/NO |
| Width 1 - 1,5 m | Ширина од 1 до 1,5 метри | YES/NO |
| Light transmission in PAR < 4 (according to ASTM D-1003 method) | Непрозирна (трансмисија на светлина помалку од 4 по метода ASTM D-1003) | YES/NO |
| Reflection in PAR 25 (according to ASTM D-1003 method) | Рефлексија на светлина 25 (по метода ASTM D-1003) | YES/NO |
| Tensile strength at break minimum 24-25 Mpa (according to ASTM D-882) | Цврстина на истегнување најмалку 24-25 Mpa (по метода ASTM D-882) | YES/NO |
| Elongation at break 450-650% (according to ASTM D-882) | Издолжување до кинење 450-650% (по метода ASTM D-882) | YES/NO |

**LOT 10: Полиетиленско платно-најлон/Polyethylene cover film**

|  |  |  |
| --- | --- | --- |
| **Technical specification**  **min. requirements** | **Спецификација** | **min. requirements** |
| **Polyethylene cover film (57.168 m2)** | **Полиетиленско платно-најлон (57.168 m2)** |  |
| Thickness: 5 layers, 150 micron | Дебелина: 5 слојно, 150 микронско | YES/NO |
| Width 8 mеters | Ширина 8 метри | YES/NO |
| Light transmission 88% | Трансмисија на светлина 88% | YES/NO |
| Light diffusion 55 % | Дифузија на светлина 55% | YES/NO |
| ANTI DRIP effect | ANTI DRIP ефект | YES/NO |
| Thermicity 85% | Термичност 85% | YES/NO |
| Reduced dust accumulation | Намалено собирање на прав | YES/NO |

**LOT 11: Полиетиленско платно-најлон/Polyethylene cover film**

|  |  |  |
| --- | --- | --- |
| **Technical specification**  **min. requirements** | **Спецификација** | **min. requirements** |
| **Polyethylene cover film (15.978 m2)** | **Полиетиленско платно-најлон (15.978 m2)** |  |
| Thickness: 5 layers, 150 micron | Дебелина: 5 слојно, 150 микронско | YES/NO |
| Width 6 mеters | Ширина 6 метри | YES/NO |
| Light transmission 88% | Трансмисија на светлина 88% | YES/NO |
| Light diffusion 55 % | Дифузија на светлина 55% | YES/NO |
| ANTI DRIP effect | ANTI DRIP ефект | YES/NO |
| Thermicity 85% | Термичност 85% | YES/NO |

**LOT 12: Црева за наводнување/Irrigation pipes**

|  |  |  |
| --- | --- | --- |
| **Technical specification**  **min. requirements** | **Спецификација** | **min. requirements** |
| **Pipe for irrigation Ø 16 with drips installed at 25 centimeters distance (26.000 m)**  Working pressure of the pipе max 4 bars | **Црево за наводнување Ø 16 со монтирани капалки на растојание од 25 сантиметри (26.000 m)**  Работен притисок на цревата максимум 4 бари | YES/NO |
| **Pipe for irrigation Ø 16 with drips installed at 20 centimeters distance (22.000 m)**  Working pressure of the pipе max 4 bars | **Црево за наводнување Ø 16 со монтирани капалки на растојание од 20 сантиметри (22.000 m)**  Работен притисок на цревата максимум 4 бари | YES/NO |
| **Pipe for irrigation Ø 16 with drips installed at 33 centimeters distance (1.200 m)**  Working pressure of the pipе max 4 bars | **Црево за наводнување Ø 16 со монтирани капалки на растојание од 33 сантиметри (1.200 m)**  Работен притисок на цревата максимум 4 бари | YES/NO |
| **Pipe for irrigation Ø 16 with self-compensatory drips installed on 40 centimeters distance (3.000 m)** Working pressure of the pipе max 4 bars | **Црево за наводнување Ø 16 со монтирани компензирачки капалки на растојание од 40 сантиметри (3.000 m)** Работен притисок на цревата максимум 4 бари | YES/NO |
| **Pipe for irrigation Ø 20 (12.500 m)**  Working pressure of the pipе max 4 bars | **Црево за наводнување Ø 20 (12.500 m)**  Работен притисок на цревата максимум 4 бари | YES/NO |
| **Pipe for irrigation Ø 50 (2.175m)**  Working pressure of the pipе at least 6 bars | **Црево за наводнување Ø 50 (2.175 m)**  Работен притисок на цревата најмалку 6 бари | YES/NO |
| **Pipe for irrigation Ø 63 (800 m)**  Working pressure of the pipе at least 6 bars | **Црево за наводнување Ø 63 (800 m)**  Работен притисок на цревата најмалку 6 бари | YES/NO |

*\*Pls. attach delivery schedule, if relevant, and cluster by lot, if partial bids will be allowed. Specify delivery locations if goods multiple destinations.*

*[Enter name of authorized staff]*

*[Designation]* [*Click here to enter a date]*

**Annex 2**

**FORM FOR SUBMITTING SUPPLIER’S QUOTATION**

***(This Form must be submitted only using the Supplier’s Official Letterhead/Stationery***

***Vakov documentza finansova ponuda da bide podnesen so kompanisko logo na Ponuduvacot I davame moznost da se podnese na makedonski )***

We, the undersigned, hereby accept in full the UNDP General Terms and Conditions, and hereby offer to supply the items listed below in conformity with the specification and requirements of UNDP as per RFQ Reference No. 42/2020 for Supply of agricultural equipment (LOTs 1 – 12)

**TABLE 1: Offer to Supply Goods Compliant with Technical Specifications and Requirements**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Item No.** | **Description/Specification of Goods** | **Quantity** | **Latest Delivery Date** | **Unit Price** | **Total Price per Item, VAT excluded** |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  | **Total Prices of Goods, VAT presented separately** | | | |  |

All other information that we have not provided automatically implies our full compliance with the requirements, terms and conditions of the RFQ.

*[Name and Signature of the Supplier’s Authorized Person]*

*[Designation]*

*[Date]*

***Stamp***

1. *Must be linked to* [*INCO Terms 2020*](https://www.kn-portal.com/incoterms_2020/) *chosen.* [↑](#footnote-ref-1)
2. *Depends on* [*INCO Terms 2020*](https://www.kn-portal.com/incoterms_2020/)*. The suggestion to use a UNDP preferred courier is only for purposes of familiarity with procedures and documentary requirements applicable to the UNDP when clearing with customs.*  [↑](#footnote-ref-2)
3. *Local vendors must comply with any applicable laws regarding doing business in other currencies. Conversion of currency into the UNDP preferred currency, if the offer is quoted differently from what is required, shall be based only on UN Operational Exchange Rate prevailing at the time of UNDP’s issuance of Purchase Order.* [↑](#footnote-ref-3)
4. *This must be reconciled with the* [*INCO Terms 2020*](https://www.kn-portal.com/incoterms_2020/) *required by the RFQ. Furthermore, VAT exemption status varies from one country to another. Pls. tick whatever is applicable to the UNDP CO/BU requiring the goods.* [↑](#footnote-ref-4)
5. *First 2 items in this list are mandatory for the supply of imported goods*  [↑](#footnote-ref-5)
6. *.* [↑](#footnote-ref-6)
7. *UNDP reserves the right not to award the contract to the lowest priced offer, if the second lowest price among the responsive offer is found to be significantly more superior, and the price is higher than the lowest priced compliant offer by not more than 10%, and the budget can sufficiently cover the price difference. The term “more superior” as used in this provision shall refer to offers that have exceeded the pre-determined requirements established in the specifications.* [↑](#footnote-ref-7)
8. *This shall be used for time-critical and/or exigent requirements (e.g., post-crisis emergencies, elections, etc.).* [↑](#footnote-ref-8)
9. *Minimum of one (1) year period and may be extended up to a maximum of three (3) years subject to satisfactory performance evaluation* [↑](#footnote-ref-9)
10. *Where the information is available in the web, a URL for the information may simply be provided.* [↑](#footnote-ref-10)
11. *This contact person and address is officially designated by UNDP. If inquiries are sent to other person/s or address/es, even if they are UNDP staff, UNDP shall have no obligation to respond nor can UNDP confirm that the query was received.* [↑](#footnote-ref-11)