Maize Sheller /Stationary Detail Specification with one week 145 operators training

|  |  |  |  |
| --- | --- | --- | --- |
| No | Description | Unit of Measure | Quantity |
| 1 | * Stationary corn sheller, steel made; * Manually powered via wood handle; * Threshing mechanism: Enclosed metal rasp bar cylinder; * Fitted with a feeding tray; * Output fitted with bagging system; * All exposed moving parts to be fully guarded ; * Dimensions (L x W x H) : 30 x 25 x 20 cm approximately; * Weight: 5-8 kg approximately; * Capacity: 100 kg/h approximately | pcs | 25 |
| 2 | One week Operating of Maize Sheller training | trainees | 145 |
|  |  |  |  |