{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["TOUBA KOLONG"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"TOUBA KOLONG","index":0,"n_rows":56,"n_cols":7,"rows_kept":56,"cut":false,"hidden":false,"merged":[[0,0,0,6],[2,0,2,6],[4,0,4,6],[41,3,41,5],[49,3,49,5]]}
["PROGRAM FOR ACCELERATED COMMUNITY DEVELOPMENT (PACD)"]
[]
["RURAL ELECTRIFICATION PROJECT (PHASE 2)"]
[]
["PROPOSED 160KVA TRANSFORMER & LV NETWORK FOR TOUBA KOLONG"]
[null,"                                     "]
["ITEM","         MATERIALS & DESCRIPTION","SIZE","UNIT","QTY","UNIT PRICE","TOTAL"]
["A","ELECTRICAL WORKS"]
[1,"TRANSFORMER (30KV)","160kva","pcs",1]
[2,"ARRESTORS","30KV","set",1]
[3,"FUSE CUT-OUT","30KV","set",1]
[4,"PC CONNECTORS",null,"pcs",6]
[5,"MOSDOFAR","30KV","pcs",1]
[6,"MAIN LINE TAP FOR BARE CONDUCTOR","70/95mm","pcs",12]
[7,"EARTHING LESS THAN 10 OHM",null,null,1]
[8,"MV STEEL POLE","850dan","pcs",1]
[9,"MV STEEL POLE","1600dan","pcs",0]
[10,"MV POLE FOUNDATION",null,null,1]
[10,"ADDITIONAL CONCRETE POLE","28'","pcs",0]
[11,"ADDITIONAL CONCRETE POLE","32'","pcs",1]
[13,"POLES TO BE RELOCATED",null,"pcs",6]
[14,"POLES TO BE SHIFTED",null,"pcs",13]
[12,"POLES TO BE REPLACED",null,"pcs",0]
[13,"BOLT & NUT","9 x 5/8","pcs",68]
[14,"SUPPLY OF SUSPENSION ASSEMBLY","ES 1500","pcs",53]
[15,"SUPPLY OF SINGLE ANCHOR ASSEMBLY","EA 1500","pcs",25]
[16,"SUPPLY OF DOUBLE ANCHOR ASSEMBLY","EAD 1500","pcs",1]
[17,"SUPPLY OF CONNECTOR","2S70,150","pcs",48]
[18,"RILSAN TIE","C55,96","pcs",207]
[19,"END CAP","CRR1670","pcs",52]
[20,"TWISTED CABLE 4X 70mm",null,"meters",3381]
[21,"TRIMMING & CUTTING",null,null,1]
[22,"LABOUR COST",null,null,1]
[23,"TRANSPORTATION",null,null,1]
[null,"SUB-TOTAL",{"$nulls":4},{"$f":"SUM(G9:G34)","v":0}]
[]
["B","CIVIL WORKS"]
[null,"DEMOLITION, EXCAVATION, FILLING AND SITE CLEARANCE"]
[1,"CLEAR ALL SHRUBS, WEEDS AND DEBRIS AROUND AREA OF PIT",null,"m2",70]
[2,"EXCAVATE TO RECEIVE FOUNDATION PIT (500 x 600 x 1400mm) ",null,"m3",29]
[3,"SPREAD NEATLY EXCAVATED MATERIALS AROUND AREA OF PIT",null,"m3",29]
[4,"ALLOW FOR REMOVAL, SHIFTING AND REALIGNMENT OF EXISTING POLES AND MAKE GOOD AREAS AFFECTED",null,"lumpsum"]
[]
[null,"CONCRETE"]
[null,"PLAIN IN-SITU CONCRETE 20N/MM2 20MM AGGREGATE SIZE SCREEN GRAVEL MIX RATIO 1:2:4"]
[1,"POLE FOUNDATION FOOTING FOR ANGLE AND DEAD END POLES (500X600X1400MM)","28'/32'","m3",8]
[2,"POLE FOUNDATION FOOTING FOR INTERMEDIATE POLES (500X600X500MM)","28'/32'","m3",8]
[3,"BOULDER STONES FOR INTERMEDIATE POLES (500X600X900MM)",null,"m3",14]
[4,"POLE FOUNDATION FOR MV POLES AND TRANSFORMER POLES ","28'/32'","m3",1]
[5,"SITE CLEANING UPON COMPLETION OF THE WORK",null,"lumpsum"]
[null,"SUB-TOTAL"]
[null,"TOTAL"]
[]
[null,"ALLOW FOR CONTINGENCY",null,0.1]
[]
[null,"GRAND TOTAL"]