{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":78,"n_cols":5,"rows_kept":78,"cut":false,"hidden":false,"merged":[[29,1,54,1],[3,1,7,1],[0,0,0,4],[2,0,2,2],[55,0,77,0],[55,1,77,1],[29,0,54,0]]}
["Hiring Project to Restore Agricultural Oasis No. 47 in Anah"]
["Item # in BOQ","Item","Description ","Required Specifications","Offered Specifications"]
["E- Rehabilitation of The Farms Irrigation Pipes System "]
[6,"Horizontal Pump of Q= 110 m3/hr. and H= 80 m ","Rated voltage : ","380V-416V"]
[null,null,"No of phase:  ","3PH  "]
[null,null,"Frequency:  ","50Hz  "]
[null,null,"Make:  ","Original manufacturer "]
[null,null," Required Brand:  "," Grundfos, Wilo, caprari, KSB \" Germany Origin\", Standart, Mas or equivalent which should be approved by the supervisory committee before starting supplying process"]
[null,null,"Rated speed: ","1500 rpm"]
[null,null," Gland type : ","Mechanical seal"]
[null,null,"Enclosure class: ","(IEC 34-5) IP 55"]
[null,null," Insulation class:  "," F "]
[null,null,"Pump liquid:  ","Water "]
[null,null," Suction hole:  ","PN 150 DN16"]
[null,null," Delivery hole: ","PN125DN16"]
[null,null," Motor power :  ","35 KW"]
[null,null,"Rated flow : ","110m3/h"]
[null,null,"Rated head : ","80M "]
[null,null," Material:  ","Cast Iron"]
[null,null,"Shaft:  "," STAINLESS STEEL- GG25 (AISI420)"]
[null,null," Impeller:   "," BRONZE"]
[null,null,"The bearing shall be grease type lubrications:"," Yes/Required"]
[null,null,"Engine coil","Made of copper"]
[null,null,"The shaft of the pump shall be with direct coupling to the motor:","Yes/Required"]
[null,null," Efficiency: ","Not less than 75%"]
[null,null," The motor shall have IEC standard dimensions "," Yes/Required"]
[null,null,"Type of control panel:  ","Soft with all protection devices and metering"]
[null,null,"Submit Manufacturer certification and test reports by BV: ","Yes/Required"]
[null,null," Submit Detail drawing brochure catalogue:   "," Yes/Required"]
[null,"Horizontal Pump of Q= 70 m3/hr. and H= 30 m ","Rated voltage : ","380V-416V"]
[null,null,"No of phase:  ","3PH  "]
[null,null,"Frequency:  ","50Hz  "]
[null,null,"Make:  ","Original manufacturer "]
[null,null," Required Brand:  "," Grundfos, Wilo, caprari, KSB \" Germany Origin\", Standart, Mas or equivalent which should be approved by the supervisory committee before starting supplying process"]
[null,null,"Rated speed: ","1500 rpm"]
[null,null," Gland type : ","Mechanical seal"]
[null,null,"Enclosure class: ","(IEC 34-5) IP 55"]
[null,null," Insulation class:  "," F "]
[null,null,"Pump liquid:  ","Water "]
[null,null," Suction hole:  ","PN 150 DN16"]
[null,null," Delivery hole: ","PN125DN16"]
[null,null," Motor power :  ","20 KW"]
[null,null,"Rated flow : ","70 m3/h"]
[null,null,"Rated head : ","30M "]
[null,null," Material:  ","Cast Iron"]
[null,null,"Shaft:  "," STAINLESS STEEL- GG25 (AISI420)"]
[null,null," Impeller:   "," BRONZE"]
[null,null,"The bearing shall be grease type lubrications:"," Yes/Required"]
[null,null,"Engine coil","Made of copper"]
[null,null,"The shaft of the pump shall be with direct coupling to the motor:","Yes/Required"]
[null,null," Efficiency: ","Not less than 75%"]
[null,null," The motor shall have IEC standard dimensions "," Yes/Required"]
[null,null,"Type of control panel:  ","Soft with all protection devices and metering"]
[null,null,"Submit Manufacturer certification and test reports by BV: ","Yes/Required"]
[null,null," Submit Detail drawing brochure catalogue:   "," Yes/Required"]
[8,"Submersible Pump of Q= 200 m3/hr. and H= 20 m ","Type:"," Submersible water pump"]
[null,null,"Capacity: ","200 m3/hr with 20m head"]
[null,null,"Motor Power:","22.5 KW"]
[null,null,"Materials: ","Cast Iron"]
[null,null,"Motor speed: ","1500 rpm"]
[null,null,"Accessories:"," with complete accessories (Valves and distributers)"]
[null,null,"Connections: ","water connections and supply steel base for fixing the pump"]
[null,null,"Suction hole :","8 inch "]
[null,null,"Delivery hole:","6 inch "]
[null,null,"Protected against water leakage"," Yes/Required"]
[null,null,"Impeller: ","BRONZE"]
[null,null,"Shaft: ","Stainless steel"]
[null,null,"Motor coil: ","Made of copper"]
[null,null,"Rated voltage :","380V-400V"]
[null,null,"No of phase: ","3PH "]
[null,null,"Frequency:  ","50Hz "]
[null,null,"Make: ","Original manufacturer"]
[null,null,"Required Brand: "," Grundfos, Wilo, caprari, KSB \" Germany Origin\", Standart, Mas or equivalent which should be approved by the supervisory committee before starting supplying process"]
[null,null,"Enclosure class:","(IEC 34-5) IP 55"]
[null,null,"Insulation class: ","F"]
[null,null,"Pump liquid: ","Water"]
[null,null,"Submit Manufacturer certification and test reports by BV  :"," Yes/Required"]
[null,null,"Submit Detail drawing brochure catalogue:"," Yes/Required"]