{"text_format":"5","workbook":"xlsx","n_sheets":2,"sheets":["BoQ Summary","BoQ"],"props":{"creator":"GC","last_modified_by":"GC"},"read":"whole","date_system":"1900"}

{"sheet":"BoQ Summary","index":0,"n_rows":6,"n_cols":3,"rows_kept":6,"merged":[[5,0,5,1]]}
["SUMMARY TABLE"]
["Section","Description","TOTAL PRICE (USD)"]
[1,"CIVIL WORKS",{"$f":"+BoQ!G43","v":0}]
[2,"MECHANICAL WORKS",{"$f":"+BoQ!G108","v":0}]
[3,"ELECTRICAL WORKS",{"$f":"+BoQ!G174","v":0}]
["TOTAL ESTIMATED PRICE (Section 1 + 2 + 3)",null,{"$f":"SUM(C3:C5)","v":0}]

{"sheet":"BoQ","index":1,"n_rows":174,"n_cols":7,"rows_kept":174,"merged":[[0,0,0,6],[2,0,2,6],[3,0,3,6],[6,0,6,5],[7,0,7,6],[41,0,41,5],[42,0,42,5],[43,0,43,6],[44,0,44,6],[45,0,45,6],[67,0,67,5],[68,0,68,6],[90,0,90,5],[91,0,91,6],[106,0,106,5],[107,0,107,5],[108,0,108,6],[109,0,109,6],[110,0,110,6],[118,0,118,5],[120,0,120,6],[125,0,125,5],[127,0,127,6],[140,0,140,5],[141,0,141,6],[146,0,146,5],[148,0,148,6],[155,0,155,5],[157,0,157,6],[169,0,169,5],[170,0,170,6],[172,0,172,5],[173,0,173,5]]}
["Bill of Quantities - Construction Works of Container Office Building in Hatay"]
["No","Item No","Description","Unit","Quantity","Unit Price\n(USD)","TOTAL\n(USD)"]
["SECTION-1 CIVIL WORKS"]
["Demolition and Removal Works"]
[1,"DRW.01","Demolition and removal of existing concrete slab and wall","m³",{"v":120,"d":"120.00"},null,{"$f":"+E5*F5","v":{"v":0,"d":"0.00"}}]
[2,"DRW.02","Removal of existing canopy","L.s",{"v":1,"d":"1.00"},null,{"$f":"+E6*F6","v":{"v":0,"d":"0.00"}}]
["Subtotal for Demolition and Removal Works",{"$nulls":5},{"$f":"SUM(G5:G6)","v":{"v":0,"d":"0.00"}}]
["Construction and Architectural Works"]
[1,"CAW.01","Excavation works","m³",255.25,null,{"$f":"+E9*F9","v":{"v":0,"d":"0.00"}}]
[2,"CAW.02","Filling with light aggregate (sieved coal clinker)","m³",{"v":382.5,"d":"382.50"},null,{"$f":"+E10*F10","v":{"v":0,"d":"0.00"}}]
[3,"CAW.03","Ready-mixed concrete (C8/10)","m³",{"v":25.5,"d":"25.50"},null,{"$f":"+E11*F11","v":{"v":0,"d":"0.00"}}]
[4,"CAW.04","Ready-mixed concrete (C25/30)","m³",{"v":115,"d":"115.00"},null,{"$f":"+E12*F12","v":{"v":0,"d":"0.00"}}]
[5,"CAW.05","Rebars Ø8-12mm","ton",{"v":3.5,"d":"3.50"},null,{"$f":"+E13*F13","v":{"v":0,"d":"0.00"}}]
[6,"CAW.06","Rebars Ø14-28mm","ton",{"v":3.8,"d":"3.80"},null,{"$f":"+E14*F14","v":{"v":0,"d":"0.00"}}]
[7,"CAW.07","Timber formwork","m²",{"v":306,"d":"306.00"},null,{"$f":"+E15*F15","v":{"v":0,"d":"0.00"}}]
[8,"CAW.08","Structural steelwork","ton",{"v":7,"d":"7.00"},null,{"$f":"+E16*F16","v":{"v":0,"d":"0.00"}}]
[9,"CAW.09","Perlite and satin plaster","m²",{"v":175,"d":"175.00"},null,{"$f":"+E17*F17","v":{"v":0,"d":"0.00"}}]
[10,"CAW.10","Satin plaster coating (average thickness of 1 mm)","m²",{"v":250,"d":"250.00"},null,{"$f":"+E18*F18","v":{"v":0,"d":"0.00"}}]
[11,"CAW.11","12.5mm thick drywall","m²",{"v":175,"d":"175.00"},null,{"$f":"+E19*F19","v":{"v":0,"d":"0.00"}}]
[12,"CAW.12","Roofing with 0.70 mm thick trapezoidal aluminium plates","m²",{"v":230,"d":"230.00"},null,{"$f":"+E20*F20","v":{"v":0,"d":"0.00"}}]
[13,"CAW.13","Aluminium lay-on suspended ceiling (60x60cm, 0.5mm thickness)","m²",{"v":220,"d":"220.00"},null,{"$f":"+E21*F21","v":{"v":0,"d":"0.00"}}]
[14,"CAW.14","Mortise lock with cylinder (for interior doors, narrow type)","pcs",{"v":6,"d":"6.00"},null,{"$f":"+E22*F22","v":{"v":0,"d":"0.00"}}]
[15,"CAW.15","Door handles and panels (chrome plated)","pcs",{"v":6,"d":"6.00"},null,{"$f":"+E23*F23","v":{"v":0,"d":"0.00"}}]
[16,"CAW.16","Facade cladding with mineral-filled composite aluminium sheets (with 5cm thick rockwool thermal insulation sheets)","m²",{"v":98,"d":"98.00"},null,{"$f":"+E24*F24","v":{"v":0,"d":"0.00"}}]
[17,"CAW.17","Gutter and down pipe made from 0.5 mm thick shop-painted galvanized sheet","m",{"v":48.8,"d":"48.80"},null,{"$f":"+E25*F25","v":{"v":0,"d":"0.00"}}]
[18,"CAW.18","Wall construction with 190mm thick horizontally perforated bricks (190x190x135mm)","m²",{"v":75,"d":"75.00"},null,{"$f":"+E26*F26","v":{"v":0,"d":"0.00"}}]
[19,"CAW.19","Wall or floor covering with natural stone mosaics (split surface)","m²",{"v":75,"d":"75.00"},null,{"$f":"+E27*F27","v":{"v":0,"d":"0.00"}}]
[20,"CAW.20","External thermal insulation","m²",{"v":75,"d":"75.00"},null,{"$f":"+E28*F28","v":{"v":0,"d":"0.00"}}]
[21,"CAW.21","Interior door frame and moldings with solid wood panel","m²",{"v":5,"d":"5.00"},null,{"$f":"+E29*F29","v":{"v":0,"d":"0.00"}}]
[22,"CAW.22","Exterior door frame and moldings with solid wood panel","m²",{"v":5,"d":"5.00"},null,{"$f":"+E30*F30","v":{"v":0,"d":"0.00"}}]
[23,"CAW.23","Interior wooden door leaf with a solid top","m²",{"v":13,"d":"13.00"},null,{"$f":"+E31*F31","v":{"v":0,"d":"0.00"}}]
[24,"CAW.24","Exterior door leaf with a solid top from wood","m²",{"v":12,"d":"12.00"},null,{"$f":"+E32*F32","v":{"v":0,"d":"0.00"}}]
[25,"CAW.25","Colour-matte and anodized heat insulated aluminium joinery","kg",{"v":1680,"d":"1,680.00"},null,{"$f":"+E33*F33","v":{"v":0,"d":"0.00"}}]
[26,"CAW.26","Window sill with white marble plates (3cm thickness)","m²",{"v":20,"d":"20.00"},null,{"$f":"+E34*F34","v":{"v":0,"d":"0.00"}}]
[27,"CAW.27","Double glazed window unit (4+4 mm thickness, 12 mm space)","m²",{"v":80,"d":"80.00"},null,{"$f":"+E35*F35","v":{"v":0,"d":"0.00"}}]
[28,"CAW.28","Water-based silk matt paint on interior surfaces","m²",{"v":375,"d":"375.00"},null,{"$f":"+E36*F36","v":{"v":0,"d":"0.00"}}]
[29,"CAW.29","2 cm thick plaster on interior or exterior surfaces (ready rough/ fine plaster)","m²",{"v":150,"d":"150.00"},null,{"$f":"+E37*F37","v":{"v":0,"d":"0.00"}}]
[30,"CAW.30","Glazed porcelain floor tiling (60x60cm)","m²",{"v":27,"d":"27.00"},null,{"$f":"+E38*F38","v":{"v":0,"d":"0.00"}}]
[31,"CAW.31","Glazed porcelain floor tiling (30x60cm)","m²",{"v":116,"d":"116.00"},null,{"$f":"+E39*F39","v":{"v":0,"d":"0.00"}}]
[32,"CAW.32","Unglazed rectified porcelain floor tiling (60x60cm)","m²",{"v":266,"d":"266.00"},null,{"$f":"+E40*F40","v":{"v":0,"d":"0.00"}}]
[33,"CAW.33","Wooden kitchen cupboard","m²",{"v":3.2,"d":"3.20"},null,{"$f":"+E41*F41","v":{"v":0,"d":"0.00"}}]
["Subtotal for Construction and Architectural Works",{"$nulls":5},{"$f":"SUM(G9:G41)","v":{"v":0,"d":"0.00"}}]
["TOTAL FOR CIVIL WORKS",{"$nulls":5},{"$f":"+G42+G7","v":{"v":0,"d":"0.00"}}]
[]
["SECTION-2 MECHANICAL WORKS"]
["Heating Installations"]
[34,"MWH.01","Heating boiler","pcs",{"v":1,"d":"1.00"},null,{"$f":"+E47*F47","v":{"v":0,"d":"0.00"}}]
[35,"MWH.02","Panel radiator (Type 22) 600","m",{"v":21,"d":"21.00"},null,{"$f":"+E48*F48","v":{"v":0,"d":"0.00"}}]
[36,"MWH.03","Corner type thermostatic radiator taps 1/2\"","pcs",{"v":14,"d":"14.00"},null,{"$f":"+E49*F49","v":{"v":0,"d":"0.00"}}]
[37,"MWH.04","Corner type thermostatic radiator return valve 1/2\"","pcs",{"v":14,"d":"14.00"},null,{"$f":"+E50*F50","v":{"v":0,"d":"0.00"}}]
[38,"MWH.05","Collector pipe ø83 / 3.25 mm","m",{"v":5,"d":"5.00"},null,{"$f":"+E51*F51","v":{"v":0,"d":"0.00"}}]
[39,"MWH.06","Collector outlet (diameter: 40 mm)","pcs",{"v":10,"d":"10.00"},null,{"$f":"+E52*F52","v":{"v":0,"d":"0.00"}}]
[40,"MWH.07","1\" collector with 6 outlet and mini ball valves","pcs",{"v":2,"d":"2.00"},null,{"$f":"+E53*F53","v":{"v":0,"d":"0.00"}}]
[41,"MWH.08","1\" collector with 8 outlet and mini ball valves","pcs",{"v":2,"d":"2.00"},null,{"$f":"+E54*F54","v":{"v":0,"d":"0.00"}}]
[42,"MWH.09","Thermometer 100mm dia.","pcs",{"v":1,"d":"1.00"},null,{"$f":"+E55*F55","v":{"v":0,"d":"0.00"}}]
[43,"MWH.10","Manometer (diameter: 100mm, graduated up to 5 Atm)","pcs",{"v":1,"d":"1.00"},null,{"$f":"+E56*F56","v":{"v":0,"d":"0.00"}}]
[44,"MWH.11","Cylindrical aeration tank 5.0L","pcs",{"v":1,"d":"1.00"},null,{"$f":"+E57*F57","v":{"v":0,"d":"0.00"}}]
[45,"MWH.12","Filling and draining tap 3/4\"","pcs",{"v":1,"d":"1.00"},null,{"$f":"+E58*F58","v":{"v":0,"d":"0.00"}}]
[46,"MWH.13","Double-stage burner (150-250 kW)","pcs",{"v":1,"d":"1.00"},null,{"$f":"+E59*F59","v":{"v":0,"d":"0.00"}}]
[47,"MWH.14","PE-Xb Pipe (with oxygen barrier, 16x2,0 mm)","m",{"v":186,"d":"186.00"},null,{"$f":"+E60*F60","v":{"v":0,"d":"0.00"}}]
[48,"MWH.15","Spiral protective sheathing","m",{"v":186,"d":"186.00"},null,{"$f":"+E61*F61","v":{"v":0,"d":"0.00"}}]
[49,"MWH.16","Ball valve 1/2\" - PN 16","pcs",{"v":4,"d":"4.00"},null,{"$f":"+E62*F62","v":{"v":0,"d":"0.00"}}]
[50,"MWH.17","Ball valve 40Ø mm (1 1/2\") PN 10-16 ","pcs",{"v":6,"d":"6.00"},null,{"$f":"+E63*F63","v":{"v":0,"d":"0.00"}}]
[51,"MWH.18","Silt Trap, die casting, with screw (dimeter:40 mm)","pcs",{"v":1,"d":"1.00"},null,{"$f":"+E64*F64","v":{"v":0,"d":"0.00"}}]
[52,"MWH.19","Check valve, brass casting, dia 40 mm","pcs",{"v":1,"d":"1.00"},null,{"$f":"+E65*F65","v":{"v":0,"d":"0.00"}}]
[53,"MWH.20","Automatic air release valve (for water) 1/2\"","pcs",{"v":2,"d":"2.00"},null,{"$f":"+E66*F66","v":{"v":0,"d":"0.00"}}]
[54,"MWH.21","Circulation pump with frequency converter (0.5-3.5 m3/h – 1-3 mSS )","pcs",{"v":2,"d":"2.00"},null,{"$f":"+E67*F67","v":{"v":0,"d":"0.00"}}]
["Subtotal for Heating Installations",{"$nulls":5},{"$f":"SUM(G47:G67)","v":{"v":0,"d":"0.00"}}]
["Sanitary and Plumbing"]
[55,"MWD.01","Semi Pedestal Glazed Faience Washbasin unit (extra class) 45x55 cm","pcs",{"v":4,"d":"4.00"},null,{"$f":"+E70*F70","v":{"v":0,"d":"0.00"}}]
[56,"MWD.02","Approximately 50x60 cm  Handicapped Glazed Faience Washbasin (extra class washbasins)","pcs",{"v":2,"d":"2.00"},null,{"$f":"+E71*F71","v":{"v":0,"d":"0.00"}}]
[57,"MWD.03","Washbasin fittings","set",{"v":4,"d":"4.00"},null,{"$f":"+E72*F72","v":{"v":0,"d":"0.00"}}]
[58,"MWD.04","Mirror (Crystal glass) 40x50 cm","pcs",{"v":4,"d":"4.00"},null,{"$f":"+E73*F73","v":{"v":0,"d":"0.00"}}]
[59,"MWD.05","Mirror for handicapped 50x70cm","pcs",{"v":2,"d":"2.00"},null,{"$f":"+E74*F74","v":{"v":0,"d":"0.00"}}]
[60,"MWD.06","Shelf; ceramic,50x10 cm","pcs",{"v":6,"d":"6.00"},null,{"$f":"+E75*F75","v":{"v":0,"d":"0.00"}}]
[61,"MWD.07","Closet with reservoir (suitable for handicapped)","set",{"v":2,"d":"2.00"},null,{"$f":"+E76*F76","v":{"v":0,"d":"0.00"}}]
[62,"MWD.08","Sink (with drainboard on one side) stainless steel, 50x100 cm","pcs",{"v":2,"d":"2.00"},null,{"$f":"+E77*F77","v":{"v":0,"d":"0.00"}}]
[63,"MWD.09","Sink fitting including basin mixer","pcs",{"v":2,"d":"2.00"},null,{"$f":"+E78*F78","v":{"v":0,"d":"0.00"}}]
[64,"MWD.10","Laundry tap  - 1/2\"","pcs",{"v":1,"d":"1.00"},null,{"$f":"+E79*F79","v":{"v":0,"d":"0.00"}}]
[65,"MWD.11","Soap holder 16x31cm","pcs",{"v":2,"d":"2.00"},null,{"$f":"+E80*F80","v":{"v":0,"d":"0.00"}}]
[66,"MWD.12","Toilet-paper holder for WC (stainless steel) (Physically Handicapped)","pcs",{"v":2,"d":"2.00"},null,{"$f":"+E81*F81","v":{"v":0,"d":"0.00"}}]
[67,"MWD.13","Clothes hanger (stainless steel)","pcs",{"v":4,"d":"4.00"},null,{"$f":"+E82*F82","v":{"v":0,"d":"0.00"}}]
[68,"MWD.14","Hold Bar for Physically Handicapped ","pcs",{"v":4,"d":"4.00"},null,{"$f":"+E83*F83","v":{"v":0,"d":"0.00"}}]
[69,"MWD.15","Toilet Hold Bar for Physically Handicapped ","pcs",{"v":4,"d":"4.00"},null,{"$f":"+E84*F84","v":{"v":0,"d":"0.00"}}]
[70,"MWD.16","Cast iron floor drain 15x15cm, Ø70mm outlet","pcs",{"v":4,"d":"4.00"},null,{"$f":"+E85*F85","v":{"v":0,"d":"0.00"}}]
[71,"MWD.17","Polypropylene clean water pipes (PPR-C) PN20 - 25 mm dia.","m",{"v":38,"d":"38.00"},null,{"$f":"+E86*F86","v":{"v":0,"d":"0.00"}}]
[72,"MWD.18","Polypropylene clean water pipes (PPR-C) PN20 - 32 mm dia.","m",{"v":10,"d":"10.00"},null,{"$f":"+E87*F87","v":{"v":0,"d":"0.00"}}]
[73,"MWD.19","Hard PVC waste water pipe 70-75 mm dia","m",{"v":40,"d":"40.00"},null,{"$f":"+E88*F88","v":{"v":0,"d":"0.00"}}]
[74,"MWD.20","Hard PVC waste water pipe 100-100 mm dia","m",{"v":28,"d":"28.00"},null,{"$f":"+E89*F89","v":{"v":0,"d":"0.00"}}]
[75,"MWD.21","Ball valve 3/4\" - PN 16","pcs",{"v":6,"d":"6.00"},null,{"$f":"+E90*F90","v":{"v":0,"d":"0.00"}}]
["Subtotal for Sanitary and Plumbing",{"$nulls":5},{"$f":"SUM(G70:G90)","v":{"v":0,"d":"0.00"}}]
["VRF Installations"]
[76,"MWC.01","Hard PVC Domestic Water Pipe (bonding bellmouth, 25mm dia, 10 atü)","m",{"v":20,"d":"20.00"},null,{"$f":"+E93*F93","v":{"v":0,"d":"0.00"}}]
[77,"MWC.02","Hard PVC Domestic Water Pipe (bonding bellmouth, 32mm dia, 10 atü)","m",{"v":30,"d":"30.00"},null,{"$f":"+E94*F94","v":{"v":0,"d":"0.00"}}]
[78,"MWC.03","Outdoor Unit - Cooling capacity (nom):44 kW, heating capacity (nom):49 kW","pcs",{"v":1,"d":"1.00"},null,{"$f":"+E95*F95","v":{"v":0,"d":"0.00"}}]
[79,"MWC.04","Cassette type indoor unit - Cooling capacity (nom):7 kW, heating capacity (nom):7,5 kW","pcs",{"v":1,"d":"1.00"},null,{"$f":"+E96*F96","v":{"v":0,"d":"0.00"}}]
[80,"MWC.05","Cassette type indoor unit - Cooling capacity (nom):9-11 kW, heating capacity (nom):9.9-12 kW","pcs",{"v":2,"d":"2.00"},null,{"$f":"+E97*F97","v":{"v":0,"d":"0.00"}}]
[81,"MWC.06","Cassette type indoor unit - Cooling capacity (nom):11-12 kW, heating capacity (nom):12-13 kW","pcs",{"v":2,"d":"2.00"},null,{"$f":"+E98*F98","v":{"v":0,"d":"0.00"}}]
[82,"MWC.07","Remote control for indoor units and its sensor","pcs",{"v":5,"d":"5.00"},null,{"$f":"+E99*F99","v":{"v":0,"d":"0.00"}}]
[83,"MWC.08","Copper Pipe Group 3/8\" 0,8 mm (13mm isolation)","m",{"v":40,"d":"40.00"},null,{"$f":"+E100*F100","v":{"v":0,"d":"0.00"}}]
[84,"MWC.09","Copper Pipe Group 1/2\" 0,8 mm (13mm isolation)","m",{"v":5,"d":"5.00"},null,{"$f":"+E101*F101","v":{"v":0,"d":"0.00"}}]
[85,"MWC.10","Copper Pipe Group 5/8\" 1.0 mm (13mm isolation)","m",{"v":25,"d":"25.00"},null,{"$f":"+E102*F102","v":{"v":0,"d":"0.00"}}]
[86,"MWC.11","Copper Pipe Group 3/4\" 1.0 mm (13mm isolation)","m",{"v":15,"d":"15.00"},null,{"$f":"+E103*F103","v":{"v":0,"d":"0.00"}}]
[87,"MWC.12","Copper Pipe Group 1\" 1.2 mm (13mm isolation)","m",{"v":5,"d":"5.00"},null,{"$f":"+E104*F104","v":{"v":0,"d":"0.00"}}]
[88,"MWC.13","Copper Pipe Group 1 1/8\" 1.2 mm (19mm isolation)","m",{"v":10,"d":"10.00"},null,{"$f":"+E105*F105","v":{"v":0,"d":"0.00"}}]
[89,"MWC.14","Connection (joint) elements (dual) up to 25 kW","set",{"v":4,"d":"4.00"},null,{"$f":"+E106*F106","v":{"v":0,"d":"0.00"}}]
["Subtotal for VRF Installations",{"$nulls":5},{"$f":"SUM(G93:G106)","v":{"v":0,"d":"0.00"}}]
["TOTAL FOR MECHANICAL WORKS",{"$nulls":5},{"$f":"+G107+G91+G68","v":{"v":0,"d":"0.00"}}]
[]
["SECTION-3 ELECTRICAL WORKS"]
["LV Distribution Board and Tables"]
[90,"ELW.01","Special sheet board- with front cover","pcs",{"v":2,"d":"2.00"},null,{"$f":"+E112*F112","v":{"v":0,"d":"0.00"}}]
[91,"ELW.02","Flush switch box (for 12 switches)","pcs",{"v":1,"d":"1.00"},null,{"$f":"+E113*F113","v":{"v":0,"d":"0.00"}}]
[92,"ELW.03","Thermal Magnetic Switch-board back- (3x10A to 3x63A, Icu: 35 kA)","pcs",{"v":2,"d":"2.00"},null,{"$f":"+E114*F114","v":{"v":0,"d":"0.00"}}]
[93,"ELW.04","Leakage current protection switches up to 4x40 A (30 mA)","pcs",{"v":3,"d":"3.00"},null,{"$f":"+E115*F115","v":{"v":0,"d":"0.00"}}]
[94,"ELW.05","Residual Current Circuit Breakers – Up to 4x63 A (300 mA)","pcs",{"v":1,"d":"1.00"},null,{"$f":"+E116*F116","v":{"v":0,"d":"0.00"}}]
[95,"ELW.06","Panel-type surge protector, B class, 230VAC, 100 kA (I imp, 10/350µs) three phase","pcs",{"v":2,"d":"2.00"},null,{"$f":"+E117*F117","v":{"v":0,"d":"0.00"}}]
[96,"ELW.07","Automatic circuit breaker with switch (6 kA) – up to 16 A","pcs",{"v":33,"d":"33.00"},null,{"$f":"+E118*F118","v":{"v":0,"d":"0.00"}}]
["Subtotal for LV Distribution Board and Tables","Toplam  ",{"$nulls":4},{"$f":"SUM(G112:G118)","v":{"v":0,"d":"0.00"}}]
[]
["Grounding and Cable Tray System"]
[97,"ELW.08","Copper busbar for cast boxes and panel boards","kg",{"v":4,"d":"4.00"},null,{"$f":"+E122*F122","v":{"v":0,"d":"0.00"}}]
[98,"ELW.09","Cable Trays","kg",{"v":125,"d":"125.00"},null,{"$f":"+E123*F123","v":{"v":0,"d":"0.00"}}]
[99,"ELW.10","Building surrounding conductor 30x3.5mm galvanized flat steel","m",{"v":100,"d":"100.00"},null,{"$f":"+E124*F124","v":{"v":0,"d":"0.00"}}]
[100,"ELW.11","Earthing electrode (rod), electrolytic copper","pcs",{"v":4,"d":"4.00"},null,{"$f":"+E125*F125","v":{"v":0,"d":"0.00"}}]
["Subtotal for Grounding and Cable Tray System","Toplam  ",{"$nulls":4},{"$f":"SUM(G122:G125)","v":{"v":0,"d":"0.00"}}]
[]
["Strong and Weak Current Cables"]
[101,"ELW.12","1kV Underground cable (NYY)-4x10 mm²","m",{"v":100,"d":"100.00"},null,{"$f":"+E129*F129","v":{"v":0,"d":"0.00"}}]
[102,"ELW.13","Socket outlet with safety line","pcs",{"v":50,"d":"50.00"},null,{"$f":"+E130*F130","v":{"v":0,"d":"0.00"}}]
[103,"ELW.14","Weatherproof outlet in galvanized pipe (normal)","pcs",{"v":4,"d":"4.00"},null,{"$f":"+E131*F131","v":{"v":0,"d":"0.00"}}]
[104,"ELW.15","Weatherproof outlet in galvanized pipe (commutator)","pcs",{"v":4,"d":"4.00"},null,{"$f":"+E132*F132","v":{"v":0,"d":"0.00"}}]
[105,"ELW.16","Weatherproof socket outlet","pcs",{"v":50,"d":"50.00"},null,{"$f":"+E133*F133","v":{"v":0,"d":"0.00"}}]
[106,"ELW.17","Supply Line Establishment with lead-free PVC insulated cables (NHXMH, at least 300/500 V), 3x2.5 mm2","m",{"v":50,"d":"50.00"},null,{"$f":"+E134*F134","v":{"v":0,"d":"0.00"}}]
[107,"ELW.18","1kV Underground cable (N2XH, 1 kV) 5x6 mm2","m",{"v":35,"d":"35.00"},null,{"$f":"+E135*F135","v":{"v":0,"d":"0.00"}}]
[108,"ELW.19","Television outlet","pcs",{"v":4,"d":"4.00"},null,{"$f":"+E136*F136","v":{"v":0,"d":"0.00"}}]
[109,"ELW.20","2x2x0,8+0,8 mm2 Je-H(St)H Fe 180 PH 120 fire resistant halogen-free alarm cable","m",{"v":80,"d":"80.00"},null,{"$f":"+E137*F137","v":{"v":0,"d":"0.00"}}]
[110,"ELW.21","RG 6AU, 75 Impedance Coaxial Cables","m",{"v":70,"d":"70.00"},null,{"$f":"+E138*F138","v":{"v":0,"d":"0.00"}}]
[111,"ELW.22","RG 11 A/U 75 Impedance Coaxial Cables","m",{"v":45,"d":"45.00"},null,{"$f":"+E139*F139","v":{"v":0,"d":"0.00"}}]
[112,"ELW.23","UTP Cat 6 Halogen free 4x2x23 AWG cable","m",{"v":350,"d":"350.00"},null,{"$f":"+E140*F140","v":{"v":0,"d":"0.00"}}]
["Subtotal for Strong and Weak Current Cables","Toplam  ",{"$nulls":4},{"$f":"SUM(G129:G140)","v":{"v":0,"d":"0.00"}}]
["Lighting Fixtures"]
[113,"ELW.24","36W LED Luminaires - suspended ceiling ","pcs",{"v":38,"d":"38.00"},null,{"$f":"+E143*F143","v":{"v":0,"d":"0.00"}}]
[114,"ELW.25","24W LED Luminaires with sensor- ceiling (downlight)","pcs",{"v":4,"d":"4.00"},null,{"$f":"+E144*F144","v":{"v":0,"d":"0.00"}}]
[115,"ELW.26","Emergency lighting set for LED luminaires","pcs",{"v":12,"d":"12.00"},null,{"$f":"+E145*F145","v":{"v":0,"d":"0.00"}}]
[116,"ELW.27","Double Sided Emergency Routing Armature with LED (1 hour lighting duration)","pcs",{"v":2,"d":"2.00"},null,{"$f":"+E146*F146","v":{"v":0,"d":"0.00"}}]
["Subtotal for Lighting Fixtures","Toplam  ",{"$nulls":4},{"$f":"SUM(G143:G146)","v":{"v":0,"d":"0.00"}}]
[]
["Uninterruptible Power Supply and Fire Alarm System"]
[117,"ELW.28","UPS, single phase input and output 6 kVA","pcs",{"v":1,"d":"1.00"},null,{"$f":"+E150*F150","v":{"v":0,"d":"0.00"}}]
[118,"ELW.29","Conventional fire alarm button","pcs",{"v":2,"d":"2.00"},null,{"$f":"+E151*F151","v":{"v":0,"d":"0.00"}}]
[119,"ELW.30","Conventional optical smoke detector","pcs",{"v":12,"d":"12.00"},null,{"$f":"+E152*F152","v":{"v":0,"d":"0.00"}}]
[120,"ELW.31","Parallel warning light","pcs",{"v":12,"d":"12.00"},null,{"$f":"+E153*F153","v":{"v":0,"d":"0.00"}}]
[121,"ELW.32","Conventional type fire alarm station up to (including) 4 zones","pcs",{"v":1,"d":"1.00"},null,{"$f":"+E154*F154","v":{"v":0,"d":"0.00"}}]
[122,"ELW.33","External type electronic fire alarm siren with strobe lights","pcs",{"v":2,"d":"2.00"},null,{"$f":"+E155*F155","v":{"v":0,"d":"0.00"}}]
["Subtotal for Uninterruptible Power Supply and Fire Alarm System","Toplam  ",{"$nulls":4},{"$f":"SUM(G150:G155)","v":{"v":0,"d":"0.00"}}]
[]
["TV-CCTV-Phone-Data systems"]
[123,"ELW.34","Internal dome camera (min 4MP)","pcs",{"v":3,"d":"3.00"},null,{"$f":"+E159*F159","v":{"v":0,"d":"0.00"}}]
[124,"ELW.35","8 Port Managed Poe Switch","pcs",{"v":1,"d":"1.00"},null,{"$f":"+E160*F160","v":{"v":0,"d":"0.00"}}]
[125,"ELW.36","Television collective antenna station-yield 21-40 db","pcs",{"v":1,"d":"1.00"},null,{"$f":"+E161*F161","v":{"v":0,"d":"0.00"}}]
[126,"ELW.37","16 U 600mmx600mm 19\" Vertical type cabinet","pcs",{"v":1,"d":"1.00"},null,{"$f":"+E162*F162","v":{"v":0,"d":"0.00"}}]
[127,"ELW.38","Fixed shelf for 500 mm depth","pcs",{"v":3,"d":"3.00"},null,{"$f":"+E163*F163","v":{"v":0,"d":"0.00"}}]
[128,"ELW.39","Fan module with thermostat (with 2 fans)","pcs",{"v":2,"d":"2.00"},null,{"$f":"+E164*F164","v":{"v":0,"d":"0.00"}}]
[129,"ELW.40","19” rack type 8 group socket with circuit breaker","pcs",{"v":1,"d":"1.00"},null,{"$f":"+E165*F165","v":{"v":0,"d":"0.00"}}]
[130,"ELW.41","19\" 2U horizontal cable organizer","pcs",{"v":3,"d":"3.00"},null,{"$f":"+E166*F166","v":{"v":0,"d":"0.00"}}]
[131,"ELW.42","Utp Cat6 patch panel, 24 ports","pcs",{"v":2,"d":"2.00"},null,{"$f":"+E167*F167","v":{"v":0,"d":"0.00"}}]
[132,"ELW.43","SM SC-SC Patchcord, 3mt","pcs",{"v":23,"d":"23.00"},null,{"$f":"+E168*F168","v":{"v":0,"d":"0.00"}}]
[133,"ELW.44","Electronic type full automatic telephone switchboard-4/32","pcs",{"v":1,"d":"1.00"},null,{"$f":"+E169*F169","v":{"v":0,"d":"0.00"}}]
["Subtotal for TV-CCTV-Phone-Data systems","Toplam  ",{"$nulls":4},{"$f":"SUM(G159:G169)","v":{"v":0,"d":"0.00"}}]
["Generator Displacement"]
[134,"ELW.45","Displacement of existing generator","L.s.",{"v":1,"d":"1.00"},null,{"$f":"+E172*F172","v":{"v":0,"d":"0.00"}}]
["Subtotal for Generator Displacement","Toplam  ",{"$nulls":4},{"$f":"+G172","v":{"v":0,"d":"0.00"}}]
["TOTAL FOR ELECTRICAL WORKS",{"$nulls":5},{"$f":"+G119+G126+G141+G147+G156+G170+G173","v":{"v":0,"d":"0.00"}}]