{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["BILL","SUMMARY"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":10,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"BILL","index":0,"n_rows":141,"n_cols":6,"rows_kept":141,"cut":false,"hidden":false,"merged":[]}
["Item","       Description","Unit","Quantity","Rate","Amount"]
[]
[]
[null,"CONTRACTOR'S ESTABLISHMENT ON SITE AND GENERAL OBLIGATIONS"]
[]
[]
[1,"The contractor's general obligation:"]
[null,"(a) Fixed obligations","L/S",1]
[]
[null,"(b) time related obligations","Month",3]
{"$rows_empty":27}
["Item","       Description","Unit","Quantity","Rate","Amount"]
[]
[2,"SUPPLY AND INSTALL HIGH EFFICIENCY LIGHTING SYSTEMS"]
[2.1,"Remove and  replacement one-to-one of all the existing lamps at the RFM hospital with LED lamps as specified in the project specification.","No.",2009]
[]
[2.2000000000000002,"Supply and install the following luminaries complete with lamps and control gear as specified in the position as indicated on the project specification.","No.",2009]
[]
[2.2999999999999998,"The removal of the selected existing fitting to be replace with new fittings"]
["2.3 (a)","Remove and  replacement one-to-one of all the existing lamps at the RFM hospital with LED lamps as specified in the project specification. Maximum wattage 30 watts"]
["2.3 (b)","The replacement of the fittings is needed, the fittings shall be installed in the same position of the previously installed one and shall provide equal or higher lighting performance compared to the existing installation. Luminaries should comply with LED specification as well as all fixture should meet the minimum specification for the tender. Max watts 30 watts","No.",976]
{"$rows_empty":18}
[null,"Carried Forward Total to Summary",null,null,null,{"$f":"SUM(F40:F65)","v":0}]
["No.","       Description","Unit","Quantity","Rate","Amount"]
[null,"Brought Forward Total"]
[]
[3,"HIGH EFFICIENCY SPACE HEATING SYSTEMS"]
[]
[null,"The Supply and Installation of the Air-Air Heat Pumps"]
[3.1,"The supply and installation the installation of high efficiency air-air heat pumps. Installation of the high efficiency air-air heat pumps in selected rooms of the hospital where heating is currently provided through the use of electric heaters should be as per the attached specification","No",63]
[]
[null,"Pipping for the High Efficient air-air heat pumps"]
[3.2,"In addition to the internal and the external unit for the high-efficiency air conditioning systems, the tenderer shall provide and install all the needed piping for the correct operation of the system"]
["3.2(a)","PVC or copper piping for condensate drain, with supports at a maximum spacing of 1.5 m, installed with a minimum slope of 1:100 and pressure tested to ensure absence of leaks;","L/S",1]
["3.2(b)","Refrigerant piping, supported on galvanized cable tray or other equivalent support system separated from power and control cables.","L/S",1]
[]
[3.3,"Repair of Existing Air Conditioning Systems,"]
["3.3 (a)","The tenderer is requested to carry out a census of the existing air conditioning systems already installed at the Hospital (mainly: split-type air conditioners) and of their current status and to quote also.","L/S",1]
["3.3 (b)","Execution of the maintenance activities needed to fix the identified issues (e.g.: refill of refrigerant fluid, cleaning of filters, replacement of minor spare parts or consumables","L/S",1]
[]
["3.3 (c )","Supply and installation of new and energy efficient air-conditions. To replace those that has passed their life span and are not reapable ","L/S",1]
[]
[]
[]
[]
[null,"Carried Forward Total to Summary",null,null,null,{"$f":"SUM(F73:F88)","v":0}]
["No.","       Description","Unit","Quantity","Rate","Amount"]
[null,"Brought Forward Total"]
[]
[4,"REPLACEMENT OF STEAM USERS AND DISMANTLING OF STEAM BOILER AND SYSTEM"]
[4.0999999999999996,"Dismantling of Existing Coal Fired Steam Boiler and of Steam Distribution Network. This include removal of the piping and device as well removal of waste or rubble and dispose in a suitable location","L/S",1]
[4.2,"The steam users to be replaced (or retrofitted when possible) include a sterilizer, a washing machine, a dryer and the kitchen water heater. For each item the devices to be installed with the main technical specifications are presented in the ITB Specification."]
[null,"Sterilizer"]
["4.2 (a)","The provision and installation of a suitable an electric steam boiler for retrofitting through the existing sterilizing autoclave.","No.",1]
["4.2 (b)","Electrical Provision for the electric steam boiler. The installation of a new dedicated switchboard and of the needed low voltage cabling for the connection of the new device to the main switchboard of the hospital. The switchboard feeding all the sterilizers shall be provided with a demand-side management system ","L/S",1]
[null,"Washing Machine"]
["4.2 (c ) ","The tenderer shall offer the replacement of the existing steam-based washing machine with a new full-electric washing machine as per attached specification","No.",1]
["4.2 (d)","Electrical Provision for the electric steam boiler. The installation of a new dedicated switchboard and of the needed low voltage cabling for the connection of the new device to the main switchboard of the hospital. The switchboard feeding all the sterilizers shall be provided with a demand-side management system ","L/S",1]
[null,"Dryer"]
["4.2 (e )","The tenderer shall offer the replacement of the existing steam-based dryer with a new full-electric tumble dryer as per the specification ","No.",1]
["4.2 (f )","Electrical Provision for the electric steam boiler. The installation of a new dedicated switchboard and of the needed low voltage cabling for the connection of the new device to the main switchboard of the hospital. The switchboard feeding all the sterilizers shall be provided with a demand-side management system ","L/S",1]
[]
[]
[null,"Carried Forward Total"]
["No.","       Description","Unit","Quantity","Rate","Amount"]
[null,"Brought Forward Total"]
[]
[null,"Heat Pump Water Heater for Kitchen"]
["4.2 (g)","Remove the existing heat pump water heating for the kitchen","L/S",1]
["4.2 (h)","The replacement of the existing steam-water heat exchanger used to produce hot water for kitchen ","No.",1]
["4.2 (i)","Electrical Provision for the electric steam boiler. The installation of a new dedicated switchboard and of the needed low voltage cabling for the connection of the new device to the main switchboard of the hospital. ","L/S",1]
{"$rows_empty":26}
[null,"Carried Forward Total to Summary",null,null,null,{"$f":"SUM(F102:F140)","v":0}]

{"sheet":"SUMMARY","index":1,"n_rows":24,"n_cols":3,"rows_kept":24,"cut":false,"hidden":false,"merged":[[0,0,1,0],[0,2,1,2],[0,1,1,1]]}
["Item No.","Description or Specification of Item     ","Amount"]
[]
[]
[1,"CONTRACTOR'S ESTABLISHMENT ON SITE AND GENERAL OBLIGATIONS",{"$f":"BILL!$F$37","v":0}]
[]
[2,"SUPPLY AND INSTALL HIGH EFFICIENCY LIGHTING SYSTEMS",{"$f":"BILL!$F$66","v":0}]
[]
[3,"HIGH EFFICIENCY SPACE HEATING SYSTEMS",{"$f":"BILL!$F$89","v":0}]
[]
[4,"REPLACEMENT OF STEAM USERS AND DISMANTLING OF STEAM BOILER AND SYSTEM",{"$f":"BILL!$F$141","v":0}]
{"$rows_empty":7}
[null,"Add 1% Construction Levy",0]
[]
[null,"SUB TOTAL (B)",0]
[null,"Add 15% V.A.T",0]
[]
[]
[null,"TOTAL TENDER AMOUNT",0]