{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Table 1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Table 1","index":0,"n_rows":78,"n_cols":7,"rows_kept":78,"cut":false,"hidden":false,"merged":[[2,6,3,6],[0,1,0,4],[1,1,1,5],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,5,3,5]]}
[null,"Financial Offer "]
[null,"(ECA Compound)  Office  Refurbishment  "]
[null,"ACTIVITY","Qty","UNIT","UNIT","TOTAL Proice ( USD) ","Remark"]
[{"$nulls":4},"PRICE ( USD ) "]
[]
[null,"UNOCHR-EARO  Second Floor"]
[null,"Lot I:  Aluminium  partation  wall  "]
[]
[null," Aluminium  partation  wall  "]
[null,"European  standard,  100mm  thick,  double panel,modular  &  demountable  sound  proof partition  system  made  of  6mm  thick  clear  glass on  both  face  with  mechanical  monitored  blind shutter  give  exacted  description  of  panel structure.  sound  proof  test  certificate. recommended  51db."]
[1,"DOOR"]
[null,"Fabricate  and  fix aluminum  door  ,covered     with 10mm  thick   ply  wood  ,fix approved  quality  lock."]
[null,"DW1     400*365cm",1,"No"]
[]
[2,"Full  height(Floor  to  concrete  ceiling   height Partition)   (Sound Proof)"]
[null,"(refer  to attached  drawing)"]
[null,"PW1         350*365cm",4,"No"]
[null,"PW2         1100*365cm",1,"No"]
[null,"PW3         735*365cm",1,"No"]
[null,"PW4         535*365cm",2,"No"]
[null,"PW5         790*365cm",1,"No"]
[null,"PW6         330*365cm",2,"No"]
[null,"PW7         200*365cm",1,"No"]
[null,"PW8         481*365cm",1,"No"]
[]
[3,"Full  height  (Floor  to  concrete  ceiling   height\nPartition)  (Non  Sound Proof)"]
[]
[null,"PW9         350*365cm",1,"No"]
[null,"PW10      250*365cm",1,"No"]
[null,"PW15      400*365cm",1,"No"]
[]
[4,"Partition  wall  (Non  Sound Proof)"]
[null,"price  to  include"]
[null,"PW11      2200*250cm",1,"No"]
[null,"PW12      500*250cm",1,"No"]
[null,"PW13      328*250cm",1,"No"]
[null,"PW14      300*250cm",1,"No"]
[]
[null,"Total Partion Price"]
[null,"Installation of the Partitioning"]
[null,"Transportation Price"]
[null,"Insurance Price"]
[null,"Other costs"]
[null,"Total Final and All inclusive Price"]
[]
[null,"Lot II: Curtain"]
[5,"Curtain (see attached pictures)"]
[null,"Supply and fix adjustable curtain , with horizontal\nalternate strips (clear and colored ). Check measurement on site."]
[null,". Durable and easy ti clean sunscreen fabric roller shade"]
[null,". Made of 100 percent polyester"]
[null,". Filter out about 90 to 96 percent of the harmful UV rays and glare reduction"]
[null,". Allows privacy whilst still providing a view out"]
[null,". Designed to allow permissible light while giving uniform and clear appearance"]
[]
[null,"160*250cm",22,"No"]
[null,"200*250cm",9,"No"]
[null,"Total Curtain Price"]
[null,"Installation  of Curtian"]
[null,"Transportation Price"]
[null,"Insurance Price"]
[null,"Other costs"]
[null,"Total Final and All inclusive Price"]
[null,"Lot III- Carpet"]
[]
[6,"Carpet"]
[]
[null,"Supply and fix heavy duty carpet size 50*50cm with fire , health and sound rating . Attach certificates.",360,"m2"]
[]
[7,"Painting in three coats of plastic emulsion paint to all specified internal wall & ceiling surface.",481,"m2"]
[]
[8,"Suspended ceiling 600*600mm .Sound proof",360,"m2"]
[]
[null,"Total Carpet Price"]
[null,"Installation of Carpet"]
[null,"Transportation Price"]
[null,"Insurance Price"]
[null,"Other costs"]
[null,"Total Final and All inclusive Price"]