{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":483,"n_cols":8,"rows_kept":483,"cut":false,"hidden":false,"merged":[[417,0,417,7],[448,0,448,7],[478,0,478,7],[482,0,482,4],[0,0,0,7],[3,0,3,7],[51,0,51,7],[99,0,99,7],[147,0,147,7],[195,0,195,7],[247,0,247,7],[279,0,279,7],[311,0,311,7],[349,0,349,7],[386,0,386,7]]}
["Lot 1: Capital reconstruction of hydro-technical constructions d/s Smolyanka (I phase)"]
["No.","Works Description","UOM","Volume ","Cost per unit, excl. VAT ","Total, excl. VAT","VAT","Total"]
[1,2,3,4,5,6,7,8]
["Capital repair of piped regulator with crossing RTP-100 К-44 PКО+20"]
[1,"Soil excavation into the dump (excavation of the construction) by dragline excavators or back fillers, soil group 1 for work at water engineering ","1000m3",0.11749999999999999]
[2,"Dismantling of head ","100m3",1.4999999999999999E-2]
[3,"Dismantling of reinforce concrete circles","10m3",0.24]
[4,"Transportation of reinforced concrete structures at the distance of 10 km ","t",11.05]
[5,"Cleaning of the constructions from siltation by the multi-bucket excavators of cross cutting type in the soils of group 1 / high humidity boggy soil which intensely sticks to the bucket teeth and walls","1000m3",6.0000000000000001E-3]
[6,"Soil excavation (excavation) into the construction by dragline excavators or back fillers, soil group 1 for work at water engineering ","1000m3",3.7999999999999999E-2]
[7,"Fine excavation manually, manual bottom and banks stripping with soil discharge into the ditches and trenches, excavated mechanically.","100m3",0.04]
[8,"Arrangement of sand preparation                 ","100m3",8.9999999999999993E-3]
[9,"Arrangement of gravel preparation                 ","100m3",2.5999999999999999E-2]
[10,"Planning of the canal bottom and banks by the single-bucket excavators, diesel-powered, on caterpillar drive, soil group 1-2 ","1000m2",7.0000000000000007E-2]
[11,"Arrangement of sand-gravel preparation for the laying of fixing slabs                ","100m2",0.28000000000000003]
[12,"Sand-gravel mixtures for construction works N3, fraction size more than 0 to 40 mm, mark DR12","m3",5.9]
[13,"Laying of slabs under pipes ","100m3",6.3E-3]
[14,"Slabs PP-10-15                                                                   ","units",6]
[15,"Preparation of concrete (class of strength M100)","100m3",1.41E-2]
[16,"Arrangement of concrete bed","100m3",1.41E-2]
[17,"Laying of reinforced concrete pipes with a diameter of 1000 mm                                                                ","1000m",0.01]
[18,"Pipes TB-100.50-2 (the length is 5 m)                                                                 ","шт.",2]
[19,"Mounting of heads with the laying of joints by cement mortar                                      ","100м3",3.0599999999999999E-2]
[20,"Head ОP-10А                                                                 ","units",1]
[21,"Head ОP-10                                                                 ","units",1]
[22,"Joints seal by tarred rope and fiber packing ","100m",0.127]
[23,"Water isolation of concrete structures","100m2",0.98]
[24,"Back-filling of the structure","1000m3",0.1595]
[25,"Soil consolidation by (density up to 1,7 t/m3)  air rammers, soil group 1, 2                                                                    ","100m3",1655]
[26,"Laying of fixing slabs","100m3",4.24E-2]
[27,"Fixing slabs RP-15-30                                                                    ","units",10]
[28,"Fixing slabs RPU-10-15                                                                   ","units",9]
[29,"Installation of blocks Т-8                                                                    ","100m3",6.2500000000000003E-3]
[30,"Blocks Т-8                                                                 ","units",5]
[31,"Preparation of concrete","100m3",5.0000000000000001E-4]
[32,"Ready heavy concrete mixtures, concrete class B15 [M200], filler fraction  bigger than 40 mm ","m3",0.05]
[33,"Installation of posts С-1                                                                  ","100m3",1.6000000000000001E-3]
[34,"Posts С-1                                                                   ","units",4]
[35,"Simple painting of the plaster and section construction by white paints, prepared for painting ","100m2",0.18]
[36,"Marking of the construction","100units",0.01]
[37,"Arrangement of earth cofferdams by single-bucket excavators, diesel-powered, on caterpillar drive, soil group 1                                                                   ","1000m3",0.02]
[38,"Dewatering","Hours of dewatering",96]
[39,"Mounting of shutters with hoist ","t",0.35299999999999998]
[40,"Lower gate DP-20-000                                                                 ","units",1]
[41,"Priming  of metal surfaces ","100m2",8.4000000000000005E-2]
[42,"Painting of metal primed surfaces","100m2",8.4000000000000005E-2]
[43,"Leveling of earth cofferdams by earthmovers at water engineering  ","1000m3",0.02]
[44,"Planning of earth surface by the earthmovers            ","1000m2",0.1]
[45,"Panting of perennial grasses","100m2",0.97699999999999998]
[46,"Arrangement of road embankments by earthmovers           ","1000m3",6.0000000000000001E-3]
[47,"Soil (add roadway at dirt way)                                                              ","m3",6]
["Capital repair of piped regulator with crossing РТП-100 К-45 ПКО+20"]
[1,"Soil excavation to the dump (excavation of the construction) by dragline excavators or back fillers, soil group 1 for work at water engineering / high humidity boggy soil which intensely sticks to the bucket teeth and walls","1000м3",0.11749999999999999]
[2,"Dismantling of head ","100m3",1.4999999999999999E-2]
[3,"Dismantling of reinforce concrete circles","10m3",0.24]
[4,"Transportation of reinforced concrete structures at the distance of 10 km","t",11.05]
[5,"Cleaning of the constructions from siltation by the multi-bucket excavators of cross cutting type in the soils of group 1 / high humidity boggy soil which intensely sticks to the bucket teeth and walls                                                                   ","1000m3",7.0000000000000001E-3]
[6,"Soil excavation (excavation) into the construction by dragline excavators or back fillers, soil group 1 for work at water engineering","1000m3",3.7999999999999999E-2]
[7,"Fine excavation manually, manual bottom and banks stripping with soil discharge into the ditches and trenches, excavated mechanically.","100m3",0.04]
[8,"Arrangement of sand preparation                 ","100m3",8.9999999999999993E-3]
[9,"Arrangement of gravel preparation                 ","100m3",2.5999999999999999E-2]
[10,"Planning of the canal bottom and banks by the single-bucket excavators, diesel-powered, on caterpillar drive, soil group 1-2 ","1000m2",7.0000000000000007E-2]
[11,"Arrangement of sand-gravel preparation the laying of fixing slabs                ","100m2",0.28000000000000003]
[12,"Sand-gravel mixtures for construction works N3, fraction size more than 0 to 40 mm, mark DR12","m3",5.9]
[13,"Laying of slabs under pipes","100m3",6.3E-3]
[14,"Slabs PP-10-15                                                                   ","units",6]
[15,"Preparation of concrete","100m3",1.41E-2]
[16,"Arrangement of concrete bed","100m3",1.41E-2]
[17,"Laying of reinforced concrete pipes with a diameter of 1000 mm                                                                ","1000m",0.01]
[18,"Pipes ТB-100.50-2 (the length is 5 m)                                                                ","units",2]
[19,"Mounting of heads with the laying of joints by cement mortar                                                                                                   ","100m3",3.0599999999999999E-2]
[20,"Head ОP-10А                                                                 ","units",1]
[21,"Head ОP-10                                                            ","units",1]
[22,"Joints seal by tarred rope and fiber packing ","100m",0.127]
[23,"Water isolation of concrete structures","100m2",0.98]
[24,"Back-filling of the structure","1000m3",0.1595]
[25,"Soil consolidation by air rammers, soil group 1, 2                                                                   ","100m3",1.655]
[26,"Laying of fixing slabs","100m3",4.24E-2]
[27,"Fixing slabs RP-15-30                                                                    ","units",10]
[28,"Fixing slabs RPU-10-15                                                                   ","units",9]
[29,"Installation of blocks Т-8                                                                    ","100m3",6.2500000000000003E-3]
[30,"Blocks Т-8                                                                 ","units",5]
[31,"Preparation of concrete (concrete hydrotechnical BGT-200)","100m3",5.0000000000000001E-4]
[32,"Ready heavy concrete mixtures. concrete class B15 [M200]. filler fraction  bigger than 40 mm ","m3",0.05]
[33,"Installation of posts С-1                                                                  ","100m3",1.6000000000000001E-3]
[34,"Posts С-1                                                                   ","units",4]
[35,"Simple painting of the plaster and section construction by white paints, prepared for painting ","100m2",0.18]
[36,"Marking of the construction","100units",0.01]
[37,"Arrangement of earth cofferdams by single-bucket excavators, diesel-powered, on caterpillar drive, soil group 1                                                                   ","1000m3",0.02]
[38,"Dewatering","Hours of dewatering",96]
[39,"Mounting of shutters with hoist ","t",0.35299999999999998]
[40,"Lower gate DP-20-000                                                                 ","units",1]
[41,"Priming  of metal surfaces ","100m2",8.4000000000000005E-2]
[42,"Painting of metal primed surfaces","100m2",8.4000000000000005E-2]
[43,"Leveling of earth cofferdams by earthmovers at water engineering  ","1000m3",0.02]
[44,"Planning of earth surface by the earthmovers            ","1000m2",0.1]
[45,"Panting of perennial grasses","100m2",0.97699999999999998]
[46,"Arrangement of road embankments by earthmovers           ","1000m3",6.0000000000000001E-3]
[47,"Soil                                                              ","m3",6]
["Capital repair of piped regulator with crossing RТК-100 К-47 PКО+20 "]
[1,"Soil excavation to the dump (excavation of the head) by dragline excavators or back fillers, soil group 1 for work at water engineering / high humidity boggy soil which intensely sticks to the bucket teeth and walls","1000m3",0.11749999999999999]
[2,"Dismantling of heads","100m3",3.0599999999999999E-2]
[3,"Dismantling of reinforce concrete pipes with the diameter 1000 mm","1000m",0.01]
[4,"Transportation of reinforced concrete structures at the distance of 10 km","t",17.059999999999999]
[5,"Cleaning of the constructions from siltation by the multi-bucket excavators of cross cutting type in the soils of group 1 / high humidity boggy soil which intensely sticks to the bucket teeth and walls                                                                   ","1000m3",6.0000000000000001E-3]
[6,"Soil excavation (excavation) into the construction by dragline excavators or back fillers, soil group 1 for work at water engineering","1000m3",3.7999999999999999E-2]
[7,"Fine excavation manually, manual bottom and banks stripping with soil discharge into the ditches and trenches, excavated mechanically.","100m3",0.04]
[8,"Arrangement of sand preparation                 ","100m3",8.9999999999999993E-3]
[9,"Arrangement of gravel preparation                 ","100m3",2.5999999999999999E-2]
[10,"Planning of the canal bottom and banks by the single-bucket excavators, diesel-powered, on caterpillar drive, soil group 1-2","1000m2",7.0000000000000007E-2]
[11,"Arrangement of sand-gravel preparation the laying of fixing slabs                ","100m2",0.28000000000000003]
[12,"Sand-gravel mixtures for construction works N3, fraction size more than 0 to 40 mm, mark DR12","m3",5.9]
[13,"Laying of slabs under pipes","100m3",6.3E-3]
[14,"Slabs PP-10-15                                                                   ","units",6]
[15,"Preparation of concrete","100m3",1.41E-2]
[16,"Arrangement of concrete bed","100m3",1.41E-2]
[17,"Laying of reinforced concrete pipes with a diameter of 1000 mm                                                                ","1000m",0.01]
[18,"Pipes ТB-100.50-2 (the length is 5 m)                                                                ","units",2]
[19,"Mounting of heads with the laying of joints by cement mortar                                                                                                   ","100m3",3.0599999999999999E-2]
[20,"Head ОP-10А                                                                 ","units",1]
[21,"Head ОP-10                                                            ","units",1]
[22,"Joints seal by tarred rope and fiber packing ","100m",0.127]
[23,"Water isolation of concrete structures","100m2",0.98]
[24,"Back-filling of the structure","1000m3",0.1595]
[25,"Soil consolidation by air rammers, soil group 1, 2                                                                   ","100m3",1.655]
[26,"Laying of fixing slabs","100m3",4.24E-2]
[27,"Fixing slabs RP-15-30                                                                    ","units",10]
[28,"Fixing slabs RPU-10-15                                                                   ","units",9]
[29,"Installation of blocks Т-8                                                                    ","100m3",6.2500000000000003E-3]
[30,"Blocks Т-8                                                                 ","units",5]
[31,"Preparation of concrete","100m3",5.0000000000000001E-4]
[32,"Ready heavy concrete mixtures, concrete class B15 [M200], filler fraction  bigger than 40 mm ","m3",0.05]
[33,"Installation of posts С-1                                                                  ","100m3",1.6000000000000001E-3]
[34,"Posts С-1                                                                   ","units",4]
[35,"Simple painting of the plaster and section construction by white paints, prepared for painting ","100m2",0.18]
[36,"Marking of the construction","100 units",0.01]
[37,"Arrangement of earth cofferdams by single-bucket excavators, diesel-powered, on caterpillar drive, soil group 1                                                                   ","1000m3",0.02]
[38,"De-watering","Hours of dewatering",96]
[39,"Mounting of box type gates with hoist                         ","t",0.39500000000000002]
[40,"Box type gate ЗК-1,3х1,0 with hoist 3В                                                                   ","units",1]
[41,"Priming  of metal surfaces ","100m2",8.4000000000000005E-2]
[42,"Painting of metal primed surfaces","100m2",8.4000000000000005E-2]
[43,"Leveling of earth cofferdams by earthmovers at water engineering  ","1000m3",0.02]
[44,"Planning of earth surface by the earthmovers            ","1000m2",0.1]
[45,"Panting of perennial grasses","100m2",0.97699999999999998]
[46,"Arrangement of road embankments by earthmovers           ","1000m3",6.0000000000000001E-3]
[47,"Soil                                                              ","m3",6]
["Capital repair of piped regulator with crossing RТP-100 К-48 PКО+20 "]
[1,"Soil excavation to the dump (excavation of the construction) by dragline excavators or back fillers, soil group 1 for work at water engineering / high humidity boggy soil which intensely sticks to the bucket teeth and walls","1000m3",0.11749999999999999]
[2,"Dismantling of head","100m3",1.4999999999999999E-2]
[3,"Dismantling of reinforce concrete circles","10m3",0.24]
[4,"Transportation of reinforced concrete structures at the distance of 10 km","t",11.05]
[5,"Cleaning of the constructions from siltation by the multi-bucket excavators of cross cutting type in the soils of group 1 / high humidity boggy soil which intensely sticks to the bucket teeth and walls                                                                   ","1000m3",5.0000000000000001E-3]
[6,"Soil excavation (excavation) into the construction by dragline excavators or back fillers, soil group 1 for work at water engineering","1000m3",3.7999999999999999E-2]
[7,"Fine excavation manually, manual bottom and banks stripping with soil discharge into the ditches and trenches, excavated mechanically.","100m3",0.04]
[8,"Arrangement of sand preparation                 ","100m3",8.9999999999999993E-3]
[9,"Arrangement of gravel preparation                 ","100m3",2.5999999999999999E-2]
[10,"Planning of the canal bottom and banks by the single-bucket excavators, diesel-powered, on caterpillar drive, soil group 1-2","1000m2",7.0000000000000007E-2]
[11,"Arrangement of sand-gravel preparation the laying of fixing slabs                ","100m2",0.28000000000000003]
[12,"Sand-gravel mixtures for construction works N3, fraction size more than 0 to 40 mm, mark DR12","m3",5.9]
[13,"Laying of slabs under pipes","100m3",6.3E-3]
[14,"Slabs PP-10-15                                                                   ","units",6]
[15,"Preparation of concrete","100m3",1.41E-2]
[16,"Arrangement of concrete bed","100m3",1.41E-2]
[17,"Laying of reinforced concrete pipes with a diameter of 1000 mm                                                                ","1000m",0.01]
[18,"Pipes ТB-100.50-2 (the length is 5 m)                                                                ","units",2]
[19,"Mounting of heads with the laying of joints by cement mortar                                                                                                   ","100m3",3.0599999999999999E-2]
[20,"Head ОP-10А                                                                 ","units",1]
[21,"Head ОP-10                                                            ","units",1]
[22,"Joints seal by tarred rope and fiber packing ","100m",0.127]
[23,"Water isolation of concrete structures","100m2",0.98]
[24,"Back-filling of the structure","1000m3",0.1595]
[25,"Soil consolidation by air rammers, soil group 1, 2                                                                   ","100m3",1655]
[26,"Laying of fixing slabs","100m3",4.24E-2]
[27,"Fixing slabs RP-15-30                                                                    ","units",10]
[28,"Fixing slabs RPU-10-15                                                                   ","units",9]
[29,"Installation of blocks Т-8                                                                    ","100m3",6.2500000000000003E-3]
[30,"Blocks Т-8                                                                 ","units",5]
[31,"Preparation of concrete","100m3",5.0000000000000001E-4]
[32,"Ready heavy concrete mixtures, concrete class B15 [M200], filler fraction  bigger than 40 mm ","m3",0.05]
[33,"Installation of posts С-1                                                                  ","100m3",1.6000000000000001E-3]
[34,"Posts С-1                                                                   ","units",4]
[35,"Simple painting of the plaster and section construction by white paints, prepared for painting ","100m2",0.18]
[36,"Marking of the construction","100 units",0.01]
[37,"Arrangement of earth cofferdams by single-bucket excavators, diesel-powered, on caterpillar drive, soil group 1                                                                   ","1000m3",0.02]
[38,"Dewatering","Hours of dewatering",96]
[39,"Mounting of shutters with hoist ","t",0.35299999999999998]
[40,"Lower gate DP-20-000                                                                 ","units",1]
[41,"Priming  of metal surfaces ","100m2",8.4000000000000005E-2]
[42,"Painting of metal primed surfaces","100m2",8.4000000000000005E-2]
[43,"Leveling of earth cofferdams by earthmovers at water engineering  ","1000m3",0.02]
[44,"Planning of earth surface by the earthmovers            ","1000m2",0.1]
[45,"Panting of perennial grasses","100m2",0.97699999999999998]
[46,"Arrangement of road embankments by earthmovers           ","1000m3",6.0000000000000001E-3]
[47,"Soil                                                              ","m3",6]
["Capital repair of piped regulator with crossing RТP-100 К-50 PКО+20"]
[1,"Shrubs cutting by tractor brush breaker ","ha",5.0000000000000001E-3]
[2,"Sweeping of cut shrubs by tractor rakes ","hа",5.0000000000000001E-3]
[3,"Grubbing of shrubs by tractor mechanism for grubbing and collecting ","hа",5.0000000000000001E-3]
[4,"Burning with the shake over of shrubs, low forest cover and roots by tractor ","hа",5.0000000000000001E-3]
[5,"Soil excavation into the dump (excavation of the construction) by dragline excavators or back fillers, soil group 1 for work at water engineering / high humidity boggy soil which intensely sticks to the bucket teeth and walls","1000m3",0.11749999999999999]
[6,"Dismantling of head","100m3",1.4999999999999999E-2]
[7,"Dismantling of reinforce concrete circles","10m3",0.24]
[8,"Transportation of reinforced concrete structures at the distance of 10 km","t",11.05]
[9,"Cleaning of the constructions from siltation by the multi-bucket excavators of cross cutting type in the soils of group 1 / high humidity boggy soil which intensely sticks to the bucket teeth and walls                                                                   ","1000m3",8.0000000000000002E-3]
[10,"Soil excavation (excavation) into the construction by dragline excavators or back fillers, soil group 1 for work at water engineering","1000m3",3.7999999999999999E-2]
[11,"Fine excavation manually, manual bottom and banks stripping with soil discharge into the ditches and trenches, excavated mechanically.","100m3",0.04]
[12,"Arrangement of sand preparation                 ","100m3",8.9999999999999993E-3]
[13,"Arrangement of gravel preparation                 ","100m3",2.5999999999999999E-2]
[14,"Planning of the canal bottom and banks by the single-bucket excavators, diesel-powered, on caterpillar drive, soil group 1-2","1000m2",7.0000000000000007E-2]
[15,"Arrangement of sand-gravel preparation the laying of fixing slabs                ","100m2",0.28000000000000003]
[16,"Sand-gravel mixtures for construction works N3, fraction size more than 0 to 40 mm, mark DR12","m3",5.9]
[17,"Laying of slabs under pipes","100m3",6.3E-3]
[18,"Slabs PP-10-15                                                                   ","units",6]
[19,"Preparation of concrete","100m3",1.41E-2]
[20,"Arrangement of concrete bed","100m3",1.41E-2]
[21,"Laying of reinforced concrete pipes with a diameter of 1000 mm                                                                ","1000m",0.01]
[22,"Pipes ТB-100.50-2 (the length is 5 m)                                                                ","units",2]
[23,"Mounting of heads with the laying of joints by cement mortar                                                                                                   ","100m3",3.0599999999999999E-2]
[24,"Head ОP-10А                                                                 ","units",1]
[25,"Head ОP-10                                                            ","units",1]
[26,"Joints seal by tarred rope and fiber packing ","100m",0.127]
[27,"Water isolation of concrete structures","100m2",0.98]
[28,"Back-filling of the construction","1000m3",0.1595]
[29,"Soil consolidation by air rammers, soil group 1, 2                                                                   ","100m3",1.655]
[30,"Laying of fixing slabs","100m3",4.24E-2]
[31,"Fixing slabs RP-15-30                                                                    ","units",10]
[32,"Fixing slabs RPU-10-15                                                                   ","units",9]
[33,"Installation of blocks Т-8                                                                    ","100m3",6.2500000000000003E-3]
[34,"Blocks Т-8                                                                 ","units",5]
[35,"Preparation of concrete","100m3",5.0000000000000001E-4]
[36,"Ready heavy concrete mixtures, concrete class B15 [M200], filler fraction  bigger than 40 mm ","m3",0.05]
[37,"Installation of posts С-1                                                                  ","100m3",1.6000000000000001E-3]
[38,"Posts С-1                                                                   ","units",4]
[39,"Simple painting of the plaster and section construction by white paints, prepared for painting ","100m2",0.18]
[40,"Marking of the construction","100units",0.01]
[41,"Arrangement of earth cofferdams by single-bucket excavators, diesel-powered, on caterpillar drive, soil group 1                                                                   ","1000m3",0.02]
[42,"De-watering","Hours of dewatering",96]
[43,"Mounting of shutters with hoist ","t",0.35299999999999998]
[44,"Lower gate DP-20-000                                                                 ","units",1]
[45,"Priming  of metal surfaces ","100m2",8.4000000000000005E-2]
[46,"Painting of metal primed surfaces","100m2",8.4000000000000005E-2]
[47,"Leveling of earth cofferdams by earthmovers at water engineering  ","1000m2",0.02]
[48,"Planning of earth surface by the earthmovers            ","1000m2",0.1]
[49,"Panting of perennial grasses","100m2",0.97699999999999998]
[50,"Arrangement of road embankments by earthmovers           ","1000m3",6.0000000000000001E-3]
[51,"Soil                                                              ","m3",6]
["Capital repair of piped regulator with crossing RТP-100  К-46 PК0+30 "]
[1,"Shrubs cutting by tractor brush breaker ","hа",1E-3]
[2,"Sweeping of cut shrubs by tractor rakes ","hа",1E-3]
[3,"Grubbing of shrubs by tractor mechanism for grubbing and collecting ","hа",1E-3]
[4,"Burning with the shake over of shrubs, low forest cover and roots by tractor ","hа",1E-3]
[5,"Cleaning of the constructions from siltation by the multi-bucket excavators of cross cutting type in the soils of group 1 / high humidity boggy soil which intensely sticks to the bucket teeth and walls                                                                                                                                    ","1000m3",7.4999999999999997E-3]
[6,"Soil excavation (the excavation of head) into the dump by dragline excavators or back fillers, soil group 1","1000m3",8.0000000000000002E-3]
[7,"Manual excavation of head","100m3",0.01]
[8,"Joints seal by tarred rope and fiber packing","100m",4.7E-2]
[9,"Back-filling of the construction ","1000m3",8.9999999999999993E-3]
[10,"Soil consolidation by air rammers, soil group 1, 2                                                                   ","100m3",0.09]
[11,"Planning of the canal bottom and banks by the single-bucket excavators, diesel-powered, on caterpillar drive, soil group 1-2","1000m2",7.0000000000000007E-2]
[12,"Arrangement of sand-gravel preparation the laying of fixing slabs          ","100m2",0.59]
[13,"Sand-gravel mixtures for construction works N3, fraction size more than 0 to 40 mm, mark DR12","m3",12.39]
[14,"Laying of fixing slabs                                                                    ","100m3",4.24E-2]
[15,"Fixing slabs RP-15-30                                                                   ","units",10]
[16,"Fixing slabs RPU-10-15                                                                  ","units",9]
[17,"Installation of blocks Т-8                                                                    ","100m3",6.2500000000000003E-3]
[18,"Blocks Т-8                                                                    ","units",5]
[19,"Preparation of concrete","100m3",6.0000000000000001E-3]
[20,"Ready heavy concrete mixtures, concrete class B15 [M200], filler fraction  bigger than 40 mm                                                              ","m3",0.6]
[21,"Installation of posts С-1                                                                  ","100m3",1.6000000000000001E-3]
[22,"Posts С-1                                                                   ","units",4]
[23,"Simple painting of the plaster and section construction by white paints, prepared for painting ","100m2",0.18]
[24,"Marking of the construction","100units",0.01]
[25,"Arrangement of earth cofferdams by single-bucket excavators, diesel-powered, on caterpillar drive, soil group 1                                                                   ","1000m3",0.02]
[26,"Dewatering","Hours of dewatering",72]
[27,"Mounting of shutters with hoist ","т",0.3]
[28,"Lower gate DP-20-000                                                                 ","units",1]
[29,"Priming  of metal surfaces ","100m2",8.4000000000000005E-2]
[30,"Painting of metal primed surfaces","100m2",8.4000000000000005E-2]
[31,"Leveling of earth cofferdams by earthmovers at water engineering  ","1000m3",0.02]
["Capital repair of piped regulator with crossing RТК-100 1-2 DU PК0+30"]
[1,"Cleaning of the constructions from siltation by the multi-bucket excavators of cross cutting type in the soils of group 1 / high humidity boggy soil which intensely sticks to the bucket teeth and walls                                                                   ","1000m3",2E-3]
[2,"Soil excavation (excavation) into the construction by dragline excavators or back fillers, soil group 1 for work at water engineering","1000m3",0.01]
[3,"Fine excavation manually, manual bottom and banks stripping with soil discharge into the ditches and trenches, excavated mechanically.","100m3",0.01]
[4,"Planning of the canal bottom and banks by the single-bucket excavators, diesel-powered, on caterpillar drive, soil group 1-2","1000m2",0.1]
[5,"Arrangement of sand-gravel preparation the laying of fixing slabs          ","100m2",0.39]
[6,"Sand-gravel mixtures for construction works N3, fraction size more than 0 to 40 mm, mark DR12","m3",8.1]
[7,"Joints seal by tarred rope and fiber packing                                                                   ","100m",8.5999999999999993E-2]
[8,"Water isolation of concrete structures","100m2",0.2]
[9,"Back-filling of the construction","1000m3",1.0999999999999999E-2]
[10,"Soil consolidation by air rammers, soil group 1, 2                                                                   ","100m3",0.17]
[11,"Laying of fixing slabs","100m3",5.9520000000000003E-2]
[12,"Fixing slabs RP 15-30                                                                    ","units",12]
[13,"Fixing slabs RPU-10-15                                                                   ","units",18]
[14,"Installation of blocks Т-8                                                                    ","100m3",6.2500000000000003E-3]
[15,"Blocks Т-8                                                                 ","units",5]
[16,"Preparation of concrete","100m3",1E-3]
[17,"Ready heavy concrete mixtures, concrete class B15 [M200], filler fraction  bigger than 40 mm ","m3",0.1]
[18,"Installation of posts С-1                                                                  ","100m3",1.6000000000000001E-3]
[19,"Posts С-1                                                                   ","units",4]
[20,"Simple painting of the plaster and section construction by white paints, prepared for painting ","100m2",0.22]
[21,"Marking of the construction","100units",0.01]
[22,"Arrangement of earth cofferdams by single-bucket excavators, diesel-powered, on caterpillar drive, soil group 1                                                                   ","1000m3",2.8000000000000001E-2]
[23,"Dewatering","Hours of dewatering",72]
[24,"Mounting of box type gates with hoist                         ","t",0.39500000000000002]
[25,"Box type gate ЗК-1,3х1,0 with hoist 3В                                                                   ","units",1]
[26,"Priming  of metal surfaces ","100m2",9.6000000000000002E-2]
[27,"Painting of metal primed surfaces","100m2",9.6000000000000002E-2]
[28,"Leveling of earth cofferdams by earthmovers at water engineering  ","1000m3",2.8000000000000001E-2]
[29,"Arrangement of road embankments by earthmovers           ","1000m3",6.0000000000000001E-3]
[30,"Soil                                                                    ","m3",6]
[31,"Restoration of concrete cover","100m2",7.0000000000000007E-2]
["Capital repair of piped regulator with crossing RТК-100 1-2DU PК16+20"]
[1,"Dismantling of heads","100m3",3.0599999999999999E-2]
[2,"Cleaning of the constructions from siltation by the multi-bucket excavators of cross cutting type in the soils of group 1 / high humidity boggy soil which intensely sticks to the bucket teeth and walls                                                                   ","1000m3",4.0000000000000001E-3]
[3,"Soil excavation (excavation) into the construction by dragline excavators or back fillers, soil group 1 for work at water engineering","1000m3",1.6E-2]
[4,"Fine excavation manually, manual bottom and banks stripping with soil discharge into the ditches and trenches, excavated mechanically.","100m3",0.02]
[5,"Planning of the canal bottom and banks by the single-bucket excavators, diesel-powered, on caterpillar drive, soil group 1-2","1000m2",7.0000000000000007E-2]
[6,"Arrangement of sand-gravel preparation the laying of fixing slabs          ","100m2",0.28000000000000003]
[7,"Sand-gravel mixtures for construction works N3, fraction size more than 0 to 40 mm, mark DR12","m3",5.9]
[8,"Preparation of concrete","100m3",1.41E-2]
[9,"Arrangement of concrete bed","100m3",1.41E-2]
[10,"Mounting of heads with the laying of joints by cement mortar                                                                                                   ","100m3",3.0599999999999999E-2]
[11,"Head ОP-10А                                                                 ","units",1]
[12,"Head ОP-10                                                            ","units",1]
[13,"Joints seal by tarred rope and fiber packing ","100m",8.7999999999999995E-2]
[14,"Water isolation of concrete structures","100m2",0.4]
[15,"Back-filling of the structure","1000m3",1.7999999999999999E-2]
[16,"Soil consolidation by air rammers, soil group 1, 2                                                                   ","100m3",0.24]
[17,"Laying of fixing slabs","100m3",4.24E-2]
[18,"Fixing slabs RP-15-30                                                                    ","units",10]
[19,"Fixing slabs RPU-10-15                                                                   ","units",9]
[20,"Installation of blocks Т-8                                                                    ","100m3",6.2500000000000003E-3]
[21,"Blocks Т-8                                                                 ","units",5]
[22,"Preparation of concrete","100m3",5.0000000000000001E-4]
[23,"Ready heavy concrete mixtures, concrete class B15 [M200], filler fraction  bigger than 40 mm ","m3",0.05]
[24,"Installation of posts С-1                                                                  ","100m3",1.6000000000000001E-3]
[25,"Posts С-1                                                                   ","units",4]
[26,"Simple painting of the plaster and section construction by white paints, prepared for painting ","100m2",0.18]
[27,"Marking of the construction","100units",0.01]
[28,"Arrangement of earth cofferdams by single-bucket excavators, diesel-powered, on caterpillar drive, soil group 1                                                                   ","1000m3",0.02]
[29,"De-watering","Hours of dewatering",72]
[30,"Mounting of box type gates with hoist                         ","t",0.34200000000000003]
[31,"Box type gate ЗК-1,3х1,0 with hoist 3В                                                                   ","units",1]
[32,"Priming  of metal surfaces ","100m2",8.4000000000000005E-2]
[33,"Painting of metal primed surfaces","100m2",8.4000000000000005E-2]
[34,"Leveling of earth cofferdams by earthmovers at water engineering  ","1000m3",0.02]
[35,"Planning of earth surface by the earthmovers        ","1000m2",0.04]
[36,"Arrangement of road embankments by earthmovers           ","1000m3",6.0000000000000001E-3]
[37,"Soil                                                                    ","m3",6]
["Capital repair of piped regulator with crossing RТК-100 1-2 DU PК25+50"]
[1,"Dismantling of heads","100m3",1.4999999999999999E-2]
[2,"Cleaning of the constructions from siltation by the multi-bucket excavators of cross cutting type in the soils of group 1 / high humidity boggy soil which intensely sticks to the bucket teeth and walls                                                                   ","1000m3",4.0000000000000001E-3]
[3,"Soil excavation (excavation) into the construction by dragline excavators or back fillers, soil group 1 for work at water engineering","1000m3",8.0000000000000002E-3]
[4,"Fine excavation manually, manual bottom and banks stripping with soil discharge into the ditches and trenches, excavated mechanically.","100m3",0.01]
[5,"Planning of the canal bottom and banks by the single-bucket excavators, diesel-powered, on caterpillar drive, soil group 1-2","1000m2",7.0000000000000007E-2]
[6,"Arrangement of sand-gravel preparation the laying of fixing slabs          ","100m2",0.28000000000000003]
[7,"Sand-gravel mixtures for construction works N3, fraction size more than 0 to 40 mm, mark DR12","m3",5.9]
[8,"Preparation of concrete","100m3",7.0000000000000001E-3]
[9,"Arrangement of concrete bed","100m3",7.0000000000000001E-3]
[10,"Mounting of heads with the laying of joints by cement mortar                                                                                                   ","100m3",1.4999999999999999E-2]
[11,"Head ОP-10                                                                     ","units",1]
[12,"Joints seal by tarred rope and fiber packing ","100m",8.7999999999999995E-2]
[13,"Water isolation of concrete structures","100m2",0.2]
[14,"Back-filling of the structure","1000m3",8.9999999999999993E-3]
[15,"Soil consolidation by air rammers, soil group 1, 2                                                                   ","100m3",0.15]
[16,"Laying of fixing slabs","100m3",4.24E-2]
[17,"Fixing slabs RP-15-30                                                                    ","units",10]
[18,"Fixing slabs RPU-10-15                                                                   ","units",9]
[19,"Installation of blocks Т-8                                                                    ","100m3",6.2500000000000003E-3]
[20,"Blocks Т-8                                                                 ","units",5]
[21,"Preparation of concrete","100m3",5.0000000000000001E-4]
[22,"Ready heavy concrete mixtures, concrete class B15 [M200], filler fraction  bigger than 40 mm ","m3",0.05]
[23,"Installation of posts С-1                                                                  ","100m3",1.6000000000000001E-3]
[24,"Posts С-1                                                                   ","units",4]
[25,"Simple painting of the plaster and section construction by white paints, prepared for painting ","100m2",0.18]
[26,"Marking of the construction","100units",0.01]
[27,"Arrangement of earth cofferdams by single-bucket excavators, diesel-powered, on caterpillar drive, soil group 1                                                                   ","1000m3",0.02]
[28,"De-watering","Hours of dewatering",72]
[29,"Mounting of box type gates with hoist                         ","t",0.34200000000000003]
[30,"Box type gate ЗК-1,3х1,0 with hoist 3В                                                                   ","units",1]
[31,"Priming  of metal surfaces ","100m2",8.4000000000000005E-2]
[32,"Painting of metal primed surfaces","100m2",8.4000000000000005E-2]
[33,"Leveling of earth cofferdams by earthmovers at water engineering  ","1000m3",0.02]
[34,"Planning of earth surface by the earthmovers        ","1000m2",0.02]
[35,"Arrangement of road embankments by earthmovers           ","1000m3",6.0000000000000001E-3]
[36,"Soil                                                                    ","m3",6]
["Capital repair of piped regulator with crossing RТК-150 3 GD PК57+50"]
[1,"Deforestation","hа",0.01]
[2,"Rooting out of trees","hа",0.01]
[3,"Burning with the shake over of shrubs, low forest cover and roots by tractor","hа",0.01]
[4,"Cleaning of the constructions from siltation by the multi-bucket excavators of cross cutting type in the soils of group 1 / high humidity boggy soil which intensely sticks to the bucket teeth and walls                                                                   ","1000m3",0.01]
[5,"Planning of the canal bottom and banks by the single-bucket excavators, diesel-powered, on caterpillar drive, soil group 1-2","1000m2",0.15]
[6,"Arrangement of sand-gravel preparation the laying of fixing slabs          ","100m2",1.3]
[7,"Sand-gravel mixtures for construction works N3, fraction size more than 0 to 40 mm, mark DR12","m3",27.3]
[8,"Laying of fixing slabs","100m3",9.1759999999999994E-2]
[9,"Fixing slabs RP-15-30                                                                    ","units",26]
[10,"Fixing slabs RPU-10-15                                                                   ","units",8]
[11,"Installation of blocks Т-8                                                                    ","100m3",6.2500000000000003E-3]
[12,"Blocks Т-8                                                                 ","units",5]
[13,"Joints seal by tarred rope and fiber packing","100m",0.08]
[14,"Preparation of concrete","100m3",2E-3]
[15,"Ready heavy concrete mixtures, concrete class B15 [M200], filler fraction  bigger than 40 mm                                                         ","m3",0.2]
[16,"Arrangement of road embankments by earthmovers                                                                              ","1000m3",8.9999999999999993E-3]
[17,"Soil                                                                    ","m3",9]
[18,"Soil consolidation by air rammers, soil group 1, 2   ","100m3",0.09]
[19,"Installation of posts С-1                                                                  ","100m3",1.6000000000000001E-3]
[20,"Posts С-1                                                                   ","units",4]
[21,"Simple painting of the plaster and section construction by white paints, prepared for painting ","100m2",0.19]
[22,"Marking of the construction","100units",0.01]
[23,"Arrangement of earth cofferdams by single-bucket excavators, diesel-powered, on caterpillar drive, soil group 1                                                                   ","1000m3",2.5000000000000001E-2]
[24,"De-watering","Hours of dewatering",72]
[25,"Restoration of concrete cover","100m2",0.05]
[26,"Mounting of box type gates with hoist                         ","m",0.66700000000000004]
[27,"Box type gate ЗК-1,3х1,0 with hoist 3В                                                                   ","units",1]
[28,"Priming  of metal surfaces ","100m2",0.252]
[29,"Painting of metal primed surfaces","100m2",0.252]
[30,"Leveling of earth cofferdams by earthmovers at water engineering  ","1000м3",2.5000000000000001E-2]
["Capital repair of piped regulator with crossing RТК-150 К-24-3 PК0+30"]
[1,"Deforestation","hа",0.01]
[2,"Rooting out of trees","hа",0.01]
[3,"Burning with the shake over of shrubs, low forest cover and roots by tractor","hа",0.01]
[4,"Cleaning of the constructions from siltation by the multi-bucket excavators of cross cutting type in the soils of group 1 / high humidity boggy soil which intensely sticks to the bucket teeth and walls                                                                   ","1000m3",7.0000000000000001E-3]
[5,"Planning of the canal bottom and banks by the single-bucket excavators, diesel-powered, on caterpillar drive, soil group 1-2","1000m2",0.15]
[6,"Arrangement of sand-gravel preparation the laying of fixing slabs          ","100m2",1.3]
[7,"Sand-gravel mixtures for construction works N3, fraction size more than 0 to 40 mm, mark DR12","m3",27.3]
[8,"Laying of fixing slabs","100m3",9.1759999999999994E-2]
[9,"Fixing slabs RP-15-30                                                                    ","units",26]
[10,"Fixing slabs RPU-10-15                                                                   ","units",8]
[11,"Installation of blocks Т-8                                                                    ","100m3",6.2500000000000003E-3]
[12,"Blocks Т-8                                                                 ","units",5]
[13,"Joints seal by tarred rope and fiber packing","100m",0.08]
[14,"Preparation of concrete","100m3",2E-3]
[15,"Ready heavy concrete mixtures, concrete class B15 [M200], filler fraction  bigger than 40 mm                                                         ","m3",0.2]
[16,"Arrangement of road embankments by earthmovers                                                                              ","1000m3",5.0000000000000001E-3]
[17,"Soil                                                                    ","m3",5]
[18,"Soil consolidation by air rammers, soil group 1, 2   ","100m3",0.05]
[19,"Installation of posts С-1                                                                  ","100m3",1.6000000000000001E-3]
[20,"Posts С-1                                                                   ","units",4]
[21,"Simple painting of the plaster and section construction by white paints, prepared for painting ","100m2",0.19]
[22,"Marking of the construction","100units",0.01]
[23,"Arrangement of earth cofferdams by single-bucket excavators, diesel-powered, on caterpillar drive, soil group 1                                                                   ","1000m3",2.5000000000000001E-2]
[24,"De-watering","Hours of dewatering",72]
[25,"Restoration of concrete cover","100m2",0.05]
[26,"Mounting of box type gates with hoist                         ","t",0.66700000000000004]
[27,"Box type gate ЗК-1,3х1,0 with hoist 3В                                                                   ","units",1]
[28,"Priming  of metal surfaces ","100m2",0.252]
[29,"Painting of metal primed surfaces","100m2",0.252]
[30,"Leveling of earth cofferdams by earthmovers at water engineering  ","1000m3",2.5000000000000001E-2]
["Capital repair of piped regulator with crossing RТК-100 3-1К PК8+15"]
[1,"Shrubs cutting by tractor brush breaker ","hа",1.4999999999999999E-2]
[2,"Sweeping of cut shrubs by tractor rakes ","hа",1.4999999999999999E-2]
[3,"Grubbing of shrubs by tractor mechanism for grubbing and collecting ","hа",1.4999999999999999E-2]
[4,"Burning with the shake over of shrubs, low forest cover and roots by tractor ","hа",1.4999999999999999E-2]
[5,"Cleaning of the constructions from siltation by the multi-bucket excavators of cross cutting type in the soils of group 1 / high humidity boggy soil which intensely sticks to the bucket teeth and walls                                                                   ","1000m3",1.2E-2]
[6,"Planning of the canal bottom and banks by the single-bucket excavators, diesel-powered, on caterpillar drive, soil group 1-2","1000m2",0.08]
[7,"Arrangement of sand-gravel preparation the laying of fixing slabs          ","100m2",0.32400000000000001]
[8,"Sand-gravel mixtures for construction works N3, fraction size more than 0 to 40 mm, mark DR12","m3",6.8]
[9,"Joints seal by tarred rope and fiber packing                                                                  ","100m",8.7999999999999995E-2]
[10,"Laying of fixing slabs","100m3",3.7600000000000001E-2]
[11,"Fixing slabs RP-15-30                                                                    ","units",10]
[12,"Fixing slabs RPU-10-15                                                                   ","units",5]
[13,"Installation of blocks Т-8                                                                    ","100m3",6.2500000000000003E-3]
[14,"Blocks Т-8                                                                 ","units",5]
[15,"Preparation of concrete","100m3",5.0000000000000001E-4]
[16,"Ready heavy concrete mixtures, concrete class B15 [M200], filler fraction  bigger than 40 mm ","m3",0.05]
[17,"Installation of posts С-1                                                                  ","100m3",1.6000000000000001E-3]
[18,"Posts С-1                                                                   ","units",4]
[19,"Simple painting of the plaster and section construction by white paints, prepared for painting ","100m2",0.22]
[20,"Marking of the construction","100units",0.01]
[21,"Arrangement of earth cofferdams by single-bucket excavators, diesel-powered, on caterpillar drive, soil group 1                                                                   ","1000m3",2.8000000000000001E-2]
[22,"Dewatering","Hours of dewatering",72]
[23,"Mounting of box type gates with hoist                         ","t",0.39500000000000002]
[24,"Box type gate ЗК-1,3х1,0 with hoist 3В                                                                   ","units",1]
[25,"Priming  of metal surfaces ","100m2",8.4000000000000005E-2]
[26,"Painting of metal primed surfaces","100m2",8.4000000000000005E-2]
[27,"Leveling of earth cofferdams by earthmovers at water engineering  ","1000m3",2.8000000000000001E-2]
[28,"Arrangement of road embankments by earthmovers           ","1000m3",6.0000000000000001E-3]
[29,"Soil                                                                    ","m3",6]
["Other Expenses"]
[1,"Communication",1]
[2,"Transportation and Logistics",1]
[3,"Other (if any, with indication of cost type)",1]
["TOTAL"]