{"text_format":"2","workbook":"xlsx","n_sheets":4,"sheets":["BOQ","cover","UCAS","Summary"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":7,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"BOQ","index":0,"n_rows":19,"n_cols":1,"rows_kept":19,"cut":false,"hidden":false,"merged":[[17,0,17,2],[18,0,18,2],[7,0,7,2],[9,0,9,2],[11,0,11,2],[12,0,12,2],[14,0,14,2],[16,0,16,2]]}
{"$rows_empty":7}
["UNITED NATIONS DEVELOPMENT PROGRAMME"]
[]
["ITB 2015-239"]
[]
[" Lot 13-A"]
["WBS 1401"]
[]
[" Bill of Quantities"]
[]
["Programme Title: Right to Education in the Gaza Strip"]
["Project name: Recovery for Higher Education"]
["PAL10- 00094739- LOT 13-A\nRehabilitation Works for  UCAS-University College of Applied Science"]

{"sheet":"cover","index":1,"n_rows":15,"n_cols":1,"rows_kept":15,"cut":false,"hidden":false,"merged":[[20,0,20,8],[7,0,7,8],[12,0,12,8],[14,0,14,8],[15,0,15,8],[17,0,17,8]]}
{"$rows_empty":7}
["UNITED NATIONS DEVELOPMENT PROGRAMME"]
[]
[]
[]
[]
["ITB 2015-239"]
[]
["UCAS-University College of Applied Science"]

{"sheet":"UCAS","index":2,"n_rows":589,"n_cols":7,"rows_kept":589,"cut":false,"hidden":false,"merged":[[464,0,464,4],[474,0,474,4],[481,0,481,4],[536,0,536,4],[555,0,555,4],[483,0,483,5],[497,0,497,5],[499,0,499,5],[501,0,501,5],[506,0,506,5],[551,0,551,5],[410,0,410,4],[424,0,424,4],[430,0,430,4],[436,0,436,4],[451,0,451,4],[309,0,309,4],[348,0,348,4],[363,0,363,4],[369,0,369,4],[375,0,375,4],[334,0,338,0],[334,2,338,2],[334,3,338,3],[334,4,338,4],[334,5,338,5],[482,0,482,5],[505,0,505,4],[339,0,339,4],[340,0,340,5],[401,0,401,4],[402,0,402,5],[452,0,452,4],[453,0,453,5],[476,0,478,0],[476,2,478,2],[476,3,478,3],[476,4,478,4],[476,5,478,5],[480,0,480,4],[387,0,387,4],[400,0,400,4],[323,4,333,4],[323,5,333,5],[241,0,241,5],[313,0,322,0],[313,2,322,2],[313,3,322,3],[313,4,322,4],[313,5,322,5],[323,0,333,0],[323,2,333,2],[323,3,333,3],[254,0,254,4],[274,0,274,4],[281,0,281,4],[288,0,288,4],[297,0,297,4],[48,0,48,4],[49,0,49,5],[11,0,11,5],[22,0,22,4],[240,0,240,4],[196,0,196,4],[189,0,189,4],[82,0,82,5],[1,0,1,5],[23,0,23,5],[197,0,197,5],[125,0,125,5],[57,0,57,4],[58,0,58,5],[81,0,81,4],[190,0,190,5],[124,0,124,4],[50,0,51,0],[588,0,588,4],[520,0,520,5],[522,0,522,5],[528,0,528,5],[531,0,531,5],[537,0,537,5],[556,0,556,5],[587,0,587,4],[570,0,570,5],[574,0,574,5],[578,0,578,5]]}
["Item \nNo","Description ","Unit","Quantity ","Unit Rate \nUS $ ","Total Amount US $"]
["General Notes: "]
[null,"1- Complete detailed shop drawings should be delivered to the Engineer to take his approval prior the commencement of work. Samples of all materials shall also be delivered to the Engineer to take his approval,"]
[null,"2-Contractor shall take into consideration that all – direct and indirect works and their relevant expenses required for proper implementation of the project including temporary facilities, fencing, securing utilities (water, wastewater, telephone and electricity systems) as well as making access to project implementation location away from the one in use by the students and teachers such that the university is running safely without disturbance."]
[null," 3-The contractor will be accountable for all necessary equipment, materials and activities to assure the safety of people within the university buildings and  vicinity, where an approved safety plan will be prerequisite to initiating activities along with installing all required components and materials necessary for safety of workers, project team as well as people at university."]
[null," 4-All relevant costs  are deemed to be included in the unit price in addition to the required re-instatement works needed to bring the original facilities to its original status before addition of temporary works. "]
[null,"5-The contractor will expect that more than one contractor will be carrying out works in the university at the same time, the Contractor is presumed to make all necessary coordination and facilitate accessibility to  and other work-related issues"]
[null,"6-All works and installations listed here below should be carried out, tested and commissioned by specialized responsible skilled labors in full coordination with university engineering office , all in accordance with drawings, specifications and relevant standards, and the instruction of the  Engineer."]
[null,"7- All unite price for each Item includes remove any surplus materials and any debris for any floor safely according to specifications and/or engineer's instructions"]
[null,"9- The contractor should prepare and submit detailed work plan in coordination with University."]
[null," 8-The Engineer has the right to reject any component of the work not complying with the specifications and the terms of the contract."]
["Bill No (A) - 1. Demolition Works"]
[null,"1-Contractor shall take into consideration that all – direct and indirect works and expenses required for the completion of the coming items are included in the unit price. Measurement is engineering measurement."]
[null,"2-All works must be according to drawings, specification and engineer instructions. Rates shall include :                                                                                                                                                                   "]
[null,"3-Cleaning the site and removing all debris, surplus unwanted materials and rubbles to approved dump site. "]
[null,"4- Price include all required tests by an approved laboratory for the defected & damaged concrete element specified by the engineer."]
[null,"5- The price includes detailed Method of statement including safety plan and in coordination with the University. "]
[1.1000000000000001,"Demolish the existing columns, concrete stairs, tiles, foundation, ground beams, steel and any required work in the administration building entrance and remove all debris to approved dump site and dismantling the existing marble and handling to the university. The price also includes dismantle carefully the existing fire clay of administration roof and handling to the university including protection and preservation of all existing finishing, electrical works & mechanical utilities, fittings, equipment and machines.…etc.  \nThe price includes dismantle, reinstall and commission air conditioners, pipes, advertisement panels and any other required works to complete the job and contract items according to specifications, and engineer instruction. All works according to Engineer instructions ,and specifications","L.S",1]
[1.2,"Demolish and remove the defected parts of slabs, concrete columns, lintels, terrazzo and ceramic tiles, concrete and hollow block walls with different thicknesses and  heights in all floors of the administration building (A) ,male student building and female student ( W) buildings. The price includes removing all defected materials inside and outside the building  including but not limited to tiles, plaster, gypsum walls and ceiling, steel, foundations, ground beams, concrete debris and solid waste etc. and transporting to approved dump sites, and includes covering the steel reinforcement for the slabs and columns starters on the existing roof, dismantling the existing wooden and gypsum partitions, doors, windows, protection steel, Gypsum wall ,electrical sockets/switches, fans,  aluminum windows , wood doors and any works inconsistent with the new design & the contract items  and any required materials and handling to the university including protection and preservation of all existing finishing, electrical works & mechanical utilities, fittings, equipment and machines.…etc. All works according to Engineer instructions ,and specifications. ","L.S",1]
[1.3,"Dismantle carefully the existing fire clay roof ( female students building) and storing in good conditions(to be reinstall in administration entrance) including protection and preservation of all existing finishing, electrical works & mechanical utilities, fittings, equipment and machines.…etc. All works according to Engineer instructions ,and specifications. \nThe price includes dismantle, reinstall and commission air conditioners, pipes, advertisement panels and any other required works to complete the job according to specifications, and engineer instruction. All works according to Engineer instructions ,and specifications. ","L.S",1]
[1.4,"Excavation from natural ground level in any type of soil to required designed level. The works including: The compaction of the soil surfaces to get (98% MDD). The excavated unwanted material should be removed out from the site to the approved places. The excavated selected material should be properly stored in the vicinity of site for reuse in backfilling. All to be executed as per specifications, drawings and the engineer’s instructions.","M3",100]
[1.5,"Supply, and fill dune sand between ground beams & inside the building up to the required levels, which shall be spread in layers not exceeding 25cm each one & compacted (98%) to reach up the required levels (under floor slab), according to the specifications & the engineer's instructions.","M3",100]
["Total"]
["Bill No (A) - 2. Concrete Works."]
[null,"Rates of Concrete Works shall include:-\n1. All form works and shuttering (new lumber for shuttering painted by special oil (fuel or burnt oil is not accepted)  in any form, shape and size . Making chamfered and curved edges, allowing for and making grooves and sleeves and using Tie Rods (Batant) for concrete walls ; removal of forms and cleaning of all exposed tie wires and rods. Steel forms must be used in shuttering the external decorations."]
[null,"2. Supplying, Casting, vibrating and curing as per specifications."]
[null,"3. Approved additives and admixtures."]
[null,"4. Developing new Concrete Job Mix Designs, Sampling , testing and providing test results certificates, storing and saving of samples."]
[null,"5. Painting of exposed surfaces of underground reinforced concrete elements with two coats of hot bituminous paint (75/25) after primer layer , the strokes of each layer to be opposite to each other."]
[null,"6. Preliminary installations for Electrical, plumbing and floor drainage in floor slabs including final floor slab."]
[null,"7. Compaction and testing under the foundation, ground beams, ground slabs and Apron. the compaction should not be less than  98% of MDD."]
[null,"8. All works according to specifications , drawings and supervisor engineer instructions "]
[null,"9.Supply, fabricate and fix reinforcement steel (fy= 410 N/mm2) for all the structural elements according to drawings and engineer's instructions for any grade, size and length as detailed in the drawings, storing on site including cutting, bending and fixing in position  and providing all tying wires, spacers, shop drawings, testing and bar bending schedules .All works according to specifications , drawings and supervisor engineer instructions "]
[null,"10. In rehabilitation works, supply fabricate and fix steel dowels to the existing concrete using special materials. In case of lapping with existing steel reinforcement, rates will include cleaning rust and treatment with special materials "]
[null,"11. In case after excavation the new columns locations and relevant footings coincide with the existing ones, the contractor will make modification to adapt implementation to the existing conditions and deemed to include in his rates relevant costs accordingly.  "]
[null,"12. The works shall include removal of any existing insulation sheets, foam concrete, development of columns steel with the existing by using epoxy material , rates will include cleaning rust, treatment with special materials, the insulation shall be reinstated around the new constructed part."]
[null,"13. The unit price includes demolish and removal of any required elements to complete the work according to the new design. "]
[null,"14. All rehabilitation works will include the necessary extra steel reinforcement and concrete to be applied in layers if necessary in addition to the necessary special materials and accessories."]
[null,"15-The price include all safety measures, scaffolding and all required by the engineer "]
[2.1,"Supply and cast reinforced concrete 'B300' for Foundation and Walls  according to specifications, drawing, and Engineer instructions.","M3",8]
[2.2000000000000002,"Ditto but for ground beams including ground beam for the platform.","M3",8]
[2.2999999999999998,"Supply and cast reinforced concrete 'B 300' 32cm thick ribbed slab. Unit price shall include demolish of loss concrete parts, additional steel, special materials for rehabilitations, supply and install lightweight blocks density 450kg/m³, (size 25x40x24) and the required steel reinforcement, decorative arches in the last slab, corridor concrete parapet. Price shall include all drop beams, inverted beams, and all other beams and projections as per specifications and drawing.","M2",25]
[2.4,"Supply and cast ready mix concrete B (300) kg/cm2 for suspended solid slab 17 cm thick, including the reinforced steel, decorative arches in last slab, corridor concrete parapet, under steel balustrade for the typical slab, , all drop and inverted beams everywhere in the slab and all other materials as per specifications and drawings.","M2",150]
[2.5,"Supply and cast reinforced concrete  'B250' for lintel beams and decoration elements. Unit rate shall include cost of steel reinforcement of 4Ф10mm steel bars with Ф 8mm stirrups@20cm,scaffolding for external decoration elements,  and all works according to drawing, engineer instructions ,and specifications. ","M3",30]
[2.6,"Ditto but for all elements of stair case including the entrance stairs and ramps the price includes scaffolding, special materials and any required works to complete the job.","M3",7]
[2.7,"Rehabilitation of shear walls opening, columns and decorative concrete elements (halls)   includes supply and cast of reinforced concrete 'B350 F.F '. The Unit rate shall include shuttering, removal of loose concrete, scaffolding, cost of steel reinforcement , additional steel reinforcement, special materials to make bond between old and new concrete, cleaning of the existing steel reinforcement and special materials anti rust, special methods and materials for rehabilitation,  and all works according to drawing, engineer instructions ,and specifications. ","M3",20]
[2.8,"Jacketing and strengthening of reinforced concrete column with free flow self-compacting concrete microconcrete (350kg/cm2) manufactured by special fosroc chemical or equivalent.\nPrice includes removing plaster, loose concrete, cleaning the reinforcement with wire brush and finally with special material for rust and special material to make bond between steel bars and concrete.\nPrice includes fixing dowel bars 8mm diameter every 20m in both directions horizontal and vertical using special material to make bond between steel bars and concrete, grid of steel reinforcement 10mm diameter every 20cm in both directions horizontal and vertical with thickness of the jackets at least 10cm. \nMixing micro-concrete and water in proportion, mixing, additives for workability and self compacting, maintaining strength of cast concrete, method statement and curing period as described by manufacturer.\nPrice includes providing shuttering, disposal of debris and all activities for assuring bonding of old and new concrete.","M3",5]
[2.9,"Ditto but for circular Jackets for the existing columns. The price includes additional steel (10Y12mm and 1Y8/15cm), demolish of edges of the existing column and remove all debris to approved dump site and special materials to make bond between old and new concrete as per specifications, drawings and engineer's instructions.","M3",5]
["Total"]
["Bill No (A) - 3. Building Works"]
[null,"The price include: \n1- Supplying hollow or solid cement block from good and approved factory in perfect dimension and build it in good manner with  a compressive strength 35 kg/cm2 for hollow block and 60 kg/cm2 for solid block. This item will include cement mortars, galvanized steel ties, reinforced concrete infill (B250) between columns & block walls (10-20 cm wide) and top, bottom lintels, sills for windows, doors and decorative arches with 1Ø8mm/40cm horizontally and 2Ø8mm vertically according to drawings, pipes encasement, false columns 20x20 cm/4.0m among the parapet wall with 4Ø12mm and bituminous paper between block work and drop beams and testing as well as  all requirements needed to finish the works according to the drawings, specification and to the  supervision engineer instructions. "]
[null,"2- The unite price includes dismantle any required works and deliver to university stores and demolish any required works and remove all debris safely to approved dump site."]
[3.1,"Supply and build hollow cement blocks 40x20x 20cm ","M2",250]
[3.2,"   Supply and build solid cement block 40x20x20 cm","M2",50]
[3.3,"Supply and build hollow cement blocks 40x20x 15cm ","M2",70]
[3.4,"Supply and build hollow cement blocks 40x20x 12cm ","M2",150]
[3.5,"Supply and build hollow cement blocks 40x20x 10cm ","M2",70]
["Total"]
["Bill No (A) - 4. Carpentry works"]
[null,"The items include supplying carpentry works from good wood grade “A” including frame cover mould, architrave, sanding sealer, prime coats, at least two coats of oil paint, 15cm aluminum kick plate 1mm thick from both sides , hard ware,  lock type Wally switch or equivalent and brass hinges 10cm height, door stopper and all other fitting according to specification and drawing."]
[null,"NOTES :\n* Sizes of carpentry works given in the bills of quantities are skeleton sizes and shall be as per drawings.\n* Sizes of doors and other items mentioned in the bills of quantities shall allow for tolerance to suit the structural openings shown in the Drawings.\n* Wooden doors and pair of doors shall be measured in number for each structural opening, unless stated otherwise in the bills of quantities.\nRates for carpentry and joinery work shall include:\n1. Shop and coordinated drawings.\n2.  Allowance for plastering and tiling and the like.\n3. Cutting and fitting around obstructions, bedding and painting.\n4. Grounds, blocking and backings."]
[null,"5. Plugging concrete, block work, and stonework, and making well, frame insulation beneath tiles.\n6. Ironmongery including wally cylindrical locks ,wally or equal handles, stoppers, screws, temporary fixing, refixing, oiling and adjusting.\n7. Providing master key for each floor.\n8. Providing 3 keys for each lock including tagging.\n9. Preparing surfaces to receive finishes.\n10. Painting, varnishing, polishing, oiling, and the like, to any area or width in any location including work in multicolor and cutting in edges and putty.                        11. Dismantle or removing any defected parts or elements, and preparing for new installment. "]
[4.0999999999999996," Supply, fix & paint flushed wooden Single door,  size (90x220cm) and 45mm thick to match the existing, Plywood laminated both sides as detailed on the drawings and as specified; complete including frames, trims, hardwood lippd, hardware locked type Ferro switch or equivalent, brass hinges, clear glass window 20*30 cm 6 mm thickness and door stops. the price includes painting one priming coat and two oil finishing  coats, All works according to specifications, approved drawings and engineer instructions.","No",25]
[4.2,"Ditto But 100x220 cm. ","No",5]
[4.3,"Ditto But  80 x 220cm without glass window.","NO",25]
[4.4000000000000004,"Ditto But double leave  120 x 220cm.","NO",20]
[4.5,"Maintenance wooden door overall size 90 x 220 x 4.5cm thick. The Price includes remove & replacement of the defected parts of wooden door,frame, accessories or/and switch,  dismantle and supply and install of ceramic tiles, supply and install granite tile to match the existing (25cm length, 5cm wide 2cm thick.) around the bottom of the frame  15 cm aluminum kick plate from both sides, all accessories, materials and  all related works  as per drawings, specification and Engineer’s Instructions.","No",120]
[4.5999999999999996,"Ditto but door size 100 x 220 x 4.5cm thick. .","No",15]
[4.7,"Supply, fix & paint flushed wooden (hard wood- zany) double door,  size (215x230cm) and 45mm thick to match the existing , composed with brushed glass 6mm, Plywood laminated both sides as detailed on the drawings and as specified; complete including frames,  trims, hardwood lippd, hardware locked type Ferro switch or equivalent, high quality brass hinges, and door stops. the price includes painting one priming coat and two lazour finishing  coats and lucker, All works according to specifications, approved drawings and engineer instructions.","No",5]
[4.8,"Ditto but  size 100x200cm","No",2]
[4.9000000000000004,"Ditto but  size 120x200cm","No",2]
[4.0999999999999996," Supply and fix soft wood rubbing rails size 150mm x 20mm with round edges, smooth surface , apply two coats of sanding sealer, one coat of  lacquer paint. sand lightly and apply two coats of varnish, drill and fix to concrete or block walls using expansion steel bolts as per specification and drawings..","LM",450]
[4.1100000000000003,"Supply and install wall mounted magnetic white marker board Lina series, 25 mm profile callboard MG 3612/L size 120x360 cm) with silver anodized elegant aluminum frame (19x25mm thick) and four strong rounded plastic (up) corners fixed internally with screws to the wall, and also with silver anodized aluminum try fixed by sliding through the profile which used for chalks, markers and duster and has UPVC edges for safety. The writing surface coated of steel polyester fixed by using automatic gluing machines to 11mm thick MDF wood covered automatically by aluminum foils.  Price to include all related works as per drawings, specification and Engineer’s Instructions.","No",5]
[4.12,"Ditto but 240*120 cm.","No",10]
[4.13,"Supply and fix 500x120x20mm soft wood coat hook rail smoothed , plugged and screwed to wall at 30cm center to center including priming and painting with brass coat hook 3mm thick, screwed to rail at 15cm center to center as per specifications and drawings and to be approved by the engineer.","No",100]
[4.1399999999999997,"Supply and fix framed fibber bulletin board (cork sheet 2 mm thick) size 1.2 x 1.00 m from Callboard (BC129) or equivalent. Price includes aluminum frame 5 x 1.5 cm silver painted, Plywood veneer 5 mm thick on the back, and all necessary fixings, fittings, accessories. ","No",10]
[4.1500000000000004,"Ditto but 50*50 cm","No",10]
[4.16,"Ditto but 120*240 cm","No",5]
[4.17,"Ditto but 70*70 cm","No",5]
[4.18," Supply and install 80*50mm softwood (Swedish) rail for handrails with round edges to match the existing, smooth surface, apply one coat of sanding sealer, two coat of approved lazoure paint and one coat of lucker, using stainless  steel bolts the price also includes dismantle and remove all defected parts according to  specifications and engineer instructions. ","L.M",100]
[4.1900000000000004,"Supply and install hard wood-zany frame width ( 50mm*30mm) T section to fix the glass & the Polycarbonates, the price includes all accessories, painting one priming coat and two lazour finishing  coats and lucker , All works according to specifications,  and engineer instructions.","L.M",200]
["Total"]
["Bill No (A) - 5. Aluminum & Metal works"]
[null,"NOTES :"]
[null,"*All Aluminum profile, sections and accessories shall be best quality and free from manufacturing defects and shall be completed with proper manner and accordance with the specifications."]
[null,"*All Aluminum profile sections  shall be (Kalel or equivalent) \" 4500\" - \"7000\" - \"8300\" - \"8100\" to match the existing and thickness not less than 1.5mm according to items"]
[null,"1- Color of aluminum according to site (to match the existing)"]
[null,"2-    All accessories, wheels, rails, hinges, handles, locks, brushes, rubber EPDM, and angles must be the original of profile, 6mm thick 80% grey glazing sheets."]
[null,"3-   Dimensions shown on the detailed drawings are the architectural dimensions of the doors or windows' leaves, not including frames."]
[null,"4-   All doors should be provided with high quality auto-close jack machine "]
[null,"5-All external windows are double and reflected glass (interior side clear glass  4 mm and exterior side glass  6mm )"]
[null,"6-Price includes dismantling all damaged windows and delivering to university."]
[null,"7- Windows dimensions more than 1m square includes internal aluminum partitions."]
[null,"8-Price includes scaffolding where needed"]
[null,"9-Price includes removing the existing old damaged windows if needed."]
[null,"10-Supplying missing parts, dismantling and refixing the defected elements after complete maintenance with complete accessories to complete the job included in the unit price."]
[null,"11- Steel work should be properly treated and prepared, painted with two coats of oil paint, one primer (polyzinc) and one undercoat. The price shall include removing the damaged aluminum and steel works and handing to the university Store."]
[5.0999999999999996,"Supply and fix aluminum partitions type 2000 including double clear glass 6mm and 4mm one of them brushed by sand, composite panels at bottom of partitions, doors, locks, high quality jack for door , ironmongery, hardware and all required accessories, to match existing partitions and as per specification, and/or  the engineer instructions. ","M2",450]
[5.2,"Supply and install aluminum door type 2000 (200*240cm) complete with frame including double clear glass 6mm and 4mm one of them brushed by sand, composite panels at bottom of the door, jack and all ironmongery, hardware and all required accessories as per specifications, drawing and/or  the engineer’s instructions","NO",5]
[5.3,"Supply and install aluminum door type 2000 (180*240cm) complete with frame including double clear glass 6mm and 4mm one of them brushed by sand, composite panels at bottom of the door, jack and all ironmongery, hardware and all required accessories as per specifications, drawing and/or  the engineer’s instructions","NO",3]
[5.4,"Supply and install aluminum door type 2000 (140*240cm) complete with frame including double clear glass 6mm and 4mm one of them brushed by sand, composite panels at bottom of the door, jack and all ironmongery, hardware and all required accessories as per specifications, drawing and/or  the engineer’s instructions","NO",3]
[5.5,"Ditto but over all size  120 x 235cm","No",5]
[5.6,"Ditto but overall size 100 x235cm ","No",10]
[5.7,"Supply and install  aluminum partitions Greek type P100 (or equivalent)  including two layers of clear glass 6 mm, silver aluminum curtains between the two layers of glass equipped with a special profile size 6.6*14 cm, for wiring private channels separated from each other to pass the phone lines, computers, electricity, composite panels at bottom of partitions, doors, locks, high quality jack, ironmongery, hardware and all required accessories,  as per specification, and/or  the engineer’s instructions. \n","M2",300]
[5.8,"Supply and install Aluminum window complete with frame section Type \"7000\" to match the existing( Ambatia),  sliding leaves ,obscure reflector glass  6mm  to match the existing thick, ironmongery and hardware and as per specifications, drawing and/or  the engineer’s instructions according to drawings and specifications.","M2",150]
[5.9,"Ditto but Aluminum type 4500 to match the existing, top hinged type, powder coated color, the price includes reflector glass 6mm,jack , ironmongery and hardware and all accessories as per specifications, drawing and/or  the engineer’s instructions.","M2",80]
[5.0999999999999996,"Supply and install Aluminum windows leave only  section Type \"7000\" to match the existing( Ambatia),  sliding leaves ,obscure reflector glass  6mm  to match the existing thick, ironmongery and hardware and as per specifications, drawing and/or  the engineer’s instructions according to drawings and specifications.","M2",70]
[5.1100000000000003,"Supply and install Aluminum curtain wall window section Type \"4500\" according to attached drawings (to match the existing), the price includes the price includes reflector glass 6mm,jack , ironmongery and hardware and all accessories as per specifications, drawing and/or  the engineer’s instructions.","M2",40]
[5.12,"Supply and install clear glass 4mm for windows to match the existing the price includes remove all broken glass to approved dump site, complete maintenance and all required accessories according to specifications and engineer instructions.","M2",60]
[5.13,"Ditto but for clear glass 6mm.","M2",40]
[5.14,"Ditto but for reflector glass 6mm.","M2",100]
[5.15,"Supply and fix colored aluminum  doors for the ducts of water (to match the existing). overall size 70 x 120cm, complete with frame the price includes, fiber glass 4mm thick, lock, Handel, hinged,  ironmongery and hardware. and as per specification and drawing. ","M2",10]
[5.16,"Maintenance of the ducts doors, the price includes supply and replace all defected parts and all required accessories according to specifications and engineer instructions. ","M2",35]
[5.17,"Supply and fix colored aluminum door type 4500 , overall size 80 x 220cm, complete with frame, white color, clear glass brushed with sand 6mm thick, fiber glass ironmongery and hardware. and as per specification and drawing. ","No",5]
[5.18,"Supply and install  aluminum strip door (okerdion) P100 (Greece type) the width of each panel not exceed than 65 cm . The number of panels according to submitted shop drawings the price includes double glass 4mm,upper and lower rails,  ironmongery and hardware and as per specifications, drawing and/or  the engineer’s instructions.","M2",25]
[5.19,"Maintenance and fix powder coated colored aluminum window  Kalel 7000, complete with frame,  sliding leaves ,with obscure glass 4mm thick, ironmongery and hardware, the price include replacement of defected parts and as per specifications, drawing and/or  the engineer’s instructions.","m2",150]
[5.2,"Maintenance and fix powder coated colored aluminum window Kalel 4500, complete with frame,  jack,obscure glass 6mm thick, ironmongery and hardware and  the price include replacement of defected parts as per specifications, drawing and/or  the engineer’s instructions.","m2",75]
[5.21,"Maintenance and fix powder coated colored aluminum partitions and doors type 2000 including supply and replace all defected parts, clear glass 6mm, fiber glass 4mm panels at bottom of partitions, doors, locks, jack, ironmongery, hardware and all required accessories, to match existing partitions and as per specification, and/or  the engineer instructions. ","M2",100]
[5.22,"Maintenance and fix Aluminum curtain wall window section Type\" 8100\",\"8300\" . The price includes, scaffolding, dismantle, reinstall, supply and install any missing parts, clear glass 6mm , jack, lock,....etc. and any required accessories according to specifications and engineer instructions.","M2",100]
[5.23,"Dismantle and reinstall the existing glass after brushing by sand with shapes as required by the engineer (to match existing). The price includes complete maintenance of aluminum elements,  and any required accessories according to specifications and engineer instructions.","M2",25]
[5.24,"Supply and install Polycarbonates brushed by sand,  4mm thickness  with required shapes by the engineer (to match existing). The price includes any required accessories according to specifications and engineer instructions.","M2",70]
[5.25,"Ditto but for 6mm glass.","M2",40]
[5.26,"Supply and fix galvanized steel balustrade for stair case to match the existing , the price includes painting with one primer (poly Zinc),  under coats and minimum two coats of oil paint, hardwood (Zaan) handrails (to match the existing) with round edges, smooth surface, apply one coat of sanding sealer, two coat of approved lazoure paint and one coat of lucker and required accessories and material to complete the job as per specifications, drawings and engineer instructions. ","L.M",200]
[5.27,"Supply and fix steel protection for windows over all size 250x110 cm to match the existing the price includes painting with one primer (poly Zinc),  under coats and minimum two coats of oil paint  and required accessories and material to complete the job as per specifications and engineer instructions. ","M2",80]
["Total"]
["Bill No (A) - 6. Finishing works"]
[null,"A- Plaster works"]
[null,"All works must be according to drawings, specification and engineer instructions. Rates shall include :                                                                                                                                                         "]
[null,"1-Supply of all needed materials, including galvanized angles for the corners, windows and external decoration  as well as the use of   galvanized wire mesh  between concrete and block work. "]
[null,"2-Preparation works by covering all conduits of electricity, water supplies , etc.,  with  a galvanized wire mesh at least 20cm width  coated by mortar (1:1) cement : sand and the work  includes removal of  wires and  nails and cleaning of surfaces to be ready for plastering."]
[null,"3- Contractor shall take into consideration that all – direct and indirect works and expenses required for the completion of the coming items are included in the unit price."]
[null,"4-Trimming of concrete chippings, removing the wires and etc. and cleaning  of  existing surfaces to be ready for plastering."]
[null,"5- Checking out all of the preliminary installation in ceilings and walls such as electrical, water supply and waste water pipes and repairing the damages if any."]
[null,"6- Curing with water for at least three days for each coat."]
[null,"This should be done prior to commencement of plastering and after obtaining a written approval from the supervision engineer.\n7- The unit price includes scaffolding, removal all Tyrolean existing finish layer, maintenance all existing plaster after removal specified area, repairing cracks, preparing the surface to install the new layer, covering the windows by polytherene sheets, dismantle, refix and commission air conditioners, pipes, advertisement panels and any other required works to complete the job according to specifications, and engineer instruction."]
[null,"8-The unit price includes removal of damaged or burnet plaster by sand gun, haking deteriorated  loose plaster layers and remove all debris to approved dump site\n9- The unite price includes maintenance for block works and any defected ribs (slab blocks) ."]
[null,"B- Tiles works"]
[null,"All works must be according to drawings, specification and engineer instructions.\n Rates shall include :                                                                        "]
[null,"1. Samples for approval and all the required tests."]
[null,"2. Cleaning, mechanical polishing and pointing using grout."]
[null,"3.Insulation works under ceramic floor tiles for all wet areas and kitchens using primer coat, two hot bitumen coats (75/25)"]
[null," 4. Plastic angle beads for ceramic wall tiles at the corners and top and sides of ceramic edges."]
[null,"5. Local marble must be Grade (A), free from cracks, holes and pits, clay flaws, homogeneous in color, and approved by the Engineer."]
[null,"6. Measuring the stockpiled quantities of tiles and obtaining the engineer approval prior to shipment to the site."]
[null,"7.Transporting and carefully  handling the stored quantities to the site."]
[null,"8.Black Basalt mixed with white marble chips, size 4mm, shall be used in precast terrazzo tiles and skirting. Price of tiles shall include all tests required as directed by the Engineer."]
[null,"9.Only grade A imported glazed ceramic tiles (floor and wall) shall be used, and approved by the Engineer . "]
[null,"10.Price shall include Skirting, polish, and remove existing tiles out of site.\n"]
[6.1,"Supply and make internal plastering 13 mm thick  for walls, Ceiling, soffits and drop beams. The work includes rough primer nail rendering to form a key with  (mix 1:1) cement sand, second layer 13mm: Base-Coat \"Rendering\" with (1:3:0.25) cement: sand : lime and third layer: Finishing Coat with (1:1:1) cement: sand : lime .  Works include removal of all damaged and burnt existing plastering, transfer to approved dump site and all materials needed to finish the works according to specifications , drawings and supervisor engineer instructions.","M2",1200]
[6.2,"Supply and make external plastering 20mm thick to walls with 3 faces : the first is the rough nail rendering (mix 1:1) cement sand; the second is 5mm thick mortar (mix 1: 2)  cement: sand, the third is the undercoat 13mm (mix 1: 3 :0.25) cement:sand:lime all is according to specifications , drawings and supervisor engineer instructions.","M2",150]
[6.3,"Supply and make external plastering 20mm thick to walls with four faces : the first is the rough nail rendering (mix 1:1) cement sand; the second is 5mm thick mortar (mix 1: 2)  cement: sand, the third is the undercoat 13mm (mix 1: 3 :0.25) cement:sand:lime, the forth is two coats of Tyrolean finish ( mix 1: 3) white cement to fine aggregate (Quartiz) and all is according to specifications , drawings and supervisor engineer's instructions","M2",200]
[6.4,"Supply and make (Marmarina Finish) for external elevations to match the existing. The price includes scaffolding, removal all existing damaged finish layer, maintenance all existing plaster after removal existing finish layer, repairing cracks, preparing the surface to install the new layer, covering the windows by polytherene sheets, dismantle, refix and commission air conditioners, pipes, advertisement panels, galvanized metal lath, angle beads, plaster stops, Water Proofing Agent and any other required works to complete the job according to specifications, and engineer instruction.","M2",5000]
[6.5,"Supply and install terrazzo Marble chips floor tiles (grade A) size 30cmx30cmx3cm laid on 2cm mortar bed and 5 cm thick sand bed and terrazzo skirting 30cmx 7cmx1cm including all materials and testing  as per specifications, drawings, and the engineer's instructions.","M2",200]
[6.6,"Supply and install colored glazed non slipping Porcelain floor tiles high quality, (full body - Spanish made Class A or equivalent) size 40x40x1.00cm or 30x30x1cm to match the existing. The price includes decoration from several colors, skirting 40cmx7cmx10mm, dismantle and removal of the existing tile to approved dump site, pointing using special pre-mix grout, final polishing and all works according to specifications and engineer instructions.","M2",1000]
[6.7,"Supply and fix colored glazed Porcelain wall tiles,  high quality, (full body - Spanish made Class A or equivalent) size 40x40x1.00cm or 30x30x1cm to match the existing. The price includes removal of the existing paints and plaster, lime free key nail then plain plaster layers, decoration from several colors and pointing using special pre-mixed grout and soft wood (Swedish) crash rails size 80mm x 50mm with round edges to match the existing, smooth surface, apply one coat of sanding sealer, two coat of approved lazoure paint and one coat of lucker, drill and fix to concrete or block walls using expansion steel bolts as specifications and supervisor engineer instructions.","M2",300]
[6.8,"Supply and install non-slipping ceramic floor tiles high quality (Spanish made Class A or equivalent), size 20x20x0.60cm to match the existing for bath rooms, toilets and kitchens to match the existing, The price including dismantle and removal of old tiles to approved dump site, skirting 7cm height wherever no wall tiles required, pointing using special pre-mix grout and  final polishing as per specifications and supervisor engineer instructions.","M2",200]
[6.9,"Ditto but size 40x40x0.6cm","M2",50]
[6.1,"Supply and fix colored glazed ceramic wall tiles (Spanish made Class A or equivalent), size 20x30x0.60cm or 20x20x0.60cm to match the existing, the price includes dismantle and removal of the existing paints and plaster to approved dump site, lime free key nail then plain plaster layers and pointing using special pre-mixed grout a as specifications and supervisor engineer instructions.","M2",200]
[6.11,"Supply and install high quality Granite (Oruz,or Jakranda type), 60cm wide, 90cm height, 3cm thick, for top cover of buffet bench. The price includes local marble grade A 3cm thick for two direction supporting, back, shelves, Granite skirting, and all accessories, fitting and making holes for sinks, water and gas supplies, stainless steel water sink (Ariston type or equivalent), water mixers (Hamat Type or equivalent), floor trap, drainage pipes 2\" connected to the nearest manhole, water supply connections (20mm, 25mm Golani pipes inside sleeves (Sharshori)) from the nearest distribution box, Aluminum shelves doors (high quality, Jordanian type) for upper and lower shelves and any required to complete the job according to the specifications and engineer instructions.","L.M",20]
[6.12,"Supply and install local marble (grade A) 28cm wide x 3cm thick for windows sills laid on 2 cm thick mortar bed. The price includes dismantle and refix of the existing windows, removal of debris to approved dump site, any needed maintenance regarding plaster & paint around the windows (internal & external), polishing and grooving of the new sill as approved by engineer and as specifications.","L.M",150]
[6.13,"Supply and install Granit (Rozabeeta) for the coping of stairs, 3cm thick, not less than 15cm wide , the frames should be double with half cycle. The price includes fixation  with spits from stainless steel with 6-5 mm in diameter that are strengthened by way holes in the marbles and any required accessories to complete the job according to the specifications and engineer instructions.","L.M",50]
[6.14,"Supply and install Granit (Rozabeeta) for stair treads , 3cm thick and 35cm wide. The price includes remove the damaged and defected treads and remove all debris to approved dump site and any required accessories required to complete the job according to the specifications and engineer instructions.","M2",20]
[6.15,"Supply and install local marble (grade A) 3cm thick for door threshold laid on 2 cm thick mortar bed including polishing and grooving according to specifications, drawings and engineer instructions.","LM",20]
[6.16,"Supply and install Italian Karara marble size 23cm wide x 3cm thick for door thresholds laid on 2.5cm thick mortar bed according to specifications, drawings and engineer instructions.","LM",50]
[6.17,"Supply and install Cream Marvil marble tiles high quality with 2cm thick, 60x30cm to match the existing dimensions for walls, the price includes remove the damaged and defected parts and remove all debris to approved dump site, white cement mortar, decorations and any required accessories to complete the job according to specifications, drawings and engineer instructions.","M2",50]
[6.18,"Ditto but sheets 3cm thick around frame of the doors.","M2",20]
[6.19,"Ditto but 2cm thick of mosaic (travertine) tile around frame of elevator doors.","M2",20]
[6.2,"Supply and install high quality granite ( Raw Silk type) with 3cm thick for elevators walls, the price includes remove the damaged and defected parts and remove all debris to approved dump site, white cement mortar, decorations and any required accessories to complete the job according to specifications, drawings and engineer instructions.","M2",30]
[6.21,"Supply and install Berlato marble 3cm thick for window sills laid on 2 cm thick mortar bed. The price includes dismantle and refix of the existing windows, remove the damaged and defected parts and remove all debris to approved dump site, any needed maintenance regarding plaster & paint around the windows (internal & external), polishing and grooving of the new sill as approved by engineer and as specifications.","M2",15]
[6.22,"Supply and lay precast terrazzo stair treads size 36 cm wide x 5cm thick chamfered once, rebated once and laid on 2cm thick mortar bed same color and kind of the floor tiles and the price includes terrazzo stair risers size 10.36cm high x2cm thick laid and skirting 7/20cm high x2cm thick as per specifications, drawings and the engineer‘s instructions.","L.M",20]
[6.23,"Reinstall, the fire clay roof tiles(Bricks), that were dismantled from Floor W300, in the entrance of building A100, the price includes reinstall wood trusses, and joints, and elements or accessories needed to complete the work. Roofing tiles should be fixed according to the required slopes and proper fixation at slope variation places with all insulation and protection elements. Supply and install special insulation sheets for ceiling covering with all required materials to prevent water leakage to the wood. The price includes approved lazour paints, the installation of electrical connections  according to the specifications, drawings, and the instruction of the engineer. Supply and install water drainage system including all required fittings and pipes of galvanized steel (1.5 mm min. thick.) including all 3 inch galvanized steel pipes of 3.2mm thick. all according to the instructions of the supervisor engineer. The price include replacement of any defected elements and supplying all missing parts (bricks, wood,..etc..), and a complete ceiling from approved wood (alent faider) 10 cm * 1cm includes painting as required by the engineer. .The contractor must approve all wooden sections before any installation and/or fixing process. Measuring will be according to the horizontal area, and the contractor should submit a shop drawing before starting the works.","M2",80]
[6.24,"Supply and fix fire rated gypsum boards one side for ceiling including suspension system. The price includes any decoration shape, dismantle and remove the existing defected parts, hot galvanized metal studs standing each 50cm frame \"C\" section in two direction, angles..etc.... (each 60*40cm for both sides), 1.5mm thick steel channels, bolts, screws,  including one undercoat primer, putty, two coats of Supercryle, all works according to specification, drawings and engineer instructions","M2",600]
[6.25," Supply and install European gypsum board false ceiling of 60*60cm manufactured by Armstrong Prima-Dune or equivalent ,with exposed suspension system manufactured by Raysound including galvanized steel hanger wire, hold down clip, wall molding, main and cross bar. The suspension parts will be selected by the Engineer. The works shall include the Gypsum border to close the sides according to specification and engineer instructions.","M2",1500]
[6.26,"Supply and install decorated polystyrene ceiling tiles for false ceiling of 60*60cm (to match the existing) manufactured by Armstrong Prima-Dune or approved equivalent. The price includes complete maintenance for the suspension system including replacement of any defected hot galvanized steel hanger wire, hold down clip, wall molding, main and cross bar according to engineer approval.\nThe contractor must visit the site before pricing \nMeasurement according to supplied panels.","M2",600]
[6.27,"Supply and fix fire rated gypsum boards for the partitions (two sides) with thickness of 12cm, The price includes hot galvanized metal studs standing frame \"C\" section in two direction, angles..etc... (each 60*60cm for both sides), 1.5mm thick steel channels, bolts, screws, 7 cm PVC skirting, including putty, two coats of Supercryle and tambortexs one undercoat primer and two coat of oil paint, all electrical works and materials needed, all according to specification, drawings and engineer instructions.","M2",400]
[6.28,"Supply and install  decoration Gypsum board ceiling (Suspension system) in A700 to match the existing adjacent computer lab , The price includes hot galvanized metal studs standing frame (each 60*60cm for both sides), bolts, screws, hot galvanized  supports, \"C\" section, angles..etc., and putty and two coats of emulsion  paints, the ceiling will be in shapes with different levels, as shown in drawing, described to be approved by the engineer . ","M2",80]
[6.29,"Supply and install of double wall cladding fire rated gypsum boards. The price includes fixing insulation polystyrene layer 5cm thick under gypsum board, all electrical works and materials needed to match the existing, dismantling and refixing the existing window and any needed materials to prevent any water leakage, local marble under the window, hot galvanized metal studs standing frame \"C\" section in two direction, angles..etc.... (each 60*60cm for both sides), 1.5mm thick steel channels, bolts, screws, remove the existing skirting to approved dump site, 7 cm PVC skirting, including putty, two coats of Supercryle and tambortexs one undercoat primer and two coat of oil paint, all electrical works and materials needed, all works according to specification, drawings and engineer instructions.","M2",80]
[6.3,"Supply and install of wall cladding  plywood, 17mm thick, covered of beech veneer (Zan) to match the existing, the price includes dismantle and remove the defected parts of the existing, aluminum and stainless separator, decorations, applying one coat of sanding sealer, two coat of approved lazoure paint and one coat of lucker and  required accessories and materials to complete the job as per specification, drawings and engineer instructions. ","M2",320]
[6.31,"Supply and install counter for the platform in the main hall of hardwood (Zan) with clear glass 4mm as described in the details per specifications, drawings and engineer instructions. \n\n","LM",8,null,null," سيتم اضافة التفاصيل في الاجتماع التمهيدي أو قبلها من طرف الجامعة"]
[6.32,"Supply and install gypsum frame cornice 10cm wide in shapes from two sides as to be approved by the engineer. The price includes putty and two coats of acrylic paint (Supercryle), smoothing and required accessories according to specifications,  and engineer instructions. ","L.M",400]
[6.33,"Ditto but 5 cm wide.","L.M",400]
[6.34,"Ditto but 3 cm wide.","L.M",1100]
["6.35","Supply and install high quality moquette  6 mm thick, 1.8kg/m2 (Super lugo or equivalent), the price includes removal of old moqutte and handling to the university upper Aluminum angles for upper steps edges 30*30*1.25mm, stainless steel rod 14mm for lower edge, skirting, sticking materials, cleaning and preparation the surface to install the moquette according to specifications and engineer instructions.","m2",1300]
[6.36,"Supply and installation of counter service of industrial marble type (Corian) with width of 80 cm of defined colors,  The price includes local marble grade A 3cm thick for two direction supporting,  aluminum columns with rounded edges on top of Corian each 1m with glass 6mm fixed between columns, and all needed accessories, per drawings and engineer instructions.","L M",18]
[6.37,"Supply and install aluminum and fiber curtains (Type Sun Strip Blinds or Zebra Blinds or equivalent), the price includes the upper rail 4cm Dia. of hot galvanized steel hidden inside aluminum rectangular section box 9*3.5cm, lower part of 1.2cm Dia. hot galvanized circular section and any required accessories and materials to complete the job as per specifications and engineer instructions. ","M2",90]
[6.38,"Supply and install of high quality Blackout  curtains (colored cloth) on original rail, Turkish or equivalent height 270 cm the price includes galvanized corrugated steel pipes 1\" diam. and 1 mm thick. , covered with colored plc. coater, rings of copp loops.  6 loops/meter, tiebacks of the same type of the curtains' fabric and all accessories and materials required to complete the job according to specification, and engineer instructions.\nNote: Measurement per pipe length.","LM",250]
[6.39,"Ditto but for 220cm height cloth curtain (water proof) Turkish or equivalent.","LM",120]
[6.4,"Supply and install of high quality strip curtains ( sun strip or equivalent) height 270 cm the price includes supply and install  steel pipes 1 \" diam. and 1 mm thick. , covered with colored plc. coater, rings of copp loops.  6 loops/meter , tiebacks of the same type of the curtains' fabric and all accessories and materials required to complete the job according to specification, and engineer instructions.","M2",500]
[6.41,"Supply and install wooden curtains, with slices of 50mm wide, 3mm thick, upper cover of hot galvanized steel sheet painted with special paints with size of 5.5*5cm, lower slice of decorated wood 17mm, the price includes required rails, horizontal and vertical control wires accessories and materials to complete the job as per specifications and engineer instructions.","m2",80]
["Total"]
["Bill No (A) - 7. Painting works"]
[null,"Rates for painting and decorating work shall include for:     \n1-Prices of painting works  (European Type of good quality) shall include supply of all materials, scaffolds, workmanship & tools and anywhere else, needed, all according to drawings, specifications, conditions and directed instructions by the Engineer or his representative.            \n2. Preparation of surface including puttying, sealing and priming,\n3. Any area or width,\n4. Any location,\n5. Work in multi colors,\n6. Cutting in edges,\n7. Any taping and covering to protect areas and others.        \n 8-Price of painting shall include removing the old paint if needed and plaster repairing, testing, Treatment of cracks including cleaning, rubbing, open, filling with Sikaflex, closing openings,  plaster maintenance within 20*20 cm.\nAll the painting materials should be approved and tested by approved local laboratory."]
[7.1,"Supply & paint  two coats of  internal water proof colored emulsion paint (Supercryle) .The works include removing the old paint and plaster repairing, testing, treatment of cracks including cleaning, rubbing, open, filling with Sikaflex, closing openings, repairing damaged plaster up to 20x20cm and cleaning the surface  as specification and drawings.  ","M2",3000]
[7.2,"Supply and paint the internal walls with one priming coat and two finishing coats with one coat of Tambourtex between them applied with roll, the price includes the final coat of oil paints, two coats of complete putty. The price includes removing old paints by fire, plaster repairing, testing, Treatment of cracks including cleaning, rubbing, open, filling with Sikaflex, closing openings, repairing damaged plaster up to 20x20cm and cleaning the surface  as specification and engineer instructions.  ","M2",5000]
[7.3,"Supply and paint the internal walls with two coats of putty, one undercoat primer and two coats of colored oil paint . The price includes removing old paints by fire, plaster repairing, testing, Treatment of cracks including cleaning, rubbing, open, filling with Sikaflex, closing openings, repairing damaged plaster up to 20x20cm and cleaning the surface  as specification and engineer instructions.  ","M2",3000]
[7.4,"Supply and paint the internal walls and ceilings (Gypsum)with two coats of putty, one undercoat primer and two coats of  internal water proof colored emulsion paint (Supercryle). The price includes , testing, Treatment of cracks including cleaning,  closing openings, complete maintenance for the  existing Gypsum board, sand cleaning the surface  as specification and engineer instructions.  ","M2",5000]
["Total"]
["Bill No (A) 8.Mechanical Works"]
[null," (1)In general rates for plumbing works shall include for:                 \n1. Developing shop and as built drawings\n2. Cutting and forming all chases, recesses, holes, and the like,\n3. Pipe sleeves,\n4. Building of concrete and/or brick ducts in floors, walls …etc.,\n5. Excavation, forming of trenches for services, concreting, bedding and back filling and ramming after laying,\n6. Fixing brackets, clips, holder bats, hangers, and the like,\n7. Temporary and final fixing, \n8. Nails, screws, bolts, nuts, washers, holes, plugs, sleeves and the like,\n9. Building in or cutting and pinning,\n10. Testing and drawings, \n11. Painting of pipes, \n12. All work of other trades in connection with plumbing work including all making good."]
[null,"(2) Rates for manholes and pits shall include excavation, concrete, benching, plastering, backfilling and cover as per Drawings and Specifications,"]
[null,"(3)  Rates for sanitary fittings, isolated taps and gullies shall also include all pipe work in connection therewith and connections thereto including connection to the nearest manhole or gully and to the cold water storage tank."]
[null,"(4)  Rates for pipe work including pipe work in frames to shading sheds shall include for:                                                              \n1. Joints in the running length, \n2. Nipples, connections, sockets, ferrules, couplings, back nuts, unions, and the like,\n3. Bends, elbows, tees, reducers, access doors, cleaning eyes, blank caps, stop valves, and the like,\n4. Welded joints and connections including grinding,\n5. Lagging and wrapping,\n6. Excavation, bedding and backfilling."]
[8.1,"Supply and fix white glazed fireclay oriental W.C suite (Vitra type - grade A ) to replace the existing  complete with heavy duty cover, 9 liter plastic double action flushing cistern (Plason or equivalent) and fixed chromium plated tap 1/2” Tibesa type or equivalent, including all water supply   pipes 16mm(Golany) to the nearest dist. box (DB), flushing hose sprayer, angle valves, UPVC drainage pipe connecting to the nearest manhole or sewage header and remove the existing to approved dump site as per specifications and supervisor engineer instructions.","NO",4]
[8.1999999999999993,"Supply and fix white glazed fireclay European W.C. suite (Vitra type - grade A ) to replace the existing (oriental W.C) complete with heavy duty cover, 9 liter plastic double action flushing cistern (Plason or equivalent) and fixed chromium plated tap 1/2” Tibesa type or equivalent, including all water supply   pipes 16mm(Golany) to the nearest dist. box (DB), flushing hose sprayer, angle valves, UPVC drainage pipe connecting to the nearest manhole or sewage header and remove the existing to approved dump site as per specifications and supervisor engineer instructions.","NO",12]
[8.3000000000000007,"Supply, install, test and commission hand wash basin (60x42cm)  Vitra or equivalent, first class with half pedestal, completed with chrome plated mixer (hamate type or equivalent), bottle trap, soap tray, chrome plated angle valves, flexible tubes, floor drain (15x15),wall fixed mirror size(60x40) and all accessories, supports and hangers upon completing the works as per specification and engineering instruction..","No",10]
[8.4,"Supply and fix white glazed fire clay hand wash basin size 52cm x45cm (Vitra type - grade A ) or equivalent, complete with all water supply pipes 16mm (Golany) to the nearest distribution box (DB), waste fitting, trap, plug and chain, long chromium water Mixer ( Hamat type or equivalent), and the drainage line 2” to the nearest floor trap and all connections and accessories as per specifications and supervisor engineer instructions.","No.",5]
[8.5,"Supply and install plastic double action flushing cistern (Plason or equivalent) including required maintenance for water supply and drainage network and supplying any required materials (16mm Golany, 2\" pipes, 3\" pipes,4\" pipes..), flushing hose sprayer and all connections and accessories as per specifications and supervisor engineer instructions.","No.",20]
[8.6,"Maintenance for W.C , including replacement of defected heavy duty cover, plastic double action flushing cistern, and fixed chromium plated tap 1/2”,roll holder, including all water supply pipes ½\", flushing mechanism, chrome plated angle valves, hand spray with flexible chrome connection, 4” diam PVC drainage pipe to the nearest manhole as specification and engineer instructions. \n","NO",20]
[8.6999999999999993,"Supply and install hand wash basin set. The price includes high quality Marble (KRARA), 240*60cm, 2cm thick, local marble partition, 3cm thick,  No. of   3 hand wash basins (Vitra type or equivalent), 3 water mixers (Hamat Type or equivalent), No. of 3 mirrors 60*60cm, floor trap, drainage pipes 2\" connected to the nearest manhole, water supply connections (20mm, 25mm Golani pipes inside sleeves (Sharshori)) from the nearest distribution box (central building, behind Bisan building, stainless steel angels to fix mirrors and all connections and accessories as per specifications and supervisor engineer instructions.","No.",7]
[8.8000000000000007,"Supply and install high quality Mirror for the walls 6mm thick(Belgian made or equivalent). The price includes stainless steel angels for edges, and any required accessories to complete the work according to specifications and engineer instructions","M2",50]
[8.9,"Supply and fix floor trap 4inch diameter, complete with heavy duty brass grating (stainless steel cover), 4”& 2” PVC drainage pipe to the nearest manhole or next F.T and including removal of the existing to approved dump site as per specifications and supervisor engineer instructions.\n","NO",60]
[8.1,"Ditto but for maintenance for the existing floor trap 4inch diameter. The price includes supply and install heavy duty brass grating (stainless steel cover), 4”& 2” PVC drainage pipe to the nearest manhole or next F.T and including removal of the existing to approved dump site as per specifications and supervisor engineer instructions..","No",15]
[8.11,"Supply and install chrome plated mixer (hamate type or equivalent)  the price includes dismantle the existing defected water Mixer, required maintenance for water supply and drainage network and supplying any required materials (16mm Golany, 2\" pipes, 3\" pipes,4\" pipes..) and all connections and accessories as per specifications and supervisor engineer instructions.","NO",30]
[8.1199999999999992,"Maintenance for the existing water mixer. the price includes supply and replace any defected part of the existing water mixer, required maintenance for water supply and drainage network and supplying any required materials (16mm Golany, 2\" pipes, 3\" pipes,4\" pipes..) and all connections and accessories as per specifications and supervisor engineer instructions.","NO",50]
[8.1300000000000008,"Supply and install chrome plated mixer (Tebesa type or equivalent)  the price includes dismantle the existing defected water Mixer, required maintenance for water supply and drainage network and supplying any required materials (16mm Golany, 2\" pipes, 3\" pipes,4\" pipes..) and all connections and accessories as per specifications and supervisor engineer instructions.","NO",10]
[8.14,"Supply, install, test and commission one bowel stainless steel kitchen sink 50x85 cm, 2.2mm thick Foster type or equivalent complete with chrome plated hot and cold water mixer (hamate type or equivalent), Φ16mm chrome plated flexible water connections,Φ16mm chrome plated angle valves, Φ75mm, workmanship and all necessary fixing, accessories, waste pipes Φ50mm and drainage to the nearest floor trap with all required works as specification and engineer instructions. ","No.",4]
["8.15","Supply and install 160 mm  diameter UPVC Pipes with wall thickness 4.7 mm to replace the existing, the price includes  fixation in the walls, floors including all connections, tees, bends, fittings, and  4\" UPVC vent for upper end of pipes. The price includes scaffolding and removal of existing ones to approved dump site, all as per specifications, drawings and supervisor engineer instructions. ","L.M",40]
["8.16","Ditto but for 4'' UPVC SN8.","LM",50]
["8.17","Ditto but for 3'' PVC .","LM",50]
[8.18,"Supply, install, test and commission galvanized steel pipes diameter 2\" (SCHEDULE 40) complete with all  fittings (valves,elbows,tees,couplings etc..), fixing on walles or under ground, supports and disinfect water supply system and all  necessary works as shown on drawings and as per specifications and engineering instructions .","L M",30]
[8.19,"Ditto but 1.5\"","L M",30]
[8.1999999999999993,"Ditto but 1\"","L M",250]
[8.2100000000000009,"Ditto but 3/4\"","L M",100]
[8.2200000000000006,"Ditto but 1/2\"","L M",120]
[8.23,"Supply, install, test and commission, cold & hot water distribution box (size 80*60 cm) made of local marble  with aluminum door, price shall include all required and necessary 1\"copper manifolds, cold & hot water pex pipes complete with flexible sleeves (sharbool), with gate valve (Sagiv or equivalent) on each branch pipe, automatic air vents, main gate valves, pressure reducing valves as per specifications and engineer instructions.","No",5]
[8.24,"Supply, install, test and commission  gate valve of diameter 2\" Sagiv or equivalent with supports and all  necessary works as shown on drawings and as per specifications and engineering instructions. ","No",5]
[8.25,"Ditto but 1.5\"","No",5]
[8.26,"Ditto but 1\"","No",5]
[8.27,"Ditto but 3/4\"","No",5]
[8.2799999999999994,"Ditto but 1/2\"","No",5]
[8.2899999999999991,"Supply, install, test and commission  water heater Ariston type or equivalent capacity 60 liters including, valves, check valve, flexible connection,  supports and all  necessary accessories as shown on drawings and as per specifications and engineering instructions.","No",8]
[8.3000000000000007,"Supply, install, and test fire hose reel cabinets, wall recessed composed of 25m length 25mm rubber hose, angle globe valve, a jet nozzle with an incorporated cock, a compartment including 2\" landing valve, connection to existing network and all required accessories to complete the job according to specifications, and engineers' instructions.","No",15]
[8.31,"Supply and install double flanged ends ¾” for fire hydrant. The price shall includes supply and install any required fittings, valve, testing and any required accessories according to specifications, and engineer instructions.","No",2]
[8.32,"Extension of the existing gas pipeline Italian quality diameter 8 mm coated with a layer of plastic, price include Installation of valve at the end of the line and work to include all installations, including sleeve pipe diameter of 3/4 inch inside floor and all accessories needed.","L M",70]
[8.33,"Supply and installation of gas pipelines feeding pipes of galvanized steel Scodiom (SCHEDULE 40) diameter 0.5\" and accessories of elbows and  so on and prices include drilling, burial and cracking in the walls and testing the work after completion of the work and what it takes to complete the work to the fullest. Work also includes the fixing of the pipes with appropriate  (HANGERS) with suitable dimensions and distances  price include Installation of valve at the end of the line and work to include all installations, including sleeve pipe diameter of 3/4 inch inside floor and all accessories needed. according to the specifications, drawings and instructions of the supervising engineer.","L M",20]
[8.34,"Supply and fix fire extinguisher, 6kg capacity filled with CO2, fixed at 2m height.  According to, specification, drawings and as per Palestinian fire defiance requirements. ","No",5]
[8.35,"Ditto but filled with powder.","No",5]
[8.36,"Supply, install and join, 200mm UPVC pipes SN8 for the sewer networks with watertight and flexible joints sealed with approved gasket rubber ring including\ndewatering, excavation in any ground, shoring, shuttering, safety measures, testing, providing specified bedded and covered by 20 cm of clean dune sand at the bottom, above and around the pipes. Kurkar will be used for the rest of trench with layers not exceeding 20cm, of 98 % MDD, leveling the road after backfilling dismantling & reinstall for interlock if needed. All in accordance with the drawings, specifications and Engineer’s instruction","LM",20]
[8.3699999999999992,"Supply, install and operation of water pump  Duty/Stand by, on the existing system, each pump is  10m3 / h pressure (45m) outlet diameter 2 \", to be installed next to the water pool in college to deliver water from pond to the top of the new building , price include dismantling of the old pumps and deliver them to the university store and work covers all fittings and valves and expansion tank.  \nAnd Control Panel complete with main and sub-circuit breakers, contactors, under voltage Relays, overloads, timers, indication lambs, bus bars, fuses, 2  Ammeter, horn alarm, Voltmeter  with selector switch, ON / OFF push buttons, Auto manual selector switch, the work includes all necessary power and control cables from pump to control panel to complete and operate the system efficiently and according to the instructions of the supervising engineer. ","NO",2]
[8.3800000000000008,"Supply and install galvanized protection steel box with thickness of 1.5mm for water valves ,the price include galvanized steel angels 40*40*3mm, hinges, lock, ironmongeries, and all required accessories to complete the work according to engineer instructions.","NO",1]
["Total",{"$nulls":4},{"$f":"SUM(F203:F240)","v":0}]
["Bill No (A) 9. Electrical works"]
[null,"General:\n*The items in general shall also include conduits, connection boxes, controls, wires, connectors, clamps, bolts, and connecting the cables to switchboards and common electric network are included in the unit price.\n*Complete detailed shop drawings should be delivered to the Engineer to take his approval prior the commencement of work. Samples of all materials shall also be delivered to the Engineer to take his approval,\n* As-built drawings shall be submitted after handing over the work.\n* All the electrical works shall be executed according to Standards, drawings, specifications and supervisor engineer instructions.\n* Dismantling &Removing old lighting unit (fluorescent light fixture, glops, ….. Etc ) and move to school stores as per engineer instructions."]
[null,"The prices of all Electrical works listed below include:\n• Execution of the works include all fittings and accessories required for installing and operation.\n• All materials are supplied (such as wires, pipes, electrical equipment … etc )   should be of excellent quality and approved by the supervising engineer.\n• The work includes maintenance period for each device according to tradition in the field.\n• Oversees the installation and maintenance, a specialist in the field of devices.\n• Provide a guarantee for electrical equipment of duration according to tradition in the field.\n• Contractor shall submit shop drawings for all electrical works to be approved by the Engineer before executing the work.\n• As-built drawings shall be submitted after handing over the work.\n• Contractor is not allowed to dismantling any electrical installations or connections without supervising engineer permission."]
[null,"LIGHTINGS WORKS"]
["9.1","Supply, install connect and operate surface mounted LED lighting fixture 32W or 36W, European made. Model Fortan LED  # 386671 or equivalent (Type is LENA or equivalent).\nThe item includes PVC conduits, J.boxes, fixing screws (Galv.) and wiring and all necessary equipment for installation and operation as per drawings, specifications and engineer instructions.","NO",100]
["9.2","Ditto but 1x16 w or 18w with special reflector for black board . Model Specto LED # 343858 or equivalent (Type is LENA or equivalent).","NO",10]
["9.3","Supply, install connect and operate 3W/ 2\" Led Spot Light .\n European made ,Model # LP-COB03For equivalent (Type is LIPER or equivalent).\nThe item includes ballast, wires, PVC pipes ,boxes and all necessary equipment for installation and operation as per drawings, specifications and engineer instructions.","NO",60]
["9.4","Supply, install connect and operate 30W Square Led Downlight, Suitable to false ceiling and gypsum tiling \n(Type is LIPER or equivalent).For A100 &A700 floors.\nThe item includes ballast, wires, PVC pipes ,boxes and all necessary equipment for installation and operation as per drawings, specifications and engineer instructions.","NO",90]
["9.5","Supply, install connect and operate 4*20W Square Adjustable Down Lighter, Suitable to false ceiling and gypsum board(Type is GAASH #5R3B40 or equivalent).For A700.\nThe item includes ballast, wires, PVC pipes ,boxes and all necessary equipment for installation and operation as per drawings, specifications and engineer instructions.","NO",4]
["9.6","Supply, install connect and operate 20W/ 6\" Circular Led Downlight, Suitable to false ceiling and gypsum board Model # LPDL-20A-Y (Type is LIPER or equivalent).\nThe item includes ballast, wires, PVC pipes ,boxes and all necessary equipment for installation and operation as per drawings, specifications and engineer instructions.","NO",24]
["9.7","Supply, install connect and operate Led lighting fixture 36W , (60*60 CM) European made. Model PLANO LED  # 313979 or equivalent (Type is LENA or equivalent).\nThe item includes PVC conduits, J.boxes, fixing screws (Galv.) and wiring and all necessary equipment for installation and operation as per drawings, specifications and engineer instructions.","No",105]
["9.8","Supply, install connect and operate Circular Surface mounted Globe with Led lamp 16 W OSRAM made (Type is GA'ASH No. 552100 or equivalent)\nThe item includes all necessary equipment for installation and operation as per drawings, specifications and engineer instructions.","No",15]
["9.9","Supply, install connect and operate Emergency LED lighting fixture 2w, 180 minutes duration Surface or wall mounted with  lamps and self adhesive original sticker - according to the direction of flow- with  legend complete with all necessary wiring and accessories.\n(Type is LENA or equivalent)","No",2]
["Total"]
[null,"LIGHTING SWITCHES AND OUTLETS WORKS"]
["9.10","Supply, install connect and operate Single pole one way internal switch, 220v, 10A, complete with PVC conduits, J.boxes, wiring, cover and all necessary accessories. \n(Type is  BTICINO MATIX or equivalent).","No",15]
["9.11","Ditto  as 10 but without wire, only replacement of the old one complete with base & cover","No",25]
["9.12","Ditto as (10) but water proof type.","No",5]
["9.13","Ditto, as (10) but one way, two pole switch","No",15]
["9.14","Ditto  as (13) but without wire, only replacement of the old one complete with base & cover","No",25]
["9.15","ditto , as (13) but water proof two pole.","No",5]
["9.16","Ditto, as (10) but one way, three pole switch","No",8]
["9.17","Ditto  as (16) but without wire, only replacement of the old one complete with base & cover  ","No",10]
["9.18","Ditto, as (10) but two way switch, two poles.","No",10]
["9.19","Ditto as (10), but push button with illuminated lamp required for stair case lighting fixtures, the item includes one stair case timer.","No",8]
["9.20","Supply, install connect and operate Electrical Heater Switch 230V, 20A, with pilot lamp, with water Proof cover.\n(Type is BTICINO MATIX or equivalent)","No",3]
["9.21","Supply, install connect and operate Single internal socket outlet 16A, 220v, 2p+E for flush, wall, or surface mounted , complete with PVC conduits, J.boxes, wiring, and all necessary accessories. (Type is BTICINO MATIX  or equivalent).","No.",50]
["9.22","Ditto  as (21) but without wire, only replacement of the old one complete with base & cover   ","No.",20]
["9.23","Ditto as item (21) but double internal socket outlets","No.",20]
["9.24","Ditto as item (21) but water and dust proof","No.",5]
["9.25","Ditto as item (21) but 20A AC Switched Outlet with 4 mm2 wires.","No.",10]
["9.26","Supply, install connect and operate Ceiling Fan CHMC made 120cm diameter or equivalent\nThe item includes switch and all necessary equipment for installation and operation as per drawings, specifications and engineer instructions.","No.",20]
["9.27","Supply, install connect and operate 6\" Extract Fan VENTA made or equivalent\nThe item includes external cover with louver of galvanized steel painted with suitable color to external elevation of the building size of 40x40 cm and all necessary equipment for installation and operation as per drawings, specifications and engineer instructions.","No.",6]
["Total"]
[null,"Telephone,satalite , and Computer"]
["9.28","Supply, install and connect wall mounted telephone socket outlet 6 pin complete with PVC conduits, J.boxes, 2 pairs cable (Teldor) from the location of telephone socket to sub-telephone box or telephone exchanger in the same socket's floor, and all necessary accessories (Type is BTICINO MATIX original   or equivalent). ","No.",55]
["9.29","Supply, install and connect internal  complete computer sockets (single) with RJ45 cat 6 female connectors, cover, Original Italian GEWISS (RJ45 Data Socket Cat6  (Product Code: GW20684)), connect it to the patch panel in Rack with U/FTP Teldor cables cat 6 as shown in the network drawings, all sockets must be tested and labeled(cables, sockets).(cable must has one meter extra length inside the Rack)","No.",75]
["9.30","Supply, install and connect IDF/MDF  Rack  : - 8U Rack ,depth  50 cm , with removable sides  including the following :\n fan, rack mounted power distributer , 24 port patch panel with female RJ45 cat 6 connector type 3M original, 24 port switch Cisco WS-C2960S-24TS-S  , with Lan Base Image  , 24 x patch cable 30cm  cat 6 original , 1x UPS 700 va rackmount, cat 6 FTP cable from the main rack to the new rack at the roof APC Smart.","No.",2]
["9.31","Supply, install and connect IDF/MDF  Rack  : - 10U Rack  , with removable sides  including the following :\n- 2 fan, rack mounted power distributer\n- 2 panels of 24 port patch panel with female RJ45 cat 6 connector type 3M original.\n- 2 switch 24 port Cisco WS-C2960S-24TS-S switch , with Lan Base Image including 48 x patch cable 30cm  cat 6 original .\n-  1x UPS 700 va rackmount, cat 6 FTP cable from the main rack to the new rack at the roof APC Smart.","No.",1]
["9.32","Supply, install and connect Sub-telephone boxes (GEWISS # PT48)  complete with all connection strips, termination and all necessary accessories \n","No.",3]
["Total"]
[null,"CABLES"]
[null,"Supply, install and connect of the following cables with all required electrical PVC pipes and civil works, the item includes dismantling and re install the existing cables and laying under ground PVC piping system, manholes, excavation, warning tapes, backfilling and all required civil works to finish the work according  specifications and demands of the supervising engineer,  to connect cables terminals from source to destination. According to drawings, specifications, instructions, and demands of the supervising engineer. as follow:"]
["9.33","  N2XY-XLPE cable 5*16 mm2","M.R",80]
["9.34","  N2XY-XLPE cable 5*10 mm2","M.R",60]
["9.35","Supply, install and connect Telephone Cable (J-Y (ST) Y (1G 20*2*0.6)) Teldor cable. The item includes 2\" PVC pipe and all necessary equipment for installation and operation as per drawings, specifications and engineer instructions.","M.R",80]
["9.36","Supply, install and connect Telephone Cable (J-Y (ST) Y (1G 40*2*0.6)) Teldor cable. The item includes 2\" PVC pipe and all necessary equipment for installation and operation as per drawings, specifications and engineer instructions.","M.R",80]
["Total"]
[null,"FIRE ALARM , Sound System , CCTV"]
["9.37","Supply, install and connect Addressable Smoke Detector type MORLEY-IAS Model # MI-PSE or equivalent\nThe item includes all necessary equipment for installation and operation as per drawings, specifications and engineer instructions.","No.",30]
["9.38","Ditto  but heat detector.","No.",7]
["9.39","Supply, install  break glass call point as per drawings the unit shall be standard type for interior use with key operated test facility, with plastic coated glass and one spare coated glasses.","No.",6]
["9.40","Supply, install 95 db electronic horn ultra sound for indoor used. ","No.",5]
["9.41","Removing and Supply, install and connect ceiling mounted loud speaker 150 mm Diam.  with nominal max. power of 4/6W including all required cables (2,5 mm2) , junction boxes conduits and,  metal front protection mesh,  clips for quick attachment , line transformer all necessary accessories (Type is Bosch,Cotina or equivalent)","No.",30]
["9.42","Supply, install and connect PVC pipes and boxes for CCTV SYSTEM Networks in the Halls (A700, W600, A100). \nThe item includes all necessary electrical and civil works and equipment for installation and operation as per drawings, specifications and engineer instructions.","L.S",1]
["9.43","Supply, install and connect wall and Ceil mounted female VGA sockets  that include VGA  cable  (0,8 mm) between two VGA connectors, and double male VGA  audio connectors 2 meters (each) to connect from computer to wall mounted VGA socket and from VGA Audio socket to LCD.","No.",15]
["Total"]
[null," POWER SYSTEM AND ELECTRICAL BOARDS WORKS"]
["9.44","Supply and install electrical switch board of size 80x60x25cm one door, the frame work is made of galvanized steel sheets 2mm  thickness, painted by antistatic and insulation paint. The item includes busbars, wiring, insulations, plastic ducts, terminal blocks and all necessary equipment and civil works for installation and operation as per drawings, specifications and engineer instructions  (Type is MOELLER or equivalent) ","No",2]
["9.45","Ditto but size 60x40x20cm","No",2]
["9.46","Supply , install and connect MCB 4*63A MOELLER made # FAZ-C63/4","No",2]
["9.47","Ditto but MCB 3*32A MOELLER made # FAZ-C32/3","No",2]
["9.48","Ditto but MCB 3*40A MOELLER made # FAZ-C40/3","No",2]
["9.49","Ditto but MCB 3*25A MOELLER made # FAZ-C25/3","No",2]
["9.50","Ditto but ELCB 4*40A MOELLER made # FIM-40/4/0.03-A","No",5]
["9.51","Ditto but MCB 1*16A MOELLER made # FAZ-C16/1","No",20]
["9.52","Ditto but MCB 1*20A MOELLER made # FAZ-C20/1","No",5]
["9.53","Ditto but MCB 1*10A MOELLER made # FAZ-C10/1","No",20]
["Total"]
[null,"PV SOLAR SYSTEM COMPONENTS"]
[null,"General:\n* The system is designed to cover the lighting loads in the Fourth floor of the Administration Building in Islamic University . The system will be of grid system, which will allow for many power sources options.\n* Contractor shall submit shop drawings of all electrical ,civil and solar photovoltaic complete system works, including a single line diagram showing all the components of the PV system, DC and AC distribution boards, PV panels lay out and backup systems and wires cross section for all the system to be approved by the Engineer before executing the work. As well as the catalogs of each component showing the requested specifications stated at the bill of quantity.\n* As-built drawings shall be submitted after handing over the work.\n"]
[null,"*  The items include Dismantling &Removing old damaged components such (PV solar panels, Batteries , wires , structure , ….. Etc ) and move to University store as per engineer instructions.\n*   Upon completion of the installation and connections, the contractor shall finish all commissioning works and operate and programing the existing system with the new installed components to be compatible to the existing loads\nThe contractor shall organize an on site training program involving nominated employer's staff. Such a program shall be carried out during the commissioning phase. The cost of the training shall be deemed to have been included in the tendered rates.\nmake all commissioning works ond operate the existing system with the new installed components to be compatible to the designed loads"]
["9.54","PV Modules – 6 KWp:","Module",18]
[null,"Supply, install, connect and operate Mono Crystalline Photovoltaic Solar Modules with all mounting structure and other material needed to have complete job ready for installing high quality PV modules with total arrays capacity  6 KWp. (Type is Canadian Solar  or equivalent), the Item Includes supply, install &connect the following: "]
[null,"• Water proof PV junction boxes IP65(combiner) for each array including DC Fuses, DC switch disconnectors, bus bars ,terminals, ducts, supports &labels suitable to the PV arrays loads."]
[null,"• Solar DC cables appropriately sized to connect the PV solar cells together and to the J.B and from J.B to the inverter to have a complete operational circuit with all conduits, clamps , trays and cable end terminations  which shall be DC plug and socket connectors ."]
[null,"The DC cables must be sized in accordance with the installation requirements applicable on site, the allowable voltage drop for DC cables between PV Arrays and inverter less than 3%."]
[null,"• 25 mm2 flexible copper cable from the structure to the electrode."]
[null,"• Panels numbers based on 320 Wp for each solar panel."]
[null,"The contractor should provide certified panel characteristics, test certificates performance , spare parts regular (as recommended by manufacturer), maintenance catalogues and manufacturers warrantee for each solar panel for a period not less than 20 years."]
[null,"The items include Dismantling &Removing old damaged components such (PV solar panels, wires , structure , ….. Etc ) and move to University store as per engineer instructions."]
[null,"All works and materials must be according to the drawings, specifications and supervisor engineer instruction’s and approval. "]
["9.55","Battery Banks:","Module",15]
[null,"Supply, install, connect and operate (OPZv) or (AGM) deep cycle Batteries with a 12-volt dc, the total capacity of battery bank must include 60 % DOD @ C10. The battery bank voltage is 48 Vdc. The works includes removing old batteries with all connections."]
[null,"Type is (SUNLIGHT or equivalent).The battery must provide high-quality and achieving superior performance, the manufacturing date must be new and not more than 6 months, suitable for every type of applications specially for solar renewable energy, designed Service Life 10 years with low internal resistance, designed to be deeply discharged and recharged hundreds of times. "]
[null,"The Battery should provide benefits of being maintenance free, case flame retardant & non-hazardous. The Item Includes supply, install &connect the following:"]
[null,"• All necessary DC cables between the batteries together and to the battery fuse box to have a complete operational circuit with all conduits, clamps, stainless steel bolts, washers and cable end terminations needed to fix, all DC cables must be sized in accordance with the installation requirements applicable on site ,the allowable voltage drop must be less than 3%."]
[null,"• Battery mounting structure from hot galvanized steel stand with shelves and dividers for hosting the batteries and all other material needed to have a complete job ready ."]
[null,"• Complete earth system for neutrals including (electrodes 15mm2, manhole with iron cover, earth joints, clamps, conduits and 50 mm2 flexible copper wire from the neutral bus bar in the battery fuse box to the electrode. All precaution to have the resistance < 2Ω."]
[null,"• The number of batteries based on 100 amp-hours of capacity for each one."]
[null,"The contractor should provide certified characteristics, shop test performance curves, spare parts regular (as recommended by manufacturer , maintenance catalogues and manufacturers warrantee for each inverter for a period not less than 10 years. "]
[null,"The items include Dismantling &Removing old damaged components such (DC wires,Cables,Batteries , structure , ….. Etc ) and move to University store as per engineer instructions."]
[null," All works and materials must be according to the drawings, catalogues, specifications and supervisor engineer instruction’s and approval."]
["9.56","PV Mounting structure:","L.S",1]
[null,"Removing and dismantling all the damaged steel supports and angles from the existing PV mounting steel structure.\nThe works includes maintenance works for the existing structure and supply new hot galvanized steel foundation to be replaced by the damaged peaces to be suitable to the dimension of selected PV modules and PV numbers to complete the works. The mounting provides a fixed inclination of the modules from 30 degree to 32 degree with vertical supports, plates, screws and casting concrete foundations B250 (0.4*0.4*0.2) m3 for each leg, the structure profile includes bracing and double hot galvanized angles for dividers. The mounting structure components are bonded together to guarantee potential equalization."]
[null," The price includes supply and install a complete earth system (electrodes 15mm2, manhole with iron cover, earth joints, clamps and 25 mm2 flexible copper cable from the structure to the electrode, all necessary copper wires to connect arrays and modules in one loop for earthen."]
[null," All precaution to have the resistance < 2Ω."]
[null,"All works and materials must be according to drawings, specifications and supervisor instructions and approval."]
["ELECTRICAL WORKS TOTAL ($)"]
[" Electrical works at Floor A500"]
[null,"LIGHTINGS WORKS"]
["9.57.1","Supply, install connect and operate Led lighting fixture 36W ,(60*60 CM) European made. Model PLANO LED  # 313979 or equivalent (Type is LENA or equivalent).\nThe item includes PVC conduits, J.boxes, fixing screws (Galv.) and wiring and all necessary equipment for installation and operation as per drawings, specifications and engineer instructions.","NO",55]
["9.57.2","Supply, install connect and operate 3W/ 2\" Led Spot Light .\n European made ,Model # LP-COB03For equivalent (Type is LIPER or equivalent).\nThe item includes ballast, wires, PVC pipes ,boxes and all necessary equipment for installation and operation as per drawings, specifications and engineer instructions.","NO",120]
["9.57.3","Ditto but  5W/ 3\" Led Spot Light . European made ,Model # LP-DL05EH or equivalent (Type is LIPER or equivalent).\n","NO",50]
["9.57.4","Ditto but  20W/ 6\" Led Spot Light . European made ,Model #  LPDL-20A-Y or equivalent (Type is LIPER or equivalent).\n","NO",50]
["9.57.5","Supply, install connect and operate Circular Surface mounted Globe with Led lamp 16 W OSRAM made (Type is GA'ASH No. 552100 or equivalent)\nThe item includes all necessary equipment for installation and operation as per drawings, specifications and engineer instructions.","No",8]
["9.57.6","Supply, install connect and operate Emergency LED lighting fixture 2w, 180 minutes duration Surface or wall mounted with  lamps and self adhesive original sticker - according to the direction of flow- with  legend complete with all necessary wiring and accessories.\n(Type is LENA or equivalent)","No",2]
["ELECTRICAL WORKS TOTAL ($)"]
[null,"LIGHTING SWITCHES AND OUTLETS WORKS"]
["9.57.7","Supply, install connect and operate Single pole one way internal switch, 220v, 10A, complete with PVC conduits, J.boxes, wiring, cover and all necessary accessories. \n(Type is  BTICINO MATIX or equivalent).","No",15]
["9.57.8","Ditto but water proof type.","No",5]
["9.57.9","Ditto but one way, two pole switch","No",25]
["9.57.10","ditto but water proof two pole.","No",5]
["9.57.11","Ditto but one way, three pole switch","No",20]
["9.57.12","Ditto but two way switch, single pole.","No",10]
["9.57.13","Ditto, but push button with illuminated lamp required for stair case lighting fixtures, the item includes one stair case timer.","No",5]
["9.57.14","Supply, install connect and operate Electrical Heater Switch 230V, 20A, with pilot lamp, with water Proof cover.\n(Type is BTICINO MATIX or equivalent)","No",2]
["9.57.15","Supply, install connect and operate Single internal socket outlet 16A, 220v, 2p+E for flush, wall, or surface mounted , complete with PVC conduits, J.boxes, wiring, and all necessary accessories. (Type is BTICINO MATIX  or equivalent).","No.",80]
["9.57.16","Ditto but double internal socket outlets","No.",20]
["9.57.17","Ditto but water and dust proof","No.",3]
["9.57.18","Ditto but 20A AC Switched Outlet with 4 mm2 wires.","No.",20]
["9.57.19","Supply, install connect and operate 6\" Extract Fan VENTA made or equivalent\nThe item includes external cover with louver of galvanized steel painted with suitable color to external elevation of the building size of 40x40 cm and all necessary equipment for installation and operation as per drawings, specifications and engineer instructions.","No.",3]
["ELECTRICAL WORKS TOTAL ($)"]
[null,"Telephone,satalite , and Computer"]
["9.57.20","Supply, install and connect wall mounted telephone socket outlet 6 pin complete with PVC conduits, J.boxes, 2 pairs cable (Teldor) from the location of telephone socket to sub-telephone box or telephone exchanger in the same socket's floor, and all necessary accessories (Type is BTICINO MATIX original   or equivalent). ","No.",30]
["9.57.21","Supply, install and connect internal  complete computer sockets (single) with RJ45 cat 6 female connectors, cover, Original Italian GEWISS (RJ45 Data Socket Cat6  (Product Code: GW20684)), connect it to the patch panel in Rack with U/FTP Teldor cables cat 6 as shown in the network drawings, all sockets must be tested and labeled(cables, sockets).(cable must has one meter extra length inside the Rack)","No.",40]
["9.57.22","Supply, install and connect IDF/MDF  Rack  : - 10U Rack  , with removable sides  including the following :\n- 2 fan, rack mounted power distributer\n- 2 panels of 24 port patch panel with female RJ45 cat 6 connector type 3M original.\n- 2 switch 24 port Cisco WS-C2960S-24TS-S switch , with Lan Base Image including 48 x patch cable 30cm  cat 6 original .\n-  1x UPS 700 va rackmount, cat 6 FTP cable from the main rack to the new rack at the roof APC Smart.","No.",1]
["9.57.23","Supply, install and connect Sub-telephone boxes (GEWISS # PT48)  complete with all connection strips, termination and all necessary accessories \n","No.",2]
["ELECTRICAL WORKS TOTAL ($)"]
[null,"CABLES"]
[null,"Supply, install and connect of the following cables with all required electrical PVC pipes and civil works, the item includes dismantling and re install the existing cables and laying under ground PVC piping system, manholes, excavation, warning tapes, backfilling and all required civil works to finish the work according  specifications and demands of the supervising engineer,  to connect cables terminals from source to destination. According to drawings, specifications, instructions, and demands of the supervising engineer. as follow:"]
["9.57.24","  N2XY-XLPE cable 5*16 mm2","M.R",60]
["9.57.25","  N2XY-XLPE cable 5*6 mm2","M.R",50]
["9.57.26","Supply, install and connect Telephone Cable (J-Y (ST) Y (1G 40*2*0.6)) Tudor cable. The item includes 2\" PVC pipe and all necessary equipment for installation and operation as per drawings, specifications and engineer instructions.","M.R",80]
["ELECTRICAL WORKS TOTAL ($)"]
[null,"FIRE ALARM , Sound System , CCTV"]
[null,"Supply, install, test and commissioning    fire alarm system as per drawings including fire resist PVC pipes, pull boxes special wires and  all necessary accessories (Type is MORLEY or equivalent), which includes :"]
["9.57.27","2 zones conventional Fire alarm control panel  complete with brand name original batteries, the item include 2pair cable for the fire alarm control panel to all parts of the system and all necessary accessories needed to complete the job ","No.",1]
["9.57.28","Supply, install and connect Addressable Smoke Detector type MORLEY-IAS Model # MI-PSE or equivalent\nThe item includes all necessary equipment for installation and operation as per drawings, specifications and engineer instructions.","No.",20]
["9.57.29","Ditto  but heat detector.","No.",3]
["9.57.30","Supply, install  break glass call point as per drawings the unit shall be standard type for interior use with key operated test facility, with plastic coated glass and one spare coated glasses.","No.",15]
["9.57.31","Supply, install 95 db electronic horn ultra sound for indoor used. ","No.",2]
["9.57.32","Supply, install and connect ceiling mounted loud speaker 150 mm Diam.  with nominal max. power of 4/6W including all required cables (2,5 mm2) , junction boxes conduits and,  metal front protection mesh,  clips for quick attachment , line transformer all necessary accessories (Type is Bosch,Cotina or equivalent)","No.",20]
["9.57.33","Supply, install and connect wall and Ceil mounted female VGA sockets  that include VGA  cable  (0,8 mm) between two VGA connectors, and double male VGA  audio connectors 2 meters (each) to connect from computer to wall mounted VGA socket and from VGA Audio socket to LCD.","No.",6]
["9.57.34","Supply, install and connect Satellite socket outlet, complete with PVC conduits, and satellite cable from satellite switch to socket outlet and  all necessary accessories (Type is   GEWISS verna or equivalent).\nNote: cables from satellite socket to multis switches must have twow meters extra-length inside the box.","No.",6]
["9.57.35","Supply, install and connect PVC pipes and boxes for CCTV SYSTEM Networks in the Halls (A700, W600, A100). \nThe item includes all necessary electrical and civil works and equipment for installation and operation as per drawings, specifications and engineer instructions.","L.S",1]
["ELECTRICAL WORKS TOTAL ($)"]
[null," POWER SYSTEM AND ELECTRICAL BOARDS WORKS"]
["9.57.36","Supply and install electrical switch board of size 80x60x25cm one door, the frame work is made of galvanized steel sheets 2mm  thickness, painted by antistatic and insulation paint. The item includes busbars, wiring, insulations, plastic ducts, terminal blocks and all necessary equipment and civil works for installation and operation as per drawings, specifications and engineer instructions  (Type is MOELLER or equivalent) ","No",1]
["9.57.37","Ditto but size 60x40x20cm","No",2]
["9.57.38","Supply , install and connect MCCB 3*63A MOELLER made # NZMB1-A63","No",1]
["9.57.39","Ditto but MCB 3*50A MOELLER made # FAZ-C50/3","No",2]
["9.57.40","Ditto but MCB 3*32A MOELLER made # FAZ-C32/3","No",1]
["9.57.41","Ditto but MCB 3*40A MOELLER made # FAZ-C40/3","No",1]
["9.57.42","Ditto but MCB 3*25A MOELLER made # FAZ-C25/3","No",2]
["9.57.43","Ditto but ELCB 4*40A MOELLER made # FIM-40/4/0.03-A","No",4]
["9.57.44","Ditto but MCB 1*16A MOELLER made # FAZ-C16/1","No",20]
["9.57.45","Ditto but MCB 1*20A MOELLER made # FAZ-C20/1","No",20]
["9.57.46","Ditto but MCB 1*10A MOELLER made # FAZ-C10/1","No",20]
["ELECTRICAL WORKS TOTAL ($)"]
["TOTAL At A500 ($)"]
["Electrical works at Floor A900"]
[null,"LIGHTINGS WORKS"]
["9.58.1","Supply, install connect and operate Led lighting fixture 36W ,(60*60 CM) European made. Model PLANO LED  # 313979 or equivalent (Type is LENA or equivalent).\nThe item includes PVC conduits, J.boxes, fixing screws (Galv.) and wiring and all necessary equipment for installation and operation as per drawings, specifications and engineer instructions.","NO",37]
["9.58.2","Supply, install connect and operate 3W/ 2\" Led Spot Light .\n European made ,Model # LP-COB03For equivalent (Type is LIPER or equivalent).\nThe item includes ballast, wires, PVC pipes ,boxes and all necessary equipment for installation and operation as per drawings, specifications and engineer instructions.","NO",140]
["9.58.3","Ditto but  5W/ 3\" Led Spot Light . European made ,Model # LP-DL05EH or equivalent (Type is LIPER or equivalent).\n","NO",30]
["9.58.4","Ditto but  20W/ 6\" Led Spot Light . European made ,Model #  LPDL-20A-Y or equivalent (Type is LIPER or equivalent).\n","NO",50]
["9.58.5","Supply, install connect and operate Circular Surface mounted Globe with Led lamp 16 W OSRAM made (Type is GA'ASH No. 552100 or equivalent)\nThe item includes all necessary equipment for installation and operation as per drawings, specifications and engineer instructions.","No",10]
["9.58.6","Supply, install connect and operate Emergency LED lighting fixture 2w, 180 minutes duration Surface or wall mounted with  lamps and self adhesive original sticker - according to the direction of flow- with  legend complete with all necessary wiring and accessories.(Type is LENA or equivalent)","No",3]
["ELECTRICAL WORKS TOTAL ($)"]
[null,"LIGHTING SWITCHES AND OUTLETS WORKS"]
["9.58.7","Supply, install connect and operate Single pole one way internal switch, 220v, 10A, complete with PVC conduits, J.boxes, wiring, cover and all necessary accessories. \n(Type is  BTICINO MATIX or equivalent).","No",12]
["9.58.8","Ditto but water proof type.","No",3]
["9.58.9","Ditto but one way, two pole switch","No",22]
["9.58.10","ditto but water proof two pole.","No",5]
["9.58.11","Ditto but one way, three pole switch","No",8]
["9.58.12","Ditto but two way switch, single pole.","No",8]
["9.58.13","Ditto, but push button with illuminated lamp required for stair case lighting fixtures, the item includes one stair case timer.","No",5]
["9.58.14","Supply, install connect and operate Electrical Heater Switch 230V, 20A, with pilot lamp, with water Proof cover.\n(Type is BTICINO MATIX or equivalent)","No",2]
["9.58.15","Supply, install connect and operate Single internal socket outlet 16A, 220v, 2p+E for flush, wall, or surface mounted , complete with PVC conduits, J.boxes, wiring, and all necessary accessories. (Type is BTICINO MATIX  or equivalent).","No.",30]
["9.58.16","Ditto but double internal socket outlets","No.",10]
["9.58.17","Ditto but water and dust proof","No.",3]
["9.58.18","Supply, install connect and operate 6\" Extract Fan VENTA made or equivalent\nThe item includes external cover with louver of galvanized steel painted with suitable color to external elevation of the building size of 40x40 cm and all necessary equipment for installation and operation as per drawings, specifications and engineer instructions.","No.",3]
["ELECTRICAL WORKS TOTAL ($)"]
[null,"Telephone,satalite , and Computer"]
["9.58.19","Supply, install and connect wall mounted telephone socket outlet 6 pin complete with PVC conduits, J.boxes, 2 pairs cable (Teldor) from the location of telephone socket to sub-telephone box or telephone exchanger in the same socket's floor, and all necessary accessories (Type is BTICINO MATIX original   or equivalent). ","No.",18]
["9.58.20","Supply, install and connect internal  complete computer sockets (single) with RJ45 cat 6 female connectors, cover, Original Italian GEWISS (RJ45 Data Socket Cat6  (Product Code: GW20684)), connect it to the patch panel in Rack with U/FTP Teldor cables cat 6 as shown in the network drawings, all sockets must be tested and labeled(cables, sockets).(cable must has one meter extra length inside the Rack)","No.",22]
["9.58.21","Supply, install and connect IDF/MDF  Rack  : - 8U Rack ,depth  50 cm , with removable sides  including the following :\n fan, rack mounted power distributer , 24 port patch panel with female RJ45 cat 6 connector type 3M original, 24 port switch Cisco WS-C2960S-24TS-S  , with Lan Base Image  , 24 x patch cable 30cm  cat 6 original , 1x UPS 700 va rackmount, cat 6 FTP cable from the main rack to the new rack at the roof APC Smart.","No.",1]
["9.58.22","Supply, install and connect Sub-telephone boxes (GEWISS # PT48)  complete with all connection strips, termination and all necessary accessories \n","No.",1]
["ELECTRICAL WORKS TOTAL ($)"]
[null,"CABLES"]
[null,"Supply, install and connect of the following cables with all required electrical PVC pipes and civil works, the item includes dismantling and re install the existing cables and laying under ground PVC piping system, manholes, excavation, warning tapes, backfilling and all required civil works to finish the work according  specifications and demands of the supervising engineer,  to connect cables terminals from source to destination. According to drawings, specifications, instructions, and demands of the supervising engineer. as follow:"]
["9.58.23","  N2XY-XLPE cable 5*16 mm2","M.R",20]
["9.58.24","  N2XY-XLPE cable 5*6 mm2","M.R",20]
["9.58.25","Supply, install and connect Telephone Cable (J-Y (ST) Y (1G 20*2*0.6)) Teldor cable. The item includes 2\" PVC pipe and all necessary equipment for installation and operation as per drawings, specifications and engineer instructions.","M.R",50]
["ELECTRICAL WORKS TOTAL ($)"]
[null,"FIRE ALARM , Sound System , CCTV"]
[null,"Supply, install, test and commissioning    fire alarm system as per drawings including fire resist PVC pipes, pull boxes special wires and  all necessary accessories (Type is MORLEY or equivalent), which includes :"]
["9.58.26","Supply, install and connect Addressable Smoke Detector type MORLEY-IAS Model # MI-PSE or equivalent\nThe item includes all necessary equipment for installation and operation as per drawings, specifications and engineer instructions.","No.",12]
["9.58.27","Ditto  but heat detector.","No.",2]
["9.58.28","Supply, install  break glass call point as per drawings the unit shall be standard type for interior use with key operated test facility, with plastic coated glass and one spare coated glasses.","No.",2]
["9.58.29","Supply, install 95 db electronic horn ultra sound for indoor used. ","No.",2]
["9.58.30","Supply, install , connect, and test  240 W Mixer amplifier (Type is Bosch PLE-2MA240 Mixing amplifier or equivalent)\nWhich has the following specifications\n▶ 4 microphone/line inputs, plus 3 music source inputs\n▶ 100 V and telephone input with priority & VOX\n▶  Announcement only output, 3-wire volume override\n▶ Voice-activated emergency override\n▶ Including case for the amplifier","No.",1]
["9.58.31","Aluminum Rack With Lock and two doors to putting mixer and transmitter mic.with power point and strip","No.",1]
["9.58.32","Supply, install , connect Microphone desk stand including 2 dynamic microphone with high level of sensitivity, Pushbuttons for momentary and latching microphone actions, 5-meter cable for amplifier connection with 5-pin DIN connector (Type is  SHURE, BOSCH or equivalent)","No.",2]
["9.58.33","Remove and Supply, install and connect ceiling mounted loud speaker 150 mm Diam.  with nominal max. power of 4/6W including all required cables (2,5 mm2) , junction boxes conduits and,  metal front protection mesh,  clips for quick attachment , line transformer all necessary accessories (Type is Bosch,Cotina or equivalent)","No.",20]
["9.58.34","Supply, install and connect wall and Ceil mounted female VGA sockets  that include VGA  cable  (0,8 mm) between two VGA connectors, and double male VGA  audio connectors 2 meters (each) to connect from computer to wall mounted VGA socket and from VGA Audio socket to LCD.","No.",15]
["9.58.35","Supply, install and connect Satellite socket outlet, complete with PVC conduits, and satellite cable from satellite switch to socket outlet and  all necessary accessories (Type is   GEWISS verna or equivalent).\nNote: cables from satellite socket to multis switches must have twow meters extra-length inside the box.","No.",10]
["9.58.36","Supply, install and connect Microphone socket outlet, female plug, including all required cables , junction boxes, waterproof junction box inside the stage, conduits and all necessary accessories   (Type is GEWISS verna  or equivalent).\nnote: Sockets must be connected with existed Amplifier","No.",10]
["9.58.37","Supply, install and connect PVC pipes and boxes for CCTV SYSTEM Networks in the Halls (A900). \nThe item includes all necessary electrical and civil works and equipment for installation and operation as per drawings, specifications and engineer instructions.","L.S",1]
["ELECTRICAL WORKS TOTAL ($)"]
[" TOTAL At A900 ($)"]
["Electrical works at Toilets"]
[null," POWER SYSTEM AND ELECTRICAL PANELS WORKS"]
["9.59.1","Supply, install, connect and operate waterproof surface mounted LED lighting fixture 32W or 36W, European made. IP66 Model CODAR RS LED  # 337680 or equivalent (Type is LENA or equivalent).\nThe item includes PVC conduits, J.boxes, fixing screws (Galv.) and wiring and all necessary equipment for installation and removing old electrical equipment and operation as per drawings, specifications and engineer instructions.","No.",8]
["9.59.2","Supply, install connect and operate Circular Surface mounted Globe with Led lamp 16 W OSRAM made (Type is GA'ASH No. 552100 or equivalent)The item includes all necessary equipment for installation and operation as per drawings, specifications and engineer instructions.","No.",25]
["9.59.3","Supply, install connect and operate Single pole one way internal switch, 220v, 10A, complete with PVC conduits, J.boxes, wiring, cover and all necessary accessories. \n(Type is  BTICINO MATIX or equivalent).","No",10]
["9.59.4","Ditto but water proof type.","No",10]
["9.59.5","ditto but water proof two pole.","No",10]
["9.59.6","Supply, install connect and operate Single internal socket outlet 16A, 220v, 2p+E for flush, wall, or surface mounted , waterproof Type IP65, complete with PVC conduits, J.boxes, wiring, and all necessary accessories. (Type is BTICINO MATIX  or equivalent).","No",15]
["9.59.7","Supply, install and connect Addressable Smoke or Heat Detector type MORLEY-IAS Model # MI-PSE or equivalent\nThe item includes all necessary equipment for installation and operation as per drawings, specifications and engineer instructions.","No.",9]
["9.59.8","Dismantle, remove and reinstall new panel door size 60*80 cm from hot galvanized steel sheets 2mm thickness, painted by antistatic and insulation paint with all necessary equipment’s and civil works for installation and operation as per specifications and engineer instructions  (Type is MOELLER or equivalent)","No.",3]
["9.59.9","Ditto , but 40*60 cm","No.",3]
["ELECTRICAL WORKS TOTAL ($)"]
[null," POWER SYSTEM AND ELECTRICAL PANELS WORKS"]
["9.60","Supply, install, connect and operate in the Existing ATS switchboard of the university new Automatic Transfer Switch (ATS) 3 phase, motorized type with overload made of two identical switches 4 poles each,400v, 1250A rating including mechanical and electrically interlock, the work includes automatic changeover control unit (ACU) with all required Timers,Relays,adjastable under voltage Relay and all protection devices to complete the work as per the engineer instructions .(Type is moeller # N4−4−AE1250 or equivalent)\nThe item includes all needed busbar & wires depending on new circuit breakers range inside the panel.\nThe existing electrical board must be rearranged and labeled  According to specifications, instructions and demands of the supervisor engineer\n\n\n\n","Set",1]
["9.61","Supply, install, connect 3 indication lamps R S T with resistance 220V,with LTL fuse3x36/6A ","SET",2]
["9.62","Supply, install, connect Current transformer (1250/5A).","NO",6]
["9.63","Supply, install, connect Amper Meter (0-1250).","NO",6]
["9.64","Supply, install, connect Voltmeter 0-500V with 7 positions selector switch with LTL fuse3x36/6A.","SET",2]
["9.65","Supply, install and connect of electrical cable XLPE / CU 3x240+120+120mm2 from main distribution board to ATS panel with all required PVC pipes and civil works, the item includes laying under ground PVC piping system, excavation, warning tapes, backfilling and all required civil works to finish the work according  specifications and demands of the supervising engineer. The price include reinstatement and repair any damage of the infrastructures works to the exist pavement.","M.R",20]
["9.66","Dismantling, removing and rearranging all electrical components such (CU bus bars, CU wires, Insulators, Power and Control wires ...etc.) in the existing main distribution board that need to separate the loads into two parts to achieve load balance with all needed new electrical component such (CU bus bars , CU wires, Insulators , Power and Control wires ...etc.) depending on the new amber ratings new electrical component such (CU bus bars , CU wires, Insulators , Power and Control wires ...etc.)\nThe item includes supply and installs new circuit breaker (N4−4−A1000) type is Moeller or equivalent with all needed bus bars and wires depending on new circuit breaker range.\nAll works must be according to specifications, instructions and demands of the supervisor engineer\n\n","L.S.",1]
["9.67","Dismantling, Removing and Re-Installing of the  65KVA generator from the ground to the up surface of the existing electricity room with all necessary cables and connections for fuel network. the item includes supply and install all required vibrations dumpers with skin of rubber resistance (6 units) to be installed under the generator.","L.S.",1]
["ELECTRICAL WORKS TOTAL ($)"]
[null,"Fire Pumps Networks"]
["9.68","Supply, Install, connect and test branded firefighting network pump station including the 2 pumps and their motors (Type is Speroni, Armstrong, or equivalent) pumps of \n50m head and 5 m3/hr. The price should include:  \n1- 4X1 1/2\" Ball Valve                                                        \n2- 2X1 1/2\" Strainer                                                            \n3- 2X1 1/2\" Flexible Connections                                      \n4- 2X1 1/2\" Check Valve                                                     \n5- 2X2\" Pressure gauges  ,\n6- 2X 200 LTR 10 bar Membrane Pressure Tank with all its accessories, pressure switches and level switches including all necessary wiring and conduits to control panel and all related protection needed.\n","Set",3]
[null,"7- Control Panel complete with main and sub-circuit breakers, contactors, under voltage Relays, overloads, timers, indication lambs, bus bars, fuses, 2  Ammeter, horn alarm, Voltmeter  with selector switch, ON / OFF push buttons, Auto manual selector switch, the work includes all necessary power and control cables from pump to control panel."]
[null,"\nThe working principle is to control the operating of the fire pumping station sequentially with the 2 pumps; the first pump will start working according to the pressure switch when the pressure drops in the system after that when the pressure is law the second pump will start working in parallel with the other pump. The pumps will stop working when there is no water from the source regarding to the level switch. All according to the drawings, specifications, and Engineers instructions\nThe price includes dismantle and remove and deliver the existing pump to the university and all required accessories and fitting and connections to complete the job according to the specifications and engineer instructions.\n\n"]
["9.69","Supply, Install, connect and test branded Electrical Jockey firefighting pump (Type is Speroni, Armstrong, or equivalent) pumps of \n50m head and 1 m3/hr. The price should includes all needed accessories and connections and fittings with all needed conduits and cables to complete the job according to the specifications and engineer instructions. \n","No",3]
["ELECTRICAL WORKS TOTAL ($)"]
[" TOTAL ($)"]
["Bill No (A) - 10. HVAC works"]
["HVAC at Floor A-100 "]
[null,"- All of works are performed in accordance with the plans and technical specifications of the project and properly approved by the Engineer ."]
[null,"-Offered prices include the following:"]
[null,"All following items shall be executed according to drawings, specifications and as directed by the Engineer. Prices shall include all required works, fittings , connections , accessories and testing."]
[null,"Contractor shall submit shop drawings for all Mechanical installations to be approved by the Engineer before executing the work.  As-made drawings shall be submitted after completing the work."]
[null,"All refrigerant should be (environmentally friendly)."]
[null,"All work s should be executed in accordance the plans and technical specifications for the project, according to the approval of the supervisor engineer.\nPrices include the following:\n-  All PVC pipes and connections of condensate water.\n-  All mechanical and electrical connections for the installation, test and operation.\n-  Restoration all the places in the walls and   Install Plastic ducts as suitable dimensions for the refrigerant pipes and electricity cables and water pipes according the supervisor engineer."]
[null,"Install condensing water drainage network and connect it to the nearest point of drainage rain water (for all units internal and external units) and according to the supervisor engineer"]
[null,"The Contractor shall submit samples of all materials with catalogs showing illustrative specifications"]
[null,"insulate pipes and tubes as a properly engineering (water condensation and gas Refrigeration)."]
[null,"The price includes all gas pipes (liquid & suction) and lengths depending on drawings and to ensure fit with distances and diameters according to the manufacturer's instructions for units"]
[null,"Wrapping All pipes and refrigerant lines with insulation as a special appropriate for the engineering assets and the approval of the supervisor engineer"]
[null,"Paint all the copper pipes of the same color paint pipes (welding places) before the isolating"]
[null,"Submit (CALCULATION SHEET) of the system from the manufacturer of the units to be clear and detailed"]
["Out Door Roof Top Unit: SEMI CENTRAL"]
[10.1,"Supply , install, test and commission Complete HVAC  system (Semi central air-conditioning)/HEAT PUMP DUCTED SPLIT DOUBLE SKIN for the ground floor mounted on Roof, consist of (outdoor and indoor unit) connected through copper refrigerant pipe),the unit should be tights installed completed with all necessary supports, hangers, insulation if needed, fasteners, drain connections, all pipes , sleeves and thermostat.\nEach unit includes (two compressors ) And working (cooling / heating) , compressors should be(scroll type) COPELAND  or equivalent with control Panel ,compressors should be a European or American manufactured , and all aluminum fins should be (anodized) or treatment and resistant for rust and corrosion salts with every needed for installation and operation of connections and copper pipes and all required electrical cables according to drawings and engineers approval , and all necessary connections to operate the system.\n The system include \nCooling capacity: ( 48000  BTU) \nAir flow (1600 CFM).","No",4]
["Duct Works :"]
[10.199999999999999,"Supply and install galvanized insulated sheet ducts (thick : 0.8 mm) ,with a proper gages as specified for supply and return air  including all accessories, galvanized hangers, bolts, flexible connector, thermal insulation materials of 1\" inch thickness density (24 Kg/m³)including volume control damper (VCD)on all branches and According to drawings and engineers approval.","m2",120]
["Air Distributing Equipment"]
[10.3,"Supply and install anodized finish aluminum supply  Ceiling Diffuser (four way), should be fitted with opposite blade damper air volume controller.  Including air box . According to the drawings     size : 40 x 40","No",12]
[10.4,"Ditto, but,  size : 45 x 45","No",4]
[10.5,"Supply and install anodized finish aluminum grill for  return air ,should be fitted with opposite blade damper air volume controller.  Including air box . According to the drawings                                  size : 60 x 60","No",8]
["Total"]
["HVAC at Floor A-500 "]
[null,"- All of works are performed in accordance with the plans and technical specifications of the project and properly approved by the Engineer ."]
[null,"-Offered prices include the following:"]
[null,"All following items shall be executed according to drawings, specifications and as directed by the Engineer. Prices shall include all required works, fittings , connections , accessories and testing."]
[null,"Contractor shall submit shop drawings for all Mechanical installations to be approved by the Engineer before executing the work.  As-made drawings shall be submitted after completing the work."]
[null,"All refrigerant should be (environmentally friendly)."]
[null,"All work s should be executed in accordance the plans and technical specifications for the project, according to the approval of the supervisor engineer.\nPrices include the following:\n-  All PVC pipes and connections of condensate water.\n-  All mechanical and electrical connections for the installation, test and operation.\n-  Restoration all the places in the walls and   Install Plastic ducts as suitable dimensions for the refrigerant pipes and electricity cables and water pipes according the supervisor engineer."]
[null,"Install condensing water drainage network and connect it to the nearest point of drainage rain water (for all units internal and external units) and according to the supervisor engineer"]
[null,"The Contractor shall submit samples of all materials with catalogs showing illustrative specifications"]
[null,"insulate pipes and tubes as a properly engineering (water condensation and gas Refrigeration)."]
[null,"The price includes all gas pipes (liquid & suction) and lengths depending on drawings and to ensure fit with distances and diameters according to the manufacturer's instructions for units"]
[null,"Wrapping All pipes and refrigerant lines with insulation as a special appropriate for the engineering assets and the approval of the supervisor engineer"]
[null,"Paint all the copper pipes of the same color paint pipes (welding places) before the isolating"]
[null,"Submit (CALCULATION SHEET) of the system from the manufacturer of the units to be clear and detailed"]
["Out Door Roof Top Unit:"]
[10.6,"Supply , install, test and commission Complete HVAC  system (central air-conditioning) Variable Refrigerant Flow (VRF) for the fourth floor mounted on Roof, consist of (two external units) connected through a complex (Refnet Header),the unit should be tights installed completed with all necessary supports, hangers, insulation if needed, fasteners, drain connections, all pipes , sleeves and thermostat.\nEach unit includes (two compressors ) And working (cooling / heating) , compressors should be(inverter type) with control Panel with a common (Microprocessor) the compressors should be a European or American manufactured or made by the same manufacturer of the units, and ​​all aluminum fins should be (anodized) or treatment and resistant for rust and corrosion salts with every needed for installation and operation of connections and copper pipes and all required electrical cables according to drawings and engineers approval , and all necessary connections to operate the system.\n The system include (measurement control) and equipped with a computer (Laptop ) and provider of Building Management System – (BMS) and all necessary software for the operation and as instructed by the supervising engineer .\nNumber (2) the ability of cooling : (30KW) Total Load (60 KW).","No",1]
["Internal Units"]
[10.7,"Supply, installation and operate internal air conditioning unit (Wall Mounted- VRF TYPE) Model (Decorative) with remote control (cooling / heating) from the same type of external units to be equipped with all the filters required with every needed to install and operate the unit and all needed Pipes a, electrical cables between the indoor unit and outdoor unit and insulation the condensate water properly and on each unit should include all needed Refnet Joint (number 2) and valves (2) and as instructed by the supervising engineer.\nCooling Capacity: (3.5 KW).\nAir flow: (380 CFM). \n","No",5]
[10.8,"Ditto but (2 KW)\nAir flow: (250 CFM).","No",6]
[10.9,"Ditto but (Cassette unit type) with built in condensate water pump (5.25 KW)\nAir flow: (535 CFM).","No",3]
[10.1,"Ditto but (2.6 KW)\nAir flow: (300 CFM).","No",4]
[10.11,"Ditto but (2 KW)\nAir flow: (250 CFM).","No",4]
["Extract Fan \n"]
[10.119999999999999,"Supply , install, test and commission Wall Mounted Extract Fan for (W.C), to be tights installed completed with all necessary supports, sleeves, dampers, and all required electrical cables , and should be working with ducted-split According to drawings and engineers approval.\nAir flow: (180  CFM).","No",1]
[10.130000000000001,"Ditto but for (W.C)\nAir flow: (100 CFM).","No",2]
["Duct Works :"]
[10.14,"Supply and install galvanized insulated sheet ducts (thick : 0.7 mm) ,with a proper gages as specified for supply and return air  including all accessories, galvanized hangers, bolts, flexible connector, thermal insulation materials of 1\" inch thickness including volume control damper (VCD)on all branches and According to drawings and engineers approval.","No",2]
[10.15,"Ditto, but duct for extract air fan ,without insulation.","No",10]
[10.16,"Supply, install and test UPVC pipes dia 4\" class 8 bar for drainage, fixed in walls, floors, exposed or in shafts including all exposed elbows and turns provided with perforated caps on roof, clean outs. Including floor drains, floor clean outs  completed with all necessary finishing and cover. Prices to include all concrete encasement with columns, Walls,...etc.","L M",20]
[10.17,"Ditto but dia 3\"","L M",30]
["Total"]
["HVAC at Floor Different Place"]
[null,"- All of works are performed in accordance with the plans and technical specifications of the project and properly approved by the Engineer ."]
[null,"-Offered prices include the following:"]
[null,"All following items shall be executed according to drawings, specifications and as directed by the Engineer. Prices shall include all required works, fittings , connections , accessories and testing."]
[null,"Contractor shall submit shop drawings for all Mechanical installations to be approved by the Engineer before executing the work.  As-made drawings shall be submitted after completing the work."]
[null,"All refrigerant should be (environmentally friendly)."]
[null,"All work s should be executed in accordance the plans and technical specifications for the project, according to the approval of the supervisor engineer.\nPrices include the following:\n-  All PVC pipes and connections of condensate water.\n-  All mechanical and electrical connections for the installation, test and operation.\n-  Restoration all the places in the walls and   Install Plastic ducts as suitable dimensions for the refrigerant pipes and electricity cables and water pipes according the supervisor engineer."]
[null,"Install condensing water drainage network and connect it to the nearest point of drainage rain water (for all units internal and external units) and according to the supervisor engineer"]
[null,"The Contractor shall submit samples of all materials with catalogs showing illustrative specifications"]
[null,"insulate pipes and tubes as a properly engineering (water condensation and gas Refrigeration)."]
[null,"The price includes all gas pipes (liquid & suction) and lengths depending on drawings and to ensure fit with distances and diameters according to the manufacturer's instructions for units"]
[null,"Wrapping All pipes and refrigerant lines with insulation as a special appropriate for the engineering assets and the approval of the supervisor engineer"]
[null,"Paint all the copper pipes of the same color paint pipes (welding places) before the isolating"]
[null,"Submit (CALCULATION SHEET) of the system from the manufacturer of the units to be clear and detailed"]
["SPLIT Unit: "]
[10.18,null,"No",8]
[10.19,"Ditto but (24000 BTU)\nAir flow: (7 00 CFM).","No",6]
[10.199999999999999,"Ditto but (12000 BTU)\nAir flow: (360 CFM).","No",5]
["TOTAL ($)"]
["HVAC at Floor A-900"]
[null,"- All of works are performed in accordance with the plans and technical specifications of the project and properly approved by the Engineer ."]
[null,"-Offered prices include the following:"]
[null,"All following items shall be executed according to drawings, specifications and as directed by the Engineer. Prices shall include all required works, fittings , connections , accessories and testing."]
[null,"Contractor shall submit shop drawings for all Mechanical installations to be approved by the Engineer before executing the work.  As-made drawings shall be submitted after completing the work."]
[null,"All refrigerant should be (environmentally friendly)."]
[null,"All work s should be executed in accordance the plans and technical specifications for the project, according to the approval of the supervisor engineer.\nPrices include the following:\n-  All PVC pipes and connections of condensate water.\n-  All mechanical and electrical connections for the installation, test and operation.\n-  Restoration all the places in the walls and   Install Plastic ducts as suitable dimensions for the refrigerant pipes and electricity cables and water pipes according the supervisor engineer."]
[null,"Install condensing water drainage network and connect it to the nearest point of drainage rain water (for all units internal and external units) and according to the supervisor engineer"]
[null,"The Contractor shall submit samples of all materials with catalogs showing illustrative specifications"]
[null,"insulate pipes and tubes as a properly engineering (water condensation and gas Refrigeration)."]
[null,"The price includes all gas pipes (liquid & suction) and lengths depending on drawings and to ensure fit with distances and diameters according to the manufacturer's instructions for units"]
[null,"Wrapping All pipes and refrigerant lines with insulation as a special appropriate for the engineering assets and the approval of the supervisor engineer"]
[null,"Paint all the copper pipes of the same color paint pipes (welding places) before the isolating"]
[null,"Submit (CALCULATION SHEET) of the system from the manufacturer of the units to be clear and detailed"]
["Out Door Roof Top Unit: SEMI CENTRAL"]
[10.210000000000001,"Check and re- run the existing air conditioning units and maintenance work includes full unity and mobilization of gas according to the technical and engineering assets and instructions of the supervising engineer\nCooling capacity: ( 55500  BTU) \nAir flow (1800 CFM).","No",9]
[10.220000000000001,"Ditto but (49000 BTU)\nAir flow: (1600 CFM).","No",4]
[10.23,"Ditto but (41000 BTU)\nAir flow: (1600 CFM).","No",1]
["Duct Works :"]
[10.24,"Supply and install galvanized insulated sheet ducts (thick : 0.8 mm) ,with a proper gages as specified for supply and return air  including all accessories, galvanized hangers, bolts, flexible connector, thermal insulation materials of 1\" inch thickness density (24 Kg/m³)including volume control damper (VCD)on all branches and According to drawings and engineers approval.","m2",50]
[10.25,"Ditto, but duct for extract air fan ,without insulation.","m2",30]
[10.26,"Remove and re-manufacturing and isolate the old galvanized ducts  and installed according to instructions assets of workmanship and the supervising engineer Instructions","m2",100]
["Air Distributing Equipment"]
[10.27,"Supply and install anodized finish aluminum supply  Ceiling Diffuser (four way), should be fitted with opposite blade damper air volume controller.  Including air box . According to the drawings     size : 45 x 45","No",5]
[10.28,"Ditto, but,  size : 40 x 40","No",25]
[10.29,"Ditto, but,  size : 22.5 x22.5","No",2]
[10.3,"Supply and install anodized finish aluminum grill for  return air ,should be fitted with opposite blade damper air volume controller.  Including air box . According to the drawings                                  size : 30 x 80","No",1]
[10.31,"Ditto, but,  size : 30 x 60","No",2]
[10.32,"Ditto, but,  size : 25 x 60","No",1]
[10.33,"Ditto, but,  size : 60 x 60","No",3]
[10.34,"Supply and install anodized finish aluminum (Linear Return Bar  Grill) for  return air , with 5 mm thick horizontal blades at fixed inclination of 15°,12 slots complete with 15 mm width frame and connection box for duct connection should be fitted with opposite blade damper air volume controller.  Including air box . According to the drawings                                  ","LM",20]
["TOTAL ($)"]
["HVAC WORKS TOTAL ($)"]

{"sheet":"Summary","index":3,"n_rows":35,"n_cols":3,"rows_kept":35,"cut":false,"hidden":false,"merged":[[26,0,26,2],[28,0,28,2],[30,0,30,2],[32,0,32,2],[34,0,34,2],[24,0,24,2],[2,0,2,2],[15,0,15,1],[18,0,18,2],[20,0,20,2],[22,0,22,2]]}
[]
[]
["OVERALL SUMMARY"]
[]
["NO.","Description","Total price ($)"]
[1,"Demolition Works"]
[2,"Concrete Works."]
[3,"Building Works"]
[4," Carpentry works"]
[5,"Aluminum & Metal works"]
[6,"Finishing works"]
[7,"Painting works"]
[8,"Mechanical Works"]
[9,"Electrical Works"]
[10,"HVAC works"]
["Total"]
[]
[]
["Total  in  numbers: ........................................................................................................................"]
[]
["Total  in  letters:  ............................................................................................................................."]
[]
[" Name of the contractor: ………….………..……………………………………………………......"]
[]
[" Authorized signature: ……………...………………….………………………………………...….."]
[]
["Signature and Sealing:…………………………………………………...…………………….……."]
[]
["Title: ………………………………………..……………………..………………………….…………."]
[]
["Telephone:………………………………………………………………………………………..……."]
[]
["Fax: ……………………………………………………………………………………………...………."]
[]
["Mobile: …………………………………………………….…..………………………………..………."]