{"text_format":"2","workbook":"xlsx","n_sheets":7,"sheets":["Summary","A. Civil","B. Carpentry","C. Furnishing","D. Electrical","E. HVAC","List of samples required"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":10,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Summary","index":0,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":false,"merged":[[25,0,25,2],[26,0,26,2],[27,0,27,2],[0,0,0,5],[1,0,1,5],[2,0,2,5],[23,0,23,2],[24,0,24,2]]}
["Client: UNDP"]
["Project : Interior Design Works of the EEIC "]
["Location : Election Commission Building, Biratnagar, Nepal"]
[]
["SUMMARY OF COSTS"]
[]
["Sl.","Description","Total Amount"]
["A","Civil Works"]
["B","Carpentry Works"]
["C","Furnishing works"]
["D","Electrical and Allied Works"]
["E","Air-conditioning system"]
[null,"Sub-Total"]
[null,"VAT"]
[null,"TOTAL"]
[]
[]
[null,"Amount in words: ……………………………………………………………………………………………………………………….."]
[null,"…………………………………"]
[null,"Authorised Signature"]
[null,"…………………………………","…………………………………"]
[null,"Name of the Company","Company Seal"]
[]
["Notes:\n1.All Materials brought on site of works and meant to be used in the same shall be the best of their respective kinds and to the approval to the architects/Employer."]
["2. Samples of all materials shall be got approved by the Architects/Employer and shall be deposited with him before the order for the material is placed with the suppliers. The material brought on the works shall confirm in every respective with approved samples. "]
["3.Any material that have not been found to confirm to the specification will be rejected for which shall be removed from the site by the contractors within 48 hours at their own cost."]
["4.The contractor shall provide the mateials as mentioned in the specification. "]
["5. Workmanship: All works shall be to level plumb and square comers, edges and arises in all cases shall be unbroken and finished neat."]

{"sheet":"A. Civil","index":1,"n_rows":48,"n_cols":6,"rows_kept":48,"cut":false,"hidden":false,"merged":[[47,3,47,4],[0,0,0,5],[1,0,1,5],[2,0,2,5],[5,1,6,1],[5,0,6,0],[5,2,6,2],[5,3,6,3],[5,5,6,5],[4,0,4,5]]}
["Client: UNDP"]
["Project : Interior Design Works of the EEIC "]
["Location : Election Commission Building, Biratnagar,  Nepal"]
[]
["Bill No. A: Civil Works"]
["S.No","Description of Works","Unit","Quantity","Rate","Amount\n(NRS)"]
[]
[1,"Dismantling"]
[null,"Dismantling  Brick wall, partitions(low and high),furniture, ceiling,  slabs required for new construction using cutter on both side of wall for minimum disturbance to the structure retaining its services like sewer, drainage, electricity, etc. including collection transportation and disposal of dismantled debris off the site as per  drawing, specification and direction of Architect. "]
[1.1000000000000001,"Wall","Sq.M.",26]
[]
[2,"Plaster ","Sq.M.",12]
[null,"Supplyng, laying and fixing plaster  including supply of materials, labour, mixing, making grooves, strengthening joints, curing and scaffolding where required all complete as per drawing, specification and direction of Architect.\n12.5 mmthick 1:4 cement sand mortar"]
[]
[3,"Marble Works"]
[null,"Providing and Laying approved quality, pattern and colour (Similar as existing marble) 19mm thick pink indian marble on floor with  cement  mortar  of  mix  1:4  (1 Cement: 4  Coarse  Sand) backing and filling joints with necessary screeding works at necessary space with white cement slurry all complete as per the technical drawings and specification and instructions."]
[3.1,"Flooring ","Sq.m",45]
[3.2,"100mm high skirting","R.m",20]
[]
[]
[4,"Marble Polishing works","Sq.m",85]
[null,"Clean and mirror polish the existing indian marble flooring without affecting other existing structures including cutting, grinding, polishing and cleaning all complete as per specification and instruction of Architect. "]
[]
[5,"False Ceiling (Modular)","Sq.M.",85]
[null,"Supplying and installing Acoustic Board False Ceiling: 600 x 600 ceiling tile of dune or classic lite or fine fissured micro finish  acoustic board false ceiling with 44 mm high Silhoutte  black groove main Runner and Cross Tee with 3mm reveal each, with suspension hangers with spacing no larger than 400mm and  as per attached catalogue, drawing, specification and direction of Architect.15mm width Shilloutte Black groove Channel and Dune or Classic lite or Fine fissured Micro look Board"]
[null,"Make: ARMSTRONG OR EQUIVALENT "]
[]
[6,"False Ceiling (Gypsum)","Sq.M.",20]
[null,"Providing and fixing suspended Boral or equivelant gypsum board ceiling (straight, vertical & curved) , with thickness no less than 12mm with exterior surface duly taped at all joints, leveled with calcium silicate compound, with surface prepared with POP/putty along entire area to receive two coats of Primer and three coats of Emulsion Paint. frames with suspension hangers with spacing no larger than 400mm screwed to the ceiling/walls as per attached catalogue,design, drawing, specification/schedule of finishes and direction of Architect. "]
[null,"Make: BORAL or EQUIVALENT"]
[]
[7,"Wall putty","Sq.m",110]
[null,"Providing and applying wall putty work  in order to make the total plastered wall surface perfectly leveled , including cost of all materials,labour, conveyance,  scaffolding, watering, curing, etc.,  as per drawing, specification/schedule of finishes and direction of Architect."]
[null,"MAKE: JK/BIRLA/ASIAN or equivalent"]
[]
[8,"Paint"]
[8.1,"Plastic Emulsion","Sq.m",192]
[null,"Supply and applying one coat  primer and two coats of anti fungus, anti stain plastic emulsion paint  in  wall surfaces above wall putty , at any level, finished smooth including supply of materials, labour, preparation of base etc. all complete as per drawing, specification/schedule of finishes and direction of Architect."]
[null,"MAKE: ASIAN/BERGER or euivalent"]
[]
[8.1999999999999993,"Enamel","Sq.m",20]
[null,"Supply and applying one coat  primer and two coats of anti fungus, anti stain enamel paint  in  wall surfaces above wall putty , at any level, finished smooth including supply of materials, labour, preparation of base etc. all complete as per drawing, specification/schedule of finishes and direction of Architect."]
[null,"MAKE: ASIAN/BERGER or equivalent"]
[]
[9,"Stepped Seating","Sq.m",21]
[null,"Fabricate, supply and install raised seating in mock polling area made up of min. 50mmx50mm  MS square pipe steel structures and supports of 40mmx40mm square pipe  and seating top and side cover of 25mm thick seasoned pine wood planks painted with approved enamel paint with one coat of wood primer and three coat of enamel paint. The plank shall be fixed with nut and bolts in metal structure all complete as per drawing, specification and instruction of engineeer. "]
[]
[null,null,null,"SUB-TOTAL (A)"]

{"sheet":"B. Carpentry","index":2,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[[5,5,6,5],[48,3,48,4],[0,0,0,5],[1,0,1,5],[2,0,2,5],[5,0,6,0],[5,1,6,1],[5,2,6,2],[5,3,6,3],[4,0,4,5]]}
["Client: UNDP"]
["Project : Interior Design Works of the EEIC "]
["Location : Election Commission Building, Biratnagar,  Nepal"]
[]
["Bill No. B: Carpentry Works"]
["S.No","Description of Works","Unit","Quantity","Rate","Amount\n(NRS)"]
[]
[1,"Furiture works"]
[null,"Fabricate, supply and fixing furnitures made of 19mm blockboard of   approved   quality,   brand   Green   or   equivalent   as approved with 1mm laminate finish,with high quality exclusive  steel hardware fiitings and heavy section channels,  hinges,  8 mm  glass,  locks  including all accessories like buffers, push magnets, patch fittings, brackets etc where  necessary  and  all complete as approved per the drawings, specification and instructions."]
[null,"Make:\nBOARD: Greenboard or equivalent\nLAMINATE: GREENLAM or equivalent"]
[1.1000000000000001,"Polling Booth (T1)","No",4]
[1.2,"Registration Desk (T2)","No",1]
[1.3,"Storage Cabinet (1.8m x 0.84m x 0.60m) (R1)","No",1]
[1.4,"Ballot Box Stand","No",1]
[1.5,"Museum Rack (Display Cabinet) (R2)","No",3]
[1.6,"Storage Cabinet (0.85m Wx 2.10m Hx 0.60m D) (R3)","No",1]
[1.7,"Podium (T3)","No",1]
[1.8,"Builtin Cabinet (R3)","No",1]
[1.9,"Pamplet Holder","No",10]
[1.1000000000000001,"Information board","No",1]
[]
[2,"Wooden partition","Sq.M.",78]
[null,"Supply and fixing Haldu wood frame 60 x 60mm in cross section with battens no larger than 450mm c/c apart bothways horizontally and vertically including the framing above false ceiling. The partition shall consist of 10mm thick approved commercial ply along the straight surface and 2 layers of flexible ply along the curve. The surface shall be finished with 1mm thick approved Laminates on both sides to be applied with with fevicol adhesive. The partition shall have glazings of 8mm thick toughened glass with etching patterns where required. The glass shall be fixed with approved quality Sisham wood moulding of size 15mm x 35mm. This moulding shall be finished with high quality french polish over sand finished wooden surface. There shall be 4\" high sisham wood skirting flushed with the partition which shall be finished with french polish over sand finished surface all complete as per drawing, specification and direction of Architect. The length of the partitions shall be verified at site"]
[null,"Make:\nCOMMERCIAL PLY:Green Board or equivalent\nLAMINATE: GREENLAM or equivalent"]
[]
[3,"Cladding Works","Sq.M.",78]
[null,"Supply and fixing 19mm thick board with battens spaced at regular intervals horizontally and vertically. The cladding shall consist of 19mm thick approved commercial ply along the straight surface . There shall be 6mm MDF cladding over the ply and shall be finished with 1mm thick approved Laminates  to be applied with with adhesive of approved make with 1 mm thick groove finished with plastic paint matching the shade of laminate.There shall be 4\" high sisham wood skirting flushed with the partition which shall be finished with french polish over sand finished surface   all complete as per drawing, specification and direction of Architect. The length of the partitions shall be verified at site"]
[null,"Make:\nCOMMERCIAL PLY: SURYA/SAGUN/DURO or equivalent\nLAMINATE: GREENLAM or equivalent"]
[]
[4,"Wooden decorative boxing","No",1]
[null,"Provide decorative boxing for the TV."]
[null,"The cladding shall consist of 19mm thick approved commercial ply along the straight surface . There shall be 6mm MDF cladding over the ply and shall be finished with 1mm thick approved Laminates  to be applied with with adhesive of approved make with 5 mm thick groove finished with french polish(minimum five coat) of approved shade and color  all complete as per drawing, specification and direction of Architect. The length of the partitions shall be verified at site"]
[null,"Make:\nCOMMERCIAL PLY: Greenboard or equivalent\nLAMINATE: GREENLAM or equivalent"]
[]
[5,"White Board","No",2]
[null,"Supply and install whiteboards  of  900  mm  X  1200  mm   with  movable  MS  steel stand with castors on the bottom all complete as per design and specification"]
[]
[6,"Window/Door  covering wokrs","Sq.M",10]
[null,"Supply and install 19mm thick block board covering for windows and door finished with gypsumboard for wall finish. The surface shall be finished with pain including the required framing, accessories and hardwares as per drawing, specification and instruction of Architect. "]
[]
[7,"Wooden Beading/Moulding with polish","M.",25]
[null,"The cladding at walls shall have approved quality teak wood moulding of size 1\" x 3/4\". The moulding shall be finished with high quality French Polish (not less than 5 coats) over sand finished wooden surface, as per drawing, specification/schedule of finishes and direction of Architect."]
[]
[8,"Aluminum partition","Sq.m",12]
[null,"Aluminium Partition: Providing and Fixing Aluminium Partition consisting of Aluminium Sections 63.5 MM X 38.1 MM X 1.00 MM thick hollow anodised . . The Sections would be installed at an interval of 1m vertically and bottom section of size 114.60 x 44.45 x 2mm Aluminium snap beeding for glazing/panelling etc. and 5.5 mm thick float Transparent Glass including providing screwless aluminium glazing clip. Bottom upto 900mm Ht.  will be provided with 9 MM thick both side pre-laminated particle board flat pressed 3 layer of interior grade complete with fixing clips, fasteners, filling up of gaps at junction, top, bottom, & sides with required PVC/Nepprene felt etc.. The joints shall be smooth, mitred and jointed with cleat angle etc as per  direction of engineer/site Incharge.Rates shall be inclusive of frostate sticker to be applied as shown in the drawings.  "]
[]
[9,"Aluminium Door","No",1]
[null,"Aluminium Door: Providing and Fixing anodised Aluminium Door consisting of Sections 83.5 MM X 44.45 MM X 2.00 MM thick vertical, top and middle horizontal members and bottom members of size 114.60MM X 44.45MM X 2.00MM thickness. Bottom upto 3’ Ht will be provided with 12MM thick both side pre-laminated board as mentioned in the item 1 above and rest above provided with 5.5 MM thick transparent float glass. Door provided with 100 MM stainless steel dead lock Godrej make, hydraulic floor spring(godrej Make) ,(double action) heavy quality ISI marked with SS cover plate 100 MM dia Circular plate type handles (2 nos.) tower bolt of size 250 x10 mm (Barrel Type) including cutting the floor etc complete as directed by  engineer/site Incharge.  \n"]
[null,null,null,"SUB-TOTAL (B)"]

{"sheet":"C. Furnishing","index":3,"n_rows":20,"n_cols":6,"rows_kept":20,"cut":false,"hidden":false,"merged":[[5,5,6,5],[19,3,19,4],[0,0,0,5],[1,0,1,5],[2,0,2,5],[4,0,4,5],[5,0,6,0],[5,1,6,1],[5,2,6,2],[5,3,6,3]]}
["Client: UNDP"]
["Project : Interior Design Works of the EEIC "]
["Location : Election Commission Building, Biratnagar,  Nepal"]
[]
["Bill No. C: Furnishing Works"]
["S.No","Description of Works","Unit","Quantity","Rate","Amount\n(NRS)"]
[]
[1,"Vertical Blind","Sq.M.",20]
[null,"Supply and install Vertical Blinds made of glass fibre fabrics in width not less than 4\". Minimum  overlapping of 20mm in fabric. Top aluminium anodized rail of 1.4 mm thickness.  40mm wide channel with front lamination of same fabric. Runners having  stainless steel hooks with built-in shock spring and self aligning slip clutch.  End control box composed of double gear system.   Botton weight fully plastic covered linked with plastic bead chain. Approved colour and pattern as per attached drawing, specification/schedule of finishes and direction of Architect."]
[null,"MAKE: VISTA OR EQUIVALENT"]
[]
[2,"Staff Chairs","Nos.",2]
[null,"Provide revolving chair: Thick Padded Contoured Fabric/PU Seat and Mesh Back with Lumbar Support. Pneumatic Seat Height Adjustment. Height Adjustable Lower Lumbar Support. Tension Adjustable Lumbar Support. Locking Tilt Control Mechanism. Tension Control.  "]
[null," Stainless steel Chrome\n High quality black net/mesh finished on back\n Black PU on seat.\n Fine hard plastic on armrest.\n Stainless steel Chrome Base\n Size approximately: Chair H 86.5cm, Seat H: 46cm, Seat D: 49.5cm, Seat W.: 46cm "]
[null,"MAKE: KIVIK/KTM/FEATHERLITE or equivalent"]
[]
[3,"Stainless Steel Hook for headset","No",20]
[null,"Provide and install stainless steel hook of 3kg capacity with stainless screws for Headset including all accessories and hardware required as per instruction of engineer."]
[]
[null,null,null,"SUB-TOTAL (C)"]

{"sheet":"D. Electrical","index":4,"n_rows":180,"n_cols":6,"rows_kept":180,"cut":false,"hidden":false,"merged":[[54,1,54,3],[58,1,58,4],[179,3,179,4],[41,1,41,2],[0,0,0,5],[1,0,1,5],[2,0,2,5],[4,0,4,5],[5,0,6,0],[5,1,6,1],[5,2,6,2],[5,3,6,3],[5,5,6,5]]}
["Client: UNDP"]
["Project : Interior Design Works of the EEIC "]
["Location : Election Commission Building, Biratnagar,  Nepal"]
[]
["Bill No. D: Electrical and Allied Works"]
["S.No","Description of Works","Unit","Quantity","Rate","Amount\n(NRS)"]
[]
[1,"DISTRIBUTION BOARDS"]
[null,"Supply, delivery, installation of  distribution Board  wall mountable, push button lock and made of  16 SWG MS metal sheet including neutral bar and phase bar and adequate space for incomming and outgoing cable with all the chiselling  of wall fixing   mortar   and   civil   works    with   complete internal wiring as per the drawing, specification, instruction  , electricity rules all complete.(  Make: MCB Seimens,ABB or equi.)"]
[]
["a","DISTRIBUTION BOARD-DB-EEIC","Set.",1]
[null,"FDB-GF Box"]
[null,"City Supply Section"]
[null,"Circuit Breakers:"]
[null,"Incoming :   1 nos 20 A TP MCB ( 10 kA, BC)"]
[null,"Outgoings:"]
[null,"2 nos. of 16 Amp DP MCB ( 10 kA)"]
[null,"10 nos. of 6/10/16 Amp SP MCB ( 10 kA, BC)"]
[null,"2 nos. of 20 Amp DP MCB( 10 kA, BC)"]
[null,"100A TPNE Copper Busbar with accessories"]
[null,"AC Supply Section"]
[null,"Circuit Breakers:"]
[null,"Incoming :   1 nos 16 A TP MCB ( 10 kA, BC)"]
[null,"Outgoings:"]
[null,"5 nos. of 16/20 Amp DP MCB( 10 kA, BC)"]
[null,"Meters:"]
[null,"1 set. 0-500V Voltmeter with selector switch"]
[null,"1 set. 0-50A Ammeter with selector switch"]
[null,"1 set. of  50/5A ring type CT coil"]
[null,"Indicator Lamps"]
[]
["b","UPS-DB","Set.",1]
[null,"DB Box"]
[null,"Circuit Breakers:"]
[null,"Incoming :   1 nos.20 A DP MCB ( 10 kA, BC)"]
[null,"Outgoings:"]
[null,"4 nos. of 16/20 Amp SP MCB ( 10 kA, BC)"]
[]
["c","Manual Changeover Switch for Standby Generator"]
[null,"Supply, installation and connection of 63A TPN Manual Changeover ( HAVELL'S / BENTEX or equivelent ), (Based on 60 amp Mains incoming connection and 25 ~ 30 KVA Genset) ","Set",1]
[]
[2,"LOW TENSION FEEDER CABLES / WIRES/CONDUITS"]
[null,"Supply, delivery, laying, connecting, testing and commissioning     of    the     following     Armoured\n/unarmoured  PVC insulated and sheathed power cables  and  wires   through   HDP pipe/Listic (whichever applicable) including cable shoes/sockets cable clamps and necessary connecting, fixing, earthing, , chiselling of existing wall / ceiling and redoing the chiselled area with cement and sand mortar as per the drawings, site conditions, specifications, electricity rules and instructions all complete.( Cable Make: Prakash/Litmus/Pioneer or NS mark )"]
["a.","4 core, 25 sq.mm armoured. Cu cable","rm",100]
[null,"(main connection)"]
[]
["b.","4 core, 10 sq.mm unarmoured. Cu cable","rm.",35]
[null,"(MDB to FDB )"]
[]
["c.","3 x6 sq.mm unarmoured. Cu cable","rm.",65]
[null,"(FDBs to UPS DB to UPS DB & UPS   )"]
[]
["c.","1c, 6 sq.mm multistrand Cu cable  (E)","rm.",45]
[]
[3,"LIGHT  POINTS  WIRING THROUGH CONDUIT/LISTIC for UPS"]
["a","Supplying the materials and  concealed wiring through ceiling, false ceiling, wall of light points ( the point wiring should include light, fan outlet of required length from  control devices/switches to a point  )  using  2  x 2.5sq.mm  Multistrand  Flexible wire  in  a  hard   HDP  pipe  of  size 20/25 mm. copper WIRE including cable shoes/sockets cable clamps and necessary connecting,   fixing,  chiselling  of  existing  wall  / ceiling and redoing the chiselld area with cement and   sand   mortar   as   per   the   drawings,   site conditions ,specifications and instruction all complete. (Make: Cables- prakash/Litmus/Pioneer or NS:344/2052 , HDP-NS)","pt.",{"$f":"D69+D72+D75+D78+D81","v":41}]
[]
[4,"13AMP/15 AMP POWER  POINT WIRING"]
[null,"(For all the general power sockets, server and computer power sockets)"]
["4a","Supplying the materials and  concealed wiring through ceiling, false ceiling,tables  wall of power points ( the point wiring should include wiring between  the power points ) using 2 x 4 +1x2.5 sq.mm Cu wire in a HDP pipe of size   20/25 mm. dia. including  cable  shoes/sockets  cable  clamps and  necessary  connecting,  fixing,  earthing, chiselling of existing wall / ceiling and redoing the chiselled area with cement and sand mortar as per the drawings, site conditions ,specifications and instruction all complete. (Make: Cables- prakash/Litmus/Pioneer or NS:344/2052 , HDP-NS)","pt.",25]
[]
[5,"AC POWER  POINT WIRING"]
[null,"(For Air Conditioner)"]
["5a","Supplying the materials and  concealed wiring for single  phase  AC  units  through  ceiling,  false ceiling wall of power points ( the point wiring from nominated DB to indoor AC units and outdoor to indoor units interconnection  ) using 2 x4 sq. mm\n+ 1x2.5 sq.mm Flexible  multistrand in a HDP pipe of size   25 mm. dia. including cable shoes/sockets cable clamps and necessary connecting,  fixing, earthing,  chiselling  of existing wall / ceiling and redoing the chiselled area with cement and sand mortar as per the drawings, site conditions ,specifications and instruction all complete. (Make: Cables- prakash/Litmus/Pioneer or NS:344/2052 , HDP-NS)","pt.",4]
[]
[6,"LIGHT FIXTURES"]
[null,"Supply, delivery, installation, testing and commissioning  of the following light fixtures  with all the acessories  including the necessary connection, fixing and insulating materials as per the electricity rule, drawings, site conditions, specifications and instructions all complete."]
[]
["a","6\" Dia downlighter with 12w LED lights","set.",20]
[null,"Wipro, Legero (LVT 6512) or equivalent"]
[]
["b","36 watt recessed mounted LED luminaire with complete prismatic difuser suitale for modular ceiling. Size : 570mmx570mm","set.",14]
[null,"Wipro(Pure LED - LM 14)/Legero (LRP 1236   or equivalent"]
[]
["e","2\" dai Spot Light with 3 W LED warm","set.",3]
[null,"( Make: Wipro/Philips/GEor equivalent )"]
[]
["f","1x40W FTL with Acrylic cover","set.",2]
[null,"( Make: Wipro/Philips/GEor equivalent )"]
[]
["g","9\" dia Exhaust Fan","set.",2]
[null,"(Polar, Usha, Crompton or equivalent)"]
[]
[7,"SWITCHES,SOCKETS ,PLUG WITH PLATES"]
[null,"Supplying and fixing of following switches, sockets including metal boxes concealed  inside wall and accessories with necessary civil works  as per drawings, specifications, electricity rules and instructions all complete. \nMODULAR SWITCHES\nMAKE: CLIPSAL/ORANGE/OR EQUIVALENT"]
["a","1- gang one way switch","no.",2]
["c","2-gang one way switch","no.",1]
["e","3- gang one way switch","no.",1]
["f","4-gang one way switch","no.",5]
["g","6-gang one way switch","no.",1]
["k","16 A, 6 pin, power socket coupled","no.",3]
["l","13 A, 3 pin, power socket coupled","no.",22]
["m","TV Socket","no",1]
["n","2A output USB Charger Outlet (Make: Northwest or equivalent)","no",11]
[]
[8,"2amp USB CHARGING POINTS WIRING ","pt.",11]
[null,"Supplying the materials and  concealed wiring through ceiling, false ceiling, wall of USB charging points  using  2  x 2.5sq.mm  Multistrand  Flexible wire  in  a  hard   HDP  pipe  of  size 20/25 mm. copper WIRE including cable shoes/sockets cable clamps and necessary connecting,   fixing,  chiselling  of  existing  wall  / ceiling and redoing the chiselld area with cement and   sand   mortar   as   per   the   drawings,   site conditions ,specifications and instruction all complete. (Make: Cables- prakash/Litmus/Pioneer or NS:344/2052 , HDP-NS)"]
[]
[9,"Networking/Data Points Wiring","Per Point",3]
[null,"Supply, delivery, wiring, conduit laying of computer networking points with cat 6 UTP cable (from switch to individual points) through 16 / 20mm dia. HDP pipe concealed in ceilings, walls and floors including heavy type metal box and all necessary connecting, fixing, insulation all complete. (IT ROOM TO EEIC PREMISES)"]
[null,"CABLE MAKE: NEX-1/D-LINK/AMP or equivalent"]
[]
[10,"Single Gang Face Plate with Information Outlet","Nos.",{"$f":"D99","v":3}]
[null,"Supply and installation of Computer Outlets RJ 45 , CAT 6 , single , with required facia plate and flush mounting GI  boxes "]
[null,"MAKE: D-LINK/LINK-BASIC or equivalent"]
[]
[11,"Category 6 Patch Panel"]
["a.","Supply and Installation of 24-ports, rack mounted, High­impact, flame retardant,thermoplastic or Powder­coated steel, 22/24 AWG, CAT 6a RJ-45 patch panel for Data as per specification/schedule of finishes. \n(MAKE: LINK BASIC, NEX-1 or equivalent)","Nos.",1]
[]
[12,"9U Wall Mount Rack with FAN","Nos.",1]
[null,"Supply, installation, testing and commissioning of 9U rack with fan designed to integrate wall-mounting, easy equipment access, and cable management in IT network. Adjustable rack rails with square mounting holes accommodate up to 12U of standard 19\" rackmount equipment; adjustable front and rear vertical rackmount rails; Locking, reversible Plexiglas® front door (2.7mm thick) and locking, removable side panels."]
[null,"MAKE: LINK BASIC or Equivalent"]
[]
[13,"Supply and installation of following switches:"]
["c.","Cisco SG100-16 16-port Gigabit Switch","Nos.",1]
[]
[14,"TV Point wiring","Per Point",1]
[null,"Wiring for TV Point from System Room to respective locations with RG6 Coaxial Cable and Power supply wires through in 20mm HDP pipe including MS box, juntion box, pull boxin with all required materials with necessary distributor terminal in between the TV Terminals."]
[]
[15,"EARTHING","set.",2]
[null,"Supplying materials, installation, testing, commissioning of  earthing for Building earthing  / equipments body earthing  / system earthing, consisting following specified parameters: ( provisional - to be installed if the existing ssystem does not have required minimumEarth resistance of 4-6 Ohms for Mains and 1 Ohms for System)"]
[null,"Plate Earthing"]
[null,"* Earthing with COPPER earth plate 600 mm x 600 mm x 6 mm thick including accessories, and providing masonry enclosure with cover plate having locking arrangement and watering pipe ect. (but without charcoal or coke and salt) complete as required.\n* 150mm thick alternate layers of Salt and Charcoal covering earth electrode completely.\n* Brazed jointing of earth electrode with earthing conductor including copper nut-bolts.\n* Providing of perforated 25mm. dia. GI watering pipe including earth excavation, refilling with compacted soil    in layers of maximum 300mm. thickness all complete. The contractor should responsible to maintain earthing resistance less than 5 Ohm.\n* Supply and installation of SWG no 8 gauge bare copper conductor from Earthing Stationss  3 Phase Main DB, Generator neutral and body and System"]
[]
[16,"SECURITY SYSTEMS"]
[16.100000000000001,"CC Camera point wiring","pt.",4]
[null,"Supplying and laying of CAT-6 UTP cable made of Cu with 23/60 twin dc wire inside 20/25 mm. dia. HDP materials including labour charge for laying CCTV cables   with  pull  boxes,   metal   box  all complete  and concealed  wiring  through  ceiling, false ceiling, wall, table whichever applicable including cable shoes/sockets cable clamps and necessary connecting, fixing, chiselling of existing wall / ceiling  and  redoing  the chiselld  area  with cement and sand mortar as per the drawings, site conditions ,specifications and instruction all complete. All point wiring from each CCTV (IP cameras)   to  be  terminated   to  HUB  switch (Make: HDP-NS) From server room to specified location\nCABLE BRAND: PIONEER, PRAKASH OR  NS:344/2052\nCABLE MAKE: NEX-1/D-LINK/AMP or equivalent"]
[]
[16.2,"UPS Output Power points for NVR and switch","set",2]
[null,"Supply and installatiopn of UPS Output Power points for cameras with 2 x 4 sq. mm. + 1 x 2.5 sq. mm. multistrained PVC insulated copper conductor  in  a  hard   HDP  pipe  of  size 20/25 mm from UPS DB to various points."]
[null,"CABLE BRAND: PIONEER, PRAKASH OR  NS:344/2052"]
[]
[16.3,"Supply Delivery, Installation Testing and Commissioning  of CCTV  camera/  HDVR system as per the drawing, specification all complete."]
["a","Supply, installation, testing and commissioning of 2 MP Full HD Network Small IR Dome Camera. 1/3” 2 Megapixel progressive scan Aptina CMOS, H.264 & MJPEG dual-stream encoding, 25/30 fps@ 1080P (1920×1080), DWDR, Day/Night(ICR), AWB,AGC,BLC, Multiple network monitoring: Web viewer, CMS (DSS/Smart PSS) & DMSS, 3.6mm fixed lens (2.8mm, 6mm optional), Max. IR LEDs Length 30 m, Micro SD memory(-S), IP66, IK10, PoE.\nMake:  DAHUA 1200 model or equivalent","set.",6]
["b","8 Channel Network Video Recorder (NVR) with 2 TB Hard Disk"]
[null,"Supply, installation, testing and commissioning of 8Channel Network Video Recorder (NVR) with 6 TB Hard Disk.\n>Max 256Mbps incoming bandwidth\n>Up to 8ch@1080P(4ch @H.265 + 4ch @H.264) realtime live-view\n>Up to 12Mp resolution live-view & playback\n>2HDMI/1 VGA simultaneous video output\n>8 channel synchronous realtime playback, GRID interface\n>Support Multi-brand network cameras: Dahua, Arecont Vision, AXIS, Bosch, Brickcom, Canon, CP Plus, Honeywell, Panasonic, Pelco, Samsung, Sanyo, Sony, Videotec, Vivotek and etc. \n>ONVIF Version 2.4 conformance\n>3D intelligent positioning with Dahua PTZ camera\n>Support 4 SATA HDDs up to 24TB, 3 USB(2 USB3.0), 1 eSATA port\n>Support IPC UPnP, 8PoE ports \n>Support P2P, QR code scan & add\n>Multiple network monitoring: Web viewer, CMS(DSS/Smart PSS) & Smart Phone(DMSS)\n>2 TB HDD","set.",1]
[null,"MAKE : DAHUA or quivalent"]
[]
["c","24\" LED Monitor for display - Dell or equivalent\nOptimal Resolution:1920 x 1080 at 60 Hz\nAspect Ratio:Widescreen (16:9)\nPixel Pitch:0.2745mm x 0.2745mm\nBrightness:250 cd/m2 (typical)\nColor Support:16.7 million colors\nContrast Ratio:1000: 1 (typical), Dynamic Contrast Ratio : 8 Million:1 (Max)\nBacklight Technology:LED","No",1]
[]
["e.","Category 6 Patch Panel","Nos.",1]
[null,"Supply and Installation of 24-ports, rack mounted, High­impact, flame retardant,thermoplastic or Powder­coated steel, 22/24 AWG, CAT 6a RJ-45 patch panel for Data as per specification. \n(MAKE: LINK BASIC/DIGI-LINK) or equivalent"]
[]
["f.","8 Port POE Switch","Nos.",1]
[null,"16-Port Desktop Gigabit PoE Switch - 8 Ports - 10/100/1000 Base -T - 2 Layer Supported - Wall Mountable IEEE 802.3, 802.3u, 802.3x, 802.3ab,802.3az, 802.3af, and 802.3at (PoE+) Full line rate and forwarding rate of 64B frame at: 1.488 Mpps for 1000M port,  0.1488 Mpps for 100M port, 0.01488Mpps for 10M port"]
[]
[]
[16.399999999999999,"FIRE ALARM SYSTEM INSTALLATION WORKS"]
["A","Supply , delivery, installation testing and\ncommission of following accessories as per the instruction, specification, drawing all complete."]
[]
["a","Smoke Detectors"]
[null,"Supply, installation, testing and commissioning of Optical smoke detector with base; auto compensation; digital processing algorithm; protected area - up to 120 sq. m.; low profile design; LED indication with 360 visibility; sensor status indication every 8 seconds.","nos.",6]
[null,"Make: TELETEK EECTRONICS/HORING LIH/SYSTEM SENSOR or equivalent"]
[]
["b","Fire Indication Lamp"]
[null,"Supply, installation, testing and commissioning of fire remote indicator with 1 input. The device repeats the status of 1 or several automatic fire detectors (up to 3 SensoMAG detectors series). The remote indicator operates with limited current detectors.","nos.",2]
[null,"Make: TELETEK EECTRONICS/HORING LIH/SYSTEM SENSOR or equivvalent"]
[]
["c","Hooter with flash light"]
[null,"Supply, installation, testing and commissioning of indoor conventional piezo siren (sound output - 105 dB) with red flash (LED strobe).","nos.",2]
[null,"Make: TELETEK EECTRONICS/HORING LIH/SYSTEM SENSOR or equivalent"]
[]
["d","Manual Call Point"]
[null,"Supply, installation, testing and commissioning of surface mounting Manual Call Point with resettable flexible element, LED indication and special tool for resetting after alarm event. ","nos.",2]
[null,"Make: TELETEK EECTRONICS/HORING LIH/SYSTEM SENSOR or equivalent"]
[]
["e","4 zone Fire Alarm Control Panel"]
[null,"Supply, installation, testing and commissioning of 4 zone fire panel, 12 Volt battery back-up; One man test function; 4 fully monitored fire zones with up to 32 fire alarm detectors per zone and unlimited number of call points; 2 monitored siren outputs 300 mA each; 1 “fire” and 1”fault” relay output; Active EOL allowing continuous monitoring of inputs; Walk test; Multilanguage support LED indication; Security key; Metal box.","nos.",1]
[null,"Make: TELETEK EECTRONICS (MAG 4M)/HORING LIH (AH-00212 )/SYSTEM SENSOR or eequivalent"]
[]
["f","SMOKE DETECTOR/HEAT DETECTOR/ MCP/RESPONSE INDICATOR POINT WIRING"]
[null,"Supplying the 2x1 sq.mm  Flexible Cu wires materials  and   concealed  wiring  through  ceiling, false ceiling, wall, table whichever applicable  in a hard PVT conduit of size   20/25 mm. dia. as per drawing  specifications  and  instruction  all complete.\nCABLE BRAND: PIONEER, PRAKASH OR  NS:344/2052","pt.",11]
[]
["g","SOUNDER POINT WIRING","pt.",2]
[null,"Supplying the 2x1.5 sq.mm  Flexible Cu wires materials  and   concealed  wiring  through  ceiling, false ceiling, wall, table whichever applicable  in a LISTIC/HDP pipe of size   20/25 mm. dia. as per drawing  specifications  and  instruction  all complete.\nCABLE BRAND: PIONEER, PRAKASH OR  NS:344/2052"]
[]
["h","FIRE EXTINGUISHER"]
[null,"Supply, delivery and installation of 5 Kg ABC Stored Pressure Multi-purpose type Fire Extinguisher having glow sign on cylinder with fixing accessories per the drawings, specification/schedule of finishess, electricity rules and instructions all complete.","nos.",2]
[null,"Make: NAFCO or equivalent"]
[null,null,null,"SUB-TOTAL (D)"]

{"sheet":"E. HVAC","index":5,"n_rows":44,"n_cols":6,"rows_kept":44,"cut":false,"hidden":false,"merged":[[43,3,43,4],[0,0,0,5],[1,0,1,5],[2,0,2,5],[4,0,4,5],[5,0,6,0],[5,1,6,1],[5,2,6,2],[5,3,6,3],[5,5,6,5]]}
["Client: UNDP"]
["Project : Interior Design Works of the EEIC "]
["Location : Election Commission Building, Biratnagar,  Nepal"]
[]
["Bill No. C: Furnishing Works"]
["S.No","Description of Works","Unit","Quantity","Rate","Amount\n(NRS)"]
[]
[1,"PART A"]
[null,"Supply, installaton, testing and commissioning of heat pump type split HVAC system inlcusive with fully charged refrigerant (R-410A) inclusive of interconnicting power and control cables, individual wired/wireless remote contrllers and supports made of MS angle/ rods as per specifications and drawings of following capacity \nMAKE: MITSUBISHI/LG or equivalent"]
[]
[1.1000000000000001,"4-Way Ceiling Cassette Type Indoor & Outdoor Unit with Drain Pump.","set",1]
[null,"Nominal cooling capacity: 5.8 kW"]
[null,"Nominal heating  capacity: 6.3 kW"]
[null,"Refrigearnt: R410A"]
[null,"Sound Pressure Level at high speed: 32 dBA"]
[null,"Air flow rate at high speed: 477 CFM"]
[null,"Electrical power source: 1 Ph, 220-240V, 50 Hz"]
[null,"Liquid line pipe diameter: 6.4 mm"]
[null,"Gas line pipe diameter: 12.7 mm"]
[]
[]
[null,"Type: Heat Pump"]
[null,"Capacity: 1.5 Ton ± 5%"]
[]
[1.2,"4-Way Ceiling Cassette Type Indoor & Outdoor Unit with Drain Pump.","set",3]
[null,"Nominal cooling capacity: 7.1 kW"]
[null,"Nominal heating capacity: 8 kW"]
[null,"Refrigearnt: R410A"]
[null,"Sound Pressure Level at high speed: 50 dBA"]
[null,"Air flow rate at high speed: 741 CFM"]
[null,"Electrical power source: 1 Ph, 220-240V, 50 Hz"]
[null,"Liquid line pipe diameter: 9.5 mm"]
[null,"Gas line pipe diameter: 15.9 mm"]
[]
[null,"Type: Heat Pump"]
[null,"Capacity: 2.0 ± 5%"]
[]
[2,"PART B"]
[null,"Installation between indoor to outdoor unit including all required installation materials like copper tube, gas, insulation tube, electrical wiring of the following capacity:"]
[2.1,"Installation charges for Ceiling Cassette units","Nos.",4]
[2.2000000000000002,"Outdoor supporting angles","Nos.",4]
[2.2999999999999998,"Extra piping","M.",40]
[]
[null,null,null,"SUB-TOTAL (E)"]

{"sheet":"List of samples required","index":6,"n_rows":31,"n_cols":5,"rows_kept":31,"cut":false,"hidden":false,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5]]}
["Client: UNDP"]
["Project : Interior Design Works of the EEIC "]
["Location : Election Commission Building, Biratnagar,  Nepal"]
[]
[]
["S.No","Description","Qty","Capacity/Size","Make"]
["A","Samples to be provided"]
[1,"Wood "]
[2,"Marble"]
[3,"Block Board"]
[4,"Ply"]
[5,"Laminate"]
[6,"Blind"]
[7,"Gypsum board"]
[8,"Frame of grid ceiling"]
[9,"Board of grid ceiling"]
[10,"Light fixtures"]
[11,"Switches"]
[12,"Power sockets"]
[13,"USB charging outlet"]
[14,"Switch gear"]
[15,"House wires"]
[16,"Network cables"]
[]
["B","Catelogue to be provided"]
[1,"Security systems"]
[2,"Fire alarm system"]
[3,"Survelliance system"]
[4,"HVAC System"]
[5,"Network switch"]
[6,"FIre Extinguishers"]