{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":48,"n_cols":6,"rows_kept":48,"cut":false,"hidden":false,"merged":[[0,1,0,5],[19,5,20,5],[19,0,20,0],[15,0,16,0],[17,0,18,0],[15,2,16,2],[15,3,16,3],[15,4,16,4],[15,5,16,5],[17,2,18,2],[17,3,18,3],[17,4,18,4],[17,5,18,5],[13,0,14,0],[13,2,14,2],[13,3,14,3],[7,5,8,5],[13,4,14,4],[13,5,14,5],[1,1,1,5],[11,5,12,5],[9,5,10,5],[7,0,8,0],[7,2,8,2],[7,3,8,3],[21,1,21,4],[19,2,20,2],[19,4,20,4],[19,3,20,3],[7,4,8,4],[11,0,12,0],[11,2,12,2],[11,3,12,3],[11,4,12,4],[9,0,10,0],[9,2,10,2],[9,3,10,3],[9,4,10,4],[33,5,34,5],[27,1,27,5],[31,0,32,0],[31,2,32,2],[31,3,32,3],[31,4,32,4],[31,5,32,5],[29,2,30,2],[29,3,30,3],[29,4,30,4],[29,5,30,5],[29,0,30,0],[39,0,40,0],[39,2,40,2],[39,3,40,3],[39,4,40,4],[39,5,40,5],[43,5,44,5],[41,0,42,0],[41,2,42,2],[41,3,42,3],[41,4,42,4],[41,5,42,5],[45,1,45,4],[43,0,44,0],[43,2,44,2],[43,3,44,3],[43,4,44,4],[37,5,38,5],[35,0,36,0],[35,2,36,2],[35,3,36,3],[35,4,36,4],[35,5,36,5],[25,1,25,4],[37,0,38,0],[37,2,38,2],[37,3,38,3],[37,4,38,4],[33,0,34,0],[33,2,34,2],[33,3,34,3],[33,4,34,4],[3,0,4,0],[3,2,4,2],[3,3,4,3],[3,4,4,4],[3,5,4,5],[5,0,6,0],[5,2,6,2],[5,3,6,3],[5,4,6,4],[5,5,6,5]]}
[null,"Rehabilitation of Sinuni Wells"]
[null,"Estimated Bill of Quantities of Rehabilitation and Maintenance Works of 2 Bakhalif  Water Wells- Sinuni Sub-District / Ninwa Governorate "]
["#","Items Description","Unit","Qty.","Unit Price $","Total $"]
["1-","Supply submersible pump motor 18 Kwatt                           as in Annex A ","No",2]
[null,"تجهيز محرك لغطاس ابار    قدرة 18 كيلووات"]
["2-","Supply submersible water pump Original                   (H=120M ) (Q=30-35M3/sec)                                      as in annex B ","No",2]
[null,"تجهيزمضخة غطاس ابار بمواصفات :                                    (H=120M ) (Q=30-35M3/sec)"]
[3,"Supply materials, tools and manpower to install motor starter board  for (22Kwatt 30Hp )water pump auto transformer type including 100Amps 3ph MCCB with all protection units and phase faller, 2 transformers , voltage, amps ,frequency meters and indication lamps contactors must be from approving manufacture with all accessories and manpower ","No",2]
[null,"تجهيز بورد ستارتر قدرة (22) كبلو واط و(30)حصان نوع اوتو ترانسفورمر يحتوي على قاطع رئيسى (100) امبير مع اجهزة حماية  وفيزفيلر ومحولتين مع مقياس التيار والفولتية والمصابيح الااشارة وكافة الملحقات وتكون كونتاكترات من المنشاء رصين وكل ما يتطلبه العمل من اعمال الربط والفحص "]
["4-","Supply materials as requested for required work for lifting and removing existing pump old diver with pipes completely out of the well and re installation new one download of the new pump with new pipes comprehensive price to do the processing and connecting the new cable (4 * 10) mm 2 capillary Double cover rubber type between the pump and operation Board supply and install power cable e (4*16mm 2) .","No",2]
[null,"تجهيز ما يلطبه   العمل  من المواد والقيام بالاعمال رفع طاقم الغطاس القديم مع الانابيب بالكامل من البئر مع تنزيل الطاقم الجديد مع الانابيب الجديدة شاملا السعر القيام باعمال تجهيز وربط الكيبل الجديد (4*10)ملم2 نوع شعري دبل غلاف مطاطي بين الغطاس و بورد التشغيل مع ربط مصدر الطاقة ربط وتجهيز كيبل (4*16)ملم2 وكل ما يتطلبه العمل "]
["5-","Supply 3' galvanize water pipe heavy type from good manufacturer (Saudi Arabia or Turkish)","ML",200]
[null,"تجهيز انابيب قطر 3انج حديد مغلون نوع ثقيل خاص بالابار ومن منشاء جيد (تركي او سعودي)"]
[6,"supply and install Change over board ATS  100Amps  contactors must be from approving manufacture with all accessories and manpower ","No",2]
[null,"تجهيز وتركيب حنج اوفر 100امبير نوعية جيدة مع كل مايتطلبه العمل من اعمال الربط والفحص والتشغيل "]
[7,"Supply materials, tools and manpower to repair and  maintenance water well generators (50KVA), including repair and maintenance of damaged parts changing  not repairable parts battery, motor starters oil ,fuel filters with all other required works to be don to operate generators  ","No",2]
[null,"قيام بتصلح وادامة المولدات الخاصة بالابار قدرة (50)كي في ئةي ويشمل العمل تصليح اجزااء المتضررة مع تبديل اجزاء التالفة او الناقصة من البطاريات ,سلف ,شاحنة باتري مع كل ما يتطلبه العما "]
[8,"Supply materials, tools and manpower to install steel door double side plate gauge 18mm dimensions (2m*2.5m)  total price includes key unit and painting  anti corrosion paint and 2liyar ,oil type paint and all other required accessories ","No",3]
[null,"تجهيز وتركيب باب حديد ركم وجهين كيج 18ملم بابعاد (2*2.5)م ا كاملا السعر يتضمن اعمال تركيب كبلون وصبغ الاساس والصبغ الدهني طبفطين  وكل ما يتطلبه العمل "]
[9,"Supply materials, tools and manpower to Install new water pipe  line diameter 6\"inch PVC from project to compound with all required work and material to excavation over damage pipe line and other repair materials ","ML",50]
[null,"تجهيز ما يتطلبه ومايلزم من المواد والقيام بالاعمال  تغير موقع الشمعة من الربط المباشر على بير رقم 2وتحويل الربط الى الخزان الكونكريتي او الحديدي في موقع شرف الدين شاملا العمل تجهيز ومد وربط انابيب قطر 3انج مغلون الى موقع الربط الذي يتم اختاره المهندس المشرف   . "]
[null,"Total Cost in US Dollars       ",null,null,null,{"$f":"SUM(F4:F21)","v":0}]
[]
[]
[]
[]
[]
[null,"Estimated Bill of Quantities of Rehabilitation and Maintenance Works of No.1and No.7 Sherfaden Water Wells - Senuni Sub-District / Ninwa Governorate  "]
["#",11,"Unit","Quantity","Price $","Total $"]
["1-","Supply submersible pump motor 18 Kwatt                         as in annex A ","No",2]
[null,"تجهيز محرك لغطاس ابار قدرة 18 كيلووات"]
["2-","Supply submersible water pump Original                     (H=120M ) (Q=30-35M3/sec)                                               as in Annex B ","No",2]
[null,"تجهيزمضخة غطاس ابار  بمواصفات :                                   (H=120M ) (Q=30-35M3/sec)"]
["3-","Supply materials, tools and manpower to install motor starter board  for (22Kwatt 30Hp )water pump auto transformer type including 100Amps 3ph MCCB with all protection units and phase faller, 2 transformers , voltage, amps ,frequency meters and indication lamps contactors must be from approving manufacture with all accessories and manpower ","No",2]
[null,"تجهيز بورد ستارتر قدرة (22) كبلو واط و(30)حصان نوع اوتو ترانسفورمر يحتوي على قاطع رئيسى (100) امبير مع اجهزة حماية  وفيزفيلر ومحولتين مع مقياس التيار والفولتية والمصابيح الااشارة وكافة الملحقات وتكون كونتاكترات من المنشاء رصين وكل ما يتطلبه العمل من اعمال الربط والفحص "]
["4-","Supply materials as requested for required work for lifting and removing existing pump old diver with pipes completely out of the well and re installation new one download of the new pump with new pipes comprehensive price to do the processing and connecting the new cable (4 * 10) mm 2 capillary Double cover100m  rubber type between the pump and operation Board supply and install power cable e (4*16mm 2) 40m ","No",2]
[null,"تجهيز ما يلطبه   العمل  من المواد والقيام بالاعمال رفع طاقم الغطاس القديم مع الانابيب بالكامل من البئر مع تنزيل الطاقم الجديد مع الانابيب الجديدة شاملا السعر القيام باعمال تجهيز وربط الكيبل الجديد (4*10)ملم2 نوع شعري دبل غلاف مطاطي بين الغطاس و بورد التشغيل 100متر مع ربط مصدر الطاقة ربط وتجهيز كيبل (4*16)ملم2و 40 متر وكل ما يتطلبه العمل "]
["5-","Supply 3' galvanize water pipe heavy type from good manufacturer (Saudi Arabia or Turkish)","ML",200]
[null,"تجهيز انابيب قطر 3انج حديد مغلون نوع ثقيل خاص بالابار ومن منشاء جيد (تركي او سعودي)"]
["6-","Supply materials, tools and manpower to install Change over board ATS  100Amps  contactors must be from approving manufacture with all accessories and manpower ","No",2]
[null,"تجهيز وتركيب حنج اوفر 100امبير نوعية جيدة مع كل مايتطلبه العمل من اعمال الربط والفحص والتشغيل "]
["7-","Provide materials, tools and manpower to repair and  maintenance water well generators (50KVA) by changing the damaged parts, battery, motor starters oil , fuel filters with all other required works to be don and operate generators  ","No",5]
[null,"قيام بتصلح وادامة المولدات الخاصة بالابار قدرة (50)كي في ئةي ويشمل العمل تصليح اجزااء المتضررة مع تبديل اجزاء التالفة او الناقصة من البطاريات ,سلف ,شاحنة باتري مع كل ما يتطلبه العما "]
["8-","Provide  materials, tools and manpower  to relocate water tap from direct connection with water well  No.2 to the metal or concrete water tank  in Sharfadeen location. The work includes supply and install and connection of galvanize  pipe line 3\" inch and all other required works  ","ML",30]
[null,"تجهيز ما يلطه يزم من المواد والقيام بالاعمال تغير موقع الشمعة من الربط المباشر مع بئر  رقم2 وتحويل ربطه بالخزان الكنكريتي او الحديدي في الموقع ابار شرف الدين شاملا العمل تجهيز ومد وربط انابيب قطر  3 عقدة  مغلون الى الموفع العمل الذي يتم اختباره  وكل ما يتطلبه العمل "]
[null,"Total Cost in US Dollars "]
[]
[null," Estimated Total Cost of Rehabilitation Sinuni Wells in US Dollars",null,null,"LOT 1"]