{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Al-Nahrawan WTP-Add. works"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Al-Nahrawan WTP-Add. works","index":0,"n_rows":14,"n_cols":6,"rows_kept":14,"cut":false,"hidden":false,"merged":[[2,1,2,5],[0,0,0,5],[1,1,1,5]]}
[" Bill of Quantities (BOQ) "]
[null,"اسم المشروع:  تجهيز ونصب مواد أضافية لمشروع مضخات خام النهروان"]
[null,"RFQ-139/16  Supply and Installation  of additional Equipment for Al- Naharwan Water Plant, Baghdad Governorate"]
[]
["No.","Materials/Items description/ Labor ","Unit","Quantity","Unit Price","Total Cost USD "]
[1,"Supply, install Ductile Double Flanged (gear box) Butterfly Valve Dia 400mm, PN25, GG50 (Manual).          Materials: Ductile Iron EN-JS 1030 Double Flanged.         Final Inspection test according to EN-12266                   Corrosion Protection: Internally and externally epoxy coated. Brand: VAG or any equivalent manufacturer per attached catalogue Annex -(1) with warranty available on site. All that requires work and as directed by the supervising engineer.       ","Ea",4,null,{"$f":"D6*E6","v":0}]
[2,"Supply, install Ductile valve (gear box) Butterfly Valve/ Dia 500mm, PN25, GG50 Double Flanged (Manual). Materials: Ductile Iron EN-JS 1030.    Final Inspection test acc. to EN-12266.  Corrosion Protection: Internally and externally epoxy coated. Brand: VAG or any equivalent manufacturer as per attached catalogue Annex -(1) with warranty available on site.  All that requires installation work and as directed by the supervising engineer.                                                            ","Ea",2,null,{"$f":"D7*E7","v":0}]
[3,"Supply, install Non-return Valve Double Flanged (Anti -retraction) dia 400mm, PN16, GG50 (Standard).                Materials: Ductile Iron EN-JS 1030  ( Final Inspection test according to EN-12266.   Corrosion Protection: Inside and Outside epoxy coating. Brand type: VAG or any equivalent manufacturer as per attached catalogue Annex -(1) with warranty available on site. All that requires installation work and as directed by the supervising engineer.  ","Ea",2,null,0]
[4,"Supply, install Ductile Double Flanged valve (gear box) Butterfly Valve Dia 350mm, PN25, GG50 double Flanged (Manual) Materials: Ductile Iron EN-JS 1030.                     Final Inspection test acc. to EN-12266    Corrosion Protection: Internally and externally epoxy coated. Brand type: VAG or any equivalent manufacturer as per attached catalogue Annex -(1) with warranty available on site.  All that requires installation work and as directed by the supervising engineer.  ","Ea",2,null,0]
[5,"Supply, install Reto - Stop Non Return Valve, dia 250mm, PN16, GG50 Double Flanged. Materials: Ductile Iron EN-JS 1030, Final Inspection test acc. to EN-12266    Corrosion Protection: Inside and Outside epoxy coating.  Brand type: VAG or any equivalent manufacturer as per attached catalogue Annex -(1) with warranty available on site. All that requires installation work and as directed by the supervising engineer.  ","Ea",4,null,0]
[6,"Supply, install Ductile Butterfly Valve (gear box) Dia 300 mm, PN16, GG50 double Flanged (Manual). Materials: Ductile Iron EN-JS 1030,   Final Inspection test acc. to EN-12266.  Corrosion Protection: Inside and Outside epoxy coating.   Brand type: VAG or any equivalent manufacturer as per attached catalogue Annex -(1) with warranty available on site. All that requires work and as directed by the supervising engineer.  ","Ea",4,null,0]
[7,"Supply, install and operate the Air Conditioning Split Unit equipment, Free Stand Floor -capacity (3 tons) with the required Testing. Cost includes supplying materials, necessary tools and manpower to install the units in the Distribution Boarders' room and pumping hall with all electrical connections including the wiring and safety system. The cost includes provide circuit breaker 32 Amps capacity connect with source intake and drain water pipe to maintain its operation properly. All electrical connection and wires 3x4 mm2 should be covered by a plastic sleeve with protracted box for external part, with minimum one-year Warranty for the supplied equipment. All that requires as directed by the supervising engineer.  ","Ea",5,null,0]
[8,"Supply materials and manpower to design and install the Sign Board for Al-Nahrawn Water project to be fixed on project Site. Dimensions of board (2.5mX 1.5m). The Design should include logos of UNDP, End-User's and counterpart’s logo and to be finalized by UNDP in collaboration with the End-users in consistent with UNDP's rules and regulation for Branding. Cost includes casting the Concrete Foundation (60 cm X 60cmX 0.8m depth) inclined slip base with fixing the Post supports, type: Steel Square Tube (2.5\"X2.5\" square) 2 Each and 2m height/ each, with all necessary materials including: Anchor bolts (1\" Dia by 50 cm length) set of 4 / each post; Steel Clamps (4 Each) to use for connecting the Sign Board to the posts. All parts should be fixed and connected with screws and welding, with completion of all works under the direction of the supervisor engineer.","Ea",1,null,0]
[null,"Total Offered Price  in U.S. Dollars ",null,null,null,{"$f":"SUM(F6:F13)","v":0}]