{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":16,"n_cols":8,"rows_kept":16,"cut":false,"hidden":false,"merged":[]}
[null,null,"Bill of Quantity"]
[null,null,"Rehabilitation of the Water Lines in Tameem    تاهيل الخط الناقل في تاميم "]
[null,null," Ramadi - Anbar"]
["#","Item","Unit","Quantity","Price $","Total $"]
[1," Supply and Install Ductile Iron Pipe 600mm diameter , 25 bar atmospheric pressure as per enclosed technical specifications,which  provide the water for Al Ta'meem Area ,The works includes trench pipeline excavation 120cm deep, 100cm wide, 50 cm River sand bedding around the Pipe, 70cm selected suitable backfill material with compaction, The price should includes connection with existing pipe line from both end,testing,commissioning, removing and cleaning the pipeline alignment from the accumulated water, and all the works that required to complete the Job.Please see attached trench excavation cross- section\n ","M.l",1200,null,null,null," "]
[null," تجهيز وحفر ومد وربط انبوب دكتايل قطر 600 ملم وبضغط 25 بار  للانبوب الناقل لخط التأميم في المنطقة الواقعة في الحديقة العامة مقابل جامع الشافعي في التأميم ,يتم الفحص والتجهيز حسبب المواصفة المرفقة في الملحق أ  شاملا السعر تجهيز الحلقة المطاطية للانبوب ويكون عمق الحفر ما لا يقل عن 120 سم مع دفن الانبوب بوسادة من الرمل النهري بسمك 50 سم حول الانبوب وتكملة باقي الدفن بالتراب النظيف مع الحدل مع سحب المياه المتجمعة في مسار الانبوب والدفن وحسب مخطط المقطع العرضي المرفق مع كل متطلبات العمل."]
[2," supply and Install  600 mm diameter ductile Iron elbow 90°   of double flange with all the required works ","Ea.",2,null,null,null," "]
[null," تجهيز وربط عكس دكتايل قطر 600 ملم وبزاوية 90 درجة دبل فلانج مع كافة متطلبات العمل "]
[3," supply and Install  ductile Iron socket flange  of  600 mm diameter with all the required works.","Ea.",4]
[null," تجهيز وربط سوكت فلانج قطر 600 ملم للانبوب الدكتايل مع كافة متطلبات العمل "]
[4," supply and Install  of ductile Iron coupling  pipe of 600 mm diameter with all the required works","Ea.",4]
[null,"تجهيز وربط كوبلن جونسون للانبوب الدكتايل قطر 600 ملم مع كافة متطلبات العمل "]
["Total Cost $"]
[{"$nulls":7}," "]
[]
[{"$nulls":6}," "]