{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["for ITB","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"for ITB","index":0,"n_rows":67,"n_cols":8,"rows_kept":67,"cut":false,"hidden":false,"merged":[[35,1,35,3],[40,1,40,3],[52,1,52,3],[65,1,65,3],[65,4,65,6],[15,1,15,3],[14,1,14,3],[13,1,13,3],[12,1,12,3],[9,1,9,3],[10,1,10,3],[11,1,11,3],[45,1,45,3],[46,1,46,3],[36,1,36,3],[43,1,43,3],[44,1,44,3],[37,1,37,3],[38,1,38,3],[39,1,39,3],[41,1,41,3],[42,1,42,3],[28,7,29,7],[28,4,29,6],[28,1,29,3],[62,1,62,3],[64,1,64,3],[56,1,56,3],[59,1,59,3],[57,0,58,7],[63,1,63,3],[60,1,60,3],[61,1,61,3],[26,1,26,3],[27,1,27,3],[55,4,55,6],[55,1,55,3],[33,0,33,7],[31,0,32,7],[30,1,30,3],[49,1,49,3],[50,1,50,3],[51,1,51,3],[53,1,53,3],[54,1,54,3],[47,1,47,3],[48,1,48,3],[34,1,34,3],[16,1,16,3],[17,1,17,3],[18,1,18,3],[23,1,23,3],[25,1,25,3],[19,1,19,3],[20,1,20,3],[21,1,21,3],[22,1,22,3],[24,1,24,3],[5,7,6,7],[7,0,8,7],[1,0,4,7],[5,0,6,0],[5,1,6,3],[5,4,6,4],[5,5,6,5],[5,6,6,6]]}
[]
["BoQs Of Rehabilitation of Qayara Water Project "]
[]
[]
[]
["#","Item of Description",null,null,"Unit ","Qty.","Unit Cost","Amount"]
[]
["A. Mechanical Works "]
[]
[1,"Supply , Install and operate Multi stage pump capacity 400m³/hr and 100 head, with Bronze Impeller, Stainless steel shaft, speed 1500 rpm, IP 55, Main frequency 50Hz, Control panel for the pump; Auto/Manual type, Voltage 380-400Va, rated  V3, Power approximate 110KW, 147.5 HP, cupper coil.  The price should includes all necessary accessories and required connections to complete the Job.  certificate of origin and BV test certificate is required.",null,null,"EA ",4]
[2,"Supply, install and operate split case horizontal pump capacity 500m³/hr and 40m head, with Bronze impeller, stainless steel shaft, speed 1500rpm, IP55, main frequency 50Hz, control panel for the Pump: Auto/Manual type , Voltage 380-400Va, rated V3, power approximate 90KW, cupper coil. The price should includesreplacing the old suction pipes and strainer with suitable size and backwash system for strainer with all necessary accessories and required connections to complete the Job. certificate of origin and BV test certificate is required.",null,null,"EA ",2]
[3,"Supply, install , and operate submersible pump river type capacity 400m³/hr at 40m head, with float,  speed 1500rpm, impeller from cast iron, power input 50Hz,  Voltage 380-400Va, rated V3phase, Motor IP 68, Isolation class f. The price should include electrical motor suitable to pump capacity including the Automatic control panel with suitable circuit breaker, with all necessary accessories and required connections to complete the Job. certificate of origin and BV certificate is required.",null,null,"EA ",4]
[4,"Supply, Install, and operate chlorination dosing device 4kg/hr complete with Injector and cupper piping. The price should include 1mm steel protection cage , with all the necessary fittings, accessories and connections with the PVC pipes.",null,null,"EA ",2]
[5,"Supply, install and operate Alum dosing pump capacity 500l/hr and 50m head. The price should includes dismantling the old unit, with all the required accessories and works to complete the Job.",null,null,"EA ",2]
[6,"Supply, install and operate alum mixer of capacity 0.37-0.75 KW , speed 1420rpm, 0.9m length, stainless steel shaft. The price should include all necessary accessories and connections to complete the Job.",null,null,"EA ",4]
[7,"Supply of protective mask anti chlorine gases complete with all necessary accessories and suitable filter. Certificate of origin is required. ",null,null,"EA ",6]
[8,"Supply of sealant  Packing with graphit  size (16 mm)",null,null,"Kg",50]
[9,"Supply of sealant Packing with graphit size (14 mm)",null,null,"Kg",50]
[10,"Supply of sealant Packing with graphit  size (12 mm)",null,null,"Kg",50]
[11,"Supply of sealant  Packing with graphit size (10 mm)",null,null,"Kg",50]
[12,"Supply of sealant Packing with graphit size (8 mm)",null,null,"Kg",50]
[13,"Supply and install submersible pumps with starter for discharge open hole 2\"  the water from Sedimmation tanks . Q=40m³/hr and H=20m",null,null,"EA ",2]
[14,"Supply and install submersible pumps the open hole 1'' with starter. Q=5m³/hr and H=20m ",null,null,"EA ",2]
[15,"supply of dossing Greaser pumps large size ",null,null,"EA ",2]
[16,"supply of dossing Greaser pumps small size ",null,null,"EA ",2]
[17,"Supply of  Grease for lubrication , type LS3",null,null,"KG",100]
[18,"Supply fire extinguisher size 5 kg",null,null,"EA ",15]
[19,"Supply fire extinguisher size 10 kg",null,null,"EA ",10]
[{"$nulls":4},"Total A ",null,null,{"$f":"SUM(H10:H28)","v":0}]
[]
[]
["B. Supply Pipe & Fittings "]
[]
["All PVC Pipe and fitting should comply with PVC, AWWA Pipe:  AWWA C900, Class 200, or  equivalent PN 10 pressure class ISSO 4422/EN1452 UPVC Water Main, with bell end with gasket, and with spigot end. All Ductile Iron Pipe and fittings should comply with EN 545 , 2010. Pls see relevant annex."]
["1-","Supply ductile Iron pipe of PN10 (12 in) diameter",null,null,"L.M",60]
["2-","Supply PVC Pipes PN10 (12 in) diameter  ",null,null,"L.M",120]
["3-","Supply PVC  Pipes PN10 (10 in) diameter  ",null,null,"L.M",120]
["4-","Supply PVC Pipes PN10 (8 in) diameter ",null,null,"L.M",120]
["5-","Supply PVC Pipes PN10 (6 in) diameter  ",null,null,"L.M",300]
["6-","Supply PVC Pipes PN10 (4 in) diameter ",null,null,"L.M",2500]
["7-","Supply PVC Valve  PN10 (8 in) diameter  ",null,null,"EA",20]
["8-","Supply PVC Gate Valve  PN10 (6\" Dia)  , complete with all accessories",null,null,"EA",25]
["9-","Supply PVC Valve  PN10 (4\" Dai) , complete with all accessories ",null,null,"EA",40]
["10-","Supply ductile Iron coupling Johnson conductor complete with all accessories of PN10 (12 in) diameter",null,null,"EA",20]
["11-","Supply ductile Iron coupling Johnson conductor complete with all accessories of PN10 (10 in) diameter",null,null,"EA",20]
["12-","Supply ductile Iron coupling Johnson conductor complete with all accessories of PN10 (8 in) diameter",null,null,"EA",20]
["13-","Supply ductile Iron coupling Johnson conductor complete with all accessories of PN10 (6 in) diameter",null,null,"EA",30]
["14-","PVC mechanical coupling Joint  (12 in)",null,null,"EA",40]
["15-","PVC mechanical coupling Joint  (10 in)",null,null,"EA",40]
["16-","PVC mechanical coupling Joint (8 in)",null,null,"EA",50]
["17-","PVC  mechanical coupling Joint  (6 in)",null,null,"EA",70]
["18-","PVC mechanical coupling Joint (4 in)",null,null,"EA",110]
["19-","PVC Elbow 45 Degree  (8 in)",null,null,"EA",10]
[20,"PVC Elbow 45 Degree  (6 in)",null,null,"EA",15]
[21,"PVC Elbow 45 Degree  (4 in)",null,null,"EA",20]
[{"$nulls":4},"Total B",null,null,{"$f":"SUM(H37:H55)","v":0}]
[]
["C. Electric Works "]
[]
["1-","Supply Electric Conductor various rating capacity ",null,null,"EA",10]
["2-","Supply Circuit Breakers (800 AMP) , Schneider, ABB or equivalent ",null,null,"EA",4]
["3-","Supply Circuit Breakers (600 AMP) ,Schneider, ABB or equivalent ",null,null,"EA",6]
["4-","Supply Circuit Breakers (400 AMP) ,Schneider, ABB or equivalent ",null,null,"EA",8]
["5-","Supply, install and operate new electrical transformer capacity 1000 KVA , 11-0.4 KV with\nfollowing specifications\nH.V:11000V\nFrequenc5 50 Hz, 3ph\nL.Y:416 /240V, DYN 1l\nONAN Type of cooling From a good country of origin, with origin certificate and according to Iraqi standards D26",null,null,"EA",2]
["6-","Supply and lay Cables PVC, 3*35mm+E  for pumping room ",null,null,"L.M",100]
[{"$nulls":4},"Total C",null,null,{"$f":"SUM(H47:H65)","v":0}]
[null,null,null,"Total Cost in US Dollars",null,null,null,{"$f":"H66+H56+H29","v":0}]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}