

|  |
| --- |
|  |

**Table # 2: Technical Compliance Table**

***Tablo # 2: Teknik uyumluluk Tablosu***

Offerors shall fill out below table in English by indicating the Brand Name and Part number of the products offered as well as the specifications of the offered products corresponding to the specifications listed in below table.

*Teklif sahipleri aşağıdaki tabloyu İngilizce olarak, önerdikleri ürünlerin marka ve parça numaraları ve aynı zamanda, aşağıda belirtilen teknik özelliklere karşıllık gelecek şekide sundukları ürünlerin teknik detaylarını girerek eksiksiz olarak doldurmalıdır.*

|  |  |  |
| --- | --- | --- |
| **#** | **Requested Technical Specifications** | **Your Offer (Please fill out with the specifications you propose)** |
| **1** | **Two-person school desks for adults:*****Çift kişilik yetşkin okul sırası:***  | **Brand Name and Part No:** |
|  | 1.1 | Height of the desk: 70-80 cm |  |
| 1.2 | Desk board dimension: 110 x 45 |  |
| 1.3 | Height of the seat: 40-50 cm |  |
| 1.4 | Desk board shall be manufactured out of Werzalit material |  |
| 1.5 | All metal parts shall be coated with electrostatic powder paint |  |
| 1.6 | Color of desk board: Cream |  |
| 1.7 | Color of metal profile tubes: blue, grey or orange  |  |
| 1.8 | Shall be manufactured in compliance with TSE 4616 |  |
| 1.9 | The main metal frame including the frame of the seat shall be made from oval shaped hollow metal profile tubes with dimension of 25 x 50 x 1,5 mm |  |
| 1.10 | All metal connectors aside from the main frame shall be made from oval shaped hollow metal profile tubes with dimension of 15x30x1,5 mm |  |
| 1.11 | Seat and backrest shall be manufactured from either Werzalit or PPC material. |  |
| 1.12 | Pictures or drawings of the proposed equipment shall be presented in the proposal. |  |
| 1.13 | All goods shall be assembled at the delivery point and the cost shall be included in unit prices offered |  |
| 1.14 | All goods shall be delivered within 40 days after signature of the contract by UNDP and the Contractor |  |
| **2** | **Teacher’s desk:*****Öğretmen masası:*** | **Brand Name and Part No:** |
|  | 2.1 | Dimension: 120 L x 60 W x 75 H (cm) |  |
| 2.2 | Main metal frame shall be manufactured from hollow 30x30x1,5 mm metal profile. |  |
| 2.3 | The table must contain two drawers |  |
| 2.4 | The drawers should comprise metal handles and should have locking mechanisms. |  |
| 2.5 | All wooden boards including the table and side panels should be of 18mm thick melamine coated chipboard. |  |
| 2.6 | All sides on the edges of the table board should be PVC coated |  |
| 2.7 | All metal bearings that has direct contact with the floor should have plastic footing |  |
| 2.8 | Pictures or drawings of the proposed equipment should be presented in the proposal. |  |
| 2.9 | All goods shall be assembled at the delivery point and the cost shall be included in unit prices offered |  |
| 2.10 | All goods shall be delivered within 40 days after signature of the contract by UNDP and the Contractor |  |
| **3** | **Teacher’s chair*****Öğretmen koltuğu:*** | **Brand Name and Part No:** |
|  | 3.1 | Dimension: 52Lx50Wx45H (cm) |  |
| 3.2 | The chair height and back incline should be adjustable via dual mechanism |  |
| 3.3 | The chair and back rest should be ergonomic and monobloc; comprised of fabric covered sponge over 12 mm thick plyboard. |  |
| 3.4 | The sponge filler should be 32 density. |  |
| 3.5 | The chair bearing for footing and armbands should be chrome coated, foot bearing should be star shaped |  |
| 3.6 | The chair should have plastic trunnions under the chorome bearings. |  |
| 3.7 | The armbands should be covered with plastic. |  |
| 3.8 | Pictures or the drawings of the proposed equipment should be presented in the proposal |  |
| 3.9 | All goods shall be assembled at the delivery point and the cost shall be included in unit prices offered |  |
| 3.10 | All goods shall be delivered within 40 days after signature of the contract by UNDP and the Contractor |  |
| **4** | **Teacher’s cabinet:*****Öğretmen dolabı:*** | **Brand Name and Part No:** |
|  | 4.1 | Dimension: 80Lx40Wx190H (cm) |  |
| 4.2 | Must be wooden with melamine coated chipboards. |  |
| 4.3 | Manufactory must be via screws and/or dowel pins. |  |
| 4.4 | The cabinet should contain 4 doors with locking mechanisms installed on every door. The upper doors should be glass with wooden frames. |  |
| 4.5 | All the edges of the boards should be covered with PVC band. |  |
| 4.6 | Pictures or the drawings of the proposed equipment should be presented in the proposal |  |
| 4.7 | All goods shall be assembled at the delivery point |  |
| 4.8 | All goods shall be delivered within 40 days after signature of the contract by UNDP and the Contractor |  |
| **5** | **Projector:** ***Projektör:*** | **Brand Name and Part No:** |
|  | 5.1 | Projection system: DLP |  |
| 5.2 | Shall have 3D support |  |
| 5.3 | Min. Native resolution: 800x600 |  |
| 5.4 | Compressed resolution: 1920x1200 |  |
| 5.5 | Aspect ratio: 16:9 |  |
| 5.6 | Brightness: 3500 ANSI Lumen |  |
| 5.7 | Contrast ratio: 20.000/1 |  |
| 5.8 | Light source: Lamp |  |
| 5.9 | Light source wattage: 200 watts |  |
| 5.10 | Min. Light source life: 4000 hrs. normal 6000 hrs. economy |  |
| 5.11 | Max. weight: 3 kg |  |
| 5.12 | Two (2) years manufacturer guarantee period is required |  |
| 5.13 | All goods shall be delivered within 40 days after signature of the contract by UNDP and the Contractor |  |
|  | 5.14 | An authorization letter signed by the authorized representative of the manufacturer or dealer shall be provided, if the offeror is not an authorized firm |  |
|  | 5.15 | Brochure or Catalog shall be provided |  |
| **6** | **Projector screen:*****Projektör Perdesi:*** | **Brand Name and Part No:** |
|  | 6.1 | Min. Dimensions: 180 x 180 cm |  |
| 6.2 | With aluminum alloy roller  |  |
| 6.3 | With Pull stop-start feature to easy adjust projection height |  |
| 6.4 | With wall bracket attachment and hanging ceiling D hooks for simple installation |  |
| 6.5 | With standard black masking borders on all sides for excess light absorption |  |
| 6.6 | Matte Polysilicate based screen fabric with black backing |  |
| 6.7 | Two (2) years manufacturer guarantee period is required |  |
| 6.8 | All goods shall be delivered within 40 days after signature of the contract by UNDP and the Contractor |  |
|  | 6.9 | Brochure or Catalog shall be provided |  |
| **7** | **Split system air conditioner:*****Split Klima:*** | **Brand Name and Part No:** |
|  | 7.1 | Type: Residential Inverter |  |
| 7.2 | Cooling capacity: 9000 BTU |  |
| 7.3 | Energy consumption class (cooling): A++ |  |
| 7.4 | Energy consumption class (heating): A |  |
| 7.5 | Rated EER (W/W): 6.1 |  |
| 7.6 | Refrigerant: Eco friendly R410A  |  |
| 7.7 | Filter Type: Catechin, ionizer, washable filter |  |
| 7.8 | Operation: Remote and LCD display |  |
| 7.9 | Noise level (indoor): ≤ 50 dBA |  |
| 7.10 | A/C units should have built in electronic shock guard mechanisms |  |
| 7.11 | The A/C units are required to be installed at the designated locations. Cost of installation and tubing shall be included in the price offer |  |
| 7.12 | Two (2) years manufacturer guarantee period is required |  |
| 7.13 | All goods shall be delivered within 40 days after signature of the contract by UNDP and the Contractor |  |
|  | 7.14 | An authorization letter signed by the authorized representative of the manufacturer or dealer shall be provided, if the offeror is not an authorized firm |  |
|  | 7.15 | Brochure or Catalog shall be provided |  |
| **8** | **75” Smart Interactive Board:****75” Akıllı Tahta** | **Brand Name and Part No:** |
|  | 8.1 | Horizontal Frequency: 135 KHz |  |
| 8.2 | Maximum Pıxel Frequency: 78 MHz |  |
| 8.3 | Vertical Frequency: 60 Hz |  |
| 8.4 | Scree Size: 75” |  |
| 8.5 | LED Type: DLED |  |
| 8.6 | Panel Technology: IPS |  |
| 8.7 | Panel Type: 16/7 |  |
| 8.8 | Bezel Type: Touch Bezel Type |  |
| 8.9 | Horizontal-Vertical use: Horizontal |  |
| 8.10 | Resolution: 3840 x 2160 (16:9) - UHD |  |
| 8.11 | Active Area: 1650 mm (H) x 928 mm (V) |  |
| 8.12 | Brightness: 350 cd/m2 |  |
| 8.13 | Contrast Ratio: 1200:1 |  |
| 8.14 | Panel Lifetime: 30,000 hours |  |
| 8.15 | Viewing angle: 178° |  |
| 8.16 | Color Value: 8-bit, 16.7 Million Color |  |
| 8.17 | Areas of Usage: Indoor |  |
| 8.18 | Monitor Connectivity:* RGB Input: Dsub 15 PIN VGA CON., YPbPr
* RGB Output: N/A
* Video input: HDMI2.0, DP1.2a, 1xUSB3.0, 1xUSB2.0
* Video output: DP1.2a, HDMI out
* Audio input: Line-in Jack
* Audio output: Line-out Jack
* External Control: RS232 (Dsub 9P), RJ12, Ethernet
 |  |
| 8.19 | Mechanical Features:* Size: 1731 mm (L) x 1008 mm (H) x 119 mm (D)
* Package Size: 1948 mm (L) x 1248 mm (H) x 310 mm (D)
* Product Weight: 80 kg
 |  |
| 8.20 | Working Conditions:Temperature conditions: +40°C / 0°CHumidity: %90 |  |
| 8.21 | Mechanical Features: IR Touch Screeen, Joystick, IR Extension support, Rocker Button, Removable Power Chord, Gutters for easy carrying, Removable Logo, internal USB cover, Chord Holder |  |
| 8.22 | Optional Features: OPS Compatibility |  |
| 8.23 | Power:* Power Supply: 110 VAC - 240 Vac
* Power Consumption (Deep Standby): ≤0.5W
 |  |
| 8.24 | Accessories:Standard: QSG, Guarantee Certificate, User’s Manual, Power Chord, Remote Control, Battery, Wall hanging brackets, Vesa extension support, IR Extension chord |  |
| 8.25 | Touchscreen features:* Touchscreen type: infrared (IR) Technology
* Supported number of touch: 10 touch points
* Sensitiveness: Finger, Hands in Gloves, Pen
* Connectivity support: HID, TUIO, Flash
* Type of Glass: Antiglare misty glass
* Response Time: up to 450 fps
* USB 1.1 Full Speed
 |  |
| 8.26 | After-sales service certificate of the manufacturerCE Certificate of the productISO 9001:2000 or ISO 9001:2008 Certificate of the manufacturer |  |
| 8.27 | I5 Processor, 8gb RAM and 256 gb ssd hard disk shall be integrated inside the product |  |
| 8.28 | Win 10 pro shall be installed |  |
| 8.29 | Authorized seller certificate shall be provided |  |
|  | 8.30 | All goods shall be assembled at the delivery point and the cost shall be included in unit prices offered |  |
|  | 8.31 | All goods shall be delivered within 40 days after signature of the contract by UNDP and the Contractor |  |
|  | 8.32 | An authorization letter signed by the authorized representative of the manufacturer or dealer shall be provided, if the offeror is not an authorized firm |  |
|  | 8.33 | Brochure or Catalog shall be provided |  |

Date / *Tarih:*

Signature and Stamp / *İmza ve Mühür:*

Name and Last Name /*Ad, Soyad:*

Title / *Unvan:*

Offeror’s Legal Company Name /*Teklif Sahibinin Yasal Şirket Ünvanı:*

**Annex 2**

**FORM FOR SUBMITTING SUPPLIER’S QUOTATION**

***FİNANSAL TEKLİF SUNMA FORMU***

***(This Form must be submitted only using the Supplier’s Official Letterhead/Stationery)***

***(Bu form firmanın antetli kağıdında sunulmalıdır)***

We, the undersigned, hereby accept in full the UNDP General Terms and Conditions for Contracts, and hereby offer to supply the items listed below in conformity with the specification and requirements of UNDP as per RFQ Reference No. UNDP-TUR-RFQ(MC3)-2018/31:

*Aşağıda imzası bulunan bizler, UNDP Sözleşmeler için Genel Hüküm ve Koşullar’ı kabul ettiğimizi ve Teklife Davet’te belirtilen teknik şartname ve gerekliliklerle uyumlu olarak belirtilen mallara yönelik teklifimizi sunarız.*

**TABLE 1: Offer to Supply Goods Compliant with Technical Specifications and Requirements**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Item No.** | **Description/Specification of Goods** | **Qty** | **Unit** | **Unit Price****(TRY)** | **Total Price per Item****(TRY)** |
| 1 | Two-person School Desks (for adults) | 566 | EA |  |  |
| 2 | Teacher’s Desk | 84 | EA |  |  |
| 3 | Teacher’s Chair | 84 | EA |  |  |
| 4 | Teacher’s Cabinet | 79 | EA |  |  |
| 5 | Projector | 84 | EA |  |  |
| 6 | Projector Screen | 85 | EA |  |  |
| 7 | A/C Units | 91 | EA |  |  |
| 8 | Smart Board | 2 | EA |  |  |
|  | **Total Final and All-Inclusive Price Quotation (TRY)** |  |

Date / *Tarih:*

Signature and Stamp / *İmza ve Mühür:*

Name and Last Name /*Ad, Soyad:*

Title / *Unvan:*

Offeror’s Legal Company Name /*Teklif Sahibinin Yasal Şirket Ünvanı:*