**Annex 2**

**FORM FOR SUBMITTING SUPPLIER’S QUOTATION[[1]](#footnote-1)**

***(This Form must be submitted only using the Supplier’s Official Letterhead/Stationery[[2]](#footnote-2))***

We, the undersigned, hereby accept in full the UNDP General Terms and Conditions, and hereby offer to supply the items listed below in conformity with the specification and requirements of UNDP as per RFQ Reference No. 145-2020-UNDP-UKR-RFQ-RPP:

**TABLE 1: BRIEF COMPANY PROFILE**

|  |
| --- |
| **BRIEF COMPANY PROFILE**The Supplier must describe and explain how and why they are the best entity that can deliver the requirements of UNDP by indicating the following: |
| Full registration name |  |
| Year of foundation |  |
| Legal status  | If Consortium, please provide written confirmation from each member |
| Legal address |  |
| Actual address |  |
| Bank information |  |
| VAT payer status |  |
| Contact person name |  |
| Contact person email |  |
| Contact person phone |  |
| Company’s core activities |  |
| Profile – describing the nature of business, field of expertise, licenses, certifications, accreditations (If any); | Please indicate here |
| Business Licenses – Registration Papers, Tax Payment Certification, etc  |  |
| Certificates and Accreditation  | Please indicate here applicable including Quality Certificates, Patent Registrations, Environmental Sustainability Certificates, etc.  |
| Please provide contact details of at least 3 previous partners for reference | Please attach the signed reference letters (if any). |
| Company is not in the UN Security Council 1267/1989 List, UN Procurement Division List or Other UN Ineligibility List. | Please confirm (Answers: Yes, we are in the list/No, we are not in the list) |

**TABLE 2: Conformity to the specification**

|  |  |  |  |
| --- | --- | --- | --- |
| # | **Technical requirements (not less tnan)** | **Conformity**(Yes/No) | **Offered Brand, Model and Exact characteristics** |
| 1 | **IP encoder Channel 101 DE** | The purpose of the equipment is to protect official information.IP-encoder - a miniature system platform in a metal case has 2 network interfaces: USB (RNDIS) and Ethernet 10/100. The device has a mini USB type B socket for connection to a PC (workstation or laptop) using a USB cable and an RJ-45 socket for connection to an external network using a network cable |  |  |
| 2 | **Router Mikrotik RB951-Ui 2HnD**  | VPN Tunnels - yesThe presence of USB - yesIPTV (IGMP) support - availablePoE support - availableOperating frequency - 2.4 GHzNetwork interface - 10/100 Mbit Base-TxWiFi standard - 802.11 b / g / NAntenna type - built-inConnection type -WAN-port Ethernet |  |  |
| 3 | **3G Модем Geneko GWR 352** | Data transfer speed - up to 21 Mbps in 3G networksSupport VPN + IP Sec Client and server modesSupport for 2 SIM cards with switching algorithmTimer rebootAvailability of additional RS232 and USB interfacesAdditional 2nd connector for external antenna to improve the quality of 3G signal receptionAdaptation for installation on a DIN rail |  |  |
| 4 | **External 3G \ 4G antenna**  | with gain up to 10 dB is compatible with position 3 |  |  |
| 5 | **Hermobox VAGO** | Dimensions 300x330x120 mmDoor with sealant. Hinges and lock with a rotary key bolt. The internal capacity of the box includes a mount for the S300 cassette and a special seat under the front panel |  |  |
| 6 | **Ethernet patch cord 3 pcs** | Ethernet patch cord 3 pcs |  |  |
| 7 | **Installation**  | Installation of the hardware components inside the Mobile ASC’s (truck based). Set up of all necessary equipment and organization of a confidential communication channel in the network of National Confidential Communication Systems with further connection to the Unified information and analytical system of the State Migration Service of Ukraine |  |  |

**TABLE 3: Price offer**

Financial proposal for the supply of goods in accordance with the technical specification and requirements

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item No.** | **Description/Specification of Goods** | **Quantity** | **Unit Price,*****Currency* (excl. VAT)** | **Total Price per Item, *Currency* (excl. VAT)** |
| 1 | **IP encoder Channel 101 DE** | **10** |  |  |
| 2 | **Router Mikrotik RB951-Ui 2HnD**  | **10** |  |  |
| 3 | **3G Модем Geneko GWR 352** | **10** |  |  |
| 4 | **External 3G \ 4G antenna (please indicate brand and model)** | **10** |  |  |
| 5 | **Hermobox VAGO** | **10** |  |  |
| 6 | **Ethernet patch cord 3 pcs (please indicate brand and model)** | **10** |  |  |
| 7 | **Installation and transportation** | **10** |  |  |
|  | **Total Prices of Goods excl. VAT**  |  |
|  | **VAT** |  |
|  | **Total Final and All-Inclusive Price Quotation (indicate currency) incl. VAT**  |  |

**TABLE 4: Offer to Comply with Other Conditions and Related Requirements**

|  |  |
| --- | --- |
| **Other Information pertaining to our Quotation are as follows:** | **Your Responses** |
| ***Yes, we will comply*** | ***No, we cannot comply*** | ***If you cannot comply, pls. indicate counter proposal*** |
| Delivery time (Delivery of equipment must be carried out within 60 days from PO/Contact signature date) |  |  |  |
| Compliance with technical requirements |  |  |  |
| Delivery terms:DDP, Ukraine, Donetsk region, Kramatorsk  |  |  |  |
| The supplier completes, set up and places all necessary equipment inside the 10 Mobile ASCs. The format of the internal placement will be discussed with the winner of the tender. The schedule of installation of 5 sets of equipment in Sievierodonetsk, Luhansk oblast and 5 sets in Kramatorsk, Donetsk oblast should be additionally agreed with UNDP. The schedule of installation will depend on the terms of production of the Mobile ASC vehicles. |  |  |  |
| Products meet the required quality standards. |  |  |  |
| Warranty and After-Sales Requirements: Not less than 1 year of official manufacturer warranty |  |  |  |
| Availability of warranty service in Ukraine |  |  |  |
| Acceptance of terms of payment |  |  |  |
| Validity of Quotation (min. 60 days) |  |  |  |
| All Provisions of the UNDP General Terms and Conditions. <https://www.undp.org/content/undp/en/home/procurement/business/how-we-buy.html> |  |  |  |

All other information that we have not provided automatically implies our full compliance with the requirements, terms and conditions of the RFQ.

*[Name and Signature of the Supplier’s Authorized Person]*

*[Designation]*

*[Date]*

1. *This serves as a guide to the Supplier in preparing the quotation and price schedule.*  [↑](#footnote-ref-1)
2. *Official Letterhead/Stationery must indicate contact details – addresses, email, phone and fax numbers – for verification purposes*  [↑](#footnote-ref-2)