Maize Sheller /Stationary Detail Specification with one week 145 operators training

|  |  |  |  |
| --- | --- | --- | --- |
| No | Description  | Unit of Measure | Quantity |
| 1 | * Stationary corn sheller, steel made;
* Manually powered via wood handle;
* Threshing mechanism: Enclosed metal rasp bar cylinder;
* Fitted with a feeding tray;
* Output fitted with bagging system;
* All exposed moving parts to be fully guarded ;
* Dimensions (L x W x H) : 30 x 25 x 20 cm approximately;
* Weight: 5-8 kg approximately;
* Capacity: 100 kg/h approximately
 | pcs | 25 |
| 2 | One week Operating of Maize Sheller training  | trainees | 145 |
|  |  |  |  |