## **ANNEX 3: TECHNICAL AND FINANCIAL OFFER - GOODS**

*Bidders are requested to complete this form, sign it and return it as part of their bid along with Annex 2: Quotation Submission Form. The Bidder shall fill in this form in accordance with the instructions indicated. No alterations to its format shall be permitted and no substitutions shall be accepted.*

|  |  |
| --- | --- |
| Name of Bidder: | Click or tap here to enter text. |
| RFQ reference: | **B-210705** | Date: Click or tap to enter a date. |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Item No.** | **DESCRIPTION** | **Country of Origin** | **Quantity** | **Unit Price****(VND)** | **VAT** **(if any)** | **Total Price****(VND)** |
| 1 | **Provide Brandname and full technical specifications of the quoted servers:****…..****The requested specifications of the servers are listed below for reference:****General requirements**The server is 100% new, produced from 2020 or later.Provide specific brand name and model.**Designs**Rack mounted server - 2U**Processor**2x Intel® Xeon® Gold 5220R 2.2G, 24C/48T, 10.4GT/s, 35.75M Cache, Turbo, HT (150W) DDR4-2666**Memory**4x 64GB RDIMM, 3200MT/s, Dual Rank24 DIMM Slots / Support 12x NVDIMM**RAID Controller**Integrated RAID Controller 8GB NV Cache, 12Gbps SASSupports RAID levels 0, 1, 5, 6, 10, 50, 60Supports separate RAID controller with M.2 SATA-SSD slot optimized for OS boot**Internal Hard disk**2 x 960GB SSD SAS Mixed use 12Gbps 512e 2.5in Hot-Plug**Hard Disk Tray**Up to 16 Hot Plug Hard Drives**Hard Drive Support**HDD: SAS, SATA, nearline SAS SSD: SAS, SATA.Supports the following configurations:Up to 16 x 2.5” hard drives: SAS, SATAInternal Dual SD Module supports 16/32/64 GB**Expansion slot**Supports up to 8 PCIe slots**Network card**Broadcom 57412 Dual Port 10GbE SFP+ & 5720 Dual Port 1GbE BASE-T rNDC**Power Supplies**Two hot plug, redundant (1+1), 750W. power suppliesFan with hot-swappable, redundancy**Management** Management card with built-in firmware and driver. Supports up to 16GB of vFlash media. Capable of managing up to 100 servers without additional administrative software.Support multiple methods for remote administration:+) Direct connection to the management card via USB port +) Connect by Bluetooth 4.0/Wireless protocol via tablet/smartphone+) Separate NIC card, Web-based HTML5-based interfaceStandard support: HTML5-based web interface, command line interface, Redfish, RACADM utility, WS-MAN interfaces, RESTful API, HTTPS, SSL, Smart Card authentication, LDAP, Active Directory, NFS v4, SMB3.0 with NTLMv1 and NTLMv2Built-in tool to automatically update drivers and firmware from the internet.**Security Features:**Lock down mode: Prevent unauthorized access to change firmware configurationSystem Erase: Easily erase data in local storage (HDDs, SSDs, NVMs) from the admin pageBIOS Recovery: Detect unauthorized BIOS versions, restore valid BIOS version |  | **02** | ??? | ??? | ??? |
| **Warranty time****(on-site** warranty during warranty period (including but not limited to fee for sending technical staff to user’s place at 135 Nui Truc Street, Ba Dinh, Hanoi and good shipping fee to manufacturer’s designated warranty place if any) |  | 3 year warranty | (included in unit price?? / if not, put lumpsum cost here) |
|  | 5 year warranty | (included in unit price?? / if not, put lumpsum cost here) |
| 2 | **Installation and Testing requirement (**Mounting to rack in Data Center and power on)  |  | Lumpsum | (included in unit price?? / if not, put lumpsum cost here) |
| 3 | **Packing and delivery to:** Medical Data Center, Electronic Health Administration, Ministry of Health135 Nui Truc Street, Ba Dinh, Hanoi |  | Lumpsum | (included in unit price?? / if not, put lumpsum cost here) |
| 4 | **Other cost (If any please specify)** |  | ??? | ??? | ??? |
| 5 | **Delivery Time** | **?????** |
|  | **Total for 3 years warranty** |  | **?????** |
|  | **Total for 5 years warranty** |  | **?????** |
|  |  |  |  |

**Offer to Comply with Other Conditions and Related Requirements**

|  |  |
| --- | --- |
| **Other Information pertaining to our Quotation are as follows:** | **Your Responses** |
| ***Yes, we will comply*** | ***No, we cannot comply*** | ***If you cannot comply, pls. indicate counter proposal*** |
| **Place of Delivery:** Medical Data Center, Electronic Health Administration, Ministry of Health - 135 Nui Truc Street, Ba Dinh, Hanoi | ***???*** | ***???*** |  |
| **Authorized distributer**Having valid Partner Certificate or Authorized Letter of the quoted servers | ***???*** | ***???*** |  |
| Installation of and testing ordered equipment at delivery place: Medical Data Center, Electronic Health Administration, Ministry of Health - 135 Nui Truc Street, Ba Dinh, Hanoi. | ***???*** | ***???*** |  |
| Validity of Quotation (90 days) | ***???*** | ***???*** |  |
| Acceptance of all provisions of the UNDP General Terms and Conditions | ***???*** | ***???*** |  |
| Acceptance of payment terms: 100% contract value to be paid upon receiving the official invoice, satisfactory completion of the delivery and acceptance report of the ordered items certified by authorized person. | ***???*** | ***???*** |  |

All other information that we have not provided automatically implies our full compliance with the requirements, terms and conditions of the RFQ.

*[Name and Signature of the Supplier’s Authorized Person]*

*[Designation]*

*[Date]*