{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Equipment Procurement"],"not_rendered":{"charts":0,"images":8,"macros":0,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Equipment Procurement","index":0,"n_rows":148,"n_cols":11,"rows_kept":148,"cut":false,"hidden":false,"merged":[[47,1,48,1],[84,1,86,1],[84,2,86,2],[87,2,91,2],[93,1,95,1],[93,2,95,2],[2,3,3,4],[2,2,3,2],[2,0,3,1],[0,0,0,1],[1,3,1,4],[0,3,0,4]]}
["UNDP"]
["UNDP South Africa"]
["Item",null,"Quantity","Specs"]
[]
["Hardware","Mirrorless Camera",2,"Type","Single-lens reflex digital camera","G) Photo and recording media",null,null,null,"G) Photo and recording media",2]
[null,null,null,"Resolution","24 Megapixels",{"$nulls":4},"G) Camera accessories",2]
[null,null,null,"Megapixels",24,{"$nulls":4},"G) Audio visual accessories",9]
[null,null,null,"Lens Mount","Canon EF-M"]
[null,null,null,"Sensor Size","APS-C (22.3 x 14.9 mm)"]
[null,null,null,"Image Stabilization","Lens Dependent"]
[null,null,null,"View Finder","Electronic"]
[null,null,null,"LCD Screen","3\" Fully articulated"]
[null,null,null,"Touchscreen","Yes"]
[null,null,null,"Battery","Lithium Ion battery"]
[null,null,null,"Battery Model","LP-E12"]
[null,null,null,"Connectivity","WiFi"]
[null,null,null,"Built in Flash","Yes"]
[null,null,null,"Continuous Shooting","10 fps"]
[null,null,null,"Focal Length","18-150mm"]
[null,null,null,"Video Codec(s)","MPEG-4, H.264"]
[null,null,null,"Video Resolution","UHD 3840 x 2160"]
[null,null,null,"Hot Shoe","Yes"]
[null,null,null,"Manual Focus","Yes"]
[null,null,null,"Audio Inputs","Mic Input"]
[null,null,null,"Memory Card Type","SD,SDHC,SDXC"]
[null,null,null,"Uncompressed Format","Yes"]
[null,"Lens",2,"Type","50mm f1.8","G) Camera accessories"]
[null,"Microphone",2,"Acoustic Principle","Line Gradient","G) Audio visual accessories"]
[null,null,null,"Active Electronics","JFET impedance converter"]
[null,null,null,"Capsule","0.50\""]
[null,null,null,"Polar Pattern","Supercardioid"]
[null,null,null,"Address Type","End"]
[null,null,null,"Frequency Range","40Hz - 20kHz"]
[null,null,null,"Output Impedance","200Ω"]
[null,null,null,"Maximum SPL","134dB SPL (@ 1kHz, 1% THD into 1KΩ load)"]
[null,null,null,"Sensitivity","-38.0dB re 1 Volt/Pascal (12.60mV @ 94 dB SPL) +/- 2 dB @ 1kHz"]
[null,null,null,"Equivalent Noise Level (A-weighted)","20dB-A"]
[null,null,null,"Power Options","9V Battery"]
[null,null,null,"Weight","176.00gm"]
[null,null,null,"Dimensions","65.00mmH x 102.00mmW x 250.00mmD"]
[null,null,null,"Output","Minijack Output"]
[null,null,null,"Warranty","1 year with free extension to 10 years following registration here"]
[null,null,null,"Mount","Integrated cold-shoe mount (3/8” thread)"]
[null,null,null,"Microphone type","Condenser"]
[null,null,null,"Mounting","Shock mounting"]
[null,null,null,"Shield","Windshield"]
[null,null,null,"Type","3.5mm"]
[null,"Wireless Lavalier Microphone ",2,"2.4 GHz wireless microphone",null,"G) Audio visual accessories"]
[null,null,null,"Dual-Channel Wireless Receiver"]
[null,null,null,"48 Selectable UHF Channels"]
[null,null,null,"Broadcast-Quality Sound"]
[null,null,null,"Includes Two Transmitters and One Receiver"]
[null,null,null,"Selectable Stereo and Mono Mode"]
[null,null,null,"Mic and Line-in"]
[null,null,null,"Selectable Mute function"]
[null,null,null,"Easy-to-read LCD displays"]
[null,null,null,"Automatic LCD-locked Function"]
[null,null,null,"Monitoring sound by headphone output (Receiver)"]
[null,"Tripod",2,"Load Capacity","20 lbs (9.9 kg)","G) Camera accessories"]
[null,null,null,"Maximum Height","72\" (1.82 m)"]
[null,null,null,"Minimum Height","26\" (66 cm)"]
[null,null,null,"Folded Length","28\" (71.12 cm)"]
[null,null,null,"Weight","3.83 lbs (1.74 kg)"]
[null,null,null,"Head Type","3-way panhead"]
[null,null,null,"Quick Release","Yes"]
[null,null,null,"Material","Aluminum"]
[null,null,null,"Leg Stages/Sections",3]
[null,null,null,"Leg Lock Type","Flip lock"]
[null,null,null,"Tripod Feet","Rubber feet"]
[null,null,null,"Center Brace","Yes"]
[null,null,null,"Center Column Type","Geared elevator"]
[null,null,null,"Center Column Sections",1]
[null,null,null,"Bubble Level","On base and on panhead"]
[null,"Memory Card",2,"Capacity"," 64GB SDHC","G) Photo and recording media"]
[null,"Lavalier microphone",2,"Transducer","Back electret condenser","G) Audio visual accessories"]
[null,null,null,"Polar Pattern","Omnidirectional"]
[null,null,null,"Frequency Response","20 Hz to 20 kHz"]
[null,null,null,"Sensitivity","-45 dB ±3 dB"]
[null,null,null,"Impedance","1000 Ω"]
[null,null,null,"Maximum SPL","135 dB"]
[null,null,null,"Dynamic Range","105 dB"]
[null,null,null,"Operating Voltage","1.5V - 12V DC"]
[null,null,null,"Connector","1/8\" (3.5 mm)"]
[null,null,null,"Head Diameter","0.14\" (3.5 mm)"]
[null,"Lavalier microphone extension cable",2,"Connector 1","TRRS male plug (3.5mm)","G) Audio visual accessories"]
[null,null,null,"Connector 2","TRRS female jack (3.5mm)"]
[null,null,null,"Dimensions (H x W x D)","236.22 x 0.12 x 0.12\" (6000 x 3 x 3 mm))"]
[null,"SD Card reader",2,"Interface","USB 3.1/3.0","G) Audio visual accessories"]
[null,null,null,"Card Slots/Port","SD, microSD, CompactFlash, Memory Stick"]
[null,null,null,"Color","Black, White"]
[null,null,null,"Maximum Transfer Speeds*","Read: 130MB/s Write: 95MB/s"]
[null,null,null,"Warranty","Two-year Limited Warranty"]
[null,"USB stick",2,"Capacity","128 GB","G) Audio visual accessories"]
[null,"Headphone monitors",2,"Type","Supra-aural, closed-back","G) Audio visual accessories"]
[null,null,null,"Frequency Range","60 Hz - 18 kHz"]
[null,null,null,"Impedance","24 Ohms"]
[null,null,null,"Sensitivity","100dB SPL/mW"]
[null,null,null,"Maximum Input Power","1000 mW"]
[null,null,null,"Connectors","1/8\" stereo mini-jack, with 1/8\" to 1/4\" TRS phono adapter"]
[null,null,null,"Cable Length","6.5' (2 m)"]
[null,"Portable hard disk",2,"Capacity","2 TB"]
[null,null,null,"Interface","USB 3.0"]
[null,null,null,"Data Transfer Rate","USB 3.0 - Up to 5 Gb/s, USB 2.0 - Up to 480 Mb/s"]
[null,null,null,"BUS Powered","Yes"]
[null,null,null,"OS Compatibility","Windows / Mac"]
[null,null,null,"Dimensions","4.33 x 3.15 x 0.74\" / 110 x 80 x 18.8 mm"]
[null,null,null,"Weight","0.53 lb / 0.240 kg"]
[null,"Green Screen",1,"1 x 3x2m Background Stand(4Pcs Cross Bar)",null,"G) Audio visual accessories"]
[null,null,null,"1 x 3x2m Non-woven Fabrics(Green)"]
[null,null,null,"4 x Stainless Steel Clamps(Silver)"]
[null,null,null,"1 x Carry Bag"]
[null,"Lighting Kit",1,"Kit includes",null,"G) Audio visual accessories"]
[null,null,null,"2 x 15W LED heads"]
[null,null,null,"2 x Power Adapters"]
[null,null,null,"2 x 2m Light Stands"]
[null,null,null,"2 x 50x70cm Softboxes"]
[null,null,null,"2 x Softbox diffusion sheets"]
[null,null,null,"1 x Carry Bag"]
[]
[null,null,null,"Equipment specifications"]
[null,null,null,"144 LED each head"]
[null,null,null,"Power: 15W Each"]
[null,null,null,"Color Temperature: 5500K(±100)"]
[null,null,null,"Plug Type: SA Plug"]
[null,null,null,"Voltage: 100-240V 50-60Hz"]
[null,null,null,"Soft Box:"]
[null,null,null,"Size: 50x70cm"]
[null,null,null,"Color: Black & Silver"]
[null,null,null,"Light Stand:"]
[null,null,null,"Material: Aluminium alloy"]
[null,null,null,"Folded Length: 73cm"]
[null,null,null,"Height: 80cm-200cm"]
[null,"Audio Recorder",1,null,null,"G) Photo and recording media"]
[null,null,null,"- Recording Media: SD card: 16MB to 2GB, SDHC card: 4GB to 32GB"]
[null,null,null,"- Display: Backlit LCD (128 x 64 pixels)"]
[null,null,null,"- Power Requirements: AA size (LR6) battery x 2, AC adapter (AD-17 (DC5V/1A/USB-type, optional), USB bus power- Modular Mic and Input System"]
[null,null,null,"- Includes XY Microphone Module"]
[null,null,null,"- Four Simultaneous Inputs"]
[null,null,null,"- Uses SD Memory Cards"]
[null,null,null,"- Compatible with H6 Mic Modules"]
[null,"Audio Recorder Accessory Pack",1,"-Tripod Stand"]
[null,null,null,"-Padded Shell Case"]
[null,null,null,"-MA-2 Tripod-to-Mic Stand Adapter"]
[null,null,null,"-Protective Case"]
[null,null,null,"-Foam Windscreen"]
[null,null,null,"-USB Cable"]
[null,null,null,"-2 x AA Batteries"]
[null,null,null,"-Set of Download Codes for Cubase LE and WaveLab LE"]