{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Folha1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Folha1","index":0,"n_rows":11,"n_cols":4,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
["Descrição","Quant.","Un","Total"]
["Central de incêndios com bateria","1 un"]
["Botija(s) com 103Kg de gás NOVEC 1230","1 un"]
["Detetores óticos de fumo","3 un"]
["Botoneiras","2 un"]
["Sinalização passiva (sinais)","6 un"]
["Sirene de alarme com luz e som","1 un"]
["Bicos de descarga do gás a 360º","2 un"]
["Fornecimento e execução dos respetivos trabalhos de instalação da cablagem elétrica com calhas e todos os acessórios necessários.","1 un"]
["Fornecimento e execução dos respetivos trabalhos de instalação da cablagem de ligação dos componentes do sistema (central de controlo, detetores, sirene, válvula de descarga do gás) com calhas/tubos e todos os acessórios necessários.","1 un"]
["Fornecimento e execução dos respetivos trabalhos de instalação da canalização para descarga do gás com todos os acessórios necessários.","1 un"]