{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["devis"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"devis","index":0,"n_rows":19,"n_cols":6,"rows_kept":19,"cut":false,"hidden":false,"merged":[[2,0,2,5],[4,0,4,5],[18,0,25,5]]}
[]
[]
["BORDERAU DE DETAILS DU DEVIS QUANTITATIF ET ESTIMATIF              LOT N° 06 : "]
[]
["REVETEMENT MUR                                                                                                                          CARRELAGE-FAIENCE"]
[]
[]
["Code","Désignation","U","Q","Déboursé","Total"]
[]
[]
["6.1","Carrelage - faïence"]
["6.1","Fourniture et pose Chape en mortier de ciment pour  de carrelage des sols Localisation: Bureau 01, Bureau 02, Corridor, SE01-02","m²",69,null,{"$f":"E12*D12","v":0}]
["6.2","Décapage, Fourniture et pose à la colle de Carrelage en grès cérame plein masse, Dim 45x45, localisation Localisation Bureau 01, Bureau 02,Corridor, SE01-02","m²",69,null,{"$f":"E13*D13","v":0}]
["6.3","Plinthes assortir surface intérieure","ml",43.52,null,{"$f":"E14*D14","v":0}]
["6.4","Décapage,Fourniture et pose à la colle de faience , Dim 15x30, localisation SE-01visiteur","m²",21,null,{"$f":"D15*E15","v":0}]
[]
[null,"TOTAL LOT 06",null,null,null,{"$f":"SUM(F12:F16)","v":0}]
[]
["NB : L'Entrepreneur exécutera, comme étant inclus dans son prix, tous travaux ressortissant de son lot et nécessaires au parfait achèvement des travaux. Il devra signaler clairement à part, dans la présentation de son offre, toutes les prestations des travaux qui ne figureraient pas dans le présent DQ. Aussi le montant du présent LOT sera forfaitaire et non révisable après négociation."]