**ANNEX 2: QUOTATION SUBMISSION FORM**

*Bidders are requested to complete this form, including the Company Profile and Bidder’s Declaration, sign it and return it as part of their quotation along with Annex 3: Technical and Financial Offer. The Bidder shall fill in this form in accordance with the instructions indicated. No alterations to its format shall be permitted and no substitutions shall be accepted.*

|  |  |
| --- | --- |
| Name of Bidder: | Click or tap here to enter text. |
| RFQ reference: | RFQ047/22 Supply of Water purification equipment (Reverse Osmosis Systems) to Karakalpakstan, including delivery, installation, commissioning, training | Date: Click or tap to enter a date. |

**Company Profile**

|  |  |
| --- | --- |
| **Item Description** | **Detail** |
| Legal name of bidder or Lead entity for JVs | Click or tap here to enter text. |
| Legal Address, City, Country | Click or tap here to enter text. |
| Website | Click or tap here to enter text. |
| Year of Registration | Click or tap here to enter text. |
| Legal structure | Choose an item. |
| Are you a UNGM registered vendor? | [ ]  Yes [ ]  No If yes, insert UNGM Vendor Number |
| Quality Assurance Certification (e.g. ISO 9000 or Equivalent) *(If yes, provide a Copy of the valid Certificate):* | [ ]  Yes [ ]  No  |
| Does your Company hold any accreditation such as ISO 14001 or ISO 14064 or equivalent related to the environment? *(If yes, provide a Copy of the valid Certificate):* | [ ]  Yes [ ]  No |
| Does your Company have a written Statement of its Environmental Policy? *(If yes, provide a Copy)* | [ ]  Yes [ ]  No |
| Does your organization demonstrate significant commitment to sustainability through some other means, for example internal company policy documents on women empowerment, renewable energies or membership of trade institutions promoting such issues *(If yes, provide a Copy)* | [ ]  Yes [ ]  No |
| Is your company a member of the UN Global Compact  | [ ]  Yes [ ]  No |
| Bank Information | Bank Name: Click or tap here to enter text.Bank Address: Click or tap here to enter text.IBAN: Click or tap here to enter text.SWIFT/BIC: Click or tap here to enter text.Account Currency: Click or tap here to enter text.Bank Account Number: Click or tap here to enter text. |
| **Previous relevant experience: 3 contracts** |
| **Name of previous contracts** | **Client & Reference Contact Details including e-mail** | **Contract Value** | **Period of activity**  | **Types of activities undertaken** |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

**Bidder’s Declaration**

| **Yes** | **No** |  |
| --- | --- | --- |
|[ ] [ ]  **Requirements and Terms and Conditions:** I/We have read and fully understand the RFQ, including the RFQ Information and Data, Schedule of Requirements, the General Conditions of Contract, and any Special Conditions of Contract. I/we confirm that the Bidder agrees to be bound by them. |
|[ ] [ ]  I/We confirm that the Bidder has the necessary capacity, capability, and necessary licenses to fully meet or exceed the Requirements and will be available to deliver throughout the relevant Contract period. |
|[ ] [ ]  **Ethics**: In submitting this Quote I/we warrant that the bidder: has not entered into any improper, illegal, collusive or anti-competitive arrangements with any Competitor; has not directly or indirectly approached any representative of the Buyer (other than the Point of Contact) to lobby or solicit information in relation to the RFQ ;has not attempted to influence, or provide any form of personal inducement, reward or benefit to any representative of the Buyer.  |
|[ ] [ ]  I/We confirm to undertake not to engage in proscribed practices, , or any other unethical practice, with the UN or any other party, and to conduct business in a manner that averts any financial, operational, reputational or other undue risk to the UN and wehave read the United Nations Supplier Code of Conduct :<https://www.un.org/Depts/ptd/about-us/un-supplier-code-conduct> and acknowledge that it provides the minimum standards expected of suppliers to the UN. |
|[ ] [ ]  **Conflict of interest:** I/We warrant that the bidder has no actual, potential, or perceived Conflict of Interest in submitting this Quote or entering a Contract to deliver the Requirements. Where a Conflict of Interest arises during the RFQ process the bidder will report it immediately to the Procuring Organisation’s Point of Contact. |
|[ ] [ ]  **Prohibitions, Sanctions:** l/We hereby declare that our firm, its affiliates or subsidiaries or employees, including any JV/Consortium members or subcontractors or suppliers for any part of the contract is not under procurement prohibition by the United Nations, including but not limited to prohibitions derived from the Compendium of United Nations Security Council Sanctions Lists and have not been suspended, debarred, sanctioned or otherwise identified as ineligible by any UN Organization or the World Bank Group or any other international Organization. |
|[ ] [ ]  **Bankruptcy**: l/We have not declared bankruptcy, are not involved in bankruptcy or receivership proceedings, and there is no judgment or pending legal action against them that could impair their operations in the foreseeable future. |
|[ ] [ ]  **Offer Validity Period:** I/We confirm that this Quote, including the price, remains open for acceptance for the Offer Validity.  |
|[ ] [ ]  I/We understand and recognize that you are not bound to accept any Quotation you receive, and wecertify that the goods offered in our Quotation are new and unused. |
|[ ] [ ]  By signing this declaration, the signatory below represents, warrants and agrees that he/she has been authorised by the Organization/s to make this declaration on its/their behalf. |

Signature:

Name: Click or tap here to enter text.

Title: Click or tap here to enter text.

Date: Click or tap to enter a date.

## **ANNEX 3: TECHNICAL AND FINANCIAL OFFER - GOODS**

*Bidders are requested to complete this form, sign it and return it as part of their bid along with Annex 2: Quotation Submission Form. The Bidder shall fill in this form in accordance with the instructions indicated. No alterations to its format shall be permitted and no substitutions shall be accepted.*

|  |  |
| --- | --- |
| Name of Bidder: | Click or tap here to enter text. |
| RFQ reference: | RFQ/047/22 Supply of Water purification equipment (Reverse Osmosys Systems) to Karakalpakstan, including delivery, installation, commissioning, training | Date: Click or tap to enter a date. |

|  |  |
| --- | --- |
| **No.** | **SITE NO. 1:** Specification of water purification equipment (reverse osmosis system) for the site located in the village "Kuralpa" SSG "Kuralpa", Karauzyak district, Karakalpakstan, Republic of Uzbekistan |
|  | **MINIMUM TECHNICAL REQUIREMENTS** | **UOM** | **Q-TY** | **UNIT PRICE** | **TOTAL PRICE** |
| ***Indicate currency***  |
| **1** | The compact, fully automated, and pre-tested plant includes all necessary components: a control screen, pumps, dispensers, valves, filters, reagent containers, etc.**Data sheet:*** Minimum productivity: 16 m3/hour.
* The yield of desalinated water from the total amount supplied to the plant: 70%.
* Maximum salinity of desalinated water: 1000 mg/l.
* Energy consumption for the desalination process (per 1 kg of salt removed): no more than 1 kWh/kg.
* Supply voltage: 380 V.
* Mains current frequency: 50 Hz.
* Rated power (including heating): 30 kW.
* Operating pressure in the hydraulic system at the inlet to the unit: 0.7 MPa.
* Operating pressure in the hydraulic system at the outlet of the unit: 0.7 MPa.
* System mode: automatic.
* Mode of operation: round-the-clock with breaks for chemically enhanced washing.
* Place of installation: covered room.

**Equipment:*** Installation frame made of stainless material: 1 pc.
* High pressure pump 32 m3/h, 5.5 kW: 1 pc.
* Monometer sensor: 2 pcs.
* Section for cleaning with cartridge filters up to 0.5 microns: 15 pcs.
* Charcoal cleaning section with automatic head: 400 kg.
* Silica sand cleaning section with automatic head: 1100 kg.
* Antiscalant dosing station with autosampler: 25 kg.
* Desalination unit with reverse osmosis membranes: OVAY 80/40 (or equivalent): 16 pcs.

- Vertical multistage centrifugal pump 32m3, 18kW, 1 pc.- Housing: all parts (assemblies) must be pre-designed and pre-assembled.Components/Consumables:a) antiscalant (in a canister of 25 liters): 200 liters.b) 0.5 micron cartridge filters: 200 pcs.c) reverse osmosis membranes OVAY 80/40 (or equivalent): 16 pcs.**Warranty:**At least 12 consecutive months.**Manual:**All technical documentation, including the operation manual, maintenance manual and step-by-step troubleshooting instructions can be provided in English for the evaluation committee, however, when the equipment is delivered, all technical documentation must be provided in Russian.**Certification and standards:**The proposed installation must be from a manufacturer with an ISO 9001 certificate issued for a quality management system (internationally recognized quality management system certificates, ISO equivalent certificates will also be considered). | Set | 1 |  |  |
|  | Total price of the equipment |  |  |
|  | Transportarion cost (delivery address: village "Kuralpa" SSG "Kuralpa", Karauzyak district, Karakalpakstan, Republic of Uzbekistan) |  |  |
|  | Insurance *(if applicable)* |  |  |
|  | Installation, Startup, Coaching on operation |  |  |
|  | Other fees *(specify)* |  |  |
|  | VAT *(if applicable)* |  |  |
|  | **Amount of the Offer for Site No. 1, including VAT** *(if applicable)* |  |  |
| **No.** | **SITE 2:** Specification of water purification equipment (reverse osmosis system) for the the site located in the village “Ak-Kudyk” SSG “Kokuzek” Kegeyli district, Karakalpakstan, Republic of Uzbekistan |
|  | **MINIMUM TECHNICAL REQUIREMENTS** | **UOM** | **Q-TY** | **UNIT PRICE** | **TOTAL PRICE** |
| ***Indicate currency*** |
| **2** | Compact, fully automated and pre-tested plant including all necessary components: control screen, pumps, dispensers, valves, filters, reagent containers, etc.**Data sheet:**- Minimum productivity: 8 m3/hour.- The yield of desalinated water from the total amount supplied to the plant: 70%.- Maximum salinity of desalinated water: 1000 mg/l.- Energy consumption for the desalination process (per 1 kg of salt removed): no more than 1 kWh/kg.- Supply voltage: 380 V.- Mains current frequency: 50 Hz.- Rated power (including heating): 30 kW.- Operating pressure in the hydraulic system at the inlet to the unit: 0.7 MPa.- Operating pressure in the hydraulic system at the outlet of the unit: 1.0 MPa.- System mode: automatic.- Mode of operation: round-the-clock with breaks for chemically enhanced washing.- Place of installation: covered room.**Equipment:**- Installation frame made of stainless material: 1 pc.- High pressure pump 16 m3/h, 3.0 kW: 1 pc.- Monometer sensor: 2 pcs.- Section for cleaning with cartridge filters up to 0.5 microns: 10 pcs.- Charcoal cleaning section with automatic head: 260 kg.- Silica sand cleaning section with automatic head: 900 kg.- Antiscalant dosing station with autosampler: 25 kg.- Desalination unit with reverse osmosis membranes: OVAY 80/40 (or equivalent): 8 pcs.- Vertical multistage centrifugal pump 11kW: 1 pc.- Housing: all parts (assemblies) must be pre-designed and pre-assembled.Components/Consumables:a) antiscalant (in a canister of 25 liters): 200 liters.b) 0.5 micron cartridge filters: 200 pcs.c) reverse osmosis membranes OVAY 80/40 (or equivalent): 8 pcs.**Warranty:**At least 12 consecutive months.**Manual:**All technical documentation, including the operation manual, maintenance manual and step-by-step troubleshooting instructions can be provided in English for the evaluation committee, however, when the equipment is delivered, all technical documentation must be provided in Russian.Certification and standards:The proposed installation must be from a manufacturer with an ISO 9001 certificate issued for a quality management system (internationally recognized quality management system certificates, ISO equivalent certificates will also be considered). | Set | 1 |  |  |
|  | Total price of the equipment |  |  |
|  | Transportarion cost (delivery address: village “Ak-Kudyk” SSG “Kokuzek” Kegeyli district, Karakalpakstan, Republic of Uzbekistan) |  |  |
|  | Insurance *(if applicable)* |  |  |
|  | Installation, Startup, Coaching on operation |  |  |
|  | Other fees *(specify)* |  |  |
|  | VAT *(if applicable)* |  |  |
|  | **Amount of the Offer for Site No. 2, including VAT** *(if applicable)* |  |  |
|  | **THE TOTAL AMOUNT OF THE OFFER FOR TWO SITES, INCLUDING ALL EXPENSES** |  |  |

**Compliance with Requirements**

|  |  |
| --- | --- |
|  | **You Responses** |
|  | **Yes, we will comply** | **No, we cannot comply** | **If you cannot comply, pls. indicate counter - offer** |
| Minimum Technical Specifications |[ ] [ ]  Click or tap here to enter text. |
| Delivery Term (INCOTERMS 2020): DAP or DDP-Karakalpakstan |[ ] [ ]  Click or tap here to enter text. |
| Delivery Lead Time; 90 calendar days |[ ] [ ]  Click or tap here to enter text. |
| Warranty: minimum 12 consequitive months |[ ] [ ]  Click or tap here to enter text. |
| Validity of Quotation: 60 calendar days |[ ] [ ]  Click or tap here to enter text. |
| Payment terms: 100% post-payment |[ ] [ ]  Click or tap here to enter text. |
| Other requirements *[pls. specify]* |[ ] [ ]  Click or tap here to enter text. |

**Other Information:**

|  |  |
| --- | --- |
| Estimated weight/volume/dimension of the Consignment:  |  Click or tap here to enter text. |
| Country/ies of Origin: (*if export licence required this must be submitted if awarded the contract*) | Click or tap here to enter text. |

|  |
| --- |
| I, the undersigned, certify that I am duly authorized to sign this quotation and bind the company below in event that the quotation is accepted. |
| *Exact name and address of company*Company NameClick or tap here to enter text.Address: Click or tap here to enter text. Click or tap here to enter text.Phone No.: Click or tap here to enter text.Email Address: Click or tap here to enter text. | Authorized Signature: Date: Click or tap here to enter text.Name: Click or tap here to enter text.Functional Title of Authorised Signatory: Click or tap here to enter text.Email Address: Click or tap here to enter text. |