{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Technical Requirement","Technical Compliance","Financial Offer "],"not_rendered":{"charts":0,"images":8,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Technical Requirement","index":0,"n_rows":10,"n_cols":3,"rows_kept":10,"cut":false,"hidden":false,"merged":[[0,1,1,1],[0,0,1,0],[0,2,1,2]]}
["No","Item Description (Name & Specifications)","Example photo"]
[]
[1,"A2 Photo Printer \nSpecification:\nNozzle Configuration: Black/Gray : 180 nozzles for each 4 black ink, Colour : 180 nozzles for each 6 colour ink\nPrint Direction: Bi-directional printing, uni-directional printing\nMaximum Print Resolution: 5760x1440 dpi\nMinimum Ink Droplet Size: 1.5pl\nPrint Speed: Draft Mode: 600 x 600dpi, 1.9 minutes *1\nNormal Mode: 1200 x 1200dpi, 3.0 minutes *1\nFine Mode: 2400 x 1200dpi, 5.6 minutes *1\nOverprint: Black Enhance Overcoat\nPrinting Method: On-demand ink jet (piezo electric), Variable-Sized Droplet Technology\nLUT: (LCCS Technology. The promotion depends on each ESC)\nMaximum Print Size: 17” wide\nColours: Cyan, Vivid Magenta, Photo Black, Matte Black, Gray, Light Gray, Yellow, Vivid Light Magenta, Light Cyan, Violet\nRated Voltage: AC 100-120V / 100-240V / 220-240V \nPaper Size & Thickness: Roll paper (Option roll paper unit), Width: 210mm (A4) - 431.8mm(17\"), Max roll diameter: 132mm\nCut Sheet : 89mm (3.5\") - 431.8mm (17\")"]
[2,"Mirrorless Digital Camera\nSpecification:\nBrand: SONY (preferably)\nType: Alpha A7 III Mirrorless; Megapixels: 24.2; Total Pixels: 25.3; Sensor Size: 35.6 × 23.8mm; Pixel Dimensions: 6000 x 4000; Pixel Size: 5.93µm; Diffraction-Limited; Aperture: f/9.6; Sensor Stabilization: Y; Lens Mount: Sony E-mount; FOVCF: 1.0x; Image Processor: BIONZ X\""]
[3,"Camera Len\nSpecifications:\nSigma Lens 16MM F1.4 DC DN Lens for Sony\nCondition: New\nWeight: 1000 Gram\nCategory: Camera Lens\nStorefront: SIGMA LENS\nDISTRIBUTOR WARRANTY\nSIGMA 16MM F/1.4 DC DN CONTEMPORARY FOR SONY E-MOUNT\n\nPerformance\nFocal Length 16mm Comparable 35mm Focal Length: 24 mm\nMaximum Aperture: f/1.4 Minimum: f/16\nCamera Mount Type Sony E\nAPS-C Compatibility Format\nAngle of View 83.2°\nMinimum Focus Distance 9.84\" (25cm)\nMagnification 0.1x\nMaximum Reproduction Ratio 1:9.9\nElements/Groups 16 / 13\nDiaphragm Blades 9, Rounded\nFeatures\nAutofocus Yes\nPhysical\nFront Thread Filter: 67 mm\nDimensions (DxL) Approx. 2.84 x 3.63\" (72.2 x 92.3 mm)\nWeight 14.29 oz (405 g)\n"]
[4,"Camera Blitz\nSpecification:\nMega Camera – FS – SONY HVL-F32M \nExternal Flash Camera – Black\nCamera flash\nCompatible with Sony ADI/P-TTL\nGuide Number: 105' at ISO 100 and 105mm\nZoom Range: 24-105mm (15mm with Panel)\nTilts -8 to 90°"]
[5,"Drone Camera\nSpecification:\nDJI Mavic Mini SE Fly More Combo Drone Camera\nAircraft\nTake-off Weight [1]: < 249 g\nDimensions: Folded: 138×81×58 mm (L×W×H); Unfolded: 159×203×56 mm (L×W×H); Unfolded (with propellers): 245×289×56 mm (L×W×H)\nDiagonal Distance: 213 mm\nMax Ascent Speed: 4 m/s (S Mode); 2 m/s (P Mode); 1.5 m/s (C Mode)\nMax Descent Speed: 3 m/s (S Mode); 1.8 m/s (P Mode): 1 m/s (C Mode)\nMax Speed (near sea level, no wind): 13 m/s (S Mode); 8 m/s (P Mode); 4 m/s (C Mode)\nMaximum Take-off Altitude”3000 m\nMax Flight Time: 30 minutes (measured while flying at 17 kph in windless conditions)\nMax Wind Speed Resistance: 8.5 m/s to 10.5m/s (Scale 5)\nMax Tilt Angle: 30° (S Mode); 20° (P Mode); 20° (C Mode)\nMax Angular Velocity: 150°/s (S Mode); 130°/s (P Mode); 30°/s (C Mode)\nOperating Temperature Range: 0° to 40°C (32° to 104°F)\nOperating Frequency: 5.725-5.850 GHz\nTransmission Power (EIRP): \n5.8 GHz: <30 dBm (FCC); <28 dBm (SRRC)\nGPS+GLONASS\nHovering Accuracy Range\nVertical: ±0.1 m (with Vision Positioning), ±0.5 m (with GPS Positioning)\nHorizontal: ±0.3 m (with Vision Positioning), ±1.5 m (with GPS Positioning)\nGimbal\nMechanical Range: Tilt: -110° to 35°; Roll: -35° to 35°; Pan: -20° to 20°\nControllable Range: Tilt: -90° to 0° (default setting) -90° to +20° (extended)\nStabilization: 3-axis (tilt, roll, pan)\nMax Control Speed (tilt): 120°/s\nAngular Vibration Range: ±0.01°\nCamera:\nSensor: 1/2.3” CMOS; Effective Pixels: 12 MP\nLens: FOV: 83°; 35 mm Format Equivalent: 24 mm; Aperture: f/2.8; Shooting Range: 1 m to ∞\nISO Range: Video: 100-3200 (Auto) 100-3200 (Manual); Photo: 100-3200 (Auto) 100-3200 (Manual)\nShutter Speed: Electronic Shutter: 4-1/8000s\nStill Image Size: 4:3: 4000×3000; 16:9: 4000×2250 Still Photography Modes: Single shot; Interval: 2/3/5/7/10/15/20/30/60 s\nVideo Resolution: 2.7K：2720×1530 24/25/30 p; FHD：1920×1080 24/25/30/48/50/60 p\nMax Video Bitrate: 40 Mbps\nSupported File System: FAT32（≤32 GB); exFAT（>32 GB）\nPhoto Format: JPEG\nVideo Format: MP4 (H.264/MPEG-4 AVC）"]
[6,"Shirt Screen Printing Polyflex 38x38\nSpecification: \nVoltage: 220 V\nTemperature varies: 0220C\nWorking measurement: 38 x 38 cm\npower: 900 W\nTime varies: 0999 sec\nWeight: 26 kg\nUse For: T-Shirt, Flat Media"]
[7,"Photocopy Machine \nSpecification:\n\nMain Function: Copy, Print, Scan, Fax\nWriting Method / Type: Laser exposure dry electrostatic transcription method / Desktop\nCPU: Cortex-A9 1.2GHz\nPrint Speed (A4) (Mono): 60 ppm\nScanning Speed (A4) 300dpi (Mono/Color) Simplex: 60/40 ipm; Duplex: 120/80 ipm\nMemory Standard 1GB (Max. 3GB)\nWarm Up Time: 25 seconds or less\nPaper Capacity: Standard: 500 sheets (Cassette) + 100 sheets (MPT); Maximum: 2,600 sheets (Main Unit + 500 sheets PF-3110 x4 + MPT)\nPaper Size: Cassette: Max. A4 (Legal) - Min. A6R; Option: Max. A4 (Legal) - Min. A5R; MPT: Max. A5 (Legal) Min. 70mm x 148mm & banner paper: Max 915mm\nPaper Weight: Cassette: 60 – 120 g/m2; Option: 60 – 120 g/m2; MPT\t60 – 220 g/m2\nDuplex Printing\tPaper size: A4/Legal - A5R; Paper weight: 60 - 120 g/m2\nOutput Capacity: Max. 500 sheets face-down; Max. 500 sheets face-down (Inner tray: 50 sheets, Finisher tray: 250 sheets)\nControl Panel: 7inch Color Touch LCD Panel\nDocument Processor: Standard (Max. 100 sheets DSDP Type)\nData Security: Data Security Kit(E) Free activation when using HD-6, HD-7 and HD-14\nDimension (W x D x H) (Main Unit): 480mm x 495mm x 610mm\nWeight (Main Unit): Approx. 24.5 kg (Excluding toner)\nPower Consumption (Standard configuration): Copy/Print: Mode:746W / 723W; Stand-by Mode: 54W/24W; Energy Saver: 0.5W\nNoise (ISO7779/ ISO9296): Print Mode: 58dB(A); Silent mode: 53dB(A); Stand-by Mode: 33dB(A)"]
[8,"Laptop\nSpecification:\nProcessor: AMD Ryzen™ 5 4500U Processor 2.3 GHz (8M Cache, up to 4.0 GHz)\nGraphics: AMD Radeon™ Graphics\nDisplay: 14.0-inch, FHD (1920 x 1080) 16:9 aspect ratio, IPS-level Panel, LED Backlit, 100% sRGB color gamut for non-OLED, Anti-glare display, Screen-to-body ratio: 90%\nMemory: 8GB LPDDR4X on board, Total system memory:12GB\nStorage: 512GB M.2 NVMe™ PCIe® 3.0 SSD\nI/O Ports: 1x USB 3.2 Gen 1 Type-A; 2x USB 3.2 Gen 2 Type-C; 1x HDMI 2.0b; Micro SD card reader\nCamera: 720p HD camera\nNetwork and Communication: Wi-Fi 6(802.11ax) +Bluetooth 5.0 (Dual band) 2*2\nBattery: 67WHrs, 4S1P, 4-cell Li-ion\nPower Supply\nTYPE-C, 65W AC Adapter, Output: 19V DC, 3.42A, 65W, Input: 100~240V AC 50/60Hz universal\nDimensions (W x D x H)\n31.90 x 21.00 x 1.43 ~ 1.43 cm (12.56\" x 8.27\" x 0.56\" ~ 0.56\")"]

{"sheet":"Technical Compliance","index":1,"n_rows":10,"n_cols":5,"rows_kept":10,"cut":false,"hidden":false,"merged":[]}
[]
["No","Item Description (Name & Minimum Specifications)","Example photo","Technical Comp (YES/NO) ","Proposed Product "]
[1,"A2 Photo Printer \nSpecification:\nNozzle Configuration: Black/Gray : 180 nozzles for each 4 black ink, Colour : 180 nozzles for each 6 colour ink\nPrint Direction: Bi-directional printing, uni-directional printing\nMaximum Print Resolution: 5760x1440 dpi\nMinimum Ink Droplet Size: 1.5pl\nPrint Speed: Draft Mode: 600 x 600dpi, 1.9 minutes *1\nNormal Mode: 1200 x 1200dpi, 3.0 minutes *1\nFine Mode: 2400 x 1200dpi, 5.6 minutes *1\nOverprint: Black Enhance Overcoat\nPrinting Method: On-demand ink jet (piezo electric), Variable-Sized Droplet Technology\nLUT: (LCCS Technology. The promotion depends on each ESC)\nMaximum Print Size: 17” wide\nColours: Cyan, Vivid Magenta, Photo Black, Matte Black, Gray, Light Gray, Yellow, Vivid Light Magenta, Light Cyan, Violet\nRated Voltage: AC 100-120V / 100-240V / 220-240V \nPaper Size & Thickness: Roll paper (Option roll paper unit), Width: 210mm (A4) - 431.8mm(17\"), Max roll diameter: 132mm\nCut Sheet : 89mm (3.5\") - 431.8mm (17\")"]
[2,"Mirrorless Digital Camera\nSpecification:\nBrand: SONY (preferably)\nType: Alpha A7 III Mirrorless; Megapixels: 24.2; Total Pixels: 25.3; Sensor Size: 35.6 × 23.8mm; Pixel Dimensions: 6000 x 4000; Pixel Size: 5.93µm; Diffraction-Limited; Aperture: f/9.6; Sensor Stabilization: Y; Lens Mount: Sony E-mount; FOVCF: 1.0x; Image Processor: BIONZ X\""]
[3,"Camera Lence\nSpecifications:\nSigma Lens 16MM F1.4 DC DN Lens for Sony\nCondition: New\nWeight: 1000 Gram\nCategory: Camera Lens\nStorefront: SIGMA LENS\nDISTRIBUTOR WARRANTY\nSIGMA 16MM F/1.4 DC DN CONTEMPORARY FOR SONY E-MOUNT\n\nPerformance\nFocal Length 16mm Comparable 35mm Focal Length: 24 mm\nMaximum Aperture: f/1.4 Minimum: f/16\nCamera Mount Type Sony E\nAPS-C Compatibility Format\nAngle of View 83.2°\nMinimum Focus Distance 9.84\" (25cm)\nMagnification 0.1x\nMaximum Reproduction Ratio 1:9.9\nElements/Groups 16 / 13\nDiaphragm Blades 9, Rounded\nFeatures\nAutofocus Yes\nPhysical\nFront Thread Filter: 67 mm\nDimensions (DxL) Approx. 2.84 x 3.63\" (72.2 x 92.3 mm)\nWeight 14.29 oz (405 g)\n"]
[4,"Camera Blitz\nSpecification:\nMega Camera – FS – SONY HVL-F32M \nExternal Flash Camera – Black\nCamera flash\nCompatible with Sony ADI/P-TTL\nGuide Number: 105' at ISO 100 and 105mm\nZoom Range: 24-105mm (15mm with Panel)\nTilts -8 to 90°"]
[5,"Drone Camera\nSpecification:\nDJI Mavic Mini SE Fly More Combo Drone Camera\nAircraft\nTake-off Weight [1]: < 249 g\nDimensions: Folded: 138×81×58 mm (L×W×H); Unfolded: 159×203×56 mm (L×W×H); Unfolded (with propellers): 245×289×56 mm (L×W×H)\nDiagonal Distance: 213 mm\nMax Ascent Speed: 4 m/s (S Mode); 2 m/s (P Mode); 1.5 m/s (C Mode)\nMax Descent Speed: 3 m/s (S Mode); 1.8 m/s (P Mode): 1 m/s (C Mode)\nMax Speed (near sea level, no wind): 13 m/s (S Mode); 8 m/s (P Mode); 4 m/s (C Mode)\nMaximum Take-off Altitude”3000 m\nMax Flight Time: 30 minutes (measured while flying at 17 kph in windless conditions)\nMax Wind Speed Resistance: 8.5 m/s to 10.5m/s (Scale 5)\nMax Tilt Angle: 30° (S Mode); 20° (P Mode); 20° (C Mode)\nMax Angular Velocity: 150°/s (S Mode); 130°/s (P Mode); 30°/s (C Mode)\nOperating Temperature Range: 0° to 40°C (32° to 104°F)\nOperating Frequency: 5.725-5.850 GHz\nTransmission Power (EIRP): \n5.8 GHz: <30 dBm (FCC); <28 dBm (SRRC)\nGPS+GLONASS\nHovering Accuracy Range\nVertical: ±0.1 m (with Vision Positioning), ±0.5 m (with GPS Positioning)\nHorizontal: ±0.3 m (with Vision Positioning), ±1.5 m (with GPS Positioning)\nGimbal\nMechanical Range: Tilt: -110° to 35°; Roll: -35° to 35°; Pan: -20° to 20°\nControllable Range: Tilt: -90° to 0° (default setting) -90° to +20° (extended)\nStabilization: 3-axis (tilt, roll, pan)\nMax Control Speed (tilt): 120°/s\nAngular Vibration Range: ±0.01°\nCamera:\nSensor: 1/2.3” CMOS; Effective Pixels: 12 MP\nLens: FOV: 83°; 35 mm Format Equivalent: 24 mm; Aperture: f/2.8; Shooting Range: 1 m to ∞\nISO Range: Video: 100-3200 (Auto) 100-3200 (Manual); Photo: 100-3200 (Auto) 100-3200 (Manual)\nShutter Speed: Electronic Shutter: 4-1/8000s\nStill Image Size: 4:3: 4000×3000; 16:9: 4000×2250 Still Photography Modes: Single shot; Interval: 2/3/5/7/10/15/20/30/60 s\nVideo Resolution: 2.7K：2720×1530 24/25/30 p; FHD：1920×1080 24/25/30/48/50/60 p\nMax Video Bitrate: 40 Mbps\nSupported File System: FAT32（≤32 GB); exFAT（>32 GB）\nPhoto Format: JPEG\nVideo Format: MP4 (H.264/MPEG-4 AVC）"]
[6,"Shirt Screen Printing Polyflex 38x38\nSpecification: \nVoltage: 220 V\nTemperature varies: 0220C\nWorking measurement: 38 x 38 cm\npower: 900 W\nTime varies: 0999 sec\nWeight: 26 kg\nUse For: T-Shirt, Flat Media"]
[7,"Photocopy Machine \nSpecification:\n\nMain Function: Copy, Print, Scan, Fax\nWriting Method / Type: Laser exposure dry electrostatic transcription method / Desktop\nCPU: Cortex-A9 1.2GHz\nPrint Speed (A4) (Mono): 60 ppm\nScanning Speed (A4) 300dpi (Mono/Color) Simplex: 60/40 ipm; Duplex: 120/80 ipm\nMemory Standard 1GB (Max. 3GB)\nWarm Up Time: 25 seconds or less\nPaper Capacity: Standard: 500 sheets (Cassette) + 100 sheets (MPT); Maximum: 2,600 sheets (Main Unit + 500 sheets PF-3110 x4 + MPT)\nPaper Size: Cassette: Max. A4 (Legal) - Min. A6R; Option: Max. A4 (Legal) - Min. A5R; MPT: Max. A5 (Legal) Min. 70mm x 148mm & banner paper: Max 915mm\nPaper Weight: Cassette: 60 – 120 g/m2; Option: 60 – 120 g/m2; MPT\t60 – 220 g/m2\nDuplex Printing\tPaper size: A4/Legal - A5R; Paper weight: 60 - 120 g/m2\nOutput Capacity: Max. 500 sheets face-down; Max. 500 sheets face-down (Inner tray: 50 sheets, Finisher tray: 250 sheets)\nControl Panel: 7inch Color Touch LCD Panel\nDocument Processor: Standard (Max. 100 sheets DSDP Type)\nData Security: Data Security Kit(E) Free activation when using HD-6, HD-7 and HD-14\nDimension (W x D x H) (Main Unit): 480mm x 495mm x 610mm\nWeight (Main Unit): Approx. 24.5 kg (Excluding toner)\nPower Consumption (Standard configuration): Copy/Print: Mode:746W / 723W; Stand-by Mode: 54W/24W; Energy Saver: 0.5W\nNoise (ISO7779/ ISO9296): Print Mode: 58dB(A); Silent mode: 53dB(A); Stand-by Mode: 33dB(A)"]
[8,"Laptop\nSpecification:\nProcessor: AMD Ryzen™ 5 4500U Processor 2.3 GHz (8M Cache, up to 4.0 GHz)\nGraphics: AMD Radeon™ Graphics\nDisplay: 14.0-inch, FHD (1920 x 1080) 16:9 aspect ratio, IPS-level Panel, LED Backlit, 100% sRGB color gamut for non-OLED, Anti-glare display, Screen-to-body ratio: 90%\nMemory: 8GB LPDDR4X on board, Total system memory:12GB\nStorage: 512GB M.2 NVMe™ PCIe® 3.0 SSD\nI/O Ports: 1x USB 3.2 Gen 1 Type-A; 2x USB 3.2 Gen 2 Type-C; 1x HDMI 2.0b; Micro SD card reader\nCamera: 720p HD camera\nNetwork and Communication: Wi-Fi 6(802.11ax) +Bluetooth 5.0 (Dual band) 2*2\nBattery: 67WHrs, 4S1P, 4-cell Li-ion\nPower Supply\nTYPE-C, 65W AC Adapter, Output: 19V DC, 3.42A, 65W, Input: 100~240V AC 50/60Hz universal\nDimensions (W x D x H)\n31.90 x 21.00 x 1.43 ~ 1.43 cm (12.56\" x 8.27\" x 0.56\" ~ 0.56\")"]

{"sheet":"Financial Offer ","index":2,"n_rows":10,"n_cols":5,"rows_kept":10,"cut":false,"hidden":false,"merged":[[9,0,9,3]]}
["No","Description (Name & Specifications)","Qty","Cost/Unit","Total Cost"]
[1,"A2 Photo Printer ",1]
[2,"Mirrorless Digital Camera",1]
[3,"Camera Lence",1]
[4,"Camera Blitz",1]
[5,"Drone Camera",1]
[6,"Shirt Screen Printing Polyflex 38x38",1]
[7,"Photocopy Machine ",1]
[8,"Laptop",1]
["Shipping Cost "]