{"text_format":"2","workbook":"xlsx","n_sheets":4,"sheets":["LOT 1","LOT 2","LOT 3","LOT 4"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"LOT 1","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"cut":false,"hidden":false,"merged":[[23,1,24,1],[23,2,24,2],[6,1,9,1],[6,2,9,2],[6,4,9,4],[10,1,11,1],[10,2,11,2],[10,4,11,4],[12,4,14,4],[12,1,14,1],[12,2,14,2],[16,1,17,1],[16,2,17,2],[16,4,17,4],[19,1,22,1],[19,2,22,2],[19,4,22,4],[35,4,37,4],[40,4,46,4],[38,4,39,4],[38,2,39,2],[38,1,39,1],[40,2,46,2],[40,1,46,1],[25,6,27,6],[6,5,9,5],[6,6,9,6],[10,5,11,5],[10,6,11,6],[12,5,14,5],[12,6,14,6],[16,5,17,5],[16,6,17,6],[19,5,22,5],[19,6,22,6],[23,5,24,5],[23,6,24,6],[62,1,62,5],[63,1,63,5],[64,1,64,5],[1,1,1,6],[2,1,2,6],[3,1,3,6],[38,5,39,5],[38,6,39,6],[40,5,46,5],[40,6,46,6],[28,5,29,5],[28,6,29,6],[30,5,31,5],[30,6,31,6],[35,5,37,5],[35,6,37,6],[5,2,5,3],[18,2,18,3],[34,2,34,3],[49,2,49,3],[61,1,61,5],[25,5,27,5],[23,4,24,4],[25,1,27,1],[25,2,27,2],[25,4,27,4],[28,1,31,1],[28,2,31,2],[28,4,29,4],[30,4,31,4],[35,1,37,1],[35,2,37,2]]}
[]
[null,"Annex 1: LOT 1: Mechanical/Electrical Design, Embedded Systems and VR Studio, Robotics Lab and Web Development"]
[null,"Delivery: Juba, South Sudan [Exact location: University of Juba]"]
[null,"NB: where specifications of a given item below relates to a particular brand, the word \"or equivalent\" apply."]
[null,"Item #","Machine/Equipment/Software","Specifications","Quantity","Unit Cost (USD)","Amount (USD)"]
[null,null,"Mechanical Design"]
[null,1,"Design computers","Workstation - desktop",20,null,{"$f":"E7*F7","v":0}]
[null,null,null,"3.1 GHz Intel Core i7,"]
[null,null,null,"8GB of 2666 MHz DDR4 RAM,"]
[null,null,null,"Integrated Intel UHD Graphics 630"]
[null,2,"Laptops","NVIDIA GeForce GTX 1650 with 4GB GDDR5 Graphics OR EQUIVALENT",5,null,{"$f":"E11*F11","v":0}]
[null,null,null,"9th Gen Intel Core i7-9750h (12MB Cache, up to 4. 5 GHz, 6 Cores) 16GB DDR4 2666MHz RAM"]
[null,3,"Projector","Wattage 50watts",1,null,0]
[null,null,null,"Brightness 3300ANSI Lumen Controller type ButtonControl Item weight 2.4Kilograms Light source wattage 210Watts"]
[null,null,null,"Minimum throw distance 2.02Metres"]
[null,4,"Softwares - Design softwares students’ version","SolidWorks student’s edition",25,null,0]
[null,5,"Softwares - Design softwares students’ version","Autodesk Inventor AutoCAD OR EQUIVALENT",25,null,0]
[null,null,null,"Fusion 360"]
[null,null,"Electric Design"]
[null,6,"Design computers","Workstation - desktop",9,null,0]
[null,null,null,"3.1 GHz Intel Core i7,"]
[null,null,null,"8GB of 2666 MHz DDR4 RAM,"]
[null,null,null,"Integrated Intel UHD Graphics 630"]
[null,7,"Laptop","NVIDIA GeForce GTX 1650 with 4GB GDDR5 Graphics OR EQUIVALENT",15,null,0]
[null,null,null,"9th Gen Intel Core i7-9750h (12MB Cache, up to 4. 5 GHz, 6 Cores) 16GB DDR4 2666MHz RAM"]
[null,8,"Projector","Wattage 50watts",1,null,0]
[null,null,null,"Brightness 3300ANSI Lumen Controller type ButtonControl Item weight 2.4Kilograms Light source wattage 210Watts"]
[null,null,null,"Minimum throw distance 2.02Metres"]
[null,10,"Softwares","Kicad","Open Source (free)"]
[null,null,null,"Free PCB development software"]
[null,null,null,"Github","Open Source (free)"]
[null,null,null,"Version control system for Project Management"]
[null,11,"Softwares","SolidWorks student’s edition",25,null,0]
[null,12,"Softwares","EagleAutoCAD ElectricalFusion 360 - Electrical",25,null,0]
[null,null,"Embedded Systems and VR Studio"]
[null,13,"Training kits for Advanced level Embedded systems, covering IoT and distributed systems","-8 and 32 bit Microcontroller units (AVR",12,null,0]
[null,null,null,"+ STM32)"]
[null,null,null,"- Sensor units:Air quality sensors,level sensors and proximity sensors among others."]
[null,null,null,"-     Actuator units:motors(stepper, servo,DC)",null,null,0]
[null,null,null,"-     Communication modules:Rf Modules(long and short range),BLEs,GSM modules."]
[null,14,"Training kits for Expert level Embedded systems, covering advanced level PCB production and IoT","-EFM32ZG-STK3200 Kit Starter EFM32",12,null,0]
[null,null,null,"Development Boards & Kits - Arm Starter Kit Silicon Labs Zero Gecko Kit ZG222F32"]
[null,null,null,"-8 and 32 bit Microcontroller units (AVR"]
[null,null,null,"+ STM32)"]
[null,null,null,"-  Sensor units:Air quality sensors,level sensors and proximity sensors among others."]
[null,null,null,"-  Actuator units:motors(stepper, servo,DC)"]
[null,null,null,"-  Communication modules:Rf Modules(long and short range),BLEs,GSM modules."]
[null,15,"Gaming computers","i7 processor, NVIDIA Graphics card, 1TB storage",2,null,0]
[null,16,"VR Kit","Resolution:1832*1920 per eye, Display panel: fast-switch LCD, Integrated positional audio, Processor: Qualcomm Snapdragon XR2 Platform, 256 GB storage.",2,null,0]
[null,null,"Robotics Lab"]
[null,17,"ROS","Robot Operating Software",25,null,0]
[null,18,"Myrobotlab.","Open-source robotics framework",25,null,0]
[null,19,"KiCad EDA Software Suite ","Electronic design software",25,null,0]
[null,20,"Processing","Graphical representation software",25,null,0]
[null,null,"Web Development"]
[null,21,"Mockplus","Free Online Software",25,null,0]
[null,22,"Javascript","Free download",25,null,0]
[null,23,"Bootstrap","Free software",25,null,0]
[null,24,"VSCode","Free software",25,null,0]
[null,25,"Git","Free Online Software",25,null,0]
[null,26,"MAMP","Free Online Software",25,null,0]
[null,"Cost of Equipment ",{"$nulls":4},{"$f":"SUM(G7:G61)","v":0}]
[null,"Transportat Cost to DAP (Incoterms 2010), University of Juba, South Sudan"]
[null,"Installation and Testing Cost"]
[null,"Total Cost of Equipment delivered to DAP (Incoterms 2010) University of Juba, South Sudan",{"$nulls":4},{"$f":"SUM(G62:G64)","v":0}]

{"sheet":"LOT 2","index":1,"n_rows":145,"n_cols":7,"rows_kept":145,"cut":false,"hidden":false,"merged":[[135,6,136,6],[137,1,140,1],[137,2,140,2],[137,4,140,4],[137,5,140,5],[137,6,140,6],[130,1,131,1],[130,2,131,2],[130,4,131,4],[130,5,131,5],[130,6,131,6],[5,2,5,3],[98,2,98,3],[110,2,110,3],[141,1,141,5],[142,1,142,5],[143,1,143,5],[144,1,144,5],[135,1,136,1],[135,2,136,2],[135,4,136,4],[135,5,136,5],[132,1,134,1],[132,2,134,2],[132,4,134,4],[132,5,134,5],[132,6,134,6],[123,1,126,1],[123,2,126,2],[123,4,126,4],[123,5,126,5],[123,6,126,6],[127,1,129,1],[127,2,129,2],[127,4,129,4],[127,5,129,5],[127,6,129,6],[117,1,119,1],[117,2,119,2],[117,4,119,4],[117,5,119,5],[117,6,119,6],[120,1,122,1],[120,2,122,2],[120,4,122,4],[120,5,122,5],[120,6,122,6],[111,6,113,6],[114,1,116,1],[114,2,116,2],[114,4,116,4],[114,5,116,5],[114,6,116,6],[108,1,109,1],[108,2,109,2],[108,4,109,4],[108,5,109,5],[108,6,109,6],[111,1,113,1],[111,2,113,2],[111,4,113,4],[111,5,113,5],[102,6,105,6],[106,1,107,1],[106,2,107,2],[106,4,107,4],[106,5,107,5],[106,6,107,6],[99,1,101,1],[99,3,101,3],[99,4,101,4],[99,5,101,5],[99,6,101,6],[102,1,105,1],[102,2,105,2],[102,4,105,4],[102,5,105,5],[93,1,94,1],[93,2,94,2],[93,4,94,4],[93,5,94,5],[93,6,94,6],[95,1,97,1],[95,2,97,2],[95,4,97,4],[95,5,97,5],[95,6,97,6],[88,1,89,1],[88,2,89,2],[88,4,89,4],[88,5,89,5],[88,6,89,6],[90,1,92,1],[90,2,92,2],[90,4,92,4],[90,5,92,5],[90,6,92,6],[79,1,80,1],[79,2,80,2],[79,4,80,4],[79,5,80,5],[79,6,80,6],[84,1,85,1],[84,2,85,2],[84,4,85,4],[84,5,85,5],[84,6,85,6],[75,1,76,1],[75,2,76,2],[75,4,76,4],[75,5,76,5],[75,6,76,6],[77,1,78,1],[77,2,78,2],[77,4,78,4],[77,5,78,5],[77,6,78,6],[71,1,72,1],[71,2,72,2],[71,4,72,4],[71,5,72,5],[71,6,72,6],[73,1,74,1],[73,2,74,2],[73,4,74,4],[73,5,74,5],[73,6,74,6],[67,1,68,1],[67,2,68,2],[67,4,68,4],[67,5,68,5],[67,6,68,6],[69,1,70,1],[69,2,70,2],[69,4,70,4],[69,5,70,5],[69,6,70,6],[63,1,64,1],[63,2,64,2],[63,4,64,4],[63,5,64,5],[63,6,64,6],[65,1,66,1],[65,2,66,2],[65,4,66,4],[65,5,66,5],[65,6,66,6],[53,1,54,1],[53,2,54,2],[53,4,54,4],[53,5,54,5],[53,6,54,6],[58,1,59,1],[58,2,59,2],[58,4,59,4],[58,5,59,5],[58,6,59,6],[47,1,48,1],[47,2,48,2],[47,4,48,4],[47,5,48,5],[47,6,48,6],[51,1,52,1],[51,2,52,2],[51,4,52,4],[51,5,52,5],[51,6,52,6],[41,1,43,1],[41,2,43,2],[41,4,43,4],[41,5,43,5],[41,6,43,6],[44,1,45,1],[44,2,45,2],[44,4,45,4],[44,5,45,5],[44,6,45,6],[33,1,36,1],[33,4,36,4],[33,5,36,5],[33,6,36,6],[37,1,40,1],[37,4,40,4],[37,5,40,5],[37,6,40,6],[24,1,25,1],[24,2,25,2],[24,4,25,4],[24,5,25,5],[24,6,25,6],[30,1,31,1],[30,2,31,2],[30,4,31,4],[30,5,31,5],[30,6,31,6],[20,2,21,2],[20,4,21,4],[20,5,21,5],[20,6,21,6],[22,1,23,1],[22,2,23,2],[22,4,23,4],[22,5,23,5],[22,6,23,6],[20,1,21,1],[1,1,1,6],[14,5,15,5],[14,6,15,6],[17,1,18,1],[17,2,18,2],[17,4,18,4],[17,5,18,5],[17,6,18,6],[6,5,7,5],[6,6,7,6],[8,2,10,2],[12,1,13,1],[12,3,13,3],[12,4,13,4],[12,5,13,5],[12,6,13,6],[6,1,10,1],[6,2,7,2],[6,4,7,4],[14,1,15,1],[14,2,15,2],[14,4,15,4],[2,1,2,6],[3,1,3,6]]}
[]
[null,"Annex 1: LOT 2: Creative Arts, Greentech and Foodtech"]
[null,"Delivery: Juba, South Sudan [Exact location: University of Juba]"]
[null,"NB: where specifications of a given item below relates to a particular brand, the word \"or equivalent\" apply."]
[null,"Item #","Description","Specifications","Quantity","Unit Cost (USD)","Amount (USD)"]
[null,null,"Creative Arts (Videography, Sound studio, Fine arts)"]
[null,1,"Highly portable camera.","DSLR Full frame camera body",2,null,{"$f":"E7*F7","v":0}]
[null,null,null,"Mirrorless camera"]
[null,null,"DSLR Lenses","50mm prime lens, F1.8",2,null,0]
[null,null,null,"75-150mm DSLR lens, Sigma 24-70mm F2.8",2,null,0]
[null,null,null,"150-300mm DSLR lens, UHD 4K 70-200mm F2.8",2,null,0]
[null,2,"Tripod; Full tripods with bag","67” Camera Tripod with Travel Bag",2,null,0]
[null,3,"External microphone","Shotgun microphone with an auxiliary jack compatible with both Camera and Camcorder",2,null,0]
[null,null,"Camera-mount microphone designed for use with DSLR. High resolution audio in either mono or mid-side stereo with an option of Rode VideoMic-R"]
[null,4,"Camera lighting","Three-Point Lighting Kit",2,null,0]
[null,null,null,"RGB LED Studio (3 point kit)"]
[null,5,"Camera lighting","Shields with concentrators",2,null,0]
[null,6,"Gimbal","Gimbal Stabilizer OR EQUIVALENT",2,null,0]
[null,null,null,"3_axis, capability including utility software and bluetooth capabilities for both android and ios compatibility"]
[null,7,"Video editing software","Compatible with newer formats such as HEVC, HDR, VR and also 4K video. Note free versions available",2,null,0]
[null,8,"Video editing software","After effects software",1,null,0]
[null,null,null,"2.5D animation software used for animation, visual effects and motion picture compositing"]
[null,9,"Video editing software","video enhancement software",1,null,0]
[null,null,null,"softwares for storyboards creation, animations and special effects"]
[null,10,"Video editing software","High resolution video editing software",1,null,{"$f":"E25*F25","v":0}]
[null,null,null,"softwares for VR Editing, creating motion graphic templates & video tilting"]
[null,11,"Softwares","Canva (free version available)",1,null,0]
[null,12,"Softwares","Blender (free)",1,null,0]
[null,13,"Softwares","Gimp (free)",1,null,0]
[null,14,"Video editing hardware","Photo and Video Editing Console, All in one console",2,null,0]
[null,15,"Video editing hardware","27″ Monitor",2,null,0]
[null,null,null,"16:9 HDR 4K IPS Monitor"]
[null,16,"Video editing hardware","Advanced Wireless Mouse",2,null,0]
[null,17,"Video editing hardware.","Desktop:",2,null,0]
[null,null,"SSD (or upgrade to an SSD USB 3.0 Or USB -C Ports","i7 four core Intel CPU (6-8 cores for desktops)"]
[null,null,null,"Nvidia GTX 1050 GPU, or better 16 GB of RAM"]
[null,null,null,"SSD (or upgrade to an SSD) USB 3.0 or USB-C ports"]
[null,18,"Video editing hardware","Laptop:",2,null,0]
[null,null,"SSD or upgrade to an SSD USB 3.0 Or USB -C Ports","i7 four core Intel CPU (6-8 cores for desktops)"]
[null,null,null,"Nvidia GTX 1050 GPU, or better 16 GB of RAM"]
[null,null,null,"SSD (or upgrade to an SSD) USB 3.0 or USB-C ports"]
[null,19,"Videography tool kit for vlogging","Youtube content creation.",2,null,0]
[null,null,null,"Mobile filming equipment (Phone gimbal, Phone sound kit,"]
[null,null,null,"Phone rig, Phone tripod, Small LED Light)"]
[null,20,"Dummy Battery","For replacement batteries",2,null,0]
[null,null,null,"Dummy Battery NP-FZ100 Cable  OR EQUIVALENT"]
[null,21,"Capture Cards","External Capture Card - Stream and record in 1080p60 HDR10 or 4K30 HDR10 with ultra-low latency",3,null,0]
[null,22,"High-Quality Memory Cards","High Speed 128 GB SD Card and above",5,null,0]
[null,null,null,"128 GB Memory Card with Read speed of 300 MB/s and Write speed of 260 MB/s"]
[null,23,"Studio pro console","Digital mixer with 12 input portable mixer with 4 programmable Midas Preamps, 8 line inputs integrated Wifi Module and USB stereo recorder suited for both live and studio applications.",1,null,0]
[null,24,"Editing consoles","As per function",2,null,0]
[null,25,"Studio microphone","Upgraded USB Condenser Microphone for Computer.",2,null,0]
[null,null,null,"Microphone with USB and 3.5 mm jack Output with tripod base frequency range 20 Hz - 20 kHZ"]
[null,26,"Midi pianos","Foldable Keyboard",2,null,0]
[null,null,null,"portable, with USB interface, 32 to 40 keys, Bluetooth MIDI Function, Multiple Playability"]
[null,27,"Sound-Drum Controller","Drum Controller, Powered via USB 2.0. ,Core i5, 4 GB RAM",1,null,0]
[null,28,"Sound Cards","For Production, Audiophile 2x4, 24-Bit/192 kHz USB audio/ MIDI Interface with Midas Mic Preamplifiers",2,null,0]
[null,29,"Speakers","For production, 7″ studio monitor speakers",2,null,0]
[null,39,"Studio microphone stands","Microphone stands",2,null,0]
[null,null,null,"Studio Flexible Broadcast Mic Stand"]
[null,31,"Mic stands","For performance, with the ability to adjust the height, Extendable & Removable Boom Arm, Portable and Easy to Assemble, Stable Tripod Base Universal Compatibility:",2,null,0]
[null,32,"Performance speakers","For performance, Performance speaker with 1300 W peak power, 12 inch woofer, 1 inch tweeter, XLR and 6.3 mm jack input, selectable output channel, advanced DSP with filtering",2,null,0]
[null,33,"Sound Cards","For performance, USB Audio adapter, compatible with PC,24-bit / 192 kHz,RGB Lighting system",2,null,0]
[null,34,"Production Softwares","Digital Audio Workstation",1,null,0]
[null,null,null,"Audio production software for song creation, mic recording, audio editing, effects, pattern-based sequencer with MIDI support and scripting"]
[null,35,"Production Softwares","Digital Audio Workstation",1,null,0]
[null,null,null,"Music and MIDI recording, arranging and editing that can host VST instruments and effects."]
[null,36,"Composition Softwares","Graphical Score Editor for creation of sheet music",1,null,0]
[null,null,null,"Music writing softwares with import and export capability of MIDI and Karaoke files."]
[null,37,"Composition Softwares","music composition software",1,null,0]
[null,null,null,"music writing softwares"]
[null,38,"Contemporary instruments","Guitar",2,null,0]
[null,null,null,"Acoustic guitar with bag, tuner, strap and picks"]
[null,39,"Contemporary instruments","Electric Guitars",2,null,0]
[null,null,null,"Semi-Hollow Electric Guitar"]
[null,40,"Contemporary instruments","Pianos",2,null,0]
[null,null,null,"Size: 29.9in * 9.1in * 2.4in Rated voltage: External power adapter"]
[null,41,"Contemporary instruments","Drum sets",2,null,0]
[null,null,null,"5-Piece 22 inch Full Acoustic Drum Kit",null,null,0]
[null,42,"Contemporary instruments","Saxophones",2,null,0]
[null,null,null,"Alto Sax Key E flat with mouthpiece, stand, reeds, cleaning clothes and carrying case",null,null,0]
[null,43,"Classical performance instruments","Cello with Hard and Soft Case, Stand, Bow, Rosin, Bridge and extra set of strings, size 4/4, hand carved solid spruce top with ebony fingerboard, pegs and tailpiece",1,null,0]
[null,44,"Classical performance instruments","Violins, Solid wood violin with Hard Case, shoulder rest, bow , wiping rag rosin and extra strings size 4/4",2,null,0]
[null,45,"Classical performance instruments","Trumpets, Professional Trumpet Large bore - 0.462”, Key C",2,null,0]
[null,46,"Painting stands","To hold canvas of various sizes.",5,null,0]
[null,null,null,"Portable Artist Easel Stand - Adjustable Height Painting Easel with Bag - Table Top Art Drawing Easels for Painting Canvas, Wedding Signs & Tabletop Easels for Display - Metal Tripod - 21x66 inches",null,null,0]
[null,47,"Armatures and wires","32.8 Feet Aluminum Wire, Wire Armature, Bendable Metal Craft Wire for Making Dolls Skeleton DIY Crafts(Silver, 3 mm Thickness) ",7,null,0]
[null,48,"Modeling tools","kit",5,null,0]
[null,49,"Wood carving tools","tool set with different knives.",5,null,{"$f":"E89*F89","v":0}]
[null,null,null,"whittling knife, detail wood carving knife, high quality SK2 carbon steel wood carving tool, polish leather strop, polishing compound, gloves, whetstone, roll bag, sandpaper, canvas sheaths",null,null,0]
[null,50,"Stone carving tools","stone bits",5,null,0]
[null,null,null,"approx.1/8\" shank works with any rotary tools and drills"]
[null,null,null,"Multi-purpose - Diamond grinding burrs made of high speed steel coated with diamond particles."]
[null,51,"Stone carving tools","chisel set",5,null,0]
[null,null,null,"10 kinds of Shape Size: Deep gouge, Medium gouge, Shallow gouge, Narrow straight chisel, Wide straight chisel, Rounded chisel, angled knives/chisels, Parting tool, Pinpoint tool",null,null,0]
[null,52,"Stone carving tools","Stone Carving Set",5,null,0]
[null,null,null,"tools average about 8-1/4\" long Hardened tools"]
[null,null,null,"tool shafts range from 5/16\" to 9/16\" in diameter and the blades measure from a sharp point up to 1-1/4\" wide"]
[null,null,"Greentech"]
[null,53,"Plastic Shredder","Plastic Type: PVS, PET, PE, PA Machine Type: Plastic shredder Max. Production Capacity:500Kg/hr",1,null,0]
[null,null,"Plastic Cutter Grinder Crusher Shredder Machine"]
[null,null,"Can have about 45 KW Motor"]
[null,54,"Soil nutrient analysis equipment","Repeatability error: ≤0.05% (0.0005 potassium dichromate solution)Detection Channels: 6Detection channels.",1,null,0]
[null,null,null,"Linear error: ≤2% (0.02 copper sulfate detection)"]
[null,null,null,"Electronic scale of 200 grams Glass pipette of 1ml, 2ml, 5ml, 10ml"]
[null,null,null,"Test sample speeds : average of 30 minutes for one sample including pretreatment time."]
[null,55,"Solar training kits","Green energy teaching equipment, Solar training kit, Solar power generation experiment box",1,null,0]
[null,null,null,"Communication line: RS232 / VGA to USB"]
[null,56,"Mini Injection Molding Machine","Ejector stroke: 100mm Ejector Force: 1000KN",1,null,0]
[null,null,null,"Theoretical shot volume: 100cm³ Injection rate: 50g/s",null,null,0]
[null,null,"Foodtech"]
[null,57,"Industrial scale","100Kgs floor pan",1,null,0]
[null,null,null,"Measuring Units: Measures in lb, oz and kg"]
[null,null,null,"Can weigh upto 200kgs Extended control board for oversize boxes with energy saving LCD Display"]
[null,58,"Industrial oven","Combination oven",1,null,0]
[null,null,null,"Power rating: 7,900 - 10,300 Watts Multi-Cook"]
[null,null,null,"Stackable oven sections"]
[null,59,"Spice / Grain grinder","Spice 3 cups",1,null,0]
[null,null,null,"19, 000 RPM"]
[null,null,null,"Power rating of 750 Watts"]
[null,60,"Planetary mixer","30 Qt. Planetary Floor Mixer with Guard & Standard Accessories.",1,null,0]
[null,null,null,"150, 245, 516 RPM"]
[null,null,null,"Gear driven transmission 10 qt and above capacity Power rating of 1,300 Watts"]
[null,61,"Kitchen weighing scale","Bowl, Timer, and Temperature Sensor, Digital Kitchen",1,null,0]
[null,null,null,"Weight (5kg)"]
[null,null,null,"Precise measurement: 11lb/5kg capacity with a division of 0.1oz/1g."]
[null,null,null,"Detachable bowl capacity of 2."]
[null,62,"Grass juicer","Wheatgrass Juicer.",1,null,0]
[null,null,null,"2800 RPM"]
[null,null,null,"80° scientific blade tooth Stainless steel juicing net Power: 370W"]
[null,63,"Juicer","At Least 1/3Hp Commercial Juicer - 16 Fruits / Minute",1,null,0]
[null,null,null,"Stainless steel blades Commercial Size 80oz Power rating 2200Watts"]
[null,64,"Food drier","Food Dehydrator Machine - 900-Watt",1,null,0]
[null,null,null,"360° Hot Air Circulation Large Capacity with 10 trays and Up to 13 lbs. of Food Dehydrate 10-layer Living Drawer (15.5\"\" X"]
[null,null,null,"15.34\"\")"]
[null,65,"Cold press oil machine","1800W Oil Press Machine 0-300℃",1,null,0]
[null,null,null,"Power: 1250-1800W Product size: 22 * 50 * 29 cm Product weight: 15kg Material: 304 stainless steel Oil yield: 90% Efficiency: 6-9kg / h"]
[null,66,"Packaging Machine","Vacuum Sealer",1,null,0]
[null,null,null,"Motor Power : 0.12 kW Vacuum Pump Rate : 3 cubic m/h"]
[null,null,null,"Chamber Dimensions : 330x275x50mm"]
[null,null,null,"Build: Stainless Steel"]
[null,"Cost of Equipment ",{"$nulls":4},{"$f":"SUM(G7:G141)","v":0}]
[null,"Transportat Cost to DAP (Incoterms 2010), University of Juba, South Sudan"]
[null,"Installation and Testing Cost"]
[null,"Total Cost of Equipment delivered to DAP (Incoterms 2010) University of Juba, South Sudan",{"$nulls":4},{"$f":"SUM(G142:G144)","v":0}]

{"sheet":"LOT 3","index":2,"n_rows":115,"n_cols":7,"rows_kept":115,"cut":false,"hidden":false,"merged":[[111,1,111,5],[112,1,112,5],[113,1,113,5],[90,2,90,3],[114,1,114,5],[105,1,107,1],[105,2,107,2],[105,4,107,4],[105,5,107,5],[95,1,96,1],[95,2,96,2],[95,4,96,4],[95,5,96,5],[105,6,107,6],[108,1,110,1],[108,2,110,2],[108,4,110,4],[108,5,110,5],[108,6,110,6],[100,1,101,1],[100,2,101,2],[100,4,101,4],[100,5,101,5],[100,6,101,6],[102,1,104,1],[102,2,104,2],[102,4,104,4],[102,5,104,5],[102,6,104,6],[95,6,96,6],[97,1,99,1],[97,2,99,2],[97,4,99,4],[97,5,99,5],[97,6,99,6],[91,6,92,6],[93,1,94,1],[93,2,94,2],[93,4,94,4],[93,5,94,5],[93,6,94,6],[82,6,86,6],[91,1,92,1],[91,2,92,2],[91,4,92,4],[91,5,92,5],[76,1,77,1],[76,2,77,2],[76,4,77,4],[76,5,77,5],[76,6,77,6],[78,1,81,1],[78,2,81,2],[78,4,81,4],[78,5,81,5],[78,6,81,6],[82,1,86,1],[82,2,86,2],[82,4,86,4],[82,5,86,5],[69,5,70,5],[69,6,70,6],[71,1,74,1],[71,2,74,2],[71,4,74,4],[71,5,74,5],[71,6,74,6],[65,1,66,1],[65,2,66,2],[65,4,66,4],[65,5,66,5],[65,6,66,6],[67,1,68,1],[67,2,68,2],[67,4,68,4],[67,5,68,5],[67,6,68,6],[69,1,70,1],[69,2,70,2],[69,4,70,4],[61,6,62,6],[63,1,64,1],[63,2,64,2],[63,4,64,4],[63,5,64,5],[63,6,64,6],[57,1,58,1],[57,2,58,2],[57,4,58,4],[57,5,58,5],[57,6,58,6],[61,1,62,1],[61,2,62,2],[61,4,62,4],[61,5,62,5],[49,1,51,1],[49,2,51,2],[49,4,51,4],[49,5,51,5],[49,6,51,6],[53,1,56,1],[53,2,56,2],[53,4,56,4],[53,5,56,5],[53,6,56,6],[39,1,44,1],[39,2,44,2],[39,4,44,4],[39,5,44,5],[39,6,44,6],[45,1,48,1],[45,2,48,2],[45,4,48,4],[45,5,48,5],[45,6,48,6],[32,1,34,1],[32,2,34,2],[32,4,33,4],[32,5,33,5],[32,6,33,6],[35,1,38,1],[35,2,38,2],[35,4,38,4],[35,5,38,5],[35,6,38,6],[24,1,27,1],[24,2,27,2],[24,4,27,4],[24,5,27,5],[24,6,27,6],[28,1,31,1],[28,2,31,2],[28,4,31,4],[28,5,31,5],[28,6,31,6],[19,1,21,1],[19,2,21,2],[19,4,21,4],[19,5,21,5],[19,6,21,6],[22,1,23,1],[22,2,23,2],[22,4,23,4],[22,5,23,5],[22,6,23,6],[16,1,18,1],[16,2,18,2],[16,4,18,4],[16,5,18,5],[16,6,18,6],[6,6,8,6],[9,1,11,1],[9,2,11,2],[9,4,11,4],[9,5,11,5],[9,6,11,6],[1,1,1,6],[2,1,2,6],[3,1,3,6],[5,2,5,3],[6,1,8,1],[6,2,8,2],[6,4,8,4],[6,5,8,5],[13,1,15,1],[13,2,15,2],[13,4,15,4],[13,5,15,5],[13,6,15,6]]}
[]
[null,"Annex 1: LOT 3: Electronic prototype, Energy and Rapid Prototyping space"]
[null,"Delivery: Juba, South Sudan [Exact location: University of Juba]"]
[null,"NB: where specifications of a given item below relates to a particular brand, the word \"or equivalent\" apply."]
[null,"Item #","Machine/Equipment/Software","Specifications","Quantity","Unit Cost (USD)","Amount (USD)"]
[null,null,"Electrical / Electronic Prototyping:"]
[null,1,"CNC drilling machine","Working power: 300W; Net weight: 35KG.",1,null,{"$f":"E7*F7","v":0}]
[null,null,null,"Spindle speed: 20000 revolve/min;"]
[null,null,null,"5. Support format: (.nc) Drill and PCB2.8 format;"]
[null,2,"Cutting machine","Overall dimension: width 280mm×length 400mm×height 250mm;",1,null,0]
[null,null,null,"Net Weight: 150KG."]
[null,null,null,"The biggest cutting plate thickness: 5mm;"]
[null,3,"Circuit board buffing machine","Power supply: AC380V/50Hz; power: 0.75KW; Dimension: 750mm×730mm×730mm; Weight: 50kg.",1,null,0]
[null,4,"Through-hole plating machine","Power: 1000W; Weight: 30Kg.",1,null,0]
[null,null,null,"power: AC220V/50Hz;"]
[null,null,null,"Air pump parameters: gas flow: 20L/min;"]
[null,5,"Screen printing machine","Net Weight: 10Kg.",1,null,{"$f":"E17*F17","v":0}]
[null,null,null,"dimension: length 500mm×width 400mm×height 380mm;"]
[null,null,null,"Screen printing area: 420mm×350mm; Regulation accuracy: 0.1mm;"]
[null,6,"Circuit board dryer","Heating power: 500W; Power supply: AC220V/50Hz; Weight: 30Kg.",1,null,0]
[null,null,null,"power: 550W;"]
[null,null,null,"Time setting: 0~999min adjustable;"]
[null,7,"Laser printer","Power supply: AC220V 50HZ; Power: printing 550W, standby 27W, energy conservation 7W;",1,null,0]
[null,null,null,"Overall dimension: 268mm×368mm×360mm; Net Weight: 20Kg."]
[null,8,"Exposure machine","Exposure light: 3KW advanced special exposure lamp;",1,null,0]
[null,null,null,"Effective wavelength: 420-640nm; Vacuum pump: vacuum degree 99.5%, power 200W;"]
[null,null,null,"Exposure time; 10-600s can be set; Power supply: 220V/AC 50Hz 3.2KW; Overall dimension: 1000mm×860mm×950mm;"]
[null,null,null,"Net Weight: 120Kg. 9.Film laminator"]
[null,9,"Film laminator","Display mode: liquid crystal display; Transfer printing speed: 0.5~1.2m/min adjustable;",1,null,0]
[null,null,null,"Heating mode: inner-heating silicon roller;"]
[null,null,null,"Working voltage: 220V/50Hz; Heating tube power: 1000W; Overall dimension: length"]
[null,null,null,"450mm×width 600mm×height 350mm; Net weight: 40KG."]
[null,10,"Spray imaging machine","Maximum imaging size: 320mm×200mm double-sided board;Imaging mode: hanging double-sided spray imaging;Imaging time: 5S~99M59S adjustable;Imaging",1,null,0]
[null,null,null,"temperature: room temperature~55°C adjustable;Heating tube: 800W 316# stainless steel heating tube;Spray motor: 100W complete anticorrosive isolation pump;Imaging liquid volume: 20L (standard);Working power:"]
[null,null,null,"AC220V/50Hz 1000W;Overall dimension: length 630mm×width 430mm×height 550mm;Net weight: 30KG.",null,null,0]
[null,11,"Spray etching machine","Dosage of etching liquid: 20L (standard);",1,null,0]
[null,null,null,"Working power: AC220V/50Hz 1000W; Overall dimension: length 630mm×width 430mm×height 550mm; weight: 30KG."]
[null,null,null,"Maximum etching size: 320mm×200mm double-sided board; Etching mode: hanging double-sided spraying etching;"]
[null,null,null,"Etching time: 5S~99M59S adjustable;"]
[null,12,"Spray stripping machine","Maximum stripping size: 320mm×200mm double-sided board; Process mode: hanging double-sided spraying stripping;",1,null,0]
[null,null,null,"Stripping time: 5S~99M59S adjustable; Stripping temperature: room temperature~55°C adjustable;"]
[null,null,null,"Heating tube: 800W titanium heating tube;"]
[null,null,null,"Spray motor: 100W complete anticorrosive isolation pump; Dosage of stripping liquid: 20L (standard);"]
[null,null,null,"Working power: AC220V/50Hz 1000W; Overall dimension: 630mm×430mm×560mm;"]
[null,null,null,"Net weight: 30KG."]
[null,13,"Tin-sinking machine","Input power: AC220V/50Hz; Entire machine power: 2200W;",1,null,0]
[null,null,null,"Overall volume: length 695mm×width 550mm×height 560mm;"]
[null,null,null,"Net weight: 75KG."]
[null,null,null,"Process dimension: 320mm×200mm double-sided board;"]
[null,14,"Spray frame cleaner","Input power: AC220V/50Hz; Entire machine power: 2200W;",1,null,0]
[null,null,null,"Overall volume: length 695mm×width 550mm×height 560mm;"]
[null,null,null,"Net weight: 75KG."]
[null,15,"Alignment table","Light tube: 20 W x 4 lampContrapuntal area: 600*700mmPower supply: AC220V/80W;Weight: 30KG.",1,null,0]
[null,16,"Digital Multimeter with clamp meters","Advanced:",2,null,0]
[null,null,null,"Automatic AC/DC voltage and range selection"]
[null,null,null,"True RMS capabilities"]
[null,null,null,"Ability to suppress false readings caused by ghost voltage"]
[null,17,"Digital Multimeter with clamp meters","Measures upto 600Vac/dc",3,null,0]
[null,null,null,"Manual selection between AC/DC and range"]
[null,18,"Digital Multimeter with clamp meters","True-rms AC/DC current, voltage, temperature, frequency clamp meter",5,null,0]
[null,null,"Energy"]
[null,19,"Oscilloscope","input power:AC220/50Hz Weight 2.8kg",3,null,0]
[null,null,null,"Display type: TFT LCD"]
[null,20,"Signal Generator","Power supply: DC5V±0.5V",3,null,0]
[null,null,null,"2 channel DDS Function Generator 1Hz-100MHz 200MSa/s",null,null,0]
[null,21,"Power supply (Variable)","Output voltage 0 ~ 30V Output current 0 ~ 5A Output power 150W",5,null,0]
[null,null,null,"Load regulation CV≤ 0.01% + 5mV, CC≤ 0.1% + 10mA",null,null,0]
[null,22,"Spectrum analyser","input power: AC220v/50HZ; Channel 2;",1,null,0]
[null,null,null,"Bandwidth 70 MHZ; Oscilloscope Type Bench",null,null,0]
[null,23,"Soldering station","input power: AC220v/50HZ; Soldering Tip Temperature 450c; ESD safe Yes;",6,null,0]
[null,null,null,"Wattage 700W;",null,null,0]
[null,24,"Circuit Board Holder","Solid metal base and ABS arm with spring-loaded clamp support 360 degree rotation",6,null,0]
[null,null,null,"Adjustable width and 4 clamping thickness size to accommodate various board sizes up to 200mm wide and up to 3mm thick"]
[null,null,null,"Equipped with 4 rubber feet under the base ensure stability"]
[null,null,null,"Lightweight and portable ideal"]
[null,25,"Smoke Absorber, Fume Extractor","absorb smoke from 4-5 inches away low noise high energy saving small vibration Long-lasting working time for over 57000 hours.",6,null,0]
[null,26,"Compressor","Weight- 25kg",1,null,0]
[null,null,null,"input power - 220v/50Hz motor rating 4.1 KW",null,null,0]
[null,27,"Solar training kits","Green energy teaching equipment, Solar training kit, Solar power generation experiment box",1,null,0]
[null,null,null,"620 * 425 * 180mm"]
[null,null,null,"Power supply:AC220V±10%, 50HZ Power: ≤500W"]
[null,null,null,"Temperature: -10°C~+40°C"]
[null,28,"Wind and Solar Energy Comprehensive Training.","Smart Grid (Solar/Wind/Fuel Cell) Training System",1,null,{"$f":"E83*F83","v":0}]
[null,null,null,"Dimension: About 1700 mm x 700 mm x 1500 mm"]
[null,null,null,"Power supply: Single phase AC220V, power < 500 VA"]
[null,null,null,"Weight: about 300kg Wind driven generator: Motor"]
[null,null,null,"output voltage: 24V Blower: 2.2kw, AC220V/50Hz Battery group Solar panel module: Power: 30W, size 550mm×505mm×30mm, Simulated light source: Power: 100w, 220VAC"]
[null,29,"Educational power training equipment","Educational Energy Power Training Equipment Fuel Cell Teaching Experiment Platform",1,null,0]
[null,30,"Renewable Energy Trainer Solar Power Teaching System","Renewable Energy Trainer Solar Power Teaching System Educational Lab Equipment",1,null,0]
[null,31,"Electrical Vehicle Training Center","Electrical Vehicle Training Center, Hybrid Car Trainer. Hybrid And Ev Training Equipment 1500*1200*1800mm",1,null,0]
[null,null,"Rapid Prototyping space"]
[null,32,"CO2 Laser cutter","36\" by 24\", 90W laser and engraving machine.",1,null,0]
[null,null,null,"Laser Classification: Class 3R, Power : 90 W, Power supply : AC 110v/220v, Motion : High Speed Stepper Motors"]
[null,33,"3D Printer","FDM 3D Printer, with accessories",2,null,0]
[null,null,null,"Build Volume: 330x240x300 mm, Bed leveling: Automatic, Build Plate: Heated, Print Technology: Fused Filament Fabrication (FFF), Max. Power: 500 W",null,null,0]
[null,34,"SLA Printer","with accessories",1,null,0]
[null,null,null,"Technology: Stereolithography (SLA), Laser Power: 250 mW, Laser spot size: 85 micrometers, XY Resolution: 25 micrometers",null,null,0]
[null,35,"3D Printer","Fully Enclosed 3D Printer-200*200mm",5,null,0]
[null,null,null,"Print chamber: Completely closed, build size: 200x200x200 mm, Build plate: Heated,"]
[null,null,null,"Filament runout sensor"]
[null,36,"Vacuum former","Heater: 2x 1500 Watts = 3000W total.",1,null,0]
[null,null,null,"Forming Area : 12” by 17”, Heater : 1500 Watts x 2 (3000 Watts), Voltage : AC 110/220, Plastics : Formable plastics (Styrene, Acrylic/Plexi-glass, Pet-G, PVC, ABS, Polyethylene, vinyl and more)"]
[null,37,"Curing Station","UV curing chamber with 360-degree automatic rotating curing chamber with 200 x 260mm size L",1,null,0]
[null,null,null,"Max. Cure Chamber: 80 degrees C/176 F, LED Wavelength: 405 nm"]
[null,null,null,",LED Power : 39 W, Turntable Diameter : 19.3 cm/7.6 in, Light Source : 13 multi-directional, LEDS Power : 90-240 VAC(50/60 Hz)"]
[null,38,"Vinylcutter","14in/35mm",1,null,0]
[null,null,null,"Voltage: 110/220 VAC 60 Hz, Cut Pressure: 10-500 g, Max Cutter Width: 11.22”/285 mm, Cutting Speed: 10-800 mm/s,"]
[null,null,null,"No. of pinch rollers : 3, Max Paper Feed : 14.76”/375 mm"]
[null,39,"3D Scanner","Scanning range: 536*378mm",1,null,0]
[null,null,null,"Scanning Range: 536x378 mm Accuracy: 0.1 mm, Resolution:"]
[null,null,null,"0.5 mm, Frame Rate: 10 fps, Output format : obj, stl, Data interface : USB 3.0"]
[null,"Cost of Equipment ",{"$nulls":4},{"$f":"SUM(G7:G111)","v":0}]
[null,"Transportat Cost to DAP (Incoterms 2010), University of Juba, South Sudan"]
[null,"Installation and Testing Cost"]
[null,"Total Cost of Equipment delivered to DAP (Incoterms 2010) University of Juba, South Sudan",{"$nulls":4},{"$f":"SUM(G112:G114)","v":0}]

{"sheet":"LOT 4","index":3,"n_rows":79,"n_cols":7,"rows_kept":79,"cut":false,"hidden":false,"merged":[[72,4,73,4],[72,5,73,5],[72,6,73,6],[1,1,1,6],[2,1,2,6],[3,1,3,6],[5,2,5,3],[21,2,21,3],[35,2,35,3],[36,1,37,1],[36,2,37,2],[36,4,37,4],[36,5,37,5],[36,6,37,6],[67,1,69,1],[67,2,69,2],[67,4,69,4],[67,5,69,5],[67,6,69,6],[32,6,34,6],[30,1,31,1],[30,2,31,2],[30,4,31,4],[30,5,31,5],[30,6,31,6],[26,6,27,6],[28,1,29,1],[28,2,29,2],[28,4,29,4],[28,5,29,5],[28,6,29,6],[26,5,27,5],[22,6,23,6],[24,1,25,1],[24,2,25,2],[24,4,25,4],[24,5,25,5],[24,6,25,6],[22,5,23,5],[75,1,75,5],[76,1,76,5],[77,1,77,5],[78,1,78,5],[22,1,23,1],[22,2,23,2],[22,4,23,4],[26,1,27,1],[26,2,27,2],[26,4,27,4],[32,1,34,1],[32,2,34,2],[32,4,34,4],[32,5,34,5],[72,1,73,1],[72,2,73,2]]}
[]
[null,"Annex 1: LOT 4 Wood workshop,textile/creative and Fabrication Workshop"]
[null,"Delivery: Juba, South Sudan [Exact location: University of Juba]"]
[null,"NB: where specifications of a given item below relates to a particular brand, the word \"or equivalent\" apply."]
[null,"Item #","Machine/Equipment/Software","Specifications","Quantity","Unit Cost (USD)","Amount (USD)"]
[null,null,"Wood workshop"]
[null,1,"CNC Router","Bed size: 8 *4ft, Nema 34 Motors. 2,2KW Spindle",1,null,{"$f":"E7*F7","v":0}]
[null,2,"Tape measure","different tape measure sets (5 meters, 8meters, inch gauge)",5,null,0]
[null,3,"Steel square",null,5,null,0]
[null,4,"Hammer set","Set of 5 pcs",5,null,0]
[null,5,"G clamps (Small)","Small",5,null,0]
[null,6,"G clamps (medium)","Medium",5,null,0]
[null,7,"G clamps (Large)","Large",5,null,0]
[null,8,"Miter saw 12 \"",null,2,null,0]
[null,9,"Cordless Drill",null,5,null,0]
[null,10,"Belt sander","2\" x 42\" Belt Sander 6\" Bench Grinder, Knife Sharpener with Large Work Table",3,null,0]
[null,11,"Bench Vice","8\" Bench Vice",2,null,0]
[null,12,"Files (set)","Flat, Round",2,null,0]
[null,13,"Cable reel with industrial sockets","40m cable with industrial sockets",2,null,0]
[null,14,"Tool chest","different hand tool sets",1,null,0]
[null,15,"Rubber mallets",null,3,null,0]
[null,null,"Textile/Creatives"]
[null,16,"Embroidery Machines","computerized Embroidery machine",4,null,0]
[null,null,null,"Power Source : 220 VAC, Embroidery size : 7.9” x 11”, Automatic thread cutter, advanced needle threader, Full color touch screen with on-screen editing functions"]
[null,17,"CNC Fabric Cutter","Automatic fabric cutter",1,null,0]
[null,null,null,"Working area : 1600 mm by 2500 mm, Cutting thickness : 0.1-25.0 mm, Rated Power : 11 kW, Max. Cutting speed : 1.2 m/s, Material Fixed Method : Vacuum absorption, Cutting accuracy : 0.1 mm, motion: servo motors",null,null,0]
[null,18,"Sewing Machines","Computerized Sewing+Embroidery+Quilting Machine",4,null,0]
[null,null,null,"Interface : LCD Touchscreen display, Function : Computerized sewing and embroidery, Power : 110/220 VAC, Working area: 4”x 4”",null,null,0]
[null,19,"Sewing Machines","Heavy duty overlock machine",2,null,0]
[null,null,null,"Stitches : 1300 /min, Variable control speed : Foot pedal, Power : 110/220 VAC, Differential feed : 0.7-2.0 mm ,Knife driver type : Lower drive (retractable knife blade)",null,null,0]
[null,20,"Sewing Machines","Heavy duty lockstitch industrial sewing machine",4,null,0]
[null,null,null,"Stitch formation : double needle lock stitch, Max. sewing speed : 3000 rpm, stitch length : 0-8 mm, needle bar stroke : 36 mm, Working table : 240mm (width)x100 mm(high)",null,null,0]
[null,21,"Laptops","NVIDIA GeForce GTX 1650 with 4GB GDDR5 Graphics",2,null,0]
[null,null,null,"9th Gen Intel Core i7-9750h (12MB Cache, up to 4. 5 GHz, 6 Cores) 16GB DDR4 2666MHz RAM"]
[null,null,null,"Or equivalent"]
[null,null,"Fabrication Workshop"]
[null,22,"High Precision CNC Milling machine","Spindle Speed (r.p.m): 50-15000 Table Travel (mm): 700*300 Number of Axes:3",1,null,0]
[null,null,null,"Spindle power: 2HP Series: 1100M",null,null,0]
[null,23,"CNC Plasma","Bed size: 8 *4ft, Nema 34 Motors, 45 Amp Plasma Source",1,null,0]
[null,24,"Welding Machine","Multi-Process MIG / STICK / TIG/ SPOT 100% Duty Cycle",2,null,0]
[null,25,"Generator Set","200 kVA Gen-set",1,null,0]
[null,26,"Angle grinders – powered tool","4.5\"",5,null,0]
[null,27,"Angle grinders – powered tool","9 \"",5,null,0]
[null,28,"Miter saw – powered tool","12\"",3,null,0]
[null,29,"Chop saw– powered tool","12\"",3,null,{"$f":"E45*F45","v":0}]
[null,30,"Step Pulley Drill Press","15-Inch Step Pulley Drill Press, 16 Speed, 1Ph 115V (354400)",3,null,0]
[null,31,"Power drills","power tools",5,null,0]
[null,32,"Cordless Drill","20V Max Cordless Drill / Driver Kit, Compact, 1/2-Inch (DCD771C2)",5,null,0]
[null,33,"Box Spanner set","Hand tool",5,null,0]
[null,34,"Adjustable Spanner set","hand tool",5,null,0]
[null,35,"Allen key set","Hand tool",5,null,0]
[null,36,"Screwdriver set","hand tool",5,null,0]
[null,37,"Tape measure","different tape measure sets (5 meters, 8meters, inch gauge)",5,null,0]
[null,38,"Steel square","Hand tool",5,null,0]
[null,39,"Hammer set","hand tool",5,null,0]
[null,40,"Hacksaw + Blades","hand tool",5,null,0]
[null,41,"Pipe wrench","Heavy Duty Adjustable Pipe Wrench Set, Wrench Tool Set / Toolbox, Hand tools for Plumbing, 3 Pack Set, 8, 10, 12 Inches Wrench Set with Storage Bag",5,null,0]
[null,42,"Rubber mallets","Hand tool",5,null,0]
[null,43,"Pliers set e.g long nose","hand tool",5,null,0]
[null,44,"G clamps (Small)","4 PCS 4 Inch C Clamp Set, Heavy Duty G-Clamps with 4-Inch Jaw Opening Sliding T-Bar Handle for DIY Carpentry Woodwork Building",5,null,0]
[null,45,"Files (set)","Flat, Round",5,null,0]
[null,46,"Cable reel with industrial sockets","40m cable with industrial sockets",5,null,0]
[null,47,"Tool chest","with 273 tools of various sets",2,null,0]
[null,48,"Bench Vice","8\" Bench Vice",3,null,0]
[null,49,"Die Grinding Wheel","Pneumatic",3,null,0]
[null,50,"Dial gauge","Dial Indicator with Magnetic Base and Point Precision Inspection Set, Long Arm 0-10mm Tester Gage Gauge 0.01mm",5,null,0]
[null,51,"Dremel tool with accessories","Cordless Rotary Tool Kit with Battery, Carrying Case, 2 Attachments, 28 Accessories - Ideal for Maximum Performance Cutting, Sanding, Sharpening & Grinding",3,null,0]
[null,52,"Belt sander","Bucktool Combo 2\" x 42\" Belt Sander 6\" Bench Grinder,",3,null,0]
[null,null,null,"Knife Sharpener with Large Work Table BG2600"]
[null,null,null,"Upgraded Mode"]
[null,53,"Bench grinder","8-Inch (DW758)",2,null,0]
[null,54,"Variable Speed Polisher with buffing","Variable Speed, Soft Start, 7-Inch/9-Inch (DWP849X)",3,null,0]
[null,55,"Drill Bits Sharpener","Portable Drill Bit Grinder End Mill Re-Sharpener with",2,null,0]
[null,null,null,"11 Collects Angle Adjustable High-precision MR-13B (110V, CBN wheel for HSS)"]
[null,56,"Magnets","Angular magnets",5,null,0]
[null,"Cost of Equipment ",{"$nulls":4},{"$f":"SUM(G7:G75)","v":0}]
[null,"Transportat Cost to DAP (Incoterms 2010), University of Juba, South Sudan"]
[null,"Installation and Testing Cost"]
[null,"Total Cost of Equipment delivered to DAP (Incoterms 2010) University of Juba, South Sudan",{"$nulls":4},{"$f":"SUM(G76:G78)","v":0}]