{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["2.1-Technical Compliance ","Sheet1"],"not_rendered":{"charts":0,"images":19,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"2.1-Technical Compliance ","index":0,"n_rows":255,"n_cols":6,"rows_kept":255,"cut":false,"hidden":false,"merged":[[250,1,257,1],[250,0,257,0],[250,2,257,2],[234,1,242,1],[234,0,242,0],[234,2,242,2],[243,1,249,1],[243,0,249,0],[243,2,249,2],[221,1,226,1],[221,0,226,0],[221,2,226,2],[227,1,233,1],[227,0,233,0],[227,2,233,2],[209,1,214,1],[209,0,214,0],[209,2,214,2],[215,1,220,1],[215,0,220,0],[215,2,220,2],[195,1,201,1],[195,0,201,0],[195,2,201,2],[202,1,208,1],[202,0,208,0],[202,2,208,2],[182,1,188,1],[182,0,188,0],[182,2,188,2],[189,1,194,1],[189,0,194,0],[189,2,194,2],[167,1,173,1],[167,0,173,0],[167,2,173,2],[174,1,181,1],[174,0,181,0],[174,2,181,2],[153,1,159,1],[153,0,159,0],[153,2,159,2],[160,1,166,1],[160,0,166,0],[160,2,166,2],[139,1,145,1],[139,0,145,0],[139,2,145,2],[146,2,152,2],[146,1,152,1],[146,0,152,0],[125,0,131,0],[125,1,131,1],[125,2,131,2],[132,1,138,1],[132,2,138,2],[132,0,138,0],[111,0,116,0],[111,1,116,1],[111,2,116,2],[117,0,124,0],[117,1,124,1],[117,2,124,2],[105,2,110,2],[105,1,110,1],[105,0,110,0],[92,1,96,1],[92,2,96,2],[92,0,96,0],[97,0,104,0],[97,1,104,1],[97,2,104,2],[87,0,91,0],[87,1,91,1],[87,2,91,2],[82,1,86,1],[82,0,86,0],[82,2,86,2],[77,1,81,1],[77,0,81,0],[77,2,81,2],[48,2,54,2],[55,2,57,2],[58,2,59,2],[62,2,66,2],[14,2,20,2],[21,2,27,2],[28,2,35,2],[36,2,47,2],[7,1,13,1],[14,1,20,1],[7,0,13,0],[14,0,20,0],[28,0,35,0],[28,1,35,1],[36,0,47,0],[5,4,5,5],[31,5,35,5],[38,4,39,4],[38,5,39,5],[49,5,51,5],[49,4,51,4],[75,0,76,0],[75,1,76,1],[75,3,76,3],[75,4,76,4],[75,5,76,5],[75,2,76,2],[21,0,27,0],[21,1,27,1],[62,0,74,0],[62,1,74,1],[58,0,59,0],[58,1,59,1],[36,1,47,1],[48,0,54,0],[48,1,54,1],[55,0,57,0],[55,1,57,1],[7,2,13,2]]}
[null,"Technical Compliance Sheet"]
[]
[null,"Project Title: ","Supply of Tailor's workshop's Operational requirements at Women Training Center (WTC) in Hun in Al-Jufra Municipality, Dirj Municipality and Alreyayna Municipality"]
[]
[]
[{"$nulls":4},"Supplier"]
["No.","DESCRIPTION","PICTURE","UNDP REQUIREMENTS SPECIFICATIONS","Technical Compliance (Yes/No)","Supplier offered Specificities "]
[1,"Training : \nThe supplier must train at least 4 trainees on how to use all the electrical appliances supplied and mentioned in this document, in addition to the supplier's obligation to provide fabric samples and all that is needed for training. and according to the approval of the UNDP's engineer. ",null,"4 trainees "]
[]
[]
[]
[]
[]
[]
[2,"Electrical Works : \nThe supplier shall provide and install the electrical connections and electrical sockets for each piece of supplied piece of equipment, according to the location of each piece of equipment in the building. Including wires and wire trunks (100 meters to 150 meters long) and according to the approval of the UNDP's engineer. ",null,"heat resistant"]
[]
[]
[]
[]
[]
[]
[3,"Double-sided board: \nSupply Double-sided board 0.9*1.2, whiteboard with base and according to the approval of the UNDP's engineer. ",null,"Whiteboard "]
[null,null,null,"Double-sided"]
[null,null,null,"Dry Erase"]
[null,null,null,"Board With Stand And Lockable Sliding"]
[null,null,null,"Size:90x120cm"]
[]
[]
[4,"blackboard calligrapher : \nSupply blackboard calligrapher. Black, red and blue colors and according to the approval of the UNDP's engineer. ",null,"Black, red and blue colors"]
{"$rows_empty":7}
[5,"First aid kit:\nSupply First aid kit (Including first aid supplies). size 40 cm * 40 cm  and according to the approval of  the UNDP's engineer. ",null,"size 38 cm * 32 cm"]
[null,null,null,"Contents:"]
[null,null,null,"plasters in a variety of different sizes and shapes"]
[null,null,null,"small, medium and large sterile gauze dressings"]
[null,null,null,"at least 2 sterile eye dressings"]
[null,null,null,"tweezers"]
[null,null,null,"alcohol-free cleansing wipes"]
[null,null,null,"sticky tape"]
[null,null,null,"antiseptic cream"]
[null,null,null,"distilled water for cleaning wounds"]
[null,null,null,"gloves"]
[null,null,null,"Cotton balls and cotton swabs"]
[6,"DRY CHEMICAL FIRE EXTINGUISHER:\nSupply fire cylinders medium size  and according to the approval of  the UNDP's engineer. ",null,"medium size - 6 kg"]
[null,null,null,"DRY CHEMICAL"]
[]
[]
[]
[]
[]
[7,"American satin fabric: \nSupply American satin fabric. Different colors, according to the approval of  the UNDP's engineer. ",null,"Different colors"]
[]
[]
[8,"Tulle Fabrics: \nSupply Tulle Fabrics. different colors, according to the approval of  the UNDP's engineer. ",null,"width : min 180 cm"]
[null,null,null,"Different colors"]
[9,"Joubert Fabrics: \nSupply Joubert Fabrics. different colors, according to the approval of  the UNDP's engineer. ",null,"Different colors"]
[10,"school uniform fabric: \nSupply school uniform fabric. Black or dark blue and, according to the approval of  the UNDP's engineer. ",null,"Different colors"]
[11,"Cloth rolling table : \nSupply cloth rolling table,2.8 m* 2 m, according to the approval of  the UNDP's engineer. ",null,"size 2.8 m * 2 m"]
{"$rows_empty":12}
[12,"Ironing board: : \nSupply Ironing board:,1.2 m* 0.4 m, according to the approval of  the UNDP's engineer. ",null,"size 1.2 m * 0.4 m"]
[]
[13,"Thermal scissors: \nSupply hot electric scissors, electric heating cloth cutter, cloth cutting tools according to the approval of  the UNDP's engineer. ",null,"Frequency:50HZ/60HZ"]
[null,null,null,"Power: Electric & Rated Voltage:110-240V"]
[null,null,null,"Function: Multi-function Cutter"]
[null,null,null,"Warranty:1 years"]
[null,null,null,"Adjustable Temperature:50-500℃"]
[14,"Iron scissors: \nSupply iron scissors, Stainless Steel, according to the approval of  the UNDP's engineer. ",null,"Stainless Steel"]
[]
[]
[]
[]
[15,"Hand Finished Scissors: \nSupply Hand Finished Scissors, Stainless Steel, according to the approval of  the UNDP's engineer. ",null,"Blade material: Stainless Steel"]
[null,null,null,"Blade thickness:3.0 mm"]
[]
[]
[]
[16,"Design Rulers: \nSupply rulers, Used for measuring & cutting fabric strips, triangles, squares & rectangles, efferent size and according to the approval of  the UNDP's engineer. ",null,"Ruler No. 1: a ruler with a side flap"]
[null,null,null,"Ruler No. 2: Armpit Reg"]
[null,null,null,"Ruler No. 3: A regular meter ruler with all sizes printed on it"]
[null,null,null,"Ruler No. 4: a jacket ruler"]
[null,null,null,"Ruler No. 5: Trousers                                            Ruler No. 6: Regular waist skirt                               Ruler No. 7: Slim waist skirt"]
[17,"Clothes measuring meter: \nSupply clothes measuring meter,1 m  and according to the approval of  the UNDP's engineer. ",null,"length : 1m"]
[null,null,null,"Thickness:‎1 Inches"]
[]
[]
[]
[]
[]
[]
[18,"Chalk: \nSupply Chalk to mark stitching lines on the fabric. And according to the approval of  the UNDP's engineer. ",null,"none"]
[]
[]
[]
[]
[]
[19,"Multi-shelves wardrobe: \nSupply Multi-shelves wardrobe, The number of shelves is not less than 20, and the dimensions of each shelf are 0.3 m * 0.3m .  according to the approval of  the UNDP's engineer. ",null,"The number of shelves is not less than 20"]
[null,null,null," the dimensions of each shelf are 0.3 m * 0.3m"]
[null,null,null,"wooden or iron"]
[]
[]
[]
[20,"Mannequin: \nSupply Mannequin display holder for clothes, dresses, and dresses to display in a standing position .  according to the approval of  the UNDP's engineer. ",null,"none"]
{"$rows_empty":7}
[21,"Zipper : \nSupply different size Zipper for Sewing,  according to the approval of  the UNDP's engineer. ",null," different size"]
[]
[]
[]
[]
[]
[]
[22,"Magnetic lights: \nSupply Magnetic electric lamp to be installed on sewing machines  . according to the approval of  the UNDP's engineer. ",null,"none"]
[]
[]
[]
[]
[]
[]
[23,"Overlock machine : \nSupply overlock machine , 3-5 strings, Max Stitch Width 4mm, Highest Speed 7000 S.P.M Operation Modes Full Automatic, Semi-Automatic, Power: 110-220V 50-60HZ 250W  and according to the approval of  the UNDP's engineer. ",null," 3-5 strings"]
[null,null,null,"Max Stitch Width 4mm"]
[null,null,null,"Highest Speed 7000 S.P.M"]
[null,null,null,"Operation Modes Full Automatic, Semi-Automatic"]
[null,null,null,"Power: 110-220V 50-60HZ 250W"]
[]
[]
[24,"Zigzag sewing and embroidery machine : \nSupply Zigzag sewing and embroidery machine, in 25 different stitches, easy stitch selection, Control stitch distance, Installing buttons, Installing a zipper, sewing light . according to the approval of  the UNDP's engineer. ",null,"Power: 110-220V 50-60HZ 250W"]
[null,null,null,"min 25 different stitches"]
[null,null,null," easy stitch selection"]
[null,null,null," Control stitch distance"]
[null,null,null,"Installing buttons"]
[null,null,null," Installing a zipper"]
[]
[25,"Trainees chairs : \nSupply trainees chairs, , black color, wrapped in sponge, complete with all fitting Furniture shall be ready to be used. according to the approval of  the UNDP's engineer. ",null,"fixed without wheels"]
[null,null,null,"black color"]
[null,null,null,"wrapped in sponge"]
[]
[]
[]
[]
[26,"Cotton sewing machine : \nSupply cotton sewing machine, Single Needle Sewing Machine, Operation Mode: Automatic, Max Stitch Length: 5mm, Max Sewing Speed: 4000-5000 (stitch/min),Power: 110-220V 50-60HZ 250W, and according to the approval of  the UNDP's engineer.  ((Half of the machines have an  external muffler motor and the rest are internal motors))",null,"Single Needle Sewing Machine"]
[null,null,null,"Operation Mode: Automatic"]
[null,null,null,"Max Stitch Length: 5mm"]
[null,null,null,"Max Sewing Speed: 4000-5000 (stitch/min)"]
[null,null,null,"Power: 110-220V 50-60HZ 250W"]
[null,null,null,"5  machines have an  external muffler motor "]
[null,null,null,"5 machines have an internal motors"]
[27," Sewing Pins : \nSupply  Sewing Pins, 34mm x 0.52mm,(Suitable for light, medium and heavy fabrics)Iron and according to the approval of  the UNDP's engineer. ",null,"34mm x 0.52mm"]
[null,null,null,"Suitable for light, medium and heavy fabrics"]
[null,null,null,"Iron"]
[]
[]
[]
[]
[28,"Buttons : \nSupply buttons, different colors & size, and according to the approval of  the UNDP's engineer. ",null,"different colors & size"]
{"$rows_empty":7}
[29,"Hand sewing needles : \nSupply  hand sewing needles, (Suitable for light, medium and heavy fabrics),Iron and according to the approval of  the UNDP's engineer. ",null,"Suitable for light, medium and heavy fabrics"]
[null,null,null,"Iron"]
[]
[]
[]
[]
[]
[30,"plastic thread regular machine: \nSupply plastic thread regular machine, Transparent and according to the approval of  the UNDP's engineer. ",null,"Transparent"]
[]
[]
[]
[]
[]
[31,"Sewing machine wire: \nSupply  sewing machine wire, different colors and and according to the approval of  the UNDP's engineer. ",null,"different colors"]
[]
[]
[]
[]
[]
[]
[32,"Sewing machine needles: \nSupply sewing machine needles (Suitable for light, medium and heavy fabrics), different size and according to the approval of  the UNDP's engineer. ",null,"Suitable for light, medium and heavy fabrics"]
[null,null,null,"different size"]
[]
[]
[]
[]
[]
[33,"Carton's Design : \nSupply Carton's Design 70 mm*100 mm and according to the approval of  the UNDP's engineer. ",null,"70 mm*100 mm"]
[]
[]
[]
[]
[]
[34,"Overlock machine wire: \nSupply overlock machine wire, different colors and according to the approval of  the UNDP's engineer. ",null,"different colors"]
[]
[]
[]
[]
[]
[35,"Steam iron: \nSupply Steam iron, 3.5 L With Steam Iron And Teflon Shoe, 220 v, and according to the approval of  the UNDP's engineer. ",null,"3.5 L"]
[null,null,null,"Steam Iron And Teflon Shoe"]
[null,null,null,"220 v"]
[]
[]
[]
[36,"Vaseline Double Face: \nSupply Vaseline Double Face, Big size , For more details see the picture  and according to the approval of  the UNDP's engineer. ",null,"Double Face"]
[null,null,null,"Big size"]
[]
[]
[]
[]
[]
[37,"Panama sewing machine (manual machine) : \nSupply panama sewing machine With all accessories including the table, and according to the approval of  the UNDP's engineer. ((Independent electric motors must be supplied with these machines for future installation))",null,"It must be the type that can be fitted with a motor"]
[null,null,null,"all accessories including the table"]
{"$rows_empty":7}
[38,"Fluca: \nSupply fluca, For more details see the picture and according to the approval of  the UNDP's engineer. ",null,"none"]
[]
[]
[]
[]
[]
[]
[39,"Straight Blade Cloth Cutting Machine: \nSupply Straight Blade Cloth Cutting Machine, different fabric Type, Automatic Grade, Motor Frequency: Heavy gauge copper winding, 750w, 220v , 8 In\", and according to the approval of  the UNDP's engineer. ",null,"Suitable for light, medium and heavy fabrics"]
[null,null,null,"Automatic Grade"]
[null,null,null,"Motor Frequency: Heavy gauge copper winding"]
[null,null,null,"750w, 220v "]
[null,null,null,"Type :8 In\""]

{"sheet":"Sheet1","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}