{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":21,"n_cols":6,"rows_kept":21,"cut":false,"hidden":false,"merged":[[17,1,17,4],[18,1,18,4],[19,1,19,4],[20,1,20,4],[16,1,16,4],[14,0,15,0],[14,2,15,2],[14,3,15,3],[14,4,15,4],[14,5,15,5],[13,0,13,5],[11,0,12,0],[11,2,12,2],[11,3,12,3],[11,4,12,4],[11,5,12,5],[10,0,10,5],[8,0,9,0],[8,2,9,2],[8,3,9,3],[8,4,9,4],[8,5,9,5],[7,0,7,5],[0,1,0,5],[1,1,1,5],[5,0,6,0],[5,2,6,2],[5,3,6,3],[5,4,6,4],[5,5,6,5]]}
[null,"ITB-042/15. Supply and Delivery of Electrical  Equipment for the Electricity Distribution Networks in Tikrit, Iraq."]
[null,"Bid Offer to Supply Goods Compliant with the Technical Specification                                                                            "]
[]
["No.","Item Description                            ","Unit","Qty","Price $","Total $"]
["ت","التفاصيل","الوحدة","الكمية","السعر","المبلغ"]
[1,"Supply New Distribution Transformer 11/0.4 KV with power 250 KVA, compatible with transformer technical specification IEC-60076, attached in Annex (A).","Unit",50]
[null,"تجهيز محولة توزيع Electrical Transformer جهد 11/ 0.4 KV وسعة 250 KVA وبموجب  المواصفة الفنية المعتمدة  IEC-60076  وبموجب المواصفات الفنية والتعليمات الواردة بالملحق المرفق  ( A )"]
[]
[2,"Supply New Electrical Galvanized Circular Steel Pole St44 or St52 , length 11m & thick 5.5mm, compatible with technical specifications, attached in Annex (B)","No.",500]
[null,"تجهيز أعمدة حديدية  مدورة مغلونة  St52 or St44 طول 11m وسمك 5,5mm بموجب المواصفات الفنية المعتمدة وبموجب الملحق المرفق (B)"]
[]
[3,"Supply New Electrical Galvanized Circular Steel Pole St44 or St52 , length 9m & thick 5mm, compatible with technical specifications, attached in Annex (B)","No.",250]
[null,"تجهيز أعمدة حديدية  مدورة مغلونة  St52 or St44 طول 9m وسمك 5mm بموجب المواصفات الفنية المعتمدة وبموجب الملحق المرفق B"]
[]
[4,"Supply Aluminum electric Wire type ACC  with sectional thick 95 mm, compatible with technical specifications, attached in Annex  (C )","KM",100]
[null,"تجهيز سلك ألمنيوم ACC مساحة مقطع  95mm2 بموجب المواصفات الفنية المعتمدة وبموجب الملحق المرفق C "]
[null,"Total Price of Goods US$"]
[null,"Add: Cost of Transportation"]
[null,"Add: Cost of Insurance"]
[null,"Add: other Charges (pls. Specify)"]
[null,"Total Final and All-Inclusif Price Bid US$"]