{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["BoQ _ITB 083 16"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"BoQ _ITB 083 16","index":0,"n_rows":37,"n_cols":6,"rows_kept":37,"cut":false,"hidden":false,"merged":[[24,0,24,5],[31,1,31,5],[0,0,0,5],[25,0,25,5],[26,0,26,5],[27,0,27,5],[28,0,28,5],[29,0,29,5],[21,1,21,4],[22,2,23,2],[22,3,23,3],[22,4,23,4],[22,5,23,5],[30,0,30,5],[22,0,23,1]]}
["Bills of Quantity (BoQ)\nRef: ITB 083/16\nRehabilitation of Rabiha Substation 33/11KV -  Ninawha Governorate\n"]
["#","Item/Description ","Unit ","Quantity ","Unit Price $","Total Price $"]
[1,"33 kV complete  switchgear :Bus bar rating  1250A , 25KA/3 sec (ABB/Siemens/Schneider or equivalent)"]
["1-1","Supply, Installation, testing, and commissioning of Incomer  with CB with P.T (100 VA) Capacity withdrawal ","No",2]
["1-2","Supply, Installation, testing, and commissioning of transformer Feeder 1250A,36kV,25kA/3sec ","No",2]
[2,"11kV complete switch gear :   Bus bar rating  1250A , 25KA/3 sec (ABB/Siemens/Schneider or equivalent)"]
["2-1","Supply, Installation, testing, and commissioning of Transformer feeder 1250A with P.T (100VA) Capacity withdraw able. ","No",2]
["2-2","Supply, Installation, testing, and commissioning of Bus coupler & Riser. 1250A","Set ",1]
["2-3","Supply, Installation, testing, and commissioning of Outgoing Feeder. 630A","No",8]
[3,"Supply, Installation, testing, and commissioning of Neutral  ground Resistance with all accessories (isolating  switch , P.T ,     C.T , lighting arrestor)      ","No",2]
[4,"Supply, Installation, testing, and commissioning of A.C Distribution  panel  0.4 kV","No",1]
[5,"Supply, Installation, testing, and commissioning of D.C Distribution  panel ( 110 V)","No",1]
[6,"Supply, Installation, testing, and commissioning of Battery charger 110VD.C , Ir=80A minimum (ABB/Siemens/Schneider or equivalent)","No",2]
[7,"Supply, Installation, testing, and commissioning of Battery  110V D.C  180 AH ,ALCAD/LC type SWEDEN origin","Set ",1]
[8,"Complete power cables :33kV as per International standard"]
["8-1","Supply, Installation,  testing,  of 33kv 1*400mm2 cable to connect  transformers inside existing cable trench's   ","Ml",500]
["8-2","Supply, Installation, and testing End  terminators (joints) for cable1* 400mm2 cable 33kv","No",24]
[9,"Supply Operating software(original) and cable for protection relay ","Set ",2]
[10,"Supply and connect ,test & operate split unit 2 ton (Carrier, LG or Media type or Equivalent) for Equipment Hall, heating and cooling identical to the Gulf specifications , work efficiency at 52 Cº , the works including supply and install steel base for the outdoor piece  with all accessories","No",4]
[11,"Supply and connect ,test & operate split unit 1 ton (Carrier, LG, or Media type or Equivalent) for operating room, heating and cooling identical to the Gulf specifications , work efficiency at 52 Cº , the works including supply and install steel base for the outdoor piece  with all accessories","No",1]
[12,"Supply materials, tools and manpower to cast reinforced concrete mix. 1:2:4 and 12mm steel bars for basements of two electrical panels thick 20cm and thick 15cm for trenches as mentioned in attached drawing.","M3",12]
[null,"Total Cost In US Dollars "]
["GENERAL IMPORTANT NOTICES:"]
[]
["1-contractor must remove existing old electrical panel boards 11Kv installing new panels "]
["2-Technical Specifications for all items compliant with attached annex A (MOE General Technical Specification)"]
["3-Equipment And Materials brands from  (Siemens-ABB –Schneider or equivalent )   "]
["4-All Supplied electrical materials should be pass MOE testing requirements"]
["5-All Supplied electrical materials should be brand new not used and compliant with Iraqi environmental condition                                                                                                                 "]
["6- Supply one copy of Drawings for all equipment’s paper and DVD (Including for all items instruments)                                                                             "]
["7- Total price shall include Transportation and insurance "]
[]
[null,"Supervisor Engineer:________________________"]
[]
[]
[]
[null,"Approved by: _________________________"]